<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="2.2225" y1="20.6375" x2="20.6375" y2="20.6375" width="0" layer="20"/>
<wire x1="20.6375" y1="20.6375" x2="20.6375" y2="2.2225" width="0" layer="20"/>
<wire x1="20.6375" y1="2.2225" x2="2.2225" y2="2.2225" width="0" layer="20"/>
<wire x1="2.2225" y1="2.2225" x2="2.2225" y2="20.6375" width="0" layer="20"/>
<text>+5V</text>
<text>GND</text>
<text>OUT</text>
</plain>
<libraries>
<library name="Cherry MX">
<packages>
<package name="MX_PCB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$2" library="Cherry MX" package="MX_PCB" value=""/>
</elements>
<signals>
<signal name="VCC">
</signal>
<signal name="GND">
</signal>
<signal name="SENS">
</signal>
<signal name="S$4">
<contactref element="E$2" pad="P$1"/>
</signal>
<signal name="S$10">
<contactref element="E$2" pad="P$2"/>
</signal>
<signal name="S$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
