(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 12)
    (no_connects 3)
    (area 36.754999 36.754999 82.625001 50.875001)
    (thickness 1.6)
    (drawings 5)
    (tracks 26)
    (zones 0)
    (modules 13)
    (nets 9)
  )
  (page User 132.004 101.6)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D1-Pad3)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "Net-(D1-Pad5)")
  (net 6 "Net-(D1-Pad6)")
  (net 7 GND)
  (net 8 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D1-Pad5)")
    (add_net "Net-(D1-Pad6)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_4UCON_19963_02x3.5mm_Straight (layer F.Cu) (tedit 597A2D7E)
    (at 40.64 43.18)
    (descr "2-way 3.5mm pitch terminal block, https://cdn-shop.adafruit.com/datasheets/19963.pdf")
    (tags "screw terminal block")
    (fp_text reference "GND 5V" (at 1.27 3.175) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.75 5.1) (layer F.Fab))
    (fp_text user %R (at 1.75 0.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Connectors_Terminal_Blocks.3dshapes/TerminalBlock_4UCON_19963_02x3.5mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_DIP_x3_W8.61mm_Slide_LowProfile (layer F.Cu) (tedit 597A2C28)
    (at 73.66 43.18)
    (descr "3x-dip-switch, Slide, row spacing 8.61 mm (338 mils), SMD, LowProfile")
    (tags "DIP Switch Slide 8.61mm 338mil SMD LowProfile")
    (attr smd)
    (fp_text reference SW1 (at 0 5.715) (layer F.SilkS))
    (fp_text value SW_DIP_x03 (at 0 5.71) (layer F.Fab))
    (pad 1 smd rect (at -4.305 -2.54) (size 2.44 1.12) (layers F.Cu F.Mask)
      (net 6 "Net-(D1-Pad6)"))
    (pad 4 smd rect (at 4.305 2.54) (size 2.44 1.12) (layers F.Cu F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at -4.305 0) (size 2.44 1.12) (layers F.Cu F.Mask)
      (net 5 "Net-(D1-Pad5)"))
    (pad 5 smd rect (at 4.305 0) (size 2.44 1.12) (layers F.Cu F.Mask)
      (net 8 +5V))
    (pad 3 smd rect (at -4.305 2.54) (size 2.44 1.12) (layers F.Cu F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 6 smd rect (at 4.305 -2.54) (size 2.44 1.12) (layers F.Cu F.Mask)
      (net 8 +5V))
    (model Buttons_Switches.3dshapes/SW_DIP_x3_W8.61mm_Slide_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_RGB_5050-6 (layer F.Cu) (tedit 597A29F2)
    (at 62.23 43.18)
    (descr http://cdn.sparkfun.com/datasheets/Components/LED/5060BRG4.pdf)
    (tags "RGB LED 5050-6")
    (attr smd)
    (fp_text reference "RGB LED" (at 0 -3.5) (layer F.SilkS))
    (fp_text value LED_RGB (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.7 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -2.4 1.7 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at 2.4 1.7 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 5 smd rect (at 2.4 0 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad5)"))
    (pad 6 smd rect (at 2.4 -1.7 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad6)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_5050-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 53.34 39.37 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 53.34 43.18 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 53.34 46.99 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 73.66 44.45)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 58.42 43.815)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbols:WEEE-Logo_4.2x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 48.26 43.815)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 597A29BA)
    (at 39.37 48.895)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 597A29C4)
    (at 80.645 48.895)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 597A29CB)
    (at 80.645 38.735)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 597A29CE)
    (at 39.37 38.735)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_text /dev/lol/TomK32 (at 63.5 48.26) (layer F.SilkS))
  (gr_line (start 82.55 36.83) (end 82.55 50.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 36.83 36.83) (end 82.55 36.83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 36.83 50.8) (end 36.83 36.83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.55 50.8) (end 36.83 50.8) (angle 90) (layer Edge.Cuts) (width 0.15))
)
