(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A2")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "V_out")
  (net 2 "Earth")
  (net 3 "V_in")
  (net 4 "Net-(C13-Pad2)")
  (net 5 "Net-(C14-Pad2)")
  (net 6 "Net-(C15-Pad2)")
  (net 7 "Net-(C16-Pad2)")
  (net 8 "Net-(C17-Pad2)")
  (net 9 "Net-(C18-Pad2)")
  (net 10 "Net-(C19-Pad2)")
  (net 11 "Net-(C20-Pad2)")
  (net 12 "Net-(C21-Pad2)")
  (net 13 "Net-(C24-Pad2)")
  (net 14 "Net-(C25-Pad2)")
  (net 15 "Net-(C26-Pad2)")
  (net 16 "Net-(C27-Pad2)")
  (net 17 "Net-(C28-Pad2)")
  (net 18 "Net-(C29-Pad2)")
  (net 19 "Net-(C30-Pad2)")
  (net 20 "Net-(C31-Pad2)")
  (net 21 "Net-(C32-Pad2)")
  (net 22 "Net-(C35-Pad2)")
  (net 23 "Net-(C36-Pad2)")
  (net 24 "Net-(C37-Pad2)")
  (net 25 "Net-(C38-Pad2)")
  (net 26 "Net-(C39-Pad2)")
  (net 27 "Net-(C40-Pad2)")
  (net 28 "Net-(C41-Pad2)")
  (net 29 "Net-(C42-Pad2)")
  (net 30 "Net-(C43-Pad2)")
  (net 31 "Net-(C2-Pad2)")
  (net 32 "Net-(C3-Pad2)")
  (net 33 "Net-(C4-Pad2)")
  (net 34 "Net-(C5-Pad2)")
  (net 35 "Net-(C6-Pad2)")
  (net 36 "Net-(C7-Pad2)")
  (net 37 "Net-(C8-Pad2)")
  (net 38 "Net-(C10-Pad1)")
  (net 39 "Net-(C10-Pad2)")
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C29" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C44" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper29" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 52.07 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J2" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.85 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 38 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 39 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C43" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C37" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper19" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C30" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 255.185 33.02)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.34 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 37 "Net-(C8-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 38 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper31" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.53 40.64)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H5" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper27" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper28" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.828885 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper6" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.0675 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 39 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 68.503888 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J3" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 32.935 33.02)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.648885 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.439164 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 33 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 34 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper40" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper17" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper16" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 73.127224)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H7" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper20" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C41" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper24" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 47.598888 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C38" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.74 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper10" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper32" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper25" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.601108 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper5" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.1025 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 34 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 35 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.6125 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 35 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 36 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C31" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.284439 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper8" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(C8-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper34" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper38" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper18" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper21" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper26" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper11" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 56.693336)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H6" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.348885 32.358888 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C33" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper14" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.188885 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.69 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper1" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper37" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.373331 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper4" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 84.937776 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J4" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 75.917777 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper2" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.701388 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper12" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C36" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper36" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 64.846112 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D3" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.512216 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper9" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper33" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 74.853888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C32" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C34" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.83 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 36 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 37 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper15" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 53.492224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper13" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.145554 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper3" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper23" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper35" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C39" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C35" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C42" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-logo:wham-logo-kicad" (layer "F.Cu")
    (at 34.29 72.39 90)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.3325 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 89.561112)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H8" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper30" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 81.28 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D4" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.070276 42.366664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 33 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 91.287776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C40" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 254 90.756155 180)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0 180) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 33.02 90.255)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 86.36)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper39" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 69.926112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper22" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.056662 37.438888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper7" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 58.42)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 244.968885 36.016664 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 261.62 96.52) (end 261.62 26.67)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 81.28) (end 43.18 81.28)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 49.53) (end 43.18 49.53)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 46.99) (end 139.7 46.99)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 46.99) (end 139.7 49.53)
    (layer "Edge.Cuts"))
  (gr_line (start 261.62 26.67) (end 25.4 26.67)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 64.77) (end 43.18 62.23)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 78.74) (end 139.7 81.28)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 78.74) (end 139.7 78.74)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 81.28) (end 43.18 78.74)
    (layer "Edge.Cuts"))
  (gr_line (start 25.4 96.52) (end 261.62 96.52)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 62.23) (end 139.7 62.23)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 64.77) (end 43.18 64.77)
    (layer "Edge.Cuts"))
  (gr_line (start 25.4 26.67) (end 25.4 96.52)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 62.23) (end 139.7 64.77)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 49.53) (end 43.18 46.99)
    (layer "Edge.Cuts"))
  (gr_text "Bias Ring \nVoltage Divider\nT. Qian 5 Dec 2023" (at 38.1 59.69 90) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 44.45) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 58.42) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 74.93) (layer "F.SilkS"))
)
