(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 677)
    (tracks 336)
    (zones 0)
    (modules 39)
    (nets 50)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (edge_width 0.05)
    (segment_width 0.1524)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.000051)
    (pad_to_paste_clearance -0.000051)
    (aux_axis_origin 0 0)
    (grid_origin 190.5 101.6)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 HT)
  (net 3 +5V)
  (net 4 "Net-(D1-Pad2)")
  (net 5 RTCI2C_CLK)
  (net 6 RTCI2C_DAT)
  (net 7 VPP)
  (net 8 ICSPDAT)
  (net 9 ICSPCLK)
  (net 10 "Net-(J3-Pad2)")
  (net 11 "Net-(J3-Pad4)")
  (net 12 "Net-(J3-Pad3)")
  (net 13 cathode0)
  (net 14 cathode9)
  (net 15 cathode8)
  (net 16 cathodeP)
  (net 17 cathode7)
  (net 18 cathode6)
  (net 19 cathode5)
  (net 20 cathode4)
  (net 21 cathode3)
  (net 22 cathode2)
  (net 23 cathode1)
  (net 24 HV_drive)
  (net 25 "Net-(Q2-Pad1)")
  (net 26 "Net-(Q3-Pad1)")
  (net 27 "Net-(Q4-Pad1)")
  (net 28 "Net-(Q5-Pad1)")
  (net 29 "Net-(Q6-Pad1)")
  (net 30 "Net-(Q7-Pad1)")
  (net 31 "Net-(Q8-Pad1)")
  (net 32 "Net-(Q9-Pad1)")
  (net 33 "Net-(Q10-Pad1)")
  (net 34 "Net-(Q11-Pad1)")
  (net 35 "Net-(Q12-Pad1)")
  (net 36 Voltage_meas)
  (net 37 nixie2)
  (net 38 nixie3)
  (net 39 nixie4)
  (net 40 nixie5)
  (net 41 nixie6)
  (net 42 nixie7)
  (net 43 nixie8)
  (net 44 nixie9)
  (net 45 nixieP)
  (net 46 BUTTON_1)
  (net 47 BUTTON_2)
  (net 48 "Net-(Q10-Pad2)")
  (net 49 "Net-(Q12-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +5V)
    (add_net BUTTON_1)
    (add_net BUTTON_2)
    (add_net GND)
    (add_net HT)
    (add_net HV_drive)
    (add_net ICSPCLK)
    (add_net ICSPDAT)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q10-Pad2)")
    (add_net "Net-(Q11-Pad1)")
    (add_net "Net-(Q12-Pad1)")
    (add_net "Net-(Q12-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(Q9-Pad1)")
    (add_net RTCI2C_CLK)
    (add_net RTCI2C_DAT)
    (add_net VPP)
    (add_net Voltage_meas)
    (add_net cathode0)
    (add_net cathode1)
    (add_net cathode2)
    (add_net cathode3)
    (add_net cathode4)
    (add_net cathode5)
    (add_net cathode6)
    (add_net cathode7)
    (add_net cathode8)
    (add_net cathode9)
    (add_net cathodeP)
    (add_net nixie2)
    (add_net nixie3)
    (add_net nixie4)
    (add_net nixie5)
    (add_net nixie6)
    (add_net nixie7)
    (add_net nixie8)
    (add_net nixie9)
    (add_net nixieP)
  )
  (module solo-nixie:L_3216Metric (layer B.Cu) (tedit 619B72B2)
    (at 196.723 106.426)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L1 (at 4.777 0) (layer B.SilkS))
    (fp_text value 10uH (at 0 -2.794) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2 0) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -2 0) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:PinHeader_1x05_P1.27mm_Vertical (layer B.Cu) (tedit 619BB32E)
    (at 193.04 88.9 90)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (fp_text reference J2 (at 0.3 1.5 90) (layer B.SilkS) hide)
    (fp_text value ICSP (at 0 -6.775 90) (layer B.Fab))
    (fp_text user clk (at -1.5 -5.1 90) (layer B.SilkS))
    (fp_text user dat (at -1.6 -3.8 90) (layer B.SilkS))
    (fp_text user gnd (at -1.7 -2.5 90) (layer B.SilkS))
    (fp_text user vcc (at -1.6 -1.143 90) (layer B.SilkS))
    (fp_text user vpp (at -1.6 0.127 90) (layer B.SilkS))
    (fp_text user %R (at 0 -2.54 180) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 ICSPCLK))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 ICSPDAT))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 VPP))
  )
  (module solo-nixie:CPH3 (layer B.Cu) (tedit 619B6D48)
    (at 196.215 98.425)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 5.385 0.075) (layer B.SilkS))
    (fp_text value CPH3459 (at 0 -3) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd roundrect (at 2.25 0) (size 1 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at -1.25 -1.5) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.25 1.5) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 HV_drive))
    (pad 3 smd roundrect (at 1.3 0) (size 2.5 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at -1.3 -0.95) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.3 0.95) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 HV_drive))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:Pin_Header_RTC_5x2.54mm_SMD (layer B.Cu) (tedit 619BB05D)
    (at 190.5 93.472 90)
    (descr "surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference RTC (at 0 6.604 90) (layer B.SilkS))
    (fp_text value RTC (at -5 -6 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd roundrect (at 0 -2.54 90) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0 2.54 90) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 RTCI2C_DAT))
    (pad 5 smd roundrect (at 0 -5.08 90) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0 0 90) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 RTCI2C_CLK))
    (pad 1 smd rect (at 0 5.08 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SW_SPST_EVQP7A (layer B.Cu) (tedit 619B6C27)
    (at 183.1 111.4 143)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (attr smd)
    (fp_text reference SW2 (at -0.195343 2.240772 143) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -3.25 143) (layer B.Fab))
    (fp_text user %R (at 0 2.5 143) (layer B.Fab))
    (pad 1 smd roundrect (at 1.8 0.72 143) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 BUTTON_2))
    (pad 1 smd roundrect (at -1.8 0.72 143) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 BUTTON_2))
    (pad 2 smd roundrect (at 1.8 -0.72 143) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.8 -0.72 143) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP7A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SW_SPST_EVQP7A (layer B.Cu) (tedit 619B6C27)
    (at 197.9 111.4 217)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (attr smd)
    (fp_text reference SW1 (at 0.060182 2.297943 37) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -3.25 37) (layer B.Fab))
    (fp_text user %R (at 0 2.5 37) (layer B.Fab))
    (pad 1 smd roundrect (at 1.8 0.72 217) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 BUTTON_1))
    (pad 1 smd roundrect (at -1.8 0.72 217) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 BUTTON_1))
    (pad 2 smd roundrect (at 1.8 -0.72 217) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.8 -0.72 217) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP7A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:LD8007 (layer F.Cu) (tedit 619E0713)
    (at 190.5 101.6)
    (fp_text reference N1 (at 0 6) (layer F.SilkS) hide)
    (fp_text value Nixie_0-9P (at 0 -6.6) (layer F.Fab) hide)
    (pad 12 smd trapezoid (at -0.092948 4.12439) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 2 HT))
    (pad 1 smd trapezoid (at 1.95609 3.575352 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 23 cathode1))
    (pad 2 smd trapezoid (at 3.525704 2.056698 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 22 cathode2))
    (pad 3 smd trapezoid (at 4.056089 -0.061954 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 21 cathode3))
    (pad 4 smd trapezoid (at 3.507051 -2.110992 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 20 cathode4))
    (pad 5 smd trapezoid (at 2.025 -3.544005 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 19 cathode5))
    (pad 6 smd trapezoid (at -0.093653 -4.07439 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 18 cathode6))
    (pad 7 smd trapezoid (at -2.142691 -3.525352 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 17 cathode7))
    (pad 8 smd trapezoid (at -3.575704 -2.043301 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 16 cathodeP))
    (pad 9 smd trapezoid (at -4.142691 -0.06125 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 15 cathode8))
    (pad 10 smd trapezoid (at -3.593653 1.987788 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 14 cathode9))
    (pad 11 smd trapezoid (at -2.074999 3.557403 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Paste F.Mask)
      (net 13 cathode0))
  )
  (module solo-nixie:USB_Micro-B_Wuerth-629105150521_CircularHoles (layer B.Cu) (tedit 619B73F2)
    (at 190.5 111.35 180)
    (descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
    (tags "usb micro receptacle")
    (attr smd)
    (fp_text reference USB (at 0 -2.569 180) (layer B.SilkS))
    (fp_text value USB_B_Micro (at 0 -5.6 180) (layer B.Fab))
    (fp_text user "PCB Edge" (at 0 -3.75 180) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.05 180) (layer B.Fab))
    (pad 6 thru_hole circle (at 3.5 -2.7 180) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.5 -2.7 180) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.5 0 180) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5 0 180) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.3 0.25 180) (size 0.45 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.65 0.25 180) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(J3-Pad4)"))
    (pad 3 smd roundrect (at 0 0.25 180) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J3-Pad3)"))
    (pad 2 smd roundrect (at -0.65 0.25 180) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J3-Pad2)"))
    (pad 1 smd rect (at -1.3 0.25 180) (size 0.45 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Wuerth-629105150521_CircularHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/micro-usb.stp
      (offset (xyz -75 0.5 -0.4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module solo-nixie:D_3220 (layer B.Cu) (tedit 619D03E5)
    (at 196.723 102.362)
    (descr "Diode SMD 3220, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 3220")
    (attr smd)
    (fp_text reference D1 (at 4.877 0) (layer B.SilkS))
    (fp_text value D (at 0 -2.6) (layer B.Fab))
    (fp_text user %R (at 0 1.6) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 1.75 2) (layers B.Cu B.Paste B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 2 0 180) (size 2 1.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_3220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm (layer B.Cu) (tedit 619B6B9B)
    (at 182.245 102.235 135)
    (descr "UQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001839B.pdf#page=464), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "UQFN NoLead")
    (attr smd)
    (fp_text reference U1 (at 0 3.556 135) (layer B.SilkS))
    (fp_text value PIC16F18346-GZ (at 0 -3.299999 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 20 smd roundrect (at -1 2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 RTCI2C_CLK))
    (pad 19 smd roundrect (at -0.5 2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 RTCI2C_DAT))
    (pad 18 smd roundrect (at 0 2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 17 smd roundrect (at 0.5 2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 16 smd roundrect (at 1 2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 ICSPDAT))
    (pad 15 smd roundrect (at 2.2 1 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 ICSPCLK))
    (pad 14 smd roundrect (at 2.2 0.5 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 HV_drive))
    (pad 13 smd roundrect (at 2.2 0 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 BUTTON_1))
    (pad 12 smd roundrect (at 2.2 -0.5 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 Voltage_meas))
    (pad 11 smd roundrect (at 2.2 -1 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 BUTTON_2))
    (pad 10 smd roundrect (at 1 -2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 nixie2))
    (pad 9 smd roundrect (at 0.5 -2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 nixie3))
    (pad 8 smd roundrect (at 0 -2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 nixie4))
    (pad 7 smd roundrect (at -0.5 -2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 nixie5))
    (pad 6 smd roundrect (at -1 -2.2 135) (size 0.25 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 nixieP))
    (pad 5 smd roundrect (at -2.2 -1 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 nixie9))
    (pad 4 smd roundrect (at -2.2 -0.5 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 nixie6))
    (pad 3 smd roundrect (at -2.2 0 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 nixie7))
    (pad 2 smd roundrect (at -2.2 0.5 135) (size 1.2 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 nixie8))
    (pad 1 smd rect (at -2.3 1 135) (size 1.4 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 VPP))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 183.947372 97.85 330)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q12 (at 0 -2.5 150) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 150) (layer F.Fab))
    (fp_text user %R (at 0 0 240) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 330) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 cathodeP))
    (pad 2 smd rect (at -1.1 0.95 330) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q12-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 330) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q12-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 183.947372 105.35 30)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q11 (at 0 -2.5 30) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 30) (layer F.Fab))
    (fp_text user %R (at 0 0 -60) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 30) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 cathode9))
    (pad 2 smd rect (at -1.1 0.95 30) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 30) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q11-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 182.9 101.6254)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q10 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 cathode8))
    (pad 2 smd rect (at -1.1 0.95) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q10-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 186.7 95 300)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q9 (at 0 -2.5 120) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 120) (layer F.Fab))
    (fp_text user %R (at 0 0 210) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 300) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 cathode7))
    (pad 2 smd rect (at -1.1 0.95 300) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 300) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q9-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 190.5 94 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 -2.5 90) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 cathode6))
    (pad 2 smd rect (at -1.1 0.95 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Q8-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 194.3 95 240)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at 0 -2.5 60) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 60) (layer F.Fab))
    (fp_text user %R (at 0 0 330) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 240) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 cathode5))
    (pad 2 smd rect (at -1.1 0.95 240) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 240) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(Q7-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 197.1 97.8 210)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 -2.5 30) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 30) (layer F.Fab))
    (fp_text user %R (at 0 0 300) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 210) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 cathode4))
    (pad 2 smd rect (at -1.1 0.95 210) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 210) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 198.1 101.6 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 cathode3))
    (pad 2 smd rect (at -1.1 0.95 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 197.052628 105.35 150)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 150) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 150) (layer F.Fab))
    (fp_text user %R (at 0 0 240) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 150) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 cathode2))
    (pad 2 smd rect (at -1.1 0.95 150) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 150) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 194.25 108.152628 120)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 120) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 120) (layer F.Fab))
    (fp_text user %R (at 0 0 210) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 120) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 cathode1))
    (pad 2 smd rect (at -1.1 0.95 120) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 120) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:SOT-23 (layer F.Cu) (tedit 619D0119)
    (at 186.75 108.152628 60)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 60) (layer F.SilkS) hide)
    (fp_text value MMBTA42 (at 0 2.5 60) (layer F.Fab))
    (fp_text user %R (at 0 0 -30) (layer F.Fab))
    (pad 3 smd rect (at 1.1 0 60) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 cathode0))
    (pad 2 smd rect (at -1.1 0.95 60) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -1.1 -0.95 60) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer B.Cu) (tedit 619D0140)
    (at 182.499 96.901 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R16 (at 0 1.397 90) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 0 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(Q12-Pad2)"))
    (pad 2 smd roundrect (at 1.2 0 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 190.5 111.76 270)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R15 (at 2.413 -0.127 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(Q10-Pad2)"))
    (pad 2 smd roundrect (at 1.2 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 180.8654 96.034975 60)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R14 (at 0 -1.7 60) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 60) (layer F.Fab))
    (fp_text user %R (at 0 0 60) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 60) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 nixieP))
    (pad 2 smd roundrect (at 1.2 0 60) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(Q12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 180.8734 107.1626 120)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R13 (at 0 -1.7 120) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 120) (layer F.Fab))
    (fp_text user %R (at 0 0 120) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 120) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 nixie9))
    (pad 2 smd roundrect (at 1.2 0 120) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 179.3748 101.6094 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R12 (at 0 -1.7 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 nixie8))
    (pad 2 smd roundrect (at 1.2 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(Q10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 184.934975 91.9654 30)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R11 (at 0 -1.7 30) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 30) (layer F.Fab))
    (fp_text user %R (at 0 0 30) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 30) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 nixie7))
    (pad 2 smd roundrect (at 1.2 0 30) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(Q9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 190.5 90.4748)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R10 (at 0 -1.7) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 nixie6))
    (pad 2 smd roundrect (at 1.2 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(Q8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 196.0626 91.948 330)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R9 (at 0 -1.7 150) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 150) (layer F.Fab))
    (fp_text user %R (at 0 0 150) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 330) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 nixie5))
    (pad 2 smd roundrect (at 1.2 0 330) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(Q7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 200.1092 96.009575 300)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R8 (at 0 -1.7 120) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 120) (layer F.Fab))
    (fp_text user %R (at 0 0 120) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 300) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 nixie4))
    (pad 2 smd roundrect (at 1.2 0 300) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 201.6506 101.5906 270)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R7 (at 0 -1.7 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 nixie3))
    (pad 2 smd roundrect (at 1.2 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 200.1346 107.165025 240)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 60) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 60) (layer F.Fab))
    (fp_text user %R (at 0 0 60) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 240) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 nixie2))
    (pad 2 smd roundrect (at 1.2 0 240) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 196.0626 111.2266 210)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 30) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 30) (layer F.Fab))
    (fp_text user %R (at 0 0 30) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 210) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 ICSPCLK))
    (pad 2 smd roundrect (at 1.2 0 210) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer F.Cu) (tedit 619D0140)
    (at 184.9374 111.2266 150)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 150) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.75 150) (layer F.Fab))
    (fp_text user %R (at 0 0 150) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 0 150) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 ICSPDAT))
    (pad 2 smd roundrect (at 1.2 0 150) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer B.Cu) (tedit 619D0140)
    (at 187.452 103.759 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R3 (at -2.921 0 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 0 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 Voltage_meas))
    (pad 2 smd roundrect (at 1.2 0 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer B.Cu) (tedit 619D0140)
    (at 192.913 98.425 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R2 (at 0 -1.27 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 0 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 HV_drive))
    (pad 2 smd roundrect (at 1.2 0 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer B.Cu) (tedit 619D0140)
    (at 189.484 103.759 270)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R1 (at 2.921 0 90) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 0 270) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 HT))
    (pad 2 smd roundrect (at 1.2 0 270) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 Voltage_meas))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer B.Cu) (tedit 619D0140)
    (at 190.5 108.331 180)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C2 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 2 smd roundrect (at 1.2 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module solo-nixie:0805_HandSoldering (layer B.Cu) (tedit 619D0140)
    (at 191.516 103.759 270)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C1 (at 2.921 0 90) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 0 270) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 HT))
    (pad 2 smd roundrect (at 1.2 0 270) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 190.5 101.6) (end 204.47 101.6) (layer Edge.Cuts) (width 0.05))
  (zone (net 48) (net_name "Net-(Q10-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.6096) (smoothing fillet) (radius 12.7))
    (polygon
      (pts
        (xy 201.168 111.76) (xy 179.832 111.76) (xy 179.832 91.44) (xy 201.168 91.44)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.6096) (smoothing fillet) (radius 12.7))
    (polygon
      (pts
        (xy 204.47 115.57) (xy 176.53 115.57) (xy 176.53 87.63) (xy 204.47 87.63)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.6096) (smoothing fillet) (radius 12.7))
    (polygon
      (pts
        (xy 204.47 115.57) (xy 176.53 115.57) (xy 176.53 87.63) (xy 204.47 87.63)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.8128) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 200.66 108.331) (xy 196.85 108.331) (xy 196.85 100.203) (xy 196.342 99.06) (xy 196.342 97.79)
        (xy 196.85 96.52) (xy 200.66 96.52)
      )
    )
  )
  (zone (net 2) (net_name HT) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.8128) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 196.469 104.013) (xy 192.659 104.013) (xy 192.659 103.632) (xy 188.468 103.632) (xy 188.468 100.965)
        (xy 196.469 100.965)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.8128) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 196.469 107.95) (xy 194.770375 109.680375) (xy 194.103625 112.315625) (xy 192.786 112.649) (xy 191.516 112.649)
        (xy 191.516 109.855) (xy 190.5 109.855) (xy 190.5 106.299) (xy 192.659 106.299) (xy 192.659 104.394)
        (xy 196.469 104.394)
      )
    )
  )
  (zone (net 2) (net_name HT) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.8128) (smoothing fillet) (radius 1.27))
    (polygon
      (pts
        (xy 192.278 102.997) (xy 190.9 104) (xy 190.72025 105.2) (xy 190.079125 105.2) (xy 190.020875 104)
        (xy 188.722 102.997) (xy 188.722 100.711) (xy 192.278 100.711)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 204.47 115.57) (xy 176.53 115.57) (xy 176.53 87.63) (xy 204.47 87.63)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.151 103.124) (xy 188.849 103.124) (xy 188.849 100.838) (xy 192.151 100.838)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 204.47 115.57) (xy 176.53 115.57) (xy 176.53 87.63) (xy 204.47 87.63)
      )
    )
  )
)
