(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 10)
    (no_connects 0)
    (area 123.749999 47.549999 139.140001 62.940001)
    (thickness 1.6)
    (drawings 18)
    (tracks 16)
    (zones 0)
    (modules 11)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 ROM_P20)
  (net 2 ~MREQ~)
  (net 3 ~ROM_CS~)
  (net 4 VCC)
  (net 5 GND)
  (net 6 ROM_P27)
  (net 7 "Net-(JP1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(JP1-Pad2)")
    (add_net ROM_P20)
    (add_net ROM_P27)
    (add_net VCC)
    (add_net ~MREQ~)
    (add_net ~ROM_CS~)
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58F537AF)
    (at 129.54 57.15 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value BAT85 (at 0.05 4.4 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 ROM_P20))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 ~MREQ~))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58F538BB)
    (at 133.35 60.96)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BAT85 (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 ROM_P20))
    (pad 2 smd rect (at 2.5 0) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 ~ROM_CS~))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 58CD4EC1)
    (at 129.54 53.34)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 2.33) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 ~MREQ~))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 58F3E549)
    (at 137.16 60.96)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J4 (at 0 -1.905) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 ~ROM_CS~))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 58CD4EC1)
    (at 137.16 53.34)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at 0 2.33) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ROM_P27))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 58F3E542)
    (at 129.54 60.96)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J6 (at 0 -1.905) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 ROM_P20))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58F539D4)
    (at 125.73 57.15 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 ROM_P20))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58F536A9)
    (at 135.89 50.8 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value 1k0 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 ROM_P27))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58F537C3)
    (at 131.445 49.53)
    (fp_text reference VCC (at 0 2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58F539C2)
    (at 125.73 53.34)
    (fp_text reference GND (at 1.905 0 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58F538ED)
    (at 133.35 53.34)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 1.905 2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X03_MALE (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 124.46 51.435) (end 128.905 51.435) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 60.325) (end 124.46 60.325) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 15.24 (width 0.3) (layer Dwgs.User)
    (gr_text "15.240 mm" (at 119.935 55.245 90) (layer Dwgs.User))
    (feature1 (pts (xy 123.825 47.625) (xy 118.585 47.625)))
    (feature2 (pts (xy 123.825 62.865) (xy 118.585 62.865)))
    (crossbar (pts (xy 121.285 62.865) (xy 121.285 47.625)))
    (arrow1a (pts (xy 121.285 47.625) (xy 121.871421 48.751504)))
    (arrow1b (pts (xy 121.285 47.625) (xy 120.698579 48.751504)))
    (arrow2a (pts (xy 121.285 62.865) (xy 121.871421 61.738496)))
    (arrow2b (pts (xy 121.285 62.865) (xy 120.698579 61.738496)))
  )
  (dimension 14.605 (width 0.3) (layer Dwgs.User)
    (gr_text "14.605 mm" (at 131.7625 43.735) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 46.99) (xy 124.46 42.385)))
    (feature2 (pts (xy 139.065 46.99) (xy 139.065 42.385)))
    (crossbar (pts (xy 139.065 45.085) (xy 124.46 45.085)))
    (arrow1a (pts (xy 124.46 45.085) (xy 125.586504 44.498579)))
    (arrow1b (pts (xy 124.46 45.085) (xy 125.586504 45.671421)))
    (arrow2a (pts (xy 139.065 45.085) (xy 137.938496 44.498579)))
    (arrow2b (pts (xy 139.065 45.085) (xy 137.938496 45.671421)))
  )
  (gr_line (start 130.175 47.625) (end 138.43 47.625) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 50.8) (end 129.54 48.26) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.825 59.69) (end 123.825 52.07) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.635 60.96) (end 127.635 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 62.865) (end 128.27 62.865) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.635 62.23) (end 128.27 62.865) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 60.325) (end 127.635 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.065 48.26) (end 139.065 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.825 52.07) (end 124.46 51.435) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.825 59.69) (end 124.46 60.325) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.065 62.23) (end 138.43 62.865) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.065 48.26) (end 138.43 47.625) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 50.8) (end 128.905 51.435) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 47.625) (end 129.54 48.26) (angle 90) (layer Edge.Cuts) (width 0.15))
)
