(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 116)
    (zones 0)
    (modules 24)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 +5VP)
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(J1-Pad2)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(R4-Pad2)")
  (net 11 "Net-(R4-Pad1)")
  (net 12 "Net-(R5-Pad1)")
  (net 13 "Net-(R6-Pad1)")
  (net 14 "Net-(U1-Pad1)")
  (net 15 "Net-(U1-Pad5)")
  (net 16 "Net-(U1-Pad7)")
  (net 17 "Net-(U1-Pad8)")
  (net 18 "Net-(U3-Pad1)")
  (net 19 "Net-(U3-Pad2)")
  (net 20 "Net-(U3-Pad3)")
  (net 21 "Net-(U3-Pad4)")
  (net 22 "Net-(U3-Pad5)")
  (net 23 "Net-(U3-Pad7)")
  (net 24 "Net-(U3-Pad8)")
  (net 25 "Net-(U3-Pad9)")
  (net 26 "Net-(U3-Pad10)")
  (net 27 "Net-(U3-Pad11)")
  (net 28 "Net-(U3-Pad12)")
  (net 29 "Net-(U3-Pad13)")
  (net 30 "Net-(U3-Pad14)")
  (net 31 "Net-(U3-Pad15)")
  (net 32 "Net-(U3-Pad16)")
  (net 33 "Net-(U3-Pad17)")
  (net 34 "Net-(U3-Pad19)")
  (net 35 "Net-(U3-Pad22)")
  (net 36 "Net-(U3-Pad23)")
  (net 37 "Net-(U3-Pad24)")
  (net 38 "Net-(U3-Pad25)")
  (net 39 "Net-(U3-Pad26)")
  (net 40 "Net-(U3-Pad27)")
  (net 41 "Net-(U3-Pad28)")
  (net 42 "Net-(U3-Pad29)")
  (net 43 "Net-(U3-Pad30)")
  (net 44 "Net-(U3-Pad33)")
  (net 45 "Net-(U3-Pad34)")
  (net 46 "Net-(U4-Pad1)")
  (net 47 "Net-(U4-Pad5)")
  (net 48 "Net-(U4-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5VP)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad24)")
    (add_net "Net-(U3-Pad25)")
    (add_net "Net-(U3-Pad26)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U3-Pad33)")
    (add_net "Net-(U3-Pad34)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad8)")
    (add_net VCC)
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F (layer F.Cu) (tedit 5B301BBE)
    (at 129.032 85.9295 90)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C1 (at -4.4945 2.54 180) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.4625 0 90) (size 2.075 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 1 VCC))
    (pad 2 smd roundrect (at 2.4625 0 90) (size 2.075 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F (layer F.Cu) (tedit 5B301BBE)
    (at 138.7615 78.994 180)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C2 (at 4.9035 1.397) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 2.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -2.4625 0 180) (size 2.075 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 1 VCC))
    (pad 2 smd roundrect (at 2.4625 0 180) (size 2.075 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 146.05 73.406 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C3 (at 4.318 5.08 180) (layer F.SilkS))
    (fp_text value 180uF (at 1.75 5.25 90) (layer F.Fab))
    (fp_text user %R (at 1.75 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 152.146 94.234)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C4 (at -2.54 3.429) (layer F.SilkS))
    (fp_text value 180uF (at 1.75 5.25) (layer F.Fab))
    (fp_text user %R (at 1.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F (layer F.Cu) (tedit 5B301BBE)
    (at 123.825 70.0265 270)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C5 (at 2.6175 -3.175) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 2.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 2.4625 0 270) (size 2.075 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.4625 0 270) (size 2.075 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.120482)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.128 71.12)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 3.184 0.254) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 135.255 91.2225 270)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 1.7415 -2.413) (layer F.SilkS))
    (fp_text value SD1206T020S1R0 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5VP))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 106.807 89.535 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at -2.286 -0.381 180) (layer F.SilkS))
    (fp_text value 44008RC (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 118.745 67.564)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at -0.127 5.08) (layer F.SilkS))
    (fp_text value Power (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT_LDM (layer F.Cu) (tedit 5C18524C)
    (at 147.955 109.22 270)
    (fp_text reference J3 (at -9.652 -11.811) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -15.24 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 5.08 -5.08 270) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.08 -5.08 270) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
  )
  (module Inductor_THT:L_Axial_L9.5mm_D4.0mm_P15.24mm_Horizontal_Fastron_SMCC (layer F.Cu) (tedit 5AE59B05)
    (at 152.146 73.406 270)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*4mm^2, Fastron, SMCC, http://cdn-reichelt.de/documents/datenblatt/B400/DS_SMCC_NEU.pdf, http://cdn-reichelt.de/documents/datenblatt/B400/LEADEDINDUCTORS.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 4mm Fastron SMCC")
    (fp_text reference L1 (at 3.302 -3.556) (layer F.SilkS))
    (fp_text value 1.8mH (at 7.62 3.12 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L9.5mm_D4.0mm_P15.24mm_Horizontal_Fastron_SMCC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 101.473 81.543 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 1.134 -1.905 180) (layer F.SilkS))
    (fp_text value R4.87k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 +5VP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 101.473 88.274 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.785 0) (layer F.SilkS))
    (fp_text value R10k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(R1-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 106.807 81.543 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 1.134 -1.905) (layer F.SilkS))
    (fp_text value R20k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 +5VP))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 122.8 84.455)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value R18.2k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.531 92.71)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.041 1.778) (layer F.SilkS))
    (fp_text value R1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 "Net-(R5-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.009 93.472)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 1.279 -1.778) (layer F.SilkS))
    (fp_text value R1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 104.775 73.5 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -6.19 1.651) (layer F.SilkS))
    (fp_text value REF195 (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +5VP))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad8)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 122.776 89.027)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -4.92 -2.159) (layer F.SilkS))
    (fp_text value INA122 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R5-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module arduino:ArduinoMicro (layer F.Cu) (tedit 5B523A25)
    (at 122.555 106.045 90)
    (fp_text reference U3 (at 11.049 -5.588 -180) (layer F.SilkS))
    (fp_text value ArduinoMicro (at 11.176 0.762 -180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U3-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(U3-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(U3-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(U3-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 -10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(U3-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 -7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at -7.62 -5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(U3-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(U3-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U3-Pad9)"))
    (pad 10 thru_hole circle (at -7.62 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U3-Pad10)"))
    (pad 11 thru_hole circle (at -7.62 5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U3-Pad11)"))
    (pad 12 thru_hole circle (at -7.62 7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U3-Pad12)"))
    (pad 13 thru_hole circle (at -7.62 10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U3-Pad13)"))
    (pad 14 thru_hole circle (at -7.62 12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad14)"))
    (pad 15 thru_hole circle (at -7.62 15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(U3-Pad15)"))
    (pad 16 thru_hole circle (at -7.62 17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(U3-Pad16)"))
    (pad 17 thru_hole circle (at -7.62 20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(U3-Pad17)"))
    (pad 18 thru_hole circle (at 7.62 20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(R6-Pad1)"))
    (pad 19 thru_hole circle (at 7.62 17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(U3-Pad19)"))
    (pad 20 thru_hole circle (at 7.62 15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +5VP))
    (pad 21 thru_hole circle (at 7.62 12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 22 thru_hole circle (at 7.62 10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(U3-Pad22)"))
    (pad 23 thru_hole circle (at 7.62 7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(U3-Pad23)"))
    (pad 24 thru_hole circle (at 7.62 5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(U3-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(U3-Pad26)"))
    (pad 27 thru_hole circle (at 7.62 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(U3-Pad27)"))
    (pad 28 thru_hole circle (at 7.62 -5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(U3-Pad28)"))
    (pad 29 thru_hole circle (at 7.62 -7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(U3-Pad29)"))
    (pad 30 thru_hole circle (at 7.62 -10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(U3-Pad30)"))
    (pad 31 thru_hole circle (at 7.62 -12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole circle (at 7.62 -15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 33 thru_hole circle (at 7.62 -17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(U3-Pad33)"))
    (pad 34 thru_hole circle (at 7.62 -20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(U3-Pad34)"))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 142.24 85.25 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 1.43 -4.318 180) (layer F.SilkS))
    (fp_text value TL061 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R6-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad8)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 128.905 67.564)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U5 (at 8.763 -1.524) (layer F.SilkS))
    (fp_text value LM7812_TO220 (at 2.54 2.5) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_1.27mm:TP_0.051_LDM (layer F.Cu) (tedit 5C198A42)
    (at 114.554 91.948)
    (fp_text reference T1 (at 2.286 1.016) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.032) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
  )
  (module Connector_PinSocket_1.27mm:TP_0.051_LDM (layer F.Cu) (tedit 5C198A42)
    (at 114.554 85.598)
    (fp_text reference T2 (at 1.651 -1.651) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.032) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad2)"))
  )
  (gr_circle (center 157.48 88.9) (end 159.0802 88.9) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 110.363 107.95) (end 111.9632 107.95) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 110.49 69.85) (end 112.0902 69.85) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 157.48 69.85) (end 159.0802 69.85) (layer Edge.Cuts) (width 0.2))
  (gr_text KRb (at 157.988 66.04) (layer F.SilkS))
  (gr_text "Prop. Valve Controller\nREV A (12/2018)\nL. De Marco " (at 112.522 77.724) (layer F.SilkS))
  (gr_text "CTRL OUT" (at 157.226 101.092) (layer F.SilkS))
  (gr_text INA122 (at 116.332 88.392) (layer F.SilkS))
  (gr_text TL061 (at 136.906 85.344) (layer F.SilkS))
  (gr_text LM7812 (at 139.7 67.564) (layer F.SilkS))
  (gr_text GND (at 115.316 70.104) (layer F.SilkS))
  (gr_text +15V (at 114.808 67.564) (layer F.SilkS))
  (gr_text REF195 (at 104.902 68.834) (layer F.SilkS))
  (gr_text 44008RC (at 108.712 91.821) (layer F.SilkS))
  (gr_line (start 99.568 116.84) (end 161.036 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.568 64.008) (end 99.568 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.036 64.008) (end 99.568 64.008) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.036 116.84) (end 161.036 64.008) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.663 62.23) (xy 163.195 62.103) (xy 162.306 119.761) (xy 97.155 119.507) (xy 97.663 62.357)
      )
    )
  )
)
