<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="73.4568" y1="0" x2="73.4568" y2="47.9298" width="0.1524" layer="20"/>
<wire x1="73.4568" y1="47.9298" x2="0.1524" y2="47.9298" width="0.1524" layer="20"/>
<wire x1="0.1524" y1="47.9298" x2="0.1524" y2="0" width="0.1524" layer="20"/>
<hole x="2.54" y="2.54" drill="3.175"/>
<hole x="71.12" y="45.72" drill="3.175"/>
<hole x="71.12" y="2.54" drill="3.175"/>
<hole x="2.54" y="45.72" drill="3.175"/>
<wire x1="25.6794" y1="16.4084" x2="48.26" y2="16.4084" width="0.1524" layer="20"/>
<wire x1="48.26" y1="16.4084" x2="48.26" y2="0" width="0.1524" layer="20"/>
<wire x1="25.6794" y1="0" x2="25.6794" y2="16.4084" width="0.1524" layer="20"/>
<wire x1="0.1524" y1="0" x2="25.6794" y2="0" width="0.1524" layer="20"/>
<wire x1="73.4568" y1="0" x2="48.26" y2="0" width="0.1524" layer="20"/>
<text>Specify 2 Oz Copper</text>
<text>GND</text>
<text>12V</text>
<text>LED 
(Remote)</text>
<text>MOTOR</text>
<text>MOTOR</text>
<text>Under
Heatsink</text>
<text>INTAKE</text>
<text>STOP</text>
<text>EXHAUST</text>
<text>EXHAUST</text>
<text>STOP</text>
<text>INTAKE</text>
<text>Switch Placement</text>
<text>Ti PowerPad</text>
<text>RV-Project.Com    Vortex I-II  Fan Controller     V2.3A    2/27/2019</text>
<text>Made in USA</text>
<text>Brushed 
Motors 
Only</text>
<text>Current Regulation
 (ILIM port) R3:
Max Current :
3.6A: 15K Resistor
3A:    20K Resistor 
2.5A: 27K Resistor
2A:   32K Resistor
</text>
<text>Use PolyCase TF-2309TX
for Cover.</text>
<text>ILIM</text>
<text>Out</text>
<text>IN</text>
<text>Out</text>
<text>5V</text>
<text>RX</text>
<text>12V</text>
<text>RX</text>
<text>5V</text>
<text>N/C</text>
<text>12V</text>
<text>IN</text>
<text>IN</text>
<text>Switch Diagram</text>
<text>LOCAL</text>
<text>Remote</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="SMD_ELECTROLYTIC_6MMDIA">
<description>Pad Size=0.4"x0.1"&lt;br&gt;Dia: 0.25" dia (6mm)</description>
</package>
<package name="1206-CAP">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;SMA diode.&lt;br&gt;
Pad Size: 0.225"x0.07"</description>
</package>
<package name="1206-RES">
</package>
<package name="ASK_MICRO_RECEIVER_DECODER_433MHZ_TYPEB">
</package>
<package name="TACTILE-PTH-12MM">
<description>Pitch: 0.2"x0.5" (2.54mmx12mm)</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SOIC8_POWERPAD">
<description>&lt;b&gt;Small Outline IC - 208mil Wide&lt;/b&gt;</description>
</package>
<package name="HEATSINK1">
</package>
<package name="1X01_HEADER">
<description>Drill: 0.039" dia</description>
</package>
<package name="KEYSTONE_15XX">
<description>Pad for Keystone Turret terminal.&lt;br&gt;
Drill: 0.094"
&lt;br&gt;1502-X, 1514-X</description>
</package>
<package name="FUSE476">
<description>Pad Size: 0.38"x0.15"</description>
</package>
<package name="SOD-123(LARGE)">
<description>Suitable for LL4148, FDLL4148, etc/&lt;br&gt;Pad Size:  0.25"x0.7"</description>
</package>
<package name="IPAK_HORIZONTAL(TO251)">
</package>
<package name="DO214AC_JBEND_NONPOLARIZED">
<description>Pad Size" 0.3"x0.1"</description>
</package>
<package name="1X02">
<description>Pitch: 0.1" (2.54mm)&lt;br&gt;Drill: 0.040" dia</description>
</package>
<package name="CREATIVECOMMONS">
</package>
<package name="RVPROJECT_LOGO">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LOGO">
<description>&lt;B&gt;Logo&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C5" library="a-lib" package="SMD_ELECTROLYTIC_6MMDIA" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="a-lib" package="1206-CAP" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="30k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX1" library="a-lib" package="ASK_MICRO_RECEIVER_DECODER_433MHZ_TYPEB" value="">
<attribute name="NAME"/>
</element>
<element name="S1" library="a-lib" package="TACTILE-PTH-12MM" value="SWITCH-MOMENTARY-212MM">
<attribute name="PROD_ID" value="SWCH-09185"/>
</element>
<element name="S2" library="a-lib" package="TACTILE-PTH-12MM" value="SWITCH-MOMENTARY-212MM">
<attribute name="PROD_ID" value="SWCH-09185"/>
</element>
<element name="S3" library="a-lib" package="TACTILE-PTH-12MM" value="SWITCH-MOMENTARY-212MM">
<attribute name="PROD_ID" value="SWCH-09185"/>
</element>
<element name="U2" library="a-lib" package="DIP08" value="TINY85-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="U3" library="a-lib" package="SOIC8_POWERPAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HS1" library="a-lib" package="HEATSINK1" value="HS407-ND">
<attribute name="VALUE" value="HS407-ND"/>
</element>
<element name="JP3" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
</element>
<element name="JP4" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
</element>
<element name="F1" library="a-lib" package="FUSE476" value="5A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="U1" library="a-lib" package="IPAK_HORIZONTAL(TO251)" value="1Amp">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="a-lib" package="DO214AC_JBEND_NONPOLARIZED" value="TVS-B">
<attribute name="NAME"/>
</element>
<element name="JP7" library="a-lib" package="KEYSTONE_15XX" value=""/>
<element name="JP8" library="a-lib" package="KEYSTONE_15XX" value=""/>
<element name="JP6" library="a-lib" package="KEYSTONE_15XX" value=""/>
<element name="JP5" library="a-lib" package="KEYSTONE_15XX" value=""/>
<element name="J1" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="LOGO3" library="a-lib" package="CREATIVECOMMONS" value="CreativeCommons"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="U$1" library="atmel" package="LOGO" value=""/>
<element name="R1" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="a-lib" package="RVPROJECT_LOGO" value="CLIPART_LOGORV-PROJECT"/>
<element name="JP2" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="C4" pad="2"/>
<contactref element="RX1" pad="GND"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="G1"/>
<contactref element="U3" pad="G2"/>
<contactref element="U3" pad="G3"/>
<contactref element="U3" pad="G4"/>
<contactref element="U3" pad="G5"/>
<contactref element="U3" pad="G6"/>
<contactref element="U3" pad="G7"/>
<contactref element="U3" pad="G8"/>
<contactref element="U3" pad="G9"/>
<contactref element="U3" pad="G10"/>
<contactref element="U3" pad="G11"/>
<contactref element="U3" pad="G12"/>
<contactref element="U3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="HS1" pad="P$1"/>
<contactref element="HS1" pad="P$2"/>
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="G"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="JP6" pad="P$1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="8"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="O"/>
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="RX1" pad="OUT1"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="RX1" pad="OUT2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="RX1" pad="OUT3"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="3"/>
<contactref element="D3" pad="C"/>
<contactref element="R5" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="2"/>
<contactref element="D4" pad="C"/>
<contactref element="R6" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="7"/>
<contactref element="D5" pad="C"/>
<contactref element="R7" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="RX1" pad="VCC"/>
<contactref element="JP2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U3" pad="6"/>
<contactref element="D6" pad="2"/>
<contactref element="JP8" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="8"/>
<contactref element="D6" pad="1"/>
<contactref element="JP7" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="JP3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="+"/>
<contactref element="U3" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="I"/>
</signal>
<signal name="N$5">
<contactref element="F1" pad="P$1"/>
<contactref element="JP5" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="JP4" pad="1"/>
<contactref element="F1" pad="P$2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$20">
<contactref element="RX1" pad="OUT4"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
