(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 449)
    (no_connects 0)
    (area 69.164999 27.254999 229.285001 163.880001)
    (thickness 1.6)
    (drawings 8)
    (tracks 2851)
    (zones 0)
    (modules 140)
    (nets 214)
  )
  (page USLetter)
  (title_block
    (title "8, 18 Bit DAC, with FPGA XEM7001 Control")
    (date 2017-03-12)
    (rev 000)
    (company "Ye Group")
    (comment 1 "Desined by: Jacob Scott")
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 69.215 163.83)
    (grid_origin 69.215 163.83)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GNDA)
  (net 3 -15V)
  (net 4 +15V)
  (net 5 "Net-(C32-Pad2)")
  (net 6 "Net-(C78-Pad1)")
  (net 7 "Net-(C79-Pad1)")
  (net 8 "Net-(FPGA1-PadGNDa)")
  (net 9 "Net-(FPGA1-PadGNDb)")
  (net 10 "Net-(FPGA1-PadP10)")
  (net 11 SCLK5)
  (net 12 "Net-(FPGA1-PadJ3)")
  (net 13 SDIN5)
  (net 14 "Net-(FPGA1-PadK1)")
  (net 15 "Net-(FPGA1-Pad3.3A)")
  (net 16 "Net-(FPGA1-Pad3.3B)")
  (net 17 SDO5)
  (net 18 "Net-(FPGA1-PadK3)")
  (net 19 ~LDAC~5)
  (net 20 "Net-(FPGA1-PadM1)")
  (net 21 ~CLR~5)
  (net 22 "Net-(FPGA1-PadL4)")
  (net 23 ~RESET~5)
  (net 24 "Net-(FPGA1-PadN1)")
  (net 25 "Net-(FPGA1-PadGNDc)")
  (net 26 "Net-(FPGA1-PadGNDd)")
  (net 27 "Net-(FPGA1-PadN3)")
  (net 28 "Net-(FPGA1-PadP1)")
  (net 29 "Net-(FPGA1-PadR1)")
  (net 30 "Net-(FPGA1-PadR2)")
  (net 31 "Net-(FPGA1-PadP3)")
  (net 32 "Net-(FPGA1-PadT2)")
  (net 33 "Net-(FPGA1-PadR3)")
  (net 34 "Net-(FPGA1-PadT3)")
  (net 35 "Net-(FPGA1-PadN4)")
  (net 36 "Net-(FPGA1-PadGNDe)")
  (net 37 "Net-(FPGA1-PadGNDf)")
  (net 38 ~RESET~6)
  (net 39 ~RESET~4)
  (net 40 ~CLR~6)
  (net 41 ~CLR~4)
  (net 42 ~LDAC~6)
  (net 43 ~LDAC~4)
  (net 44 SDO6)
  (net 45 SDO4)
  (net 46 "Net-(FPGA1-Pad3.3C)")
  (net 47 "Net-(FPGA1-Pad3.3D)")
  (net 48 SDIN6)
  (net 49 SDIN4)
  (net 50 SCLK6)
  (net 51 SCLK4)
  (net 52 ~SYNC~6)
  (net 53 ~SYNC~4)
  (net 54 "Net-(FPGA1-PadGNDg)")
  (net 55 "Net-(FPGA1-PadGNDh)")
  (net 56 "Net-(FPGA1-Pad3.3E)")
  (net 57 "Net-(FPGA1-Pad3.3F)")
  (net 58 ~RESET~1)
  (net 59 ~RESET~2)
  (net 60 ~CLR~1)
  (net 61 ~CLR~2)
  (net 62 ~LDAC~1)
  (net 63 ~LDAC~2)
  (net 64 SDO1)
  (net 65 SDO2)
  (net 66 SDIN1)
  (net 67 SDIN2)
  (net 68 SCLK1)
  (net 69 SCLK2)
  (net 70 ~SYNC~1)
  (net 71 ~SYNC~2)
  (net 72 "Net-(FPGA1-PadD4)")
  (net 73 "Net-(FPGA1-PadC4)")
  (net 74 "Net-(FPGA1-PadGNDj)")
  (net 75 "Net-(FPGA1-PadGNDk)")
  (net 76 "Net-(FPGA1-PadGNDl)")
  (net 77 "Net-(FPGA1-PadA8)")
  (net 78 ~SYNC~7)
  (net 79 "Net-(FPGA1-PadC8)")
  (net 80 SCLK7)
  (net 81 "Net-(FPGA1-PadA9)")
  (net 82 SDIN7)
  (net 83 "Net-(FPGA1-Pad3.3G)")
  (net 84 "Net-(FPGA1-Pad3.3H)")
  (net 85 "Net-(FPGA1-PadB9)")
  (net 86 SDO7)
  (net 87 "Net-(FPGA1-PadB10)")
  (net 88 ~LDAC~7)
  (net 89 "Net-(FPGA1-PadB12)")
  (net 90 ~CLR~7)
  (net 91 "Net-(FPGA1-PadC12)")
  (net 92 ~RESET~7)
  (net 93 "Net-(FPGA1-PadGNDn)")
  (net 94 "Net-(FPGA1-PadGNDm)")
  (net 95 "Net-(FPGA1-PadA13)")
  (net 96 "Net-(FPGA1-PadA14)")
  (net 97 "Net-(FPGA1-PadE13)")
  (net 98 "Net-(FPGA1-PadB14)")
  (net 99 "Net-(FPGA1-PadC14)")
  (net 100 "Net-(FPGA1-PadA15)")
  (net 101 "Net-(FPGA1-PadB15)")
  (net 102 "Net-(FPGA1-PadB16)")
  (net 103 "Net-(FPGA1-PadGNDo)")
  (net 104 "Net-(FPGA1-PadGNDp)")
  (net 105 ~RESET~3)
  (net 106 ~RESET~8)
  (net 107 ~CLR~3)
  (net 108 ~CLR~8)
  (net 109 ~LDAC~3)
  (net 110 ~LDAC~8)
  (net 111 SDO3)
  (net 112 SDO8)
  (net 113 "Net-(FPGA1-Pad3.3I)")
  (net 114 "Net-(FPGA1-Pad3.3J)")
  (net 115 SDIN3)
  (net 116 SDIN8)
  (net 117 SCLK3)
  (net 118 SCLK8)
  (net 119 ~SYNC~3)
  (net 120 "Net-(FPGA1-PadGNDq)")
  (net 121 "Net-(FPGA1-PadGNDr)")
  (net 122 Vout1)
  (net 123 Vout2)
  (net 124 Vout3)
  (net 125 Vout4)
  (net 126 Vout5)
  (net 127 Vout6)
  (net 128 Vout7)
  (net 129 Vout8)
  (net 130 "Net-(U1-Pad1)")
  (net 131 "Net-(U1-Pad3)")
  (net 132 "Net-(U1-Pad5)")
  (net 133 "Net-(U1-Pad8)")
  (net 134 "Net-(U2-Pad1)")
  (net 135 "Net-(U2-Pad3)")
  (net 136 "Net-(U2-Pad4)")
  (net 137 "Net-(U2-Pad16)")
  (net 138 "Net-(U2-Pad17)")
  (net 139 "Net-(U2-Pad20)")
  (net 140 "Net-(U3-Pad1)")
  (net 141 "Net-(U3-Pad2)")
  (net 142 "Net-(U3-Pad20)")
  (net 143 "Net-(U4-Pad1)")
  (net 144 "Net-(U4-Pad5)")
  (net 145 "Net-(U4-Pad8)")
  (net 146 +10Vref)
  (net 147 -10Vref)
  (net 148 "Net-(U6-Pad1)")
  (net 149 "Net-(U6-Pad3)")
  (net 150 "Net-(U6-Pad5)")
  (net 151 "Net-(U6-Pad8)")
  (net 152 "Net-(U7-Pad1)")
  (net 153 "Net-(U10-Pad2)")
  (net 154 "Net-(U10-Pad1)")
  (net 155 "Net-(U10-Pad7)")
  (net 156 "Net-(U10-Pad6)")
  (net 157 "Net-(U7-Pad20)")
  (net 158 "Net-(U8-Pad1)")
  (net 159 "Net-(U8-Pad2)")
  (net 160 "Net-(U8-Pad20)")
  (net 161 "Net-(U9-Pad1)")
  (net 162 "Net-(U9-Pad5)")
  (net 163 "Net-(U9-Pad8)")
  (net 164 "Net-(U11-Pad4)")
  (net 165 "Net-(U11-Pad5)")
  (net 166 "Net-(U11-Pad13)")
  (net 167 "Net-(U11-Pad10)")
  (net 168 "Net-(U11-Pad11)")
  (net 169 "Net-(U11-Pad12)")
  (net 170 "Net-(U12-Pad1)")
  (net 171 "Net-(U12-Pad3)")
  (net 172 "Net-(U12-Pad5)")
  (net 173 "Net-(U12-Pad8)")
  (net 174 "Net-(U13-Pad1)")
  (net 175 "Net-(U13-Pad3)")
  (net 176 "Net-(U13-Pad4)")
  (net 177 ~SYNC~5)
  (net 178 "Net-(U13-Pad16)")
  (net 179 "Net-(U13-Pad17)")
  (net 180 "Net-(U13-Pad20)")
  (net 181 "Net-(U14-Pad1)")
  (net 182 "Net-(U14-Pad2)")
  (net 183 "Net-(U14-Pad20)")
  (net 184 "Net-(U15-Pad1)")
  (net 185 "Net-(U15-Pad5)")
  (net 186 "Net-(U15-Pad8)")
  (net 187 "Net-(U17-Pad1)")
  (net 188 "Net-(U17-Pad3)")
  (net 189 "Net-(U17-Pad5)")
  (net 190 "Net-(U17-Pad8)")
  (net 191 "Net-(U18-Pad1)")
  (net 192 "Net-(U18-Pad3)")
  (net 193 "Net-(U18-Pad4)")
  (net 194 "Net-(U18-Pad16)")
  (net 195 "Net-(U18-Pad17)")
  (net 196 "Net-(U18-Pad20)")
  (net 197 "Net-(U19-Pad1)")
  (net 198 "Net-(U19-Pad2)")
  (net 199 ~SYNC~8)
  (net 200 "Net-(U19-Pad20)")
  (net 201 "Net-(U20-Pad1)")
  (net 202 "Net-(U20-Pad5)")
  (net 203 "Net-(U20-Pad8)")
  (net 204 GNDD)
  (net 205 "Net-(FPGA1-PadCLK1)")
  (net 206 "Net-(FPGA1-PadCLK2)")
  (net 207 "/FPGAPinout/External Clock Input/CLK")
  (net 208 "Net-(C85-Pad1)")
  (net 209 "Net-(C85-Pad2)")
  (net 210 "Net-(C86-Pad1)")
  (net 211 "Net-(JP1-Pad1)")
  (net 212 "Net-(P10-Pad1)")
  (net 213 "Net-(U23-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(C32-Pad2)")
    (add_net "Net-(C85-Pad1)")
    (add_net "Net-(C86-Pad1)")
    (add_net "Net-(FPGA1-Pad3.3A)")
    (add_net "Net-(FPGA1-Pad3.3B)")
    (add_net "Net-(FPGA1-Pad3.3C)")
    (add_net "Net-(FPGA1-Pad3.3D)")
    (add_net "Net-(FPGA1-Pad3.3E)")
    (add_net "Net-(FPGA1-Pad3.3F)")
    (add_net "Net-(FPGA1-Pad3.3G)")
    (add_net "Net-(FPGA1-Pad3.3H)")
    (add_net "Net-(FPGA1-Pad3.3I)")
    (add_net "Net-(FPGA1-Pad3.3J)")
    (add_net "Net-(FPGA1-PadA13)")
    (add_net "Net-(FPGA1-PadA14)")
    (add_net "Net-(FPGA1-PadA15)")
    (add_net "Net-(FPGA1-PadA8)")
    (add_net "Net-(FPGA1-PadA9)")
    (add_net "Net-(FPGA1-PadB10)")
    (add_net "Net-(FPGA1-PadB12)")
    (add_net "Net-(FPGA1-PadB15)")
    (add_net "Net-(FPGA1-PadB16)")
    (add_net "Net-(FPGA1-PadB9)")
    (add_net "Net-(FPGA1-PadC12)")
    (add_net "Net-(FPGA1-PadC14)")
    (add_net "Net-(FPGA1-PadC4)")
    (add_net "Net-(FPGA1-PadC8)")
    (add_net "Net-(FPGA1-PadCLK1)")
    (add_net "Net-(FPGA1-PadCLK2)")
    (add_net "Net-(FPGA1-PadD4)")
    (add_net "Net-(FPGA1-PadE13)")
    (add_net "Net-(FPGA1-PadGNDa)")
    (add_net "Net-(FPGA1-PadGNDb)")
    (add_net "Net-(FPGA1-PadGNDc)")
    (add_net "Net-(FPGA1-PadGNDd)")
    (add_net "Net-(FPGA1-PadGNDe)")
    (add_net "Net-(FPGA1-PadGNDf)")
    (add_net "Net-(FPGA1-PadGNDg)")
    (add_net "Net-(FPGA1-PadGNDh)")
    (add_net "Net-(FPGA1-PadGNDj)")
    (add_net "Net-(FPGA1-PadGNDk)")
    (add_net "Net-(FPGA1-PadGNDl)")
    (add_net "Net-(FPGA1-PadGNDm)")
    (add_net "Net-(FPGA1-PadGNDn)")
    (add_net "Net-(FPGA1-PadGNDo)")
    (add_net "Net-(FPGA1-PadGNDp)")
    (add_net "Net-(FPGA1-PadGNDq)")
    (add_net "Net-(FPGA1-PadGNDr)")
    (add_net "Net-(FPGA1-PadJ3)")
    (add_net "Net-(FPGA1-PadK1)")
    (add_net "Net-(FPGA1-PadK3)")
    (add_net "Net-(FPGA1-PadL4)")
    (add_net "Net-(FPGA1-PadM1)")
    (add_net "Net-(FPGA1-PadN1)")
    (add_net "Net-(FPGA1-PadN3)")
    (add_net "Net-(FPGA1-PadN4)")
    (add_net "Net-(FPGA1-PadP1)")
    (add_net "Net-(FPGA1-PadP10)")
    (add_net "Net-(FPGA1-PadP3)")
    (add_net "Net-(FPGA1-PadR1)")
    (add_net "Net-(FPGA1-PadR2)")
    (add_net "Net-(FPGA1-PadR3)")
    (add_net "Net-(FPGA1-PadT2)")
    (add_net "Net-(FPGA1-PadT3)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad6)")
    (add_net "Net-(U10-Pad7)")
    (add_net "Net-(U11-Pad10)")
    (add_net "Net-(U11-Pad11)")
    (add_net "Net-(U11-Pad12)")
    (add_net "Net-(U11-Pad13)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U11-Pad5)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U12-Pad3)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U12-Pad8)")
    (add_net "Net-(U13-Pad1)")
    (add_net "Net-(U13-Pad16)")
    (add_net "Net-(U13-Pad17)")
    (add_net "Net-(U13-Pad20)")
    (add_net "Net-(U13-Pad3)")
    (add_net "Net-(U13-Pad4)")
    (add_net "Net-(U14-Pad1)")
    (add_net "Net-(U14-Pad2)")
    (add_net "Net-(U14-Pad20)")
    (add_net "Net-(U15-Pad1)")
    (add_net "Net-(U15-Pad5)")
    (add_net "Net-(U15-Pad8)")
    (add_net "Net-(U17-Pad1)")
    (add_net "Net-(U17-Pad3)")
    (add_net "Net-(U17-Pad5)")
    (add_net "Net-(U17-Pad8)")
    (add_net "Net-(U18-Pad1)")
    (add_net "Net-(U18-Pad16)")
    (add_net "Net-(U18-Pad17)")
    (add_net "Net-(U18-Pad20)")
    (add_net "Net-(U18-Pad3)")
    (add_net "Net-(U18-Pad4)")
    (add_net "Net-(U19-Pad1)")
    (add_net "Net-(U19-Pad2)")
    (add_net "Net-(U19-Pad20)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U20-Pad1)")
    (add_net "Net-(U20-Pad5)")
    (add_net "Net-(U20-Pad8)")
    (add_net "Net-(U23-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad3)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad8)")
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad20)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad2)")
    (add_net "Net-(U8-Pad20)")
    (add_net "Net-(U9-Pad1)")
    (add_net "Net-(U9-Pad5)")
    (add_net "Net-(U9-Pad8)")
    (add_net SCLK1)
    (add_net SCLK2)
    (add_net SCLK3)
    (add_net SCLK4)
    (add_net SCLK5)
    (add_net SCLK6)
    (add_net SCLK7)
    (add_net SCLK8)
    (add_net SDIN1)
    (add_net SDIN2)
    (add_net SDIN3)
    (add_net SDIN4)
    (add_net SDIN5)
    (add_net SDIN6)
    (add_net SDIN7)
    (add_net SDIN8)
    (add_net SDO1)
    (add_net SDO2)
    (add_net SDO3)
    (add_net SDO4)
    (add_net SDO5)
    (add_net SDO6)
    (add_net SDO7)
    (add_net SDO8)
    (add_net ~CLR~1)
    (add_net ~CLR~2)
    (add_net ~CLR~3)
    (add_net ~CLR~4)
    (add_net ~CLR~5)
    (add_net ~CLR~6)
    (add_net ~CLR~7)
    (add_net ~CLR~8)
    (add_net ~LDAC~1)
    (add_net ~LDAC~2)
    (add_net ~LDAC~3)
    (add_net ~LDAC~4)
    (add_net ~LDAC~5)
    (add_net ~LDAC~6)
    (add_net ~LDAC~7)
    (add_net ~LDAC~8)
    (add_net ~RESET~1)
    (add_net ~RESET~2)
    (add_net ~RESET~3)
    (add_net ~RESET~4)
    (add_net ~RESET~5)
    (add_net ~RESET~6)
    (add_net ~RESET~7)
    (add_net ~RESET~8)
    (add_net ~SYNC~1)
    (add_net ~SYNC~2)
    (add_net ~SYNC~3)
    (add_net ~SYNC~4)
    (add_net ~SYNC~5)
    (add_net ~SYNC~6)
    (add_net ~SYNC~7)
    (add_net ~SYNC~8)
  )
  (net_class HF ""
    (clearance 0.5)
    (trace_width 0.35)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "/FPGAPinout/External Clock Input/CLK")
    (add_net "Net-(C85-Pad2)")
    (add_net "Net-(FPGA1-PadB14)")
    (add_net "Net-(P10-Pad1)")
  )
  (net_class POWER/GND ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +10Vref)
    (add_net +15V)
    (add_net +3V3)
    (add_net -10Vref)
    (add_net -15V)
    (add_net GNDA)
    (add_net GNDD)
    (add_net "Net-(C78-Pad1)")
    (add_net "Net-(C79-Pad1)")
  )
  (net_class Vout ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net Vout1)
    (add_net Vout2)
    (add_net Vout3)
    (add_net Vout4)
    (add_net Vout5)
    (add_net Vout6)
    (add_net Vout7)
    (add_net Vout8)
  )
  (module Connectors:1pin (layer Top) (tedit 58C6E235)
    (at 86.36 130.175)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
  )
  (module Connectors:1pin (layer Top) (tedit 58C6E240)
    (at 86.36 64.135)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
  )
  (module Connectors:1pin (layer Top) (tedit 58C6E256)
    (at 139.065 33.02)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 204 GNDD))
  )
  (module Connectors:1pin (layer Top) (tedit 58C6E286)
    (at 222.885 33.02)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 204 GNDD))
  )
  (module Connectors:1pin (layer Top) (tedit 58C6E227)
    (at 139.7 156.845)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D595)
    (at 98.679 155.956)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.397 -1.397) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D74B)
    (at 99.314 134.62)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 1.27 1.524) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.254 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D5C0)
    (at 89.535 153.67 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.651 1.397 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DB9A)
    (at 98.806 139.446)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.1115 0.1905) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D738)
    (at 89.662 136.144 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0.381 1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D5CC)
    (at 98.425 150.495 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -3.556 0.254 360) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0.127 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D6A0)
    (at 116.84 145.796 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0.889 -1.524 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D5FF)
    (at 116.7765 155.0035 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.0635 -0.0635 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D9F4)
    (at 111.76 136.144 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -3.556 -0.381 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D6FF)
    (at 93.98 143.637 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0.254 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D5A7)
    (at 93.98 160.655 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0.254 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D695)
    (at 126.111 146.939 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.254 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DE5B)
    (at 98.679 122.936)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 3.81 0.508) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.0635 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D861)
    (at 99.187 101.6)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 3.81 -2.159) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.254 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DB39)
    (at 89.535 120.5865 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 1.4605 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.1905 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DABC)
    (at 98.806 106.426)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 3.683 0.508) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D841)
    (at 89.662 103.124 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C26 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DEAC)
    (at 98.3615 117.475 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at -3.683 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0.0635 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DD3C)
    (at 116.84 112.649 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C29 (at 0.6985 -1.651 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.0635 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E310)
    (at 154.813 137.9855 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C31 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.0635 0.254 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DDF1)
    (at 116.5225 121.9835 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C34 (at 0.8255 -1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D9EE)
    (at 111.76 103.124 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C36 (at -3.683 -0.508 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5D883)
    (at 93.98 110.617 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C37 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DC01)
    (at 93.98 127.635 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C38 (at 0.127 1.5875 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.0635 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5DD60)
    (at 126.0475 113.919 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C39 (at -1.397 -1.5875 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.1905 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5EA45)
    (at 98.679 89.789)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C41 (at 3.6195 0.254) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5ED14)
    (at 99.1235 68.199)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C43 (at 3.556 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E96F)
    (at 89.535 87.4395 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C44 (at 1.524 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E2FE)
    (at 154.813 157.6705 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C45 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.254 0.127 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5ECC4)
    (at 98.806 73.3425)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C47 (at 3.556 0.4445) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5ED32)
    (at 89.662 69.977 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C48 (at 1.4605 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5EB4B)
    (at 98.425 84.3915 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C50 (at -3.683 0.0635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.0635 -0.0635 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5EC08)
    (at 116.84 79.756 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C52 (at 0.9525 -1.524 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5EBDA)
    (at 116.7765 88.9 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C54 (at 3.556 -0.0635 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5EC91)
    (at 111.887 70.0405 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C56 (at 3.556 -0.5715 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E3F5)
    (at 93.98 77.6605 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C57 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E96B)
    (at 93.98 94.6785 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C58 (at 0 1.4605 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E364)
    (at 126.0475 80.9625 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C59 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F474)
    (at 98.806 57.15)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C61 (at 3.6195 0.0635) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 -0.0635) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F303)
    (at 99.187 35.3695)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C63 (at 1.397 1.5875) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F42B)
    (at 89.535 54.483 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C64 (at 1.651 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F32F)
    (at 98.806 40.513)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C66 (at 3.556 0.3175) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0.0635) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F25A)
    (at 89.662 36.8935 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C67 (at 1.143 1.4605 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F4A7)
    (at 98.425 51.435 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C69 (at -3.683 -0.127 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0.0635 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F416)
    (at 116.84 46.609 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C70 (at 0.762 -1.5875 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F4EF)
    (at 116.713 55.9435 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C72 (at -2.159 -1.5875 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F392)
    (at 111.6965 37.084 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C74 (at 3.7084 -0.3683 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F275)
    (at 93.98 44.6405 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C75 (at 1.2065 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F444)
    (at 93.98 61.6585 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C76 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5F418)
    (at 126.111 47.879 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C77 (at 0.889 -1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E2C1)
    (at 179.578 154.4955 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C78 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C78-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E2C7)
    (at 179.578 148.1455 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C79 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C79-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E2DB)
    (at 189.738 154.4955 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C80 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0.3175 0.0635 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C5E2E0)
    (at 189.738 148.1455 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C81 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.01uF (at -0.1905 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer Top) (tedit 58C5E2D4)
    (at 184.658 159.5755)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference L1 (at 0 -2.75) (layer F.SilkS))
    (fp_text value "1k ohm" (at 0.127 -0.127) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.9 0) (size 2.2 3) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C78-Pad1)"))
    (pad 2 smd rect (at 2.9 0) (size 2.2 3) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer Top) (tedit 58C5E2CC)
    (at 184.658 143.0655)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference L2 (at 0 -2.75) (layer F.SilkS))
    (fp_text value "1k ohm" (at 0.127 0.127) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.9 0) (size 2.2 3) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C79-Pad1)"))
    (pad 2 smd rect (at 2.9 0) (size 2.2 3) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C504BB)
    (at 76.2 153.67 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P1 (at -5.207 8.382 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 122 Vout1))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C504BF)
    (at 76.2 137.16 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P2 (at -5.207 8.255 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 123 Vout2))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C5E7A6)
    (at 76.2 120.65 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P3 (at -5.461 8.509 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 124 Vout3))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C5E7A9)
    (at 76.2 104.14 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P4 (at -5.334 8.255 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 125 Vout4))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C5E7AB)
    (at 76.2 87.63 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P5 (at -5.461 8.763 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 126 Vout5))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C5E7AE)
    (at 76.2 71.12 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P6 (at -5.461 8.636 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 127 Vout6))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C5E7B0)
    (at 76.2 54.61 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P7 (at -5.207 8.636 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 128 Vout7))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer Top) (tedit 58C5E7B3)
    (at 76.2 38.1 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference P8 (at -5.207 8.382 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 129 Vout8))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINHEAD1-3 (layer Top) (tedit 58C5E2BC)
    (at 172.593 153.8605 90)
    (fp_text reference P9 (at 2.59 -3.8 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 2.4765 2.4765 90) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C78-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C79-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-220-5_Pentawatt_Multiwatt-5_Vertical_StaggeredType1 (layer Top) (tedit 58C5E2EF)
    (at 197.358 146.2405)
    (descr "TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-1")
    (tags "TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5 staggered type-1")
    (fp_text reference U22 (at 3.4 -9.32) (layer F.SilkS))
    (fp_text value LT1963A (at 3.683 -5.6515) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 +15V))
    (pad 2 thru_hole oval (at 1.7 -3.7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 +15V))
    (pad 3 thru_hole oval (at 3.4 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 4 thru_hole oval (at 5.1 -3.7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 5 thru_hole oval (at 6.8 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model TO_SOT_Packages_THT.3dshapes/TO-220-5_Pentawatt_Multiwatt-5_Vertical_StaggeredType1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58C65052)
    (at 132.08 42.545)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 0 (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5F389)
    (at 107.315 38.1 270)
    (fp_text reference U19 (at 0.3175 3.8735 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 197 "Net-(U19-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 198 "Net-(U19-Pad2)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 192 "Net-(U18-Pad3)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 193 "Net-(U18-Pad4)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 106 ~RESET~8))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 108 ~CLR~8))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 110 ~LDAC~8))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 112 SDO8))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 116 SDIN8))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 118 SCLK8))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 199 ~SYNC~8))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 194 "Net-(U18-Pad16)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 195 "Net-(U18-Pad17)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 200 "Net-(U19-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5E883)
    (at 107.315 54.61 270)
    (fp_text reference U18 (at -0.381 3.937 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 191 "Net-(U18-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 188 "Net-(U17-Pad3)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 192 "Net-(U18-Pad3)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 193 "Net-(U18-Pad4)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 92 ~RESET~7))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 90 ~CLR~7))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 88 ~LDAC~7))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 86 SDO7))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 82 SDIN7))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 80 SCLK7))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 78 ~SYNC~7))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 194 "Net-(U18-Pad16)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 195 "Net-(U18-Pad17)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 196 "Net-(U18-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5E879)
    (at 107.315 71.12 270)
    (fp_text reference U14 (at -0.254 3.937 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 181 "Net-(U14-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 182 "Net-(U14-Pad2)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 175 "Net-(U13-Pad3)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 176 "Net-(U13-Pad4)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 38 ~RESET~6))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 40 ~CLR~6))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 42 ~LDAC~6))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 44 SDO6))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 48 SDIN6))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 50 SCLK6))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 52 ~SYNC~6))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 178 "Net-(U13-Pad16)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 179 "Net-(U13-Pad17)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 183 "Net-(U14-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5E855)
    (at 107.315 87.63 270)
    (fp_text reference U13 (at -0.127 4.064 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 174 "Net-(U13-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 171 "Net-(U12-Pad3)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 175 "Net-(U13-Pad3)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 176 "Net-(U13-Pad4)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 23 ~RESET~5))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 21 ~CLR~5))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 19 ~LDAC~5))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 17 SDO5))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 13 SDIN5))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 11 SCLK5))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 177 ~SYNC~5))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 178 "Net-(U13-Pad16)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 179 "Net-(U13-Pad17)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 180 "Net-(U13-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5D9DC)
    (at 107.315 104.14 270)
    (fp_text reference U8 (at 0.381 3.937 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 158 "Net-(U8-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 159 "Net-(U8-Pad2)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 153 "Net-(U10-Pad2)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 154 "Net-(U10-Pad1)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 39 ~RESET~4))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 41 ~CLR~4))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 43 ~LDAC~4))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 45 SDO4))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 49 SDIN4))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 51 SCLK4))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 53 ~SYNC~4))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 155 "Net-(U10-Pad7)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 156 "Net-(U10-Pad6)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 160 "Net-(U8-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5DDC7)
    (at 107.315 120.65 270)
    (fp_text reference U7 (at 0.1905 -4.318 270) (layer F.SilkS))
    (fp_text value AD5781 (at -0.127 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 152 "Net-(U7-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 149 "Net-(U6-Pad3)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 153 "Net-(U10-Pad2)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 154 "Net-(U10-Pad1)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 105 ~RESET~3))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 107 ~CLR~3))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 109 ~LDAC~3))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 111 SDO3))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 115 SDIN3))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 117 SCLK3))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 119 ~SYNC~3))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 155 "Net-(U10-Pad7)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 156 "Net-(U10-Pad6)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 157 "Net-(U7-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5D6D0)
    (at 107.315 137.16 270)
    (fp_text reference U3 (at 0.381 3.937 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 140 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 141 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 135 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 136 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 59 ~RESET~2))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 61 ~CLR~2))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 63 ~LDAC~2))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 65 SDO2))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 67 SDIN2))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 69 SCLK2))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 71 ~SYNC~2))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 137 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 138 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 142 "Net-(U3-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD5781ARUZ (layer Top) (tedit 58C5D5E2)
    (at 107.315 153.67 270)
    (fp_text reference U2 (at 0 -4.191 270) (layer F.SilkS))
    (fp_text value AD5781 (at 0 -0.254 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.8194 -2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 134 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 131 "Net-(U1-Pad3)"))
    (pad 3 smd rect (at -2.8194 -1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 135 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 136 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -2.8194 -0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at -2.8194 0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 58 ~RESET~1))
    (pad 7 smd rect (at -2.8194 0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 60 ~CLR~1))
    (pad 8 smd rect (at -2.8194 1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 62 ~LDAC~1))
    (pad 9 smd rect (at -2.8194 2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -2.8194 2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at 2.8194 2.925 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 64 SDO1))
    (pad 12 smd rect (at 2.8194 2.275002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 66 SDIN1))
    (pad 13 smd rect (at 2.8194 1.625001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 68 SCLK1))
    (pad 14 smd rect (at 2.8194 0.975002 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 70 ~SYNC~1))
    (pad 15 smd rect (at 2.8194 0.325001 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 16 smd rect (at 2.8194 -0.324998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 137 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 2.8194 -0.974999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 138 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 2.8194 -1.624998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 19 smd rect (at 2.8194 -2.274999 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 20 smd rect (at 2.8194 -2.924998 270) (size 1.4732 0.3556) (layers Top F.Paste F.Mask)
      (net 139 "Net-(U2-Pad20)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5E88A)
    (at 93.345 38.1 270)
    (fp_text reference U20 (at -0.635 -3.302 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 201 "Net-(U20-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 129 Vout8))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 198 "Net-(U19-Pad2)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 202 "Net-(U20-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 129 Vout8))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 203 "Net-(U20-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5E887)
    (at 93.345 54.61 270)
    (fp_text reference U17 (at 0.381 -3.302 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 187 "Net-(U17-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 128 Vout7))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 188 "Net-(U17-Pad3)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 189 "Net-(U17-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 128 Vout7))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 190 "Net-(U17-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5ED36)
    (at 93.345 71.12 270)
    (fp_text reference U15 (at -0.254 -3.3655 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 184 "Net-(U15-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 127 Vout6))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 182 "Net-(U14-Pad2)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 185 "Net-(U15-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 127 Vout6))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 186 "Net-(U15-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5EA61)
    (at 93.345 87.63 270)
    (fp_text reference U12 (at 0 -3.2385 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0.127 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 170 "Net-(U12-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 126 Vout5))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 171 "Net-(U12-Pad3)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 172 "Net-(U12-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 126 Vout5))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 173 "Net-(U12-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5DA7E)
    (at 93.345 104.14 270)
    (fp_text reference U9 (at -0.635 -3.429 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0.127 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 161 "Net-(U9-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 125 Vout4))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 159 "Net-(U8-Pad2)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 162 "Net-(U9-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 125 Vout4))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 163 "Net-(U9-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5DE52)
    (at 93.345 120.65 270)
    (fp_text reference U6 (at 0.3175 -3.302 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 148 "Net-(U6-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 124 Vout3))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 149 "Net-(U6-Pad3)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 150 "Net-(U6-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 124 Vout3))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 151 "Net-(U6-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5D759)
    (at 93.345 137.16 270)
    (fp_text reference U4 (at -0.762 -3.429 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0.127 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 143 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 123 Vout2))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 141 "Net-(U3-Pad2)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 144 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 123 Vout2))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 145 "Net-(U4-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD8675ARZ (layer Top) (tedit 58C5D5B5)
    (at 93.345 153.67 270)
    (fp_text reference U1 (at 0.508 -3.302 270) (layer F.SilkS))
    (fp_text value AD8675 (at 0.127 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 130 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 122 Vout1))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 131 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 132 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 122 Vout1))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 133 "Net-(U1-Pad8)"))
  )
  (module KiCad_DAC_Specific:AD688ARWZ (layer Top) (tedit 58C4E355)
    (at 150.368 148.1455 270)
    (fp_text reference U11 (at 0 6.35 270) (layer F.SilkS))
    (fp_text value AD688 (at 0 -6.35 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.52755 -4.445 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 146 +10Vref))
    (pad 2 smd rect (at -4.52755 -3.175 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 3 smd rect (at -4.52755 -1.905 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 146 +10Vref))
    (pad 4 smd rect (at -4.52755 -0.635 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 164 "Net-(U11-Pad4)"))
    (pad 5 smd rect (at -4.52755 0.635 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 165 "Net-(U11-Pad5)"))
    (pad 6 smd rect (at -4.52755 1.905 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 164 "Net-(U11-Pad4)"))
    (pad 7 smd rect (at -4.52755 3.175 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C32-Pad2)"))
    (pad 8 smd rect (at -4.52755 4.445 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 166 "Net-(U11-Pad13)"))
    (pad 9 smd rect (at 4.52755 4.445 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 10 smd rect (at 4.52755 3.175 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 167 "Net-(U11-Pad10)"))
    (pad 11 smd rect (at 4.52755 1.905 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 168 "Net-(U11-Pad11)"))
    (pad 12 smd rect (at 4.52755 0.635 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 169 "Net-(U11-Pad12)"))
    (pad 13 smd rect (at 4.52755 -0.635 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 166 "Net-(U11-Pad13)"))
    (pad 14 smd rect (at 4.52755 -1.905 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 147 -10Vref))
    (pad 15 smd rect (at 4.52755 -3.175 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 147 -10Vref))
    (pad 16 smd rect (at 4.52755 -4.445 270) (size 2.2987 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
  )
  (module KiCad_DAC_Specific:AD8676ARZ (layer Top) (tedit 58C5D69A)
    (at 120.65 145.415 270)
    (fp_text reference U5 (at -0.127 -3.556 270) (layer F.SilkS))
    (fp_text value AD8676 (at 0.127 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 136 "Net-(U2-Pad4)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 135 "Net-(U2-Pad3)"))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 146 +10Vref))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 147 -10Vref))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 138 "Net-(U2-Pad17)"))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 137 "Net-(U2-Pad16)"))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
  )
  (module KiCad_DAC_Specific:AD8676ARZ (layer Top) (tedit 58C5DD3F)
    (at 120.65 112.395 270)
    (fp_text reference U10 (at -0.1905 -3.302 270) (layer F.SilkS))
    (fp_text value AD8676 (at 0 -0.127 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 154 "Net-(U10-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 153 "Net-(U10-Pad2)"))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 146 +10Vref))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 147 -10Vref))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 156 "Net-(U10-Pad6)"))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 155 "Net-(U10-Pad7)"))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
  )
  (module KiCad_DAC_Specific:AD8676ARZ (layer Top) (tedit 58C5E860)
    (at 120.65 79.375 270)
    (fp_text reference U16 (at 0.508 -3.302 270) (layer F.SilkS))
    (fp_text value AD8676 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 176 "Net-(U13-Pad4)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 175 "Net-(U13-Pad3)"))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 146 +10Vref))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 147 -10Vref))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 179 "Net-(U13-Pad17)"))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 178 "Net-(U13-Pad16)"))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
  )
  (module KiCad_DAC_Specific:AD8676ARZ (layer Top) (tedit 58C5E891)
    (at 120.65 46.355 270)
    (fp_text reference U21 (at -0.889 -3.302 270) (layer F.SilkS))
    (fp_text value AD8676 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 193 "Net-(U18-Pad4)"))
    (pad 2 smd rect (at -2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 192 "Net-(U18-Pad3)"))
    (pad 3 smd rect (at -2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 146 +10Vref))
    (pad 4 smd rect (at -2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (pad 5 smd rect (at 2.3622 1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 147 -10Vref))
    (pad 6 smd rect (at 2.3622 0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 195 "Net-(U18-Pad17)"))
    (pad 7 smd rect (at 2.3622 -0.635 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 194 "Net-(U18-Pad16)"))
    (pad 8 smd rect (at 2.3622 -1.905 270) (size 2.1844 0.5588) (layers Top F.Paste F.Mask)
      (net 4 +15V))
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5E305)
    (at 142.748 148.1455 90)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C32 (at 0 -2.55 90) (layer F.SilkS))
    (fp_text value 10uF (at 0.0635 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 90) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 90) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C32-Pad2)"))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5E2E9)
    (at 204.978 154.4955 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C83 (at 0 -2.55 270) (layer F.SilkS))
    (fp_text value 10uF (at -0.3175 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5E2E4)
    (at 196.723 154.4955 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C82 (at 0 -2.55 270) (layer F.SilkS))
    (fp_text value 10uF (at -0.127 0.0635 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5E29B)
    (at 113.919 36.5125 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C73 (at 0 -2.55 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 0.127 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5F4DA)
    (at 113.6015 54.6735 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C71 (at 3.4925 1.651 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5F497)
    (at 98.425 49.022 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C68 (at -4.2545 -0.0635 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5F326)
    (at 98.7425 42.672 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C65 (at -4.1275 -0.6985 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.0635 0.1905 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5F2A0)
    (at 98.806 33.147 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C62 (at -4.064 -0.4445 180) (layer F.SilkS))
    (fp_text value 10uF (at 0.0635 0.0635 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5F465)
    (at 98.9965 59.309 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C60 (at -4.1275 -0.3175 180) (layer F.SilkS))
    (fp_text value 10uF (at 0.127 0.0635 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5EC7A)
    (at 113.919 69.5325 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C55 (at 0 -1.9685 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5EBD6)
    (at 113.8555 87.757 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C53 (at 3.175 1.651 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5E2F9)
    (at 159.258 158.9405 90)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C51 (at 0 -2.55 90) (layer F.SilkS))
    (fp_text value 10uF (at 0.1905 0.127 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 90) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 90) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5EB36)
    (at 98.4885 82.1055 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C49 (at -4.1275 -0.127 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.1905 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5ECD2)
    (at 98.806 75.5015 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C46 (at -4.1275 -0.5715 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5ECF4)
    (at 98.806 66.2305 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C42 (at -4.318 -0.1905 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5EA2B)
    (at 99.187 92.329 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C40 (at -4.191 -0.1905 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D9EF)
    (at 113.919 102.616 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C35 (at 0.127 -2.032 270) (layer F.SilkS))
    (fp_text value 10uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5DDEE)
    (at 113.8555 120.904 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C33 (at 3.2385 1.524 270) (layer F.SilkS))
    (fp_text value 10uF (at 0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5E30B)
    (at 157.988 138.6205 90)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C30 (at 0 -2.55 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 0.1905 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 90) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 90) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5DE98)
    (at 98.298 114.935 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C27 (at -4.445 -0.127 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.1905 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5DAC1)
    (at 98.7425 108.6485 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C24 (at -4.1275 -0.5715 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.127 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D860)
    (at 98.806 99.187 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C21 (at -1.778 -3.937 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.254 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5DE44)
    (at 99.1235 125.2855 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C19 (at -4.1275 -0.254 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.127 -0.0635 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D6BB)
    (at 113.919 135.636 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C14 (at -0.127 -2.032 270) (layer F.SilkS))
    (fp_text value 10uF (at -0.381 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D5F6)
    (at 113.665 153.67 270)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C12 (at 3.175 0.635 540) (layer F.SilkS))
    (fp_text value 10uF (at -0.127 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.375 0 270) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 3 -15V))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D5D6)
    (at 98.425 147.955 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C9 (at -0.254 1.651 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D761)
    (at 98.7425 141.7955 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C6 (at -3.683 -0.254 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.254 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D753)
    (at 98.806 132.334 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C3 (at -3.683 -0.127 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.254 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer Top) (tedit 58C5D598)
    (at 99.187 158.369 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C1 (at -3.683 0 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.127 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58C6DBCA)
    (at 132.08 64.135)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 0 (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58C6DBD7)
    (at 132.08 96.52)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 0 (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58C6DBD0)
    (at 132.08 128.27)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 0 (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58C6DBDD)
    (at 211.582 133.35 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 0 (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer Top) (tedit 58D2E2A7)
    (at 222.885 156.845)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58D21EF4)
    (at 176.022 125.095)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C84 (at 3.81 0.127) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58D2223C)
    (at 164.6555 123.6345 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C85 (at 4.064 -0.254 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 208 "Net-(C85-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 209 "Net-(C85-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58D222B8)
    (at 171.8945 123.698 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C86 (at -0.9525 1.524 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 210 "Net-(C86-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0805 (layer Top) (tedit 58D2219F)
    (at 171.196 119.4435 180)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at 0 1.6 180) (layer F.SilkS))
    (fp_text value 1n4148 (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0 180) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.05 0 180) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 208 "Net-(C85-Pad1)"))
  )
  (module Diodes_SMD:D_0805 (layer Top) (tedit 58D222BD)
    (at 167.5765 122.4915)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D2 (at 1.143 -1.524) (layer F.SilkS))
    (fp_text value 1n4148 (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 208 "Net-(C85-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
  )
  (module Connectors:SMA_THT_Jack_Straight (layer Top) (tedit 58D22394)
    (at 217.2335 117.2845)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference P10 (at -5.715 2.7305) (layer F.SilkS))
    (fp_text value Trigger (at 4.6355 -0.0635 90) (layer F.SilkS))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 212 "Net-(P10-Pad1)"))
  )
  (module Connectors:SMA_THT_Jack_Straight (layer Top) (tedit 58D223C6)
    (at 189.1665 122.2375)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference P11 (at -5.842 2.794) (layer F.SilkS))
    (fp_text value "Ext. Clock IN" (at 4.6355 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 209 "Net-(C85-Pad2)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58D21B8A)
    (at 217.2335 108.585 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.2385 0 90) (layer F.SilkS))
    (fp_text value 17 (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 212 "Net-(P10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 98 "Net-(FPGA1-PadB14)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58D21B87)
    (at 213.6775 108.585 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.302 0 270) (layer F.SilkS))
    (fp_text value 33 (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 98 "Net-(FPGA1-PadB14)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58D22241)
    (at 168.402 125.0315)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 1.4605 1.9685) (layer F.SilkS))
    (fp_text value 50 (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 209 "Net-(C85-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad_DAC_Specific:LTC6957HMS-3 (layer Top) (tedit 58D2191D)
    (at 177.292 121.285)
    (fp_text reference U23 (at 0 -2.921) (layer F.SilkS))
    (fp_text value LTC6957-3 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.1844 -1.6256) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 2 smd rect (at -2.1844 -0.97536) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -2.1844 -0.32512) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 208 "Net-(C85-Pad1)"))
    (pad 4 smd rect (at -2.1844 0.32512) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 210 "Net-(C86-Pad1)"))
    (pad 5 smd rect (at -2.1844 0.97536) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 6 smd rect (at -2.1844 1.6256) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at 2.1844 1.6256) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 8 smd rect (at 2.1844 0.97536) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
    (pad 9 smd rect (at 2.1844 0.32512) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 213 "Net-(U23-Pad9)"))
    (pad 10 smd rect (at 2.1844 -0.32512) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 211 "Net-(JP1-Pad1)"))
    (pad 11 smd rect (at 2.1844 -0.97536) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 1 +3V3))
    (pad 12 smd rect (at 2.1844 -1.6256) (size 1.397 0.4318) (layers Top F.Paste F.Mask)
      (net 204 GNDD))
  )
  (module KiCad_DAC_Specific:Jumper-2 (layer Top) (tedit 58D21E76)
    (at 170.815 116.84 180)
    (fp_text reference JP1 (at 0.254 2.032 180) (layer F.SilkS))
    (fp_text value Jumper (at 0 0 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.51 1.51) (drill 1) (layers *.Cu *.Mask)
      (net 211 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.51 1.51) (drill 1) (layers *.Cu *.Mask)
      (net 207 "/FPGAPinout/External Clock Input/CLK"))
  )
  (module KiCad_DAC_Specific:XEM7001 (layer Top) (tedit 58D2E78F)
    (at 185.039 80.264)
    (fp_text reference FPGA1 (at -34.29 -29.21) (layer F.SilkS))
    (fp_text value XEM7001 (at -34.29 -30.48) (layer F.SilkS))
    (fp_text user JP3 (at 26.67 17.78) (layer F.SilkS))
    (fp_text user JP1 (at 17.78 -10.16) (layer F.SilkS))
    (fp_text user JP2 (at -24.13 -17.78) (layer F.SilkS))
    (pad GNDi thru_hole circle (at -34.29 21.59) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 204 GNDD) (zone_connect 0))
    (pad GNDi thru_hole circle (at 36.83 21.59) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 204 GNDD) (zone_connect 0))
    (pad GNDi thru_hole circle (at 36.83 -21.59) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 204 GNDD) (zone_connect 0))
    (pad GNDa thru_hole circle (at 31.75 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(FPGA1-PadGNDa)"))
    (pad GNDb thru_hole circle (at 31.75 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(FPGA1-PadGNDb)"))
    (pad CLK1 thru_hole circle (at 29.21 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 205 "Net-(FPGA1-PadCLK1)"))
    (pad P10 thru_hole circle (at 29.21 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(FPGA1-PadP10)"))
    (pad J1 thru_hole circle (at 26.67 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 110 ~LDAC~8))
    (pad J3 thru_hole circle (at 26.67 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(FPGA1-PadJ3)"))
    (pad K2 thru_hole circle (at 24.13 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 108 ~CLR~8))
    (pad K1 thru_hole circle (at 24.13 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(FPGA1-PadK1)"))
    (pad 3.3A thru_hole circle (at 21.59 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(FPGA1-Pad3.3A)"))
    (pad 3.3B thru_hole circle (at 21.59 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(FPGA1-Pad3.3B)"))
    (pad L2 thru_hole circle (at 19.05 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 106 ~RESET~8))
    (pad K3 thru_hole circle (at 19.05 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(FPGA1-PadK3)"))
    (pad L3 thru_hole circle (at 16.51 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 ~SYNC~8))
    (pad M1 thru_hole circle (at 16.51 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(FPGA1-PadM1)"))
    (pad M2 thru_hole circle (at 13.97 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 118 SCLK8))
    (pad L4 thru_hole circle (at 13.97 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(FPGA1-PadL4)"))
    (pad M4 thru_hole circle (at 11.43 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 116 SDIN8))
    (pad N1 thru_hole circle (at 11.43 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(FPGA1-PadN1)"))
    (pad GNDc thru_hole circle (at 8.89 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(FPGA1-PadGNDc)"))
    (pad GNDd thru_hole circle (at 8.89 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(FPGA1-PadGNDd)"))
    (pad N2 thru_hole circle (at 6.35 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 112 SDO8))
    (pad N3 thru_hole circle (at 6.35 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(FPGA1-PadN3)"))
    (pad P1 thru_hole circle (at 3.81 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(FPGA1-PadP1)"))
    (pad R1 thru_hole circle (at 3.81 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(FPGA1-PadR1)"))
    (pad R2 thru_hole circle (at 1.27 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(FPGA1-PadR2)"))
    (pad P3 thru_hole circle (at 1.27 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(FPGA1-PadP3)"))
    (pad T2 thru_hole circle (at -1.27 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(FPGA1-PadT2)"))
    (pad R3 thru_hole circle (at -1.27 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(FPGA1-PadR3)"))
    (pad T3 thru_hole circle (at -3.81 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(FPGA1-PadT3)"))
    (pad N4 thru_hole circle (at -3.81 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(FPGA1-PadN4)"))
    (pad GNDe thru_hole circle (at -6.35 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(FPGA1-PadGNDe)"))
    (pad GNDf thru_hole circle (at -6.35 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(FPGA1-PadGNDf)"))
    (pad P4 thru_hole circle (at -8.89 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 88 ~LDAC~7))
    (pad T4 thru_hole circle (at -8.89 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 SDO6))
    (pad P5 thru_hole circle (at -11.43 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 90 ~CLR~7))
    (pad N6 thru_hole circle (at -11.43 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 SDIN6))
    (pad R5 thru_hole circle (at -13.97 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 92 ~RESET~7))
    (pad P8 thru_hole circle (at -13.97 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 SCLK6))
    (pad T5 thru_hole circle (at -16.51 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 78 ~SYNC~7))
    (pad R6 thru_hole circle (at -16.51 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 52 ~SYNC~6))
    (pad 3.3C thru_hole circle (at -19.05 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 "Net-(FPGA1-Pad3.3C)"))
    (pad 3.3D thru_hole circle (at -19.05 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 "Net-(FPGA1-Pad3.3D)"))
    (pad T9 thru_hole circle (at -21.59 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 80 SCLK7))
    (pad R7 thru_hole circle (at -21.59 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 ~RESET~6))
    (pad T7 thru_hole circle (at -24.13 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 82 SDIN7))
    (pad R8 thru_hole circle (at -24.13 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 ~CLR~6))
    (pad T8 thru_hole circle (at -26.67 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 86 SDO7))
    (pad T10 thru_hole circle (at -26.67 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 ~LDAC~6))
    (pad GNDg thru_hole circle (at -29.21 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 54 "Net-(FPGA1-PadGNDg)"))
    (pad GNDh thru_hole circle (at -29.21 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 "Net-(FPGA1-PadGNDh)"))
    (pad 3.3E thru_hole circle (at 16.51 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 56 "Net-(FPGA1-Pad3.3E)"))
    (pad 3.3F thru_hole circle (at 19.05 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 "Net-(FPGA1-Pad3.3F)"))
    (pad H1 thru_hole circle (at 16.51 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 ~LDAC~4))
    (pad H2 thru_hole circle (at 19.05 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 ~LDAC~5))
    (pad G1 thru_hole circle (at 16.51 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 ~CLR~4))
    (pad G2 thru_hole circle (at 19.05 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 ~CLR~5))
    (pad F2 thru_hole circle (at 16.51 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 ~RESET~4))
    (pad E1 thru_hole circle (at 19.05 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 ~RESET~5))
    (pad E2 thru_hole circle (at 16.51 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 ~SYNC~4))
    (pad D1 thru_hole circle (at 19.05 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 177 ~SYNC~5))
    (pad C1 thru_hole circle (at 16.51 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 51 SCLK4))
    (pad C2 thru_hole circle (at 19.05 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 SCLK5))
    (pad B1 thru_hole circle (at 16.51 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 SDIN4))
    (pad B2 thru_hole circle (at 19.05 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 SDIN5))
    (pad A2 thru_hole circle (at 16.51 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 SDO4))
    (pad A3 thru_hole circle (at 19.05 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 SDO5))
    (pad D4 thru_hole circle (at 16.51 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 72 "Net-(FPGA1-PadD4)"))
    (pad C4 thru_hole circle (at 19.05 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 73 "Net-(FPGA1-PadC4)"))
    (pad GNDi thru_hole circle (at 16.51 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 204 GNDD))
    (pad GNDj thru_hole circle (at 19.05 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 74 "Net-(FPGA1-PadGNDj)"))
    (pad GNDk thru_hole circle (at 31.75 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 75 "Net-(FPGA1-PadGNDk)"))
    (pad GNDl thru_hole circle (at 31.75 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 76 "Net-(FPGA1-PadGNDl)"))
    (pad A8 thru_hole circle (at 29.21 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 77 "Net-(FPGA1-PadA8)"))
    (pad D9 thru_hole circle (at 29.21 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 64 SDO1))
    (pad C8 thru_hole circle (at 26.67 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 79 "Net-(FPGA1-PadC8)"))
    (pad D10 thru_hole circle (at 26.67 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 SDIN1))
    (pad A9 thru_hole circle (at 24.13 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 81 "Net-(FPGA1-PadA9)"))
    (pad C9 thru_hole circle (at 24.13 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 68 SCLK1))
    (pad 3.3G thru_hole circle (at 21.59 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 83 "Net-(FPGA1-Pad3.3G)"))
    (pad 3.3H thru_hole circle (at 21.59 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 84 "Net-(FPGA1-Pad3.3H)"))
    (pad B9 thru_hole circle (at 19.05 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 85 "Net-(FPGA1-PadB9)"))
    (pad A10 thru_hole circle (at 19.05 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 70 ~SYNC~1))
    (pad B10 thru_hole circle (at 16.51 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 87 "Net-(FPGA1-PadB10)"))
    (pad C11 thru_hole circle (at 16.51 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 ~RESET~1))
    (pad B12 thru_hole circle (at 13.97 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 89 "Net-(FPGA1-PadB12)"))
    (pad A12 thru_hole circle (at 13.97 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 60 ~CLR~1))
    (pad C12 thru_hole circle (at 11.43 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 91 "Net-(FPGA1-PadC12)"))
    (pad F13 thru_hole circle (at 11.43 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 62 ~LDAC~1))
    (pad GNDn thru_hole circle (at 8.89 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 93 "Net-(FPGA1-PadGNDn)"))
    (pad GNDm thru_hole circle (at 8.89 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 94 "Net-(FPGA1-PadGNDm)"))
    (pad A13 thru_hole circle (at 6.35 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 95 "Net-(FPGA1-PadA13)"))
    (pad A14 thru_hole circle (at 6.35 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 96 "Net-(FPGA1-PadA14)"))
    (pad E13 thru_hole circle (at 3.81 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 "Net-(FPGA1-PadE13)"))
    (pad B14 thru_hole circle (at 3.81 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 98 "Net-(FPGA1-PadB14)"))
    (pad C14 thru_hole circle (at 1.27 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 99 "Net-(FPGA1-PadC14)"))
    (pad A15 thru_hole circle (at 1.27 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 100 "Net-(FPGA1-PadA15)"))
    (pad B15 thru_hole circle (at -1.27 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 101 "Net-(FPGA1-PadB15)"))
    (pad B16 thru_hole circle (at -1.27 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 102 "Net-(FPGA1-PadB16)"))
    (pad C16 thru_hole circle (at -3.81 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 109 ~LDAC~3))
    (pad D15 thru_hole circle (at -3.81 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 65 SDO2))
    (pad GNDo thru_hole circle (at -6.35 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 103 "Net-(FPGA1-PadGNDo)"))
    (pad GNDp thru_hole circle (at -6.35 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 104 "Net-(FPGA1-PadGNDp)"))
    (pad D16 thru_hole circle (at -8.89 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 ~CLR~3))
    (pad D14 thru_hole circle (at -8.89 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 SDIN2))
    (pad E16 thru_hole circle (at -11.43 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 105 ~RESET~3))
    (pad E15 thru_hole circle (at -11.43 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 SCLK2))
    (pad G15 thru_hole circle (at -13.97 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 119 ~SYNC~3))
    (pad F14 thru_hole circle (at -13.97 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 71 ~SYNC~2))
    (pad H14 thru_hole circle (at -16.51 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 117 SCLK3))
    (pad G16 thru_hole circle (at -16.51 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 ~RESET~2))
    (pad 3.3I thru_hole circle (at -19.05 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 113 "Net-(FPGA1-Pad3.3I)"))
    (pad 3.3J thru_hole circle (at -19.05 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 114 "Net-(FPGA1-Pad3.3J)"))
    (pad H13 thru_hole circle (at -21.59 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 115 SDIN3))
    (pad H16 thru_hole circle (at -21.59 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 ~CLR~2))
    (pad F15 thru_hole circle (at -24.13 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 111 SDO3))
    (pad G14 thru_hole circle (at -24.13 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 63 ~LDAC~2))
    (pad E12 thru_hole circle (at -26.67 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 207 "/FPGAPinout/External Clock Input/CLK"))
    (pad CLK2 thru_hole circle (at -26.67 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 206 "Net-(FPGA1-PadCLK2)"))
    (pad GNDq thru_hole circle (at -29.21 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 120 "Net-(FPGA1-PadGNDq)"))
    (pad GNDr thru_hole circle (at -29.21 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 121 "Net-(FPGA1-PadGNDr)"))
    (pad GNDi thru_hole circle (at -34.29 -21.59) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 204 GNDD) (zone_connect 0))
  )
  (gr_text "Scott Designs\nOcta 18 Bit DAC\nXEM7001 FPGA Control\nREV000" (at 197.485 38.1) (layer F.SilkS))
  (dimension 136.525 (width 0.3) (layer Eco1.User)
    (gr_text "5.3750 in" (at 234.395 95.5675 270) (layer Eco1.User))
    (feature1 (pts (xy 229.235 163.83) (xy 235.745 163.83)))
    (feature2 (pts (xy 229.235 27.305) (xy 235.745 27.305)))
    (crossbar (pts (xy 233.045 27.305) (xy 233.045 163.83)))
    (arrow1a (pts (xy 233.045 163.83) (xy 232.458579 162.703496)))
    (arrow1b (pts (xy 233.045 163.83) (xy 233.631421 162.703496)))
    (arrow2a (pts (xy 233.045 27.305) (xy 232.458579 28.431504)))
    (arrow2b (pts (xy 233.045 27.305) (xy 233.631421 28.431504)))
  )
  (dimension 160.02 (width 0.3) (layer Eco1.User)
    (gr_text "6.3000 in" (at 149.225 22.78) (layer Eco1.User))
    (feature1 (pts (xy 229.235 27.305) (xy 229.235 21.43)))
    (feature2 (pts (xy 69.215 27.305) (xy 69.215 21.43)))
    (crossbar (pts (xy 69.215 24.13) (xy 229.235 24.13)))
    (arrow1a (pts (xy 229.235 24.13) (xy 228.108496 24.716421)))
    (arrow1b (pts (xy 229.235 24.13) (xy 228.108496 23.543579)))
    (arrow2a (pts (xy 69.215 24.13) (xy 70.341504 24.716421)))
    (arrow2b (pts (xy 69.215 24.13) (xy 70.341504 23.543579)))
  )
  (gr_line (start 229.235 163.83) (end 69.215 163.83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 229.235 163.195) (end 229.235 163.83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 229.235 27.305) (end 229.235 163.195) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.215 27.305) (end 229.235 27.305) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.215 27.305) (end 69.215 163.83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GNDA) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.175 127) (xy 138.43 135.255) (xy 227.965 135.255) (xy 227.965 162.56) (xy 70.485 162.56)
        (xy 70.485 28.575) (xy 130.175 28.575)
      )
    )
  )
  (zone (net 204) (net_name GNDD) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 227.965 131.445) (xy 139.7 131.445) (xy 133.985 125.73) (xy 133.985 28.575) (xy 227.965 28.575)
      )
    )
  )
)
