(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.5448)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" mixed)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" mixed)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 0.2)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.991)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "core")
				(color "FR4 natural")
				(thickness 0.202)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0152)
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 75 75)
		(pcbplotparams
			(layerselection 0x00010e8_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plot/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(J2-RF)")
	(net 3 "Net-(J1-RF)")
	(net 4 "Net-(J11-RF)")
	(net 5 "+5V")
	(net 6 "/5V0_FIL")
	(net 7 "Net-(U1-VRMS)")
	(net 8 "Net-(U1-VENV)")
	(net 9 "unconnected-(U1-NC-Pad12)")
	(net 10 "Net-(U1-RFIN)")
	(net 11 "Net-(J4-Pin_3)")
	(net 12 "Net-(U1-FLT2)")
	(net 13 "unconnected-(U1-FLT3-Pad1)")
	(net 14 "unconnected-(U1-NC-Pad7)")
	(net 15 "unconnected-(U1-NC-Pad6)")
	(net 16 "Net-(U1-FLT4)")
	(net 17 "unconnected-(U1-NC-Pad13)")
	(net 18 "unconnected-(U1-NC-Pad8)")
	(net 19 "Net-(U1-FLT1)")
	(net 20 "Net-(J4-Pin_4)")
	(net 21 "Net-(U1-EREF)")
	(net 22 "Net-(J4-Pin_5)")
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 204.4 104.5 90)
		(property "Reference" "R2"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/5V0_FIL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+5V")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 207.4 106.2 -90)
		(property "Reference" "R3"
			(at 0 -2.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(J4-Pin_5)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U1-VRMS)")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 199.4 108.5 90)
		(property "Reference" "R1"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(J2-RF)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 201.1 109.2 180)
		(property "Reference" "C1"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6200pf"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-RFIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(J2-RF)")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 211.1 112.9 90)
		(property "Reference" "R6"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(J1-RF)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(J4-Pin_4)")
			(pintype "passive")
		)
	)
	(footprint "b_all:QFN-16-1EP_3x3mm_P0.5mm_EP.9x.9mm"
		(layer "F.Cu")
		(at 204.7 109.5)
		(descr "QFN, 16 Pin (https://www.nxp.com/docs/en/package-information/98ASA00525D.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1"
			(at 0.7 3 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:QFN-16-1EP_3x3mm_P0.5mm_EP.9x.9mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "ADL5511"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0)
			(size 0.77 0.77)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.5125 -0.75)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "unconnected-(U1-FLT3-Pad1)")
			(pinfunction "FLT3")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5125 -0.25)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U1-RFIN)")
			(pinfunction "RFIN")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.5125 0.25)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U1-FLT1)")
			(pinfunction "FLT1")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -1.5125 0.75)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/5V0_FIL")
			(pinfunction "ENBL")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -0.75 1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "COMM")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -0.25 1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "unconnected-(U1-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at 0.25 1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "unconnected-(U1-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "8" smd roundrect
			(at 0.75 1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "unconnected-(U1-NC-Pad8)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "9" smd roundrect
			(at 1.5125 0.75)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-EREF)")
			(pinfunction "EREF")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at 1.5125 0.25)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-VENV)")
			(pinfunction "VENV")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 1.5125 -0.25)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U1-VRMS)")
			(pinfunction "VRMS")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 1.5125 -0.75)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "unconnected-(U1-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "13" smd roundrect
			(at 0.75 -1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "unconnected-(U1-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at 0.25 -1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U1-FLT4)")
			(pinfunction "FLT4")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -0.25 -1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/5V0_FIL")
			(pinfunction "VPOS")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -0.75 -1.5125)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U1-FLT2)")
			(pinfunction "FLT2")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 0.93 0.93)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 208.3 109.9 180)
		(property "Reference" "R5"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(J11-RF)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-VENV)")
			(pintype "passive")
		)
	)
	(footprint "b_all:SMA_Edge_062_142_0701"
		(layer "F.Cu")
		(at 195.7 109.1 90)
		(property "Reference" "J2"
			(at -2.2 1.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Edge"
			(at 0.2 -1.3 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SMA_Edge_062_142_0701"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 0 -1.4 90)
			(size 0.5 2.6)
			(layers "F.Cu" "F.Mask")
			(net 2 "Net-(J2-RF)")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2418 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at -4.2 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2418 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(model "${T_LIBS}/3d/t_RF_conn/SMA_Edge.wrl"
			(offset
				(xyz 0 3.174999952 0.3809999943)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 270 0 90)
			)
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 205.9 106 90)
		(property "Reference" "C6"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(U1-FLT4)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/5V0_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 209.6 105.7 180)
		(property "Reference" "R7"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(J11-RF)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(J4-Pin_3)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 209 108.1 -90)
		(property "Reference" "C9"
			(at 0 -2.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNI"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(J11-RF)")
			(pintype "passive")
		)
	)
	(footprint "b_all:SMA_Edge_062"
		(layer "F.Cu")
		(at 215.493 103 -90)
		(property "Reference" "J11"
			(at -4.445 4.064 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Edge"
			(at 0.2 -1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SMA_Edge_062"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 -0.1 270)
			(size 1.4986 5.2)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(J11-RF)")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2418 -0.1 270)
			(size 1.6002 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2418 -0.1 270)
			(size 1.6002 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(model "${T_LIBS}/3d/t_RF_conn/SMA_Edge.wrl"
			(offset
				(xyz 0 3.174999952 0.3809999943)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 270 0 90)
			)
		)
	)
	(footprint "Connector_PinSocket_2.00mm:PinSocket_1x05_P2.00mm_Vertical_SMD_Pin1Left"
		(layer "F.Cu")
		(at 203.6 100 90)
		(descr "surface-mounted straight socket strip, 1x05, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated")
		(tags "Surface mounted socket strip SMD 1x05 2.00mm single row style1 pin1 left")
		(property "Reference" "J4"
			(at 0 -6.8 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 6.8 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.00mm:PinSocket_1x05_P2.00mm_Vertical_SMD_Pin1Left"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.6 -4 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.6 -2 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.6 0 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.6 2 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.6 4 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x05_P2.00mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 202.4 104.7)
		(property "Reference" "C2"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/5V0_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 201.9 111 90)
		(property "Reference" "C3"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNI"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(U1-FLT1)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 208.3 112.5)
		(property "Reference" "C7"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNI"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(J1-RF)")
			(pintype "passive")
		)
	)
	(footprint "b_all:SMA_Edge_062"
		(layer "F.Cu")
		(at 215.493 116 -90)
		(property "Reference" "J1"
			(at 2 -0.007 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Edge"
			(at 0.2 -1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SMA_Edge_062"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 -0.1 270)
			(size 1.4986 5.2)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(J1-RF)")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2418 -0.1 270)
			(size 1.6002 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2418 -0.1 270)
			(size 1.6002 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(model "${T_LIBS}/3d/t_RF_conn/SMA_Edge.wrl"
			(offset
				(xyz 0 3.174999952 0.3809999943)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 270 0 90)
			)
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 208.3 111.2 180)
		(property "Reference" "R4"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Detector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(J1-RF)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U1-EREF)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 206.8 104)
		(property "Reference" "C8"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNI"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(J4-Pin_5)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 201.7 106.7 90)
		(property "Reference" "C5"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNI"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-FLT2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/5V0_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 203.7 106.4)
		(property "Reference" "C4"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6200pf"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/5V0_FIL")
			(pintype "passive")
		)
	)
	(gr_line
		(start 192.6 122)
		(end 192.6 96.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.5 122)
		(end 192.6 122)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.6 96.7)
		(end 218.5 96.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.5 96.7)
		(end 218.5 122)
		(layer "Edge.Cuts")
	)
	(gr_text "Detector"
		(at 196.15 116.3 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193 97) (xy 193 121.5) (xy 218 121.5) (xy 218 97)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193 97) (xy 193 121.5) (xy 218 121.5) (xy 218 97)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.153)
		)
		(min_thickness 0.153)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 218.1 121.6) (xy 192.9 121.6) (xy 192.9 97.2) (xy 218.1 97.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.22)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 213.8 79.3) (xy 201.6 79.3) (xy 201.6 76.3) (xy 213.8 76.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.22)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 205 121.9) (xy 192.8 121.9) (xy 192.8 118.9) (xy 205 118.9)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.22)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 259.2 79.6) (xy 247 79.6) (xy 247 76.6) (xy 259.2 76.6)
			)
		)
	)
)