(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 533)
    (zones 0)
    (modules 29)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.762)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3048)
    (uvia_drill 0.1016)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 113.03)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 +12V)
  (net 4 /Supply)
  (net 5 /Sens_A)
  (net 6 /Sens_B)
  (net 7 /Sens_C)
  (net 8 /g_C_L)
  (net 9 /SH_C)
  (net 10 /g_C_H)
  (net 11 /g_B_L)
  (net 12 /SH_B)
  (net 13 /g_B_H)
  (net 14 /g_A_L)
  (net 15 /SH_A)
  (net 16 /g_A_H)
  (net 17 "Net-(Q1-Pad1)")
  (net 18 "Net-(Q2-Pad1)")
  (net 19 "Net-(Q3-Pad1)")
  (net 20 "Net-(Q4-Pad1)")
  (net 21 "Net-(Q5-Pad1)")
  (net 22 "Net-(Q6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net +12V)
    (add_net +BATT)
    (add_net /SH_A)
    (add_net /SH_B)
    (add_net /SH_C)
    (add_net /Sens_A)
    (add_net /Sens_B)
    (add_net /Sens_C)
    (add_net /Supply)
    (add_net /g_A_H)
    (add_net /g_A_L)
    (add_net /g_B_H)
    (add_net /g_B_L)
    (add_net /g_C_H)
    (add_net /g_C_L)
    (add_net GND)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 152.4 68.58 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 157.48 109.22 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5B301BBE)
    (at 180.34 108.585 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -4.445 0 -90) (layer B.SilkS))
    (fp_text value C (at 0 -2.28) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 +BATT))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5B301BBE)
    (at 180.34 93.345 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -4.445 0 -90) (layer B.SilkS))
    (fp_text value C (at 0 -2.28) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer B.Cu) (tedit 5B301BBE)
    (at 180.34 78.105 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -4.445 0 -90) (layer B.SilkS))
    (fp_text value C (at 0 -2.28) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 +BATT))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 173.355 101.6 225)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C4 (at -5.837166 1.347038 45) (layer F.SilkS))
    (fp_text value CP1 (at 3.75 9.25 45) (layer F.Fab))
    (fp_text user %R (at 3.75 0 45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 225) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 7.5 0 225) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FK_Parts:D2Pak (layer F.Cu) (tedit 0)
    (at 188.0362 100.965 90)
    (fp_text reference Q1 (at 0 0 90) (layer F.SilkS))
    (fp_text value MOSFET_D2Pak (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at -5.08 8.1534 90) (layer F.SilkS))
    (fp_text user * (at -3.81 4.572 90) (layer F.Fab))
    (fp_text user * (at -3.81 4.572 90) (layer F.Fab))
    (fp_text user * (at -5.08 8.1534 90) (layer F.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 smd rect (at 0 -3.2512 90) (size 10.7188 7.5692) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 7 smd rect (at 3.81 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 15 /SH_A))
    (pad 6 smd rect (at 2.54 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 15 /SH_A))
    (pad 5 smd rect (at 1.27 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 15 /SH_A))
    (pad 3 smd rect (at -1.27 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 15 /SH_A))
    (pad 2 smd rect (at -2.54 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 15 /SH_A))
    (pad 1 smd rect (at -3.81 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q1-Pad1)"))
  )
  (module FK_Parts:D2Pak (layer B.Cu) (tedit 0)
    (at 190.5 100.965 90)
    (fp_text reference Q2 (at 0 0 270) (layer B.SilkS))
    (fp_text value MOSFET_D2Pak (at 0 0 270) (layer B.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User))
    (fp_text user * (at -5.08 -8.1534 270) (layer B.SilkS))
    (fp_text user * (at -3.81 -4.572 270) (layer B.Fab))
    (fp_text user * (at -3.81 -4.572 270) (layer B.Fab))
    (fp_text user * (at -5.08 -8.1534 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -2.54 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.27 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.27 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.54 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.81 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 3.2512 90) (size 10.7188 7.5692) (layers B.Cu B.Paste B.Mask)
      (net 15 /SH_A))
  )
  (module FK_Parts:D2Pak (layer F.Cu) (tedit 0)
    (at 188.0362 85.725 90)
    (fp_text reference Q3 (at 0 0 90) (layer F.SilkS))
    (fp_text value MOSFET_D2Pak (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at -5.08 8.1534 90) (layer F.SilkS))
    (fp_text user * (at -3.81 4.572 90) (layer F.Fab))
    (fp_text user * (at -3.81 4.572 90) (layer F.Fab))
    (fp_text user * (at -5.08 8.1534 90) (layer F.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 smd rect (at 0 -3.2512 90) (size 10.7188 7.5692) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 7 smd rect (at 3.81 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 12 /SH_B))
    (pad 6 smd rect (at 2.54 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 12 /SH_B))
    (pad 5 smd rect (at 1.27 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 12 /SH_B))
    (pad 3 smd rect (at -1.27 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 12 /SH_B))
    (pad 2 smd rect (at -2.54 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 12 /SH_B))
    (pad 1 smd rect (at -3.81 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q3-Pad1)"))
  )
  (module FK_Parts:D2Pak (layer B.Cu) (tedit 0)
    (at 190.5 85.725 90)
    (fp_text reference Q4 (at 0 0 270) (layer B.SilkS))
    (fp_text value MOSFET_D2Pak (at 0 0 270) (layer B.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User))
    (fp_text user * (at -5.08 -8.1534 270) (layer B.SilkS))
    (fp_text user * (at -3.81 -4.572 270) (layer B.Fab))
    (fp_text user * (at -3.81 -4.572 270) (layer B.Fab))
    (fp_text user * (at -5.08 -8.1534 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -2.54 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.27 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.27 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.54 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.81 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 3.2512 90) (size 10.7188 7.5692) (layers B.Cu B.Paste B.Mask)
      (net 12 /SH_B))
  )
  (module FK_Parts:D2Pak (layer F.Cu) (tedit 0)
    (at 188.0362 70.485 90)
    (fp_text reference Q5 (at 0 0 90) (layer F.SilkS))
    (fp_text value MOSFET_D2Pak (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at -5.08 8.1534 90) (layer F.SilkS))
    (fp_text user * (at -3.81 4.572 90) (layer F.Fab))
    (fp_text user * (at -3.81 4.572 90) (layer F.Fab))
    (fp_text user * (at -5.08 8.1534 90) (layer F.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 smd rect (at 0 -3.2512 90) (size 10.7188 7.5692) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 7 smd rect (at 3.81 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 9 /SH_C))
    (pad 6 smd rect (at 2.54 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 9 /SH_C))
    (pad 5 smd rect (at 1.27 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 9 /SH_C))
    (pad 3 smd rect (at -1.27 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 9 /SH_C))
    (pad 2 smd rect (at -2.54 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 9 /SH_C))
    (pad 1 smd rect (at -3.81 8.1534 90) (size 0.9652 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q5-Pad1)"))
  )
  (module FK_Parts:D2Pak (layer B.Cu) (tedit 0)
    (at 190.5 70.485 90)
    (fp_text reference Q6 (at 0 0 270) (layer B.SilkS))
    (fp_text value MOSFET_D2Pak (at 0 0 270) (layer B.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User))
    (fp_text user * (at -5.08 -8.1534 270) (layer B.SilkS))
    (fp_text user * (at -3.81 -4.572 270) (layer B.Fab))
    (fp_text user * (at -3.81 -4.572 270) (layer B.Fab))
    (fp_text user * (at -5.08 -8.1534 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at -2.54 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.27 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.27 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.54 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.81 -8.1534 90) (size 0.9652 3.1496) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 3.2512 90) (size 10.7188 7.5692) (layers B.Cu B.Paste B.Mask)
      (net 9 /SH_C))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 81.28 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /g_A_H))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 86.36 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /g_A_L))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 88.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /g_B_H))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 93.98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(Q4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /g_B_L))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 96.52 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(Q5-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /g_C_H))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 101.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /g_C_L))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 160.02 91.44 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 39k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Supply))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.845 91.444999 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.265001) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Supply))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.21 85.09 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 39k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /Sens_A))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /SH_A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.21 88.265 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 2.2k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /Sens_A))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.21 93.345 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 39k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /Sens_B))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /SH_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.21 96.52 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 2.2k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /Sens_B))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.21 100.33 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 39k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /Sens_C))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /SH_C))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.21 103.505 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 2.2k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /Sens_C))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 154.94 76.2 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value DCDC (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 149.86 81.28)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x10_Odd_Even (at 1.27 25.19) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /g_A_H))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SH_A))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /g_A_L))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /g_B_H))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Supply))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SH_B))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Sens_A))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /g_B_L))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Sens_B))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /g_C_H))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /Sens_C))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SH_C))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /g_C_L))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 173.355 84.455 225)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C5 (at 5.388154 -8.980256 45) (layer F.SilkS))
    (fp_text value CP1 (at 3.75 9.25 45) (layer F.Fab))
    (fp_text user %R (at 3.75 0 45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 225) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 7.5 0 225) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text B- (at 152.654 73.66) (layer F.SilkS))
  (gr_text B+ (at 156.083 73.66) (layer F.SilkS))
  (gr_text 12V (at 149.352 73.66) (layer F.SilkS))
  (gr_text SS (at 148.082 91.567 90) (layer F.SilkS))
  (gr_text SC (at 148.082 98.933 90) (layer F.SilkS))
  (gr_text SB (at 148.082 96.266 90) (layer F.SilkS))
  (gr_text SA (at 148.082 93.98 90) (layer F.SilkS))
  (gr_text 12V (at 148.082 88.773 90) (layer F.SilkS))
  (gr_text + (at 148.209 81.915 90) (layer F.SilkS))
  (gr_text GND (at 151.13 106.68) (layer F.SilkS))
  (gr_text CL (at 154.686 101.6 90) (layer F.SilkS))
  (gr_text C (at 154.686 99.187 90) (layer F.SilkS))
  (gr_text CH (at 154.686 96.647 90) (layer F.SilkS))
  (gr_text BL (at 154.686 94.107 90) (layer F.SilkS))
  (gr_text B (at 154.686 91.44 90) (layer F.SilkS))
  (gr_text BH (at 154.686 89.027 90) (layer F.SilkS))
  (gr_text AL (at 154.559 86.36 90) (layer F.SilkS))
  (gr_text A (at 154.559 83.82 90) (layer F.SilkS))
  (gr_text AH (at 154.559 81.153 90) (layer F.SilkS))
  (gr_text "Battery -" (at 172.085 63.5) (layer B.SilkS))
  (gr_text "Battery +" (at 173.355 63.5) (layer F.SilkS))
  (gr_text "Phase C" (at 206.375 78.105) (layer F.SilkS))
  (gr_text "Phase B" (at 206.375 93.345) (layer F.SilkS))
  (gr_text "Phase A" (at 206.375 108.585) (layer F.SilkS))
  (gr_line (start 212.09 62.23) (end 213.36 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.765 62.23) (end 147.32 66.675) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.32 108.585) (end 151.765 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.36 108.585) (end 208.915 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.09 62.23) (end 151.765 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.36 108.585) (end 213.36 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.765 113.03) (end 208.915 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.32 66.675) (end 147.32 108.585) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.705 109.22) (xy 166.37 109.22) (xy 165.735 108.585) (xy 165.735 65.278) (xy 179.705 65.278)
      )
    )
  )
  (zone (net 1) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.705 109.22) (xy 166.37 109.22) (xy 165.735 108.585) (xy 165.735 65.278) (xy 179.705 65.278)
      )
    )
  )
  (zone (net 9) (net_name /SH_C) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.725 76.835) (xy 198.755 76.835) (xy 198.755 64.135) (xy 212.725 64.135)
      )
    )
  )
  (zone (net 9) (net_name /SH_C) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.755 76.835) (xy 212.725 76.835) (xy 212.725 64.135) (xy 198.755 64.135)
      )
    )
  )
  (zone (net 12) (net_name /SH_B) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.725 92.075) (xy 198.755 92.075) (xy 198.755 79.375) (xy 212.725 79.375)
      )
    )
  )
  (zone (net 12) (net_name /SH_B) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.755 92.075) (xy 212.725 92.075) (xy 212.725 79.375) (xy 198.755 79.375)
      )
    )
  )
  (zone (net 15) (net_name /SH_A) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.725 107.315) (xy 198.755 107.315) (xy 198.755 94.615) (xy 212.725 94.615)
      )
    )
  )
  (zone (net 15) (net_name /SH_A) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.755 107.315) (xy 212.725 107.315) (xy 212.725 94.615) (xy 198.755 94.615)
      )
    )
  )
)
