<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>editable area</text>
<text>Acquisition Board v2.2</text>
<text>revision 2 (Feb 2014)</text>
<text>http://open-ephys.org</text>
<hole x="154.432" y="6.731" drill="3.175"/>
<hole x="154.432" y="154.305" drill="3.175"/>
<hole x="6.858" y="154.305" drill="3.175"/>
<hole x="6.731" y="6.731" drill="3.175"/>
<text>Acquisition Board v2.2</text>
<text>revision 3 (Jan 2017)</text>
<text>http://open-ephys.org</text>
<text>3.3V</text>
<text>gnd</text>
<text>5V pwr</text>
<text>ADC meets DAC GND</text>
<text>analog meets digital GND</text>
<text>i2c</text>
<text>+3.3V</text>
<text>GND</text>
<text>+5.5V</text>
<text>5V FAN</text>
<hole x="136.2" y="88.5" drill="2.5"/>
<hole x="92.2" y="88.5" drill="2.5"/>
<hole x="92.2" y="157.4" drill="3.5"/>
<hole x="136.2" y="157.4" drill="3.5"/>
<text>gnd</text>
<text>s/n</text>
<text>tested</text>
<text>gnd</text>
<text>+5V</text>
<text>dat</text>
<text>WS2812</text>
<text>extra</text>
<text>remove jumper for</text>
<text>±5V</text>
<text>ADC range select</text>
<text>0-5V straight to ADC</text>
<text>0-5V via buffer op-amp</text>
<text>gnd</text>
<text>gnd</text>
<text>o</text>
<text>i</text>
<text>led_dat</text>
<text>+5va</text>
<text>-5va</text>
<text>gnd</text>
<text>+5V</text>
<text>gnd</text>
<text>unbuffered 3.3V logic I/O  - DON'T CONNECT 5V/TTL</text>
<text>o16</text>
<text>o15</text>
<text>o14</text>
<text>o13</text>
<text>o12</text>
<text>o11</text>
<text>o10</text>
<text>o9</text>
<text>i16</text>
<text>i9</text>
<text>i10</text>
<text>i11</text>
<text>i12</text>
<text>i13</text>
<text>i14</text>
<text>i15</text>
<text>gnd</text>
<text>gnd</text>
<text>gnd</text>
<text>+3.3v</text>
<text>+5VDC jack</text>
<text>10k pull-down</text>
<wire x1="155.194" y1="160.528" x2="160.528" y2="155.194" width="0.254" layer="20"/>
<wire x1="160.528" y1="155.194" x2="160.528" y2="144.78" width="0.254" layer="20"/>
<wire x1="160.528" y1="144.78" x2="148.844" y2="144.78" width="0.254" layer="20"/>
<wire x1="148.844" y1="144.78" x2="148.844" y2="111.252" width="0.254" layer="20"/>
<wire x1="148.844" y1="111.252" x2="160.528" y2="111.252" width="0.254" layer="20"/>
<wire x1="160.528" y1="111.252" x2="160.528" y2="6.096" width="0.254" layer="20"/>
<wire x1="160.528" y1="6.096" x2="154.94" y2="0.508" width="0.254" layer="20"/>
<wire x1="6.35" y1="0.508" x2="0.508" y2="6.35" width="0.254" layer="20"/>
<wire x1="0.508" y1="6.35" x2="0.508" y2="154.686" width="0.254" layer="20"/>
<wire x1="0.508" y1="154.686" x2="6.35" y2="160.528" width="0.254" layer="20"/>
<wire x1="6.35" y1="160.528" x2="155.194" y2="160.528" width="0.254" layer="20"/>
<wire x1="0.254" y1="0.508" x2="151.13" y2="0.508" width="0.508" layer="46"/>
<wire x1="154.94" y1="0.508" x2="150.876" y2="0.508" width="0.254" layer="20"/>
<wire x1="150.876" y1="0.508" x2="149.098" y2="-1.27" width="0.254" layer="20"/>
<wire x1="149.098" y1="-1.27" x2="119.38" y2="-1.27" width="0.254" layer="20"/>
<wire x1="119.38" y1="-1.27" x2="117.602" y2="0.508" width="0.254" layer="20"/>
<wire x1="117.602" y1="0.508" x2="6.35" y2="0.508" width="0.2032" layer="20"/>
<text>+gnd</text>
</plain>
<libraries>
<library name="RHD2000_eval_board">
<description>Intan Technologies RHD2000 Eval Board</description>
<packages>
<package name="OPALKELLY_XEM6010">
</package>
<package name="PJ-102AH">
</package>
<package name="OMNETICS_PZN-12-AA">
</package>
<package name="0603">
</package>
<package name="SOIC-14">
</package>
<package name="1206">
</package>
<package name="SJ-3523">
</package>
<package name="0805">
</package>
<package name="SOT-23-6">
</package>
<package name="SOT-23-5">
</package>
<package name="TESTPOINT">
</package>
<package name="1206_POL">
</package>
<package name="TERMINAL_BLOCK_3.5MM_2_GND">
</package>
</packages>
</library>
<library name="open-ephys">
<packages>
<package name="TSSOP-24">
</package>
<package name="HDMI_A">
</package>
<package name="OPEN_EPHYS_LOGO">
</package>
<package name="SOT23-6">
</package>
<package name="MBRA210LT3-D">
</package>
<package name="BNC_RIGHT_ANGLE">
</package>
<package name="8-SOIC">
</package>
<package name="DCU">
</package>
<package name="8-MSOP">
</package>
<package name="CT/CN1812">
<description>&lt;b&gt;EPCOS SMD Varistors, MLV; Standard Series&lt;/b&gt;&lt;p&gt;
Source: www.farnell.com/datasheets/49238.pdf</description>
</package>
<package name="2-XDFN">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP5Q">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ws2812">
<packages>
<package name="WS2812_EXTENDED_PADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BRD1" library="RHD2000_eval_board" package="OPALKELLY_XEM6010" value="OPALKELLY_XEM6010"/>
<element name="J2" library="RHD2000_eval_board" package="PJ-102AH" value="DC_POWER_JACK-PJ-102AH"/>
<element name="A" library="RHD2000_eval_board" package="OMNETICS_PZN-12-AA" value="RHD2000-CABLE-DAQ-SIDE">
<attribute name="NAME"/>
</element>
<element name="B" library="RHD2000_eval_board" package="OMNETICS_PZN-12-AA" value="RHD2000-CABLE-DAQ-SIDE">
<attribute name="NAME"/>
</element>
<element name="C" library="RHD2000_eval_board" package="OMNETICS_PZN-12-AA" value="RHD2000-CABLE-DAQ-SIDE">
<attribute name="NAME"/>
</element>
<element name="D" library="RHD2000_eval_board" package="OMNETICS_PZN-12-AA" value="RHD2000-CABLE-DAQ-SIDE">
<attribute name="NAME"/>
</element>
<element name="R3" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C20" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C19" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C18" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C17" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C16" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C15" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C14" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C13" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C37" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="OPAMP_A" library="RHD2000_eval_board" package="SOIC-14" value="OPA4170">
<attribute name="VALUE"/>
</element>
<element name="R21" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R13" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R29" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R4" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C38" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R5" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C39" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R6" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C40" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R7" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C41" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R8" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C42" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R9" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C43" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R10" library="RHD2000_eval_board" package="0603" value="5.6K">
<attribute name="NAME"/>
</element>
<element name="C44" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="R22" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R14" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R30" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R23" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R15" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R31" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R24" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R16" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R32" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="OPAMP_B" library="RHD2000_eval_board" package="SOIC-14" value="OPA4170">
<attribute name="VALUE"/>
</element>
<element name="R25" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R17" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R33" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R26" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R18" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R34" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R27" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R19" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R35" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R28" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R20" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R36" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="C45" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C46" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C47" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C48" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C29" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C30" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C31" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C32" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C33" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C34" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C35" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C36" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="R37" library="RHD2000_eval_board" package="0603" value="100">
<attribute name="NAME"/>
</element>
<element name="R38" library="RHD2000_eval_board" package="0603" value="100">
<attribute name="NAME"/>
</element>
<element name="R39" library="RHD2000_eval_board" package="0603" value="1.0M">
<attribute name="NAME"/>
</element>
<element name="R40" library="RHD2000_eval_board" package="0603" value="1.0M">
<attribute name="NAME"/>
</element>
<element name="C49" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="C50" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="J1" library="RHD2000_eval_board" package="SJ-3523" value="STEREO_JACK_SJ-3523"/>
<element name="C4" library="RHD2000_eval_board" package="0603" value="10n">
<attribute name="NAME"/>
</element>
<element name="C3" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
</element>
<element name="C5" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="3.5VREG" library="RHD2000_eval_board" package="SOT-23-6" value="TPS79301">
<attribute name="NAME"/>
</element>
<element name="R2" library="RHD2000_eval_board" package="0603" value="56.0K">
<attribute name="NAME"/>
</element>
<element name="R1" library="RHD2000_eval_board" package="0603" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="RHD2000_eval_board" package="0603" value="15p">
<attribute name="NAME"/>
</element>
<element name="C9" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C7" library="RHD2000_eval_board" package="0603" value="100n"/>
<element name="C8" library="RHD2000_eval_board" package="0603" value="100n"/>
<element name="C6" library="RHD2000_eval_board" package="0603" value="100n"/>
<element name="INVERTER" library="RHD2000_eval_board" package="SOT-23-5" value="TPS60403">
<attribute name="NAME"/>
</element>
<element name="C25" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
</element>
<element name="C26" library="RHD2000_eval_board" package="1206" value="10u">
<attribute name="NAME"/>
</element>
<element name="C24" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
</element>
<element name="-5V_REG" library="RHD2000_eval_board" package="SOT-23-5" value="TPS72301">
<attribute name="NAME"/>
</element>
<element name="R11" library="RHD2000_eval_board" package="0603" value="82K">
<attribute name="NAME"/>
</element>
<element name="R12" library="RHD2000_eval_board" package="0603" value="25.5K">
<attribute name="NAME"/>
</element>
<element name="C28" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="L1" library="RHD2000_eval_board" package="0805" value="100n">
<attribute name="NAME"/>
</element>
<element name="C27" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
</element>
<element name="I2C_DATA" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="I2C_CLOCK" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="CLOCK_OUT" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT">
<attribute name="NAME"/>
</element>
<element name="H18-L34N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="F16-L10P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="F17-L10N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="J17-L36P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="U20-L51P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="D10-L33P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C10-L33N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="D11-L36P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C12-L36N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="D15-L62P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C16-L62N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="B6-L4P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="A6-L4P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C7-L5P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="A7-L5N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C9-L8P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="A9-L8N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="B12-L37P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="A12-L37N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="LED_DAT" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="A14-L50N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="B16-L63P" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="A16-L63N" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+3.3V_FPGA_2" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+3.3V_FPGA_1" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="GND_1" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="GND_2" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="ADC_!CS!" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="ADC_SCLK" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DAC_SCLK" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DAC_!SYNC!" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+1.8V_FPGA" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+1.2V_FPGA" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C1" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="GND_3" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="LS_IN" library="open-ephys" package="TSSOP-24" value="OCTAL_BUS_TRANSCEIVER"/>
<element name="TTL_IN" library="open-ephys" package="HDMI_A" value="HDMI"/>
<element name="DAC_OUT" library="open-ephys" package="HDMI_A" value="HDMI"/>
<element name="LS_OUT" library="open-ephys" package="TSSOP-24" value="OCTAL_BUS_TRANSCEIVER"/>
<element name="TTL_OUT" library="open-ephys" package="HDMI_A" value="HDMI"/>
<element name="R41" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R42" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R43" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R44" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R45" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R46" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R47" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="R48" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="U$6" library="open-ephys" package="OPEN_EPHYS_LOGO" value="OPEN_EPHYS_LOGO"/>
<element name="5.5V_BOOST" library="open-ephys" package="SOT23-6" value="LTC3426">
<attribute name="VALUE"/>
</element>
<element name="D1" library="open-ephys" package="MBRA210LT3-D" value="MBRA210LT3-D">
<attribute name="NAME"/>
</element>
<element name="L2" library="RHD2000_eval_board" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="RHD2000_eval_board" package="1206" value="10u">
<attribute name="NAME"/>
</element>
<element name="C11" library="RHD2000_eval_board" package="1206" value="10u">
<attribute name="NAME"/>
</element>
<element name="R68" library="RHD2000_eval_board" package="0603" value="95.3k">
<attribute name="NAME"/>
</element>
<element name="R69" library="RHD2000_eval_board" package="0603" value="27.4k">
<attribute name="NAME"/>
</element>
<element name="5VD" library="RHD2000_eval_board" package="SOT-23-6" value="TPS79301">
<attribute name="NAME"/>
</element>
<element name="C51" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
</element>
<element name="C52" library="RHD2000_eval_board" package="0603" value="10n">
<attribute name="NAME"/>
</element>
<element name="C53" library="RHD2000_eval_board" package="0603" value="15p">
<attribute name="NAME"/>
</element>
<element name="C54" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="R72" library="RHD2000_eval_board" package="0603" value="30.9k">
<attribute name="NAME"/>
</element>
<element name="R73" library="RHD2000_eval_board" package="0603" value="95.3k">
<attribute name="NAME"/>
</element>
<element name="5VA" library="RHD2000_eval_board" package="SOT-23-6" value="TPS79301">
<attribute name="NAME"/>
</element>
<element name="C55" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
</element>
<element name="C56" library="RHD2000_eval_board" package="0603" value="10n">
<attribute name="NAME"/>
</element>
<element name="C57" library="RHD2000_eval_board" package="0603" value="15p">
<attribute name="NAME"/>
</element>
<element name="C58" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
</element>
<element name="R74" library="RHD2000_eval_board" package="0603" value="27.4k">
<attribute name="NAME"/>
</element>
<element name="R75" library="RHD2000_eval_board" package="0603" value="95.3k">
<attribute name="NAME"/>
</element>
<element name="BNC" library="open-ephys" package="BNC_RIGHT_ANGLE" value="BNC_RIGHT_ANGLE"/>
<element name="LS_ADC" library="open-ephys" package="TSSOP-24" value="OCTAL_BUS_TRANSCEIVER"/>
<element name="LS_DAC" library="open-ephys" package="TSSOP-24" value="OCTAL_BUS_TRANSCEIVER"/>
<element name="DIGITAL_OUT_9" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_10" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_11" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_12" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_13" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_14" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_15" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="ADC_IN" library="open-ephys" package="HDMI_A" value="HDMI"/>
<element name="LS_CLK" library="open-ephys" package="TSSOP-24" value="OCTAL_BUS_TRANSCEIVER"/>
<element name="R76" library="RHD2000_eval_board" package="0603" value="51">
<attribute name="NAME"/>
</element>
<element name="DIGITAL_IN_9" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_10" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_11" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_12" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_13" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_14" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_15" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_IN_16" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="ADC_REF" library="open-ephys" package="8-SOIC" value="REF195">
<attribute name="NAME"/>
</element>
<element name="C60" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C61" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="LS_I2C" library="open-ephys" package="DCU" value="TCA9406"/>
<element name="R49" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R50" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_1" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R51" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R52" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_2" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R53" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R54" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_3" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R55" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R56" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_4" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R57" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R58" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_5" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R59" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R60" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_6" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R61" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R62" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_7" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="R63" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R64" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP_AIN_8" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="C62" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C63" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C64" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C65" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C66" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C67" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C68" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="C69" library="RHD2000_eval_board" package="0603" value="1n">
<attribute name="NAME"/>
</element>
<element name="OPAMP_C" library="RHD2000_eval_board" package="SOIC-14" value="OPA4170">
<attribute name="VALUE"/>
</element>
<element name="OPAMP_D" library="RHD2000_eval_board" package="SOIC-14" value="OPA4170">
<attribute name="VALUE"/>
</element>
<element name="C70" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C72" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C71" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C86" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C74" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C75" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="+3V5_1" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+5VA" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="-5VA" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="GND_6" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C73" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="+5VD_1" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="GND_4" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+5.5V" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="GND_5" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="+5V_RAW" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="GND_7" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="DIGITAL_OUT_16" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="C59" library="RHD2000_eval_board" package="1206_POL" value="10u">
<attribute name="NAME"/>
</element>
<element name="C76" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C77" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C78" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C79" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="U$8" library="open-ephys" package="OPEN_EPHYS_LOGO" value="OPEN_EPHYS_LOGO"/>
<element name="DAC1" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC2" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC3" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC4" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC5" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC6" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC7" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="DAC8" library="open-ephys" package="8-MSOP" value="DAC8531"/>
<element name="R77" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R78" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R79" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R80" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R81" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R82" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R83" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R84" library="RHD2000_eval_board" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND_CONN" library="RHD2000_eval_board" package="TERMINAL_BLOCK_3.5MM_2_GND" value="TERMINAL_BLOCK_2-3.5MM-GND"/>
<element name="ADC1" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC2" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC3" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC4" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC5" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC6" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC7" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="ADC8" library="open-ephys" package="8-MSOP" value="ADS8325"/>
<element name="DAC_REF" library="open-ephys" package="8-SOIC" value="REF195"/>
<element name="C12" library="RHD2000_eval_board" package="0603" value="100n"/>
<element name="C21" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="RHD2000_eval_board" package="1206_POL" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V_FAN" library="jumper" package="JP2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5VD" library="RHD2000_eval_board" package="TESTPOINT" value="TESTPOINT"/>
<element name="LS_LED" library="open-ephys" package="TSSOP-24" value="OCTAL_BUS_TRANSCEIVER"/>
<element name="R67" library="RHD2000_eval_board" package="0603" value="100"/>
<element name="C87" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C88" library="RHD2000_eval_board" package="0603" value="100n"/>
<element name="C80" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C81" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C82" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C83" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C84" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C85" library="RHD2000_eval_board" package="0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="DAISY_CHAIN_CONNECTOR" library="jumper" package="JP5Q" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R65" library="RHD2000_eval_board" package="0603" value="10k"/>
<element name="R66" library="RHD2000_eval_board" package="0603" value="100"/>
<element name="C89" library="RHD2000_eval_board" package="1206" value="22u"/>
<element name="C90" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="RHD2000_eval_board" package="0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C91" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C92" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.5VREG1" library="RHD2000_eval_board" package="SOT-23-6" value="TPS79301"/>
<element name="R70" library="RHD2000_eval_board" package="0603" value="56.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R71" library="RHD2000_eval_board" package="0603" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C93" library="RHD2000_eval_board" package="0603" value="15p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C94" library="RHD2000_eval_board" package="0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C95" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C96" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.5VREG2" library="RHD2000_eval_board" package="SOT-23-6" value="TPS79301"/>
<element name="R85" library="RHD2000_eval_board" package="0603" value="56.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R86" library="RHD2000_eval_board" package="0603" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C97" library="RHD2000_eval_board" package="0603" value="15p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C98" library="RHD2000_eval_board" package="0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C99" library="RHD2000_eval_board" package="0805" value="1.0u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C100" library="RHD2000_eval_board" package="1206" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.5VREG3" library="RHD2000_eval_board" package="SOT-23-6" value="TPS79301"/>
<element name="R87" library="RHD2000_eval_board" package="0603" value="56.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R88" library="RHD2000_eval_board" package="0603" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C101" library="RHD2000_eval_board" package="0603" value="15p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POLYFUSE" library="open-ephys" package="CT/CN1812" value="0ZCC_FUSE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ZENER" library="open-ephys" package="2-XDFN" value="TPD1E10B06"/>
<element name="LED5" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED4" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED3" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED2" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED1" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED6" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED7" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
<element name="LED8" library="ws2812" package="WS2812_EXTENDED_PADS" value="WS2812&quot;"/>
</elements>
<signals>
<signal name="+VCCO1_35">
<contactref element="BRD1" pad="JP2-35"/>
</signal>
<signal name="+VCCO1_55">
<contactref element="BRD1" pad="JP2-55"/>
</signal>
<signal name="+VCCO0_36">
<contactref element="BRD1" pad="JP3-36"/>
</signal>
<signal name="+VCCO0_56">
<contactref element="BRD1" pad="JP3-56"/>
</signal>
<signal name="RHD_A_MISO1+">
<contactref element="BRD1" pad="JP3-15"/>
<contactref element="A" pad="B4"/>
</signal>
<signal name="RHD_A_MISO1-">
<contactref element="BRD1" pad="JP3-17"/>
<contactref element="A" pad="T4"/>
</signal>
<signal name="RHD_A_MISO2+">
<contactref element="BRD1" pad="JP3-19"/>
<contactref element="A" pad="B5"/>
</signal>
<signal name="RHD_A_MISO2-">
<contactref element="BRD1" pad="JP3-21"/>
<contactref element="A" pad="T5"/>
</signal>
<signal name="RHD_A_CS+">
<contactref element="BRD1" pad="JP3-23"/>
<contactref element="A" pad="B1"/>
</signal>
<signal name="RHD_A_CS-">
<contactref element="BRD1" pad="JP3-25"/>
<contactref element="A" pad="T1"/>
</signal>
<signal name="RHD_A_SCLK+">
<contactref element="BRD1" pad="JP3-27"/>
<contactref element="A" pad="B2"/>
</signal>
<signal name="RHD_A_SCLK-">
<contactref element="BRD1" pad="JP3-29"/>
<contactref element="A" pad="T2"/>
</signal>
<signal name="RHD_A_MOSI+">
<contactref element="BRD1" pad="JP3-31"/>
<contactref element="A" pad="B3"/>
</signal>
<signal name="RHD_A_MOSI-">
<contactref element="BRD1" pad="JP3-33"/>
<contactref element="A" pad="T3"/>
</signal>
<signal name="RHD_B_MISO1+">
<contactref element="BRD1" pad="JP3-37"/>
<contactref element="B" pad="B4"/>
</signal>
<signal name="RHD_B_MISO1-">
<contactref element="BRD1" pad="JP3-39"/>
<contactref element="B" pad="T4"/>
</signal>
<signal name="RHD_B_MISO2+">
<contactref element="BRD1" pad="JP3-41"/>
<contactref element="B" pad="B5"/>
</signal>
<signal name="RHD_B_MISO2-">
<contactref element="BRD1" pad="JP3-43"/>
<contactref element="B" pad="T5"/>
</signal>
<signal name="RHD_B_CS+">
<contactref element="BRD1" pad="JP3-45"/>
<contactref element="B" pad="B1"/>
</signal>
<signal name="RHD_B_CS-">
<contactref element="BRD1" pad="JP3-47"/>
<contactref element="B" pad="T1"/>
</signal>
<signal name="RHD_B_SCLK+">
<contactref element="BRD1" pad="JP3-49"/>
<contactref element="B" pad="B2"/>
</signal>
<signal name="RHD_B_SCLK-">
<contactref element="BRD1" pad="JP3-51"/>
<contactref element="B" pad="T2"/>
</signal>
<signal name="RHD_B_MOSI+">
<contactref element="BRD1" pad="JP3-53"/>
<contactref element="B" pad="B3"/>
</signal>
<signal name="RHD_B_MOSI-">
<contactref element="BRD1" pad="JP3-57"/>
<contactref element="B" pad="T3"/>
</signal>
<signal name="RHD_C_CS+">
<contactref element="BRD1" pad="JP3-59"/>
<contactref element="C" pad="B1"/>
</signal>
<signal name="RHD_C_CS-">
<contactref element="BRD1" pad="JP3-61"/>
<contactref element="C" pad="T1"/>
</signal>
<signal name="RHD_C_SCLK+">
<contactref element="BRD1" pad="JP3-63"/>
<contactref element="C" pad="B2"/>
</signal>
<signal name="RHD_C_SCLK-">
<contactref element="BRD1" pad="JP3-65"/>
<contactref element="C" pad="T2"/>
</signal>
<signal name="RHD_C_MOSI+">
<contactref element="BRD1" pad="JP3-67"/>
<contactref element="C" pad="B3"/>
</signal>
<signal name="RHD_C_MOSI-">
<contactref element="BRD1" pad="JP3-69"/>
<contactref element="C" pad="T3"/>
</signal>
<signal name="RHD_D_CS+">
<contactref element="BRD1" pad="JP3-71"/>
<contactref element="D" pad="B1"/>
</signal>
<signal name="RHD_D_CS-">
<contactref element="BRD1" pad="JP3-73"/>
<contactref element="D" pad="T1"/>
</signal>
<signal name="RHD_D_MOSI+">
<contactref element="BRD1" pad="JP3-77"/>
<contactref element="D" pad="B3"/>
</signal>
<signal name="RHD_D_MOSI-">
<contactref element="BRD1" pad="JP3-79"/>
<contactref element="D" pad="T3"/>
</signal>
<signal name="RHD_D_SCLK-">
<contactref element="BRD1" pad="JP3-75"/>
<contactref element="D" pad="T2"/>
</signal>
<signal name="RHD_D_SCLK+">
<contactref element="BRD1" pad="JP3-76"/>
<contactref element="D" pad="B2"/>
</signal>
<signal name="RHD_C_MISO1+">
<contactref element="BRD1" pad="JP3-16"/>
<contactref element="C" pad="B4"/>
</signal>
<signal name="RHD_C_MISO1-">
<contactref element="BRD1" pad="JP3-18"/>
<contactref element="C" pad="T4"/>
</signal>
<signal name="RHD_C_MISO2+">
<contactref element="BRD1" pad="JP3-20"/>
<contactref element="C" pad="B5"/>
</signal>
<signal name="RHD_C_MISO2-">
<contactref element="BRD1" pad="JP3-22"/>
<contactref element="C" pad="T5"/>
</signal>
<signal name="RHD_D_MISO1+">
<contactref element="BRD1" pad="JP3-24"/>
<contactref element="D" pad="B4"/>
</signal>
<signal name="RHD_D_MISO1-">
<contactref element="BRD1" pad="JP3-26"/>
<contactref element="D" pad="T4"/>
</signal>
<signal name="RHD_D_MISO2+">
<contactref element="BRD1" pad="JP3-28"/>
<contactref element="D" pad="B5"/>
</signal>
<signal name="RHD_D_MISO2-">
<contactref element="BRD1" pad="JP3-30"/>
<contactref element="D" pad="T5"/>
</signal>
<signal name="GND">
<contactref element="BRD1" pad="JP3-55"/>
<contactref element="BRD1" pad="JP3-35"/>
<contactref element="BRD1" pad="JP3-78"/>
<contactref element="BRD1" pad="JP3-80"/>
<contactref element="BRD1" pad="JP3-2"/>
<contactref element="BRD1" pad="JP3-14"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="A" pad="T6"/>
<contactref element="B" pad="T6"/>
<contactref element="C" pad="T6"/>
<contactref element="D" pad="T6"/>
<contactref element="3.5VREG" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="GND_1" pad="1"/>
<contactref element="GND_2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="GND_3" pad="1"/>
<contactref element="BRD1" pad="JP2-13"/>
<contactref element="BRD1" pad="JP2-1"/>
<contactref element="C20" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="TTL_IN" pad="P$2"/>
<contactref element="LS_IN" pad="P11"/>
<contactref element="LS_IN" pad="P12"/>
<contactref element="LS_IN" pad="P13"/>
<contactref element="TTL_IN" pad="P$5"/>
<contactref element="TTL_IN" pad="P$8"/>
<contactref element="TTL_IN" pad="P$11"/>
<contactref element="TTL_IN" pad="P$17"/>
<contactref element="LS_IN" pad="P22"/>
<contactref element="LS_ADC" pad="P22"/>
<contactref element="LS_ADC" pad="P11"/>
<contactref element="LS_ADC" pad="P12"/>
<contactref element="LS_ADC" pad="P13"/>
<contactref element="ADC_REF" pad="P4"/>
<contactref element="C60" pad="2"/>
<contactref element="C61" pad="2"/>
<contactref element="BRD1" pad="JP2-78"/>
<contactref element="BRD1" pad="JP2-80"/>
<contactref element="BRD1" pad="JP2-56"/>
<contactref element="BRD1" pad="JP2-36"/>
<contactref element="BRD1" pad="JP2-14"/>
<contactref element="C37" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="DAC_OUT" pad="P$2"/>
<contactref element="DAC_OUT" pad="P$5"/>
<contactref element="DAC_OUT" pad="P$8"/>
<contactref element="DAC_OUT" pad="P$11"/>
<contactref element="DAC_OUT" pad="P$17"/>
<contactref element="LS_DAC" pad="P11"/>
<contactref element="LS_DAC" pad="P12"/>
<contactref element="LS_DAC" pad="P13"/>
<contactref element="LS_DAC" pad="P2"/>
<contactref element="LS_DAC" pad="P22"/>
<contactref element="R39" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="INVERTER" pad="4"/>
<contactref element="C25" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="-5V_REG" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="5.5V_BOOST" pad="2"/>
<contactref element="R69" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="5VD" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="R72" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="5VA" pad="2"/>
<contactref element="C56" pad="2"/>
<contactref element="R74" pad="2"/>
<contactref element="C58" pad="2"/>
<contactref element="BNC" pad="P$GND"/>
<contactref element="LS_OUT" pad="P11"/>
<contactref element="LS_OUT" pad="P12"/>
<contactref element="LS_OUT" pad="P13"/>
<contactref element="TTL_OUT" pad="P$17"/>
<contactref element="TTL_OUT" pad="P$11"/>
<contactref element="TTL_OUT" pad="P$8"/>
<contactref element="TTL_OUT" pad="P$5"/>
<contactref element="TTL_OUT" pad="P$2"/>
<contactref element="LS_OUT" pad="P22"/>
<contactref element="LS_OUT" pad="P2"/>
<contactref element="LS_CLK" pad="P22"/>
<contactref element="LS_CLK" pad="P2"/>
<contactref element="LS_CLK" pad="P11"/>
<contactref element="LS_CLK" pad="P12"/>
<contactref element="LS_CLK" pad="P13"/>
<contactref element="ADC_IN" pad="P$2"/>
<contactref element="ADC_IN" pad="P$17"/>
<contactref element="ADC_IN" pad="P$11"/>
<contactref element="ADC_IN" pad="P$8"/>
<contactref element="ADC_IN" pad="P$5"/>
<contactref element="LS_I2C" pad="P2"/>
<contactref element="C62" pad="2"/>
<contactref element="C63" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="C65" pad="2"/>
<contactref element="C66" pad="2"/>
<contactref element="C67" pad="2"/>
<contactref element="C68" pad="2"/>
<contactref element="C69" pad="2"/>
<contactref element="C70" pad="2"/>
<contactref element="C72" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="C86" pad="2"/>
<contactref element="C74" pad="2"/>
<contactref element="C75" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="GND_6" pad="1"/>
<contactref element="C73" pad="2"/>
<contactref element="GND_4" pad="1"/>
<contactref element="GND_5" pad="1"/>
<contactref element="GND_7" pad="1"/>
<contactref element="C59" pad="-"/>
<contactref element="C76" pad="2"/>
<contactref element="C77" pad="2"/>
<contactref element="C78" pad="1"/>
<contactref element="C79" pad="1"/>
<contactref element="DAC1" pad="P8"/>
<contactref element="DAC2" pad="P8"/>
<contactref element="DAC3" pad="P8"/>
<contactref element="DAC4" pad="P8"/>
<contactref element="DAC5" pad="P8"/>
<contactref element="DAC6" pad="P8"/>
<contactref element="DAC7" pad="P8"/>
<contactref element="DAC8" pad="P8"/>
<contactref element="R84" pad="1"/>
<contactref element="R77" pad="1"/>
<contactref element="R78" pad="1"/>
<contactref element="R83" pad="1"/>
<contactref element="R82" pad="1"/>
<contactref element="R81" pad="1"/>
<contactref element="R80" pad="1"/>
<contactref element="R79" pad="1"/>
<contactref element="GND_CONN" pad="2"/>
<contactref element="GND_CONN" pad="1"/>
<contactref element="ADC1" pad="P4"/>
<contactref element="ADC2" pad="P4"/>
<contactref element="ADC3" pad="P4"/>
<contactref element="ADC4" pad="P4"/>
<contactref element="ADC5" pad="P4"/>
<contactref element="ADC6" pad="P4"/>
<contactref element="ADC7" pad="P4"/>
<contactref element="ADC8" pad="P4"/>
<contactref element="ADC8" pad="P3"/>
<contactref element="ADC7" pad="P3"/>
<contactref element="ADC6" pad="P3"/>
<contactref element="ADC5" pad="P3"/>
<contactref element="ADC4" pad="P3"/>
<contactref element="ADC3" pad="P3"/>
<contactref element="ADC2" pad="P3"/>
<contactref element="ADC1" pad="P3"/>
<contactref element="DAC_REF" pad="P4"/>
<contactref element="C12" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="-"/>
<contactref element="5V_FAN" pad="3"/>
<contactref element="5V_FAN" pad="1"/>
<contactref element="LS_LED" pad="P11"/>
<contactref element="LS_LED" pad="P12"/>
<contactref element="LS_LED" pad="P13"/>
<contactref element="LS_LED" pad="P22"/>
<contactref element="LS_LED" pad="P2"/>
<contactref element="C87" pad="2"/>
<contactref element="C88" pad="2"/>
<contactref element="C80" pad="2"/>
<contactref element="C81" pad="2"/>
<contactref element="C82" pad="2"/>
<contactref element="C83" pad="2"/>
<contactref element="C84" pad="2"/>
<contactref element="C85" pad="2"/>
<contactref element="DAISY_CHAIN_CONNECTOR" pad="9"/>
<contactref element="DAISY_CHAIN_CONNECTOR" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="C89" pad="2"/>
<contactref element="C90" pad="2"/>
<contactref element="3.5VREG1" pad="2"/>
<contactref element="3.5VREG1" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C91" pad="2"/>
<contactref element="C92" pad="2"/>
<contactref element="R71" pad="1"/>
<contactref element="3.5VREG2" pad="2"/>
<contactref element="3.5VREG2" pad="2"/>
<contactref element="C94" pad="2"/>
<contactref element="C95" pad="2"/>
<contactref element="C96" pad="2"/>
<contactref element="R86" pad="1"/>
<contactref element="3.5VREG3" pad="2"/>
<contactref element="3.5VREG3" pad="2"/>
<contactref element="C98" pad="2"/>
<contactref element="C99" pad="2"/>
<contactref element="C100" pad="2"/>
<contactref element="R88" pad="1"/>
<contactref element="ZENER" pad="P$1"/>
<contactref element="LED5" pad="VSS"/>
<contactref element="LED5" pad="VSS"/>
<contactref element="LED4" pad="VSS"/>
<contactref element="LED4" pad="VSS"/>
<contactref element="LED3" pad="VSS"/>
<contactref element="LED3" pad="VSS"/>
<contactref element="LED2" pad="VSS"/>
<contactref element="LED2" pad="VSS"/>
<contactref element="LED1" pad="VSS"/>
<contactref element="LED1" pad="VSS"/>
<contactref element="LED6" pad="VSS"/>
<contactref element="LED6" pad="VSS"/>
<contactref element="LED7" pad="VSS"/>
<contactref element="LED7" pad="VSS"/>
<contactref element="LED8" pad="VSS"/>
<contactref element="LED8" pad="VSS"/>
</signal>
<signal name="+3V3">
<contactref element="BRD1" pad="JP3-9"/>
<contactref element="BRD1" pad="JP3-11"/>
<contactref element="BRD1" pad="JP3-13"/>
<contactref element="+3.3V_FPGA_1" pad="1"/>
<contactref element="+3.3V_FPGA_2" pad="1"/>
<contactref element="LS_IN" pad="P23"/>
<contactref element="LS_IN" pad="P24"/>
<contactref element="LS_ADC" pad="P24"/>
<contactref element="LS_ADC" pad="P23"/>
<contactref element="BRD1" pad="JP2-2"/>
<contactref element="BRD1" pad="JP2-4"/>
<contactref element="BRD1" pad="JP2-6"/>
<contactref element="LS_DAC" pad="P24"/>
<contactref element="LS_DAC" pad="P23"/>
<contactref element="LS_OUT" pad="P24"/>
<contactref element="LS_OUT" pad="P23"/>
<contactref element="LS_CLK" pad="P24"/>
<contactref element="LS_CLK" pad="P23"/>
<contactref element="LS_I2C" pad="P3"/>
<contactref element="LS_I2C" pad="P6"/>
<contactref element="C74" pad="1"/>
<contactref element="LS_LED" pad="P24"/>
<contactref element="LS_LED" pad="P23"/>
</signal>
<signal name="+5V">
<contactref element="BRD1" pad="JP3-5"/>
<contactref element="BRD1" pad="JP3-3"/>
<contactref element="BRD1" pad="JP3-1"/>
<contactref element="C3" pad="1"/>
<contactref element="3.5VREG" pad="1"/>
<contactref element="3.5VREG" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="5.5V_BOOST" pad="6"/>
<contactref element="5.5V_BOOST" pad="4"/>
<contactref element="C10" pad="1"/>
<contactref element="+5V_RAW" pad="1"/>
<contactref element="5V_FAN" pad="2"/>
<contactref element="C86" pad="1"/>
<contactref element="C87" pad="1"/>
<contactref element="C80" pad="1"/>
<contactref element="C81" pad="1"/>
<contactref element="C82" pad="1"/>
<contactref element="C83" pad="1"/>
<contactref element="C84" pad="1"/>
<contactref element="C85" pad="1"/>
<contactref element="C89" pad="1"/>
<contactref element="C90" pad="1"/>
<contactref element="C91" pad="1"/>
<contactref element="3.5VREG1" pad="1"/>
<contactref element="3.5VREG1" pad="3"/>
<contactref element="C95" pad="1"/>
<contactref element="3.5VREG2" pad="1"/>
<contactref element="3.5VREG2" pad="3"/>
<contactref element="C99" pad="1"/>
<contactref element="3.5VREG3" pad="1"/>
<contactref element="3.5VREG3" pad="3"/>
<contactref element="POLYFUSE" pad="2"/>
<contactref element="ZENER" pad="P$2"/>
<contactref element="LED5" pad="VDD"/>
<contactref element="LED5" pad="LEDVDD"/>
<contactref element="LED4" pad="VDD"/>
<contactref element="LED4" pad="LEDVDD"/>
<contactref element="LED3" pad="VDD"/>
<contactref element="LED3" pad="LEDVDD"/>
<contactref element="LED2" pad="VDD"/>
<contactref element="LED2" pad="LEDVDD"/>
<contactref element="LED1" pad="VDD"/>
<contactref element="LED1" pad="LEDVDD"/>
<contactref element="LED6" pad="VDD"/>
<contactref element="LED6" pad="LEDVDD"/>
<contactref element="LED7" pad="VDD"/>
<contactref element="LED7" pad="LEDVDD"/>
<contactref element="LED8" pad="VDD"/>
<contactref element="LED8" pad="LEDVDD"/>
</signal>
<signal name="N$143">
<contactref element="C4" pad="1"/>
<contactref element="3.5VREG" pad="4"/>
</signal>
<signal name="N$144">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="3.5VREG" pad="5"/>
</signal>
<signal name="DAISYCHAIN_OUT">
<contactref element="BRD1" pad="JP3-32"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="N$176">
<contactref element="BRD1" pad="JP3-38"/>
<contactref element="D10-L33P" pad="1"/>
</signal>
<signal name="N$177">
<contactref element="BRD1" pad="JP3-40"/>
<contactref element="C10-L33N" pad="1"/>
</signal>
<signal name="N$178">
<contactref element="BRD1" pad="JP3-42"/>
<contactref element="D11-L36P" pad="1"/>
</signal>
<signal name="N$179">
<contactref element="BRD1" pad="JP3-44"/>
<contactref element="C12-L36N" pad="1"/>
</signal>
<signal name="N$180">
<contactref element="BRD1" pad="JP3-46"/>
<contactref element="D15-L62P" pad="1"/>
</signal>
<signal name="N$181">
<contactref element="BRD1" pad="JP3-48"/>
<contactref element="C16-L62N" pad="1"/>
</signal>
<signal name="N$182">
<contactref element="BRD1" pad="JP3-50"/>
<contactref element="B6-L4P" pad="1"/>
</signal>
<signal name="N$183">
<contactref element="BRD1" pad="JP3-52"/>
<contactref element="A6-L4P" pad="1"/>
</signal>
<signal name="N$184">
<contactref element="BRD1" pad="JP3-54"/>
<contactref element="C7-L5P" pad="1"/>
</signal>
<signal name="N$186">
<contactref element="BRD1" pad="JP3-58"/>
<contactref element="A7-L5N" pad="1"/>
</signal>
<signal name="N$187">
<contactref element="BRD1" pad="JP3-60"/>
<contactref element="C9-L8P" pad="1"/>
</signal>
<signal name="N$188">
<contactref element="BRD1" pad="JP3-62"/>
<contactref element="A9-L8N" pad="1"/>
</signal>
<signal name="N$189">
<contactref element="BRD1" pad="JP3-64"/>
<contactref element="B12-L37P" pad="1"/>
</signal>
<signal name="N$190">
<contactref element="BRD1" pad="JP3-66"/>
<contactref element="A12-L37N" pad="1"/>
</signal>
<signal name="N$175">
<contactref element="BRD1" pad="JP3-7"/>
<contactref element="+1.8V_FPGA" pad="1"/>
</signal>
<signal name="N$185">
<contactref element="BRD1" pad="JP3-4"/>
<contactref element="+1.2V_FPGA" pad="1"/>
<contactref element="BRD1" pad="JP3-6"/>
</signal>
<signal name="N$52">
<contactref element="BRD1" pad="JP2-29"/>
<contactref element="LS_ADC" pad="P21"/>
</signal>
<signal name="N$55">
<contactref element="BRD1" pad="JP2-31"/>
<contactref element="LS_ADC" pad="P20"/>
</signal>
<signal name="N$56">
<contactref element="BRD1" pad="JP2-33"/>
<contactref element="LS_ADC" pad="P19"/>
</signal>
<signal name="N$57">
<contactref element="BRD1" pad="JP2-37"/>
<contactref element="LS_ADC" pad="P18"/>
</signal>
<signal name="N$58">
<contactref element="BRD1" pad="JP2-39"/>
<contactref element="LS_ADC" pad="P17"/>
</signal>
<signal name="N$59">
<contactref element="BRD1" pad="JP2-41"/>
<contactref element="LS_ADC" pad="P16"/>
</signal>
<signal name="N$54">
<contactref element="BRD1" pad="JP2-43"/>
<contactref element="LS_ADC" pad="P15"/>
</signal>
<signal name="N$60">
<contactref element="LS_ADC" pad="P10"/>
<contactref element="ADC8" pad="P6"/>
</signal>
<signal name="DIGITAL_IN_8_3.3V">
<contactref element="BRD1" pad="JP2-63"/>
<contactref element="LS_IN" pad="P14"/>
</signal>
<signal name="DIGITAL_IN_7_3.3V">
<contactref element="BRD1" pad="JP2-61"/>
<contactref element="LS_IN" pad="P15"/>
</signal>
<signal name="DIGITAL_IN_6_3.3V">
<contactref element="BRD1" pad="JP2-59"/>
<contactref element="LS_IN" pad="P16"/>
</signal>
<signal name="DIGITAL_IN_5_3.3V">
<contactref element="BRD1" pad="JP2-57"/>
<contactref element="LS_IN" pad="P17"/>
</signal>
<signal name="DIGITAL_IN_4_3.3V">
<contactref element="BRD1" pad="JP2-53"/>
<contactref element="LS_IN" pad="P18"/>
</signal>
<signal name="DIGITAL_IN_3_3.3V">
<contactref element="BRD1" pad="JP2-51"/>
<contactref element="LS_IN" pad="P19"/>
</signal>
<signal name="DIGITAL_IN_2_3.3V">
<contactref element="BRD1" pad="JP2-49"/>
<contactref element="LS_IN" pad="P20"/>
</signal>
<signal name="DIGITAL_IN_1_3.3V">
<contactref element="BRD1" pad="JP2-47"/>
<contactref element="LS_IN" pad="P21"/>
</signal>
<signal name="ADC_IN_1">
<contactref element="R49" pad="2"/>
<contactref element="JP_AIN_1" pad="2"/>
<contactref element="C62" pad="1"/>
<contactref element="ADC1" pad="P2"/>
</signal>
<signal name="ADC_IN_2">
<contactref element="R51" pad="2"/>
<contactref element="JP_AIN_2" pad="2"/>
<contactref element="C63" pad="1"/>
<contactref element="ADC2" pad="P2"/>
</signal>
<signal name="ADC_IN_3">
<contactref element="R53" pad="2"/>
<contactref element="JP_AIN_3" pad="2"/>
<contactref element="C64" pad="1"/>
<contactref element="ADC3" pad="P2"/>
</signal>
<signal name="ADC_IN_4">
<contactref element="R55" pad="2"/>
<contactref element="JP_AIN_4" pad="2"/>
<contactref element="C65" pad="1"/>
<contactref element="ADC4" pad="P2"/>
</signal>
<signal name="ADC_IN_5">
<contactref element="R57" pad="2"/>
<contactref element="JP_AIN_5" pad="2"/>
<contactref element="C66" pad="1"/>
<contactref element="ADC5" pad="P2"/>
</signal>
<signal name="ADC_IN_6">
<contactref element="R59" pad="2"/>
<contactref element="JP_AIN_6" pad="2"/>
<contactref element="C67" pad="1"/>
<contactref element="ADC6" pad="P2"/>
</signal>
<signal name="ADC_IN_7">
<contactref element="R61" pad="2"/>
<contactref element="JP_AIN_7" pad="2"/>
<contactref element="C68" pad="1"/>
<contactref element="ADC7" pad="P2"/>
</signal>
<signal name="ADC_IN_8">
<contactref element="R63" pad="2"/>
<contactref element="JP_AIN_8" pad="2"/>
<contactref element="C69" pad="1"/>
<contactref element="ADC8" pad="P2"/>
</signal>
<signal name="CLOCK_OUT">
<contactref element="BRD1" pad="JP2-19"/>
<contactref element="CLOCK_OUT" pad="1"/>
<contactref element="LS_CLK" pad="P17"/>
</signal>
<signal name="N$168">
<contactref element="BRD1" pad="JP2-21"/>
<contactref element="H18-L34N" pad="1"/>
</signal>
<signal name="N$169">
<contactref element="BRD1" pad="JP2-23"/>
<contactref element="F16-L10P" pad="1"/>
</signal>
<signal name="N$170">
<contactref element="BRD1" pad="JP2-25"/>
<contactref element="F17-L10N" pad="1"/>
</signal>
<signal name="N$171">
<contactref element="BRD1" pad="JP2-27"/>
<contactref element="J17-L36P" pad="1"/>
</signal>
<signal name="DIGITAL_IN_8_5V">
<contactref element="LS_IN" pad="P10"/>
<contactref element="TTL_IN" pad="P$12"/>
<contactref element="R82" pad="2"/>
</signal>
<signal name="DIGITAL_IN_7_5V">
<contactref element="LS_IN" pad="P9"/>
<contactref element="TTL_IN" pad="P$10"/>
<contactref element="R81" pad="2"/>
</signal>
<signal name="DIGITAL_IN_6_5V">
<contactref element="LS_IN" pad="P8"/>
<contactref element="TTL_IN" pad="P$9"/>
<contactref element="R80" pad="2"/>
</signal>
<signal name="DIGITAL_IN_5_5V">
<contactref element="LS_IN" pad="P7"/>
<contactref element="TTL_IN" pad="P$7"/>
<contactref element="R79" pad="2"/>
</signal>
<signal name="DIGITAL_IN_4_5V">
<contactref element="LS_IN" pad="P6"/>
<contactref element="TTL_IN" pad="P$6"/>
<contactref element="R83" pad="2"/>
</signal>
<signal name="DIGITAL_IN_3_5V">
<contactref element="LS_IN" pad="P5"/>
<contactref element="TTL_IN" pad="P$4"/>
<contactref element="R78" pad="2"/>
</signal>
<signal name="DIGITAL_IN_2_5V">
<contactref element="LS_IN" pad="P4"/>
<contactref element="TTL_IN" pad="P$3"/>
<contactref element="R77" pad="2"/>
</signal>
<signal name="DIGITAL_IN_1_5V">
<contactref element="LS_IN" pad="P3"/>
<contactref element="TTL_IN" pad="P$1"/>
<contactref element="R84" pad="2"/>
</signal>
<signal name="+5V5">
<contactref element="D1" pad="NEG"/>
<contactref element="5.5V_BOOST" pad="5"/>
<contactref element="R68" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="INVERTER" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="5VD" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="5VD" pad="3"/>
<contactref element="5VA" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="5VA" pad="3"/>
<contactref element="+5.5V" pad="1"/>
</signal>
<signal name="I2C_DATA">
<contactref element="TTL_IN" pad="P$16"/>
<contactref element="DAC_OUT" pad="P$16"/>
<contactref element="TTL_OUT" pad="P$16"/>
<contactref element="ADC_IN" pad="P$16"/>
<contactref element="LS_I2C" pad="P1"/>
</signal>
<signal name="I2C_CLOCK">
<contactref element="TTL_IN" pad="P$15"/>
<contactref element="DAC_OUT" pad="P$15"/>
<contactref element="TTL_OUT" pad="P$15"/>
<contactref element="ADC_IN" pad="P$15"/>
<contactref element="LS_I2C" pad="P8"/>
</signal>
<signal name="N$95">
<contactref element="LS_ADC" pad="P3"/>
<contactref element="ADC1" pad="P6"/>
</signal>
<signal name="N$96">
<contactref element="LS_ADC" pad="P4"/>
<contactref element="ADC2" pad="P6"/>
</signal>
<signal name="N$98">
<contactref element="LS_ADC" pad="P5"/>
<contactref element="ADC3" pad="P6"/>
</signal>
<signal name="N$141">
<contactref element="LS_ADC" pad="P6"/>
<contactref element="ADC4" pad="P6"/>
</signal>
<signal name="N$165">
<contactref element="LS_ADC" pad="P7"/>
<contactref element="ADC5" pad="P6"/>
</signal>
<signal name="N$166">
<contactref element="LS_ADC" pad="P8"/>
<contactref element="ADC6" pad="P6"/>
</signal>
<signal name="N$167">
<contactref element="LS_ADC" pad="P9"/>
<contactref element="ADC7" pad="P6"/>
</signal>
<signal name="N$212">
<contactref element="LS_ADC" pad="P14"/>
<contactref element="BRD1" pad="JP2-45"/>
</signal>
<signal name="ADC_!CS!_5V">
<contactref element="ADC_!CS!" pad="1"/>
<contactref element="LS_CLK" pad="P3"/>
<contactref element="ADC1" pad="P5"/>
<contactref element="ADC2" pad="P5"/>
<contactref element="ADC3" pad="P5"/>
<contactref element="ADC4" pad="P5"/>
<contactref element="ADC5" pad="P5"/>
<contactref element="ADC6" pad="P5"/>
<contactref element="ADC7" pad="P5"/>
<contactref element="ADC8" pad="P5"/>
</signal>
<signal name="ADC_SCLK_5V">
<contactref element="ADC_SCLK" pad="1"/>
<contactref element="LS_CLK" pad="P4"/>
<contactref element="ADC1" pad="P7"/>
<contactref element="ADC2" pad="P7"/>
<contactref element="ADC3" pad="P7"/>
<contactref element="ADC4" pad="P7"/>
<contactref element="ADC5" pad="P7"/>
<contactref element="ADC6" pad="P7"/>
<contactref element="ADC7" pad="P7"/>
<contactref element="ADC8" pad="P7"/>
</signal>
<signal name="DIGITAL_IN_9_3.3V">
<contactref element="BRD1" pad="JP2-65"/>
<contactref element="DIGITAL_IN_9" pad="1"/>
</signal>
<signal name="DIGITAL_IN_10_3.3V">
<contactref element="BRD1" pad="JP2-67"/>
<contactref element="DIGITAL_IN_10" pad="1"/>
</signal>
<signal name="DIGITAL_IN_11_3.3V">
<contactref element="BRD1" pad="JP2-69"/>
<contactref element="DIGITAL_IN_11" pad="1"/>
</signal>
<signal name="DIGITAL_IN_12_3.3V">
<contactref element="BRD1" pad="JP2-71"/>
<contactref element="DIGITAL_IN_12" pad="1"/>
</signal>
<signal name="DIGITAL_IN_13_3.3V">
<contactref element="BRD1" pad="JP2-73"/>
<contactref element="DIGITAL_IN_13" pad="1"/>
</signal>
<signal name="DIGITAL_IN_14_3.3V">
<contactref element="BRD1" pad="JP2-75"/>
<contactref element="DIGITAL_IN_14" pad="1"/>
</signal>
<signal name="DIGITAL_IN_15_3.3V">
<contactref element="BRD1" pad="JP2-77"/>
<contactref element="DIGITAL_IN_15" pad="1"/>
</signal>
<signal name="DIGITAL_IN_16_3.3V">
<contactref element="BRD1" pad="JP2-79"/>
<contactref element="DIGITAL_IN_16" pad="1"/>
</signal>
<signal name="I2C_DATA_FPGA">
<contactref element="BRD1" pad="JP2-15"/>
<contactref element="I2C_DATA" pad="1"/>
<contactref element="LS_I2C" pad="P4"/>
</signal>
<signal name="I2C_CLOCK_FPGA">
<contactref element="BRD1" pad="JP2-17"/>
<contactref element="I2C_CLOCK" pad="1"/>
<contactref element="LS_I2C" pad="P5"/>
</signal>
<signal name="DAC_!SYNC!_5V">
<contactref element="DAC_!SYNC!" pad="1"/>
<contactref element="LS_CLK" pad="P6"/>
<contactref element="DAC1" pad="P5"/>
<contactref element="DAC2" pad="P5"/>
<contactref element="DAC3" pad="P5"/>
<contactref element="DAC4" pad="P5"/>
<contactref element="DAC5" pad="P5"/>
<contactref element="DAC6" pad="P5"/>
<contactref element="DAC7" pad="P5"/>
<contactref element="DAC8" pad="P5"/>
</signal>
<signal name="DAC_SCLK_5V">
<contactref element="DAC_SCLK" pad="1"/>
<contactref element="LS_CLK" pad="P5"/>
<contactref element="DAC1" pad="P6"/>
<contactref element="DAC2" pad="P6"/>
<contactref element="DAC3" pad="P6"/>
<contactref element="DAC4" pad="P6"/>
<contactref element="DAC5" pad="P6"/>
<contactref element="DAC6" pad="P6"/>
<contactref element="DAC7" pad="P6"/>
<contactref element="DAC8" pad="P6"/>
</signal>
<signal name="N$43">
<contactref element="LS_DAC" pad="P3"/>
<contactref element="DAC1" pad="P7"/>
</signal>
<signal name="N$45">
<contactref element="BRD1" pad="JP2-22"/>
<contactref element="LS_DAC" pad="P20"/>
</signal>
<signal name="N$46">
<contactref element="LS_DAC" pad="P5"/>
<contactref element="DAC3" pad="P7"/>
</signal>
<signal name="N$47">
<contactref element="LS_DAC" pad="P6"/>
<contactref element="DAC4" pad="P7"/>
</signal>
<signal name="N$48">
<contactref element="LS_DAC" pad="P7"/>
<contactref element="DAC5" pad="P7"/>
</signal>
<signal name="N$49">
<contactref element="LS_DAC" pad="P8"/>
<contactref element="DAC6" pad="P7"/>
</signal>
<signal name="N$50">
<contactref element="LS_DAC" pad="P9"/>
<contactref element="DAC7" pad="P7"/>
</signal>
<signal name="N$51">
<contactref element="LS_DAC" pad="P10"/>
<contactref element="DAC8" pad="P7"/>
</signal>
<signal name="ADC_!CS!">
<contactref element="BRD1" pad="JP2-38"/>
<contactref element="LS_CLK" pad="P21"/>
</signal>
<signal name="ADC_SCLK">
<contactref element="BRD1" pad="JP2-40"/>
<contactref element="LS_CLK" pad="P20"/>
</signal>
<signal name="N$53">
<contactref element="R30" pad="1"/>
<contactref element="DAC_OUT" pad="P$3"/>
</signal>
<signal name="N$61">
<contactref element="R31" pad="1"/>
<contactref element="DAC_OUT" pad="P$4"/>
</signal>
<signal name="N$62">
<contactref element="R32" pad="1"/>
<contactref element="DAC_OUT" pad="P$6"/>
</signal>
<signal name="N$63">
<contactref element="R33" pad="1"/>
<contactref element="DAC_OUT" pad="P$7"/>
</signal>
<signal name="N$64">
<contactref element="R34" pad="1"/>
<contactref element="DAC_OUT" pad="P$9"/>
</signal>
<signal name="N$65">
<contactref element="R35" pad="1"/>
<contactref element="DAC_OUT" pad="P$10"/>
</signal>
<signal name="N$66">
<contactref element="R36" pad="1"/>
<contactref element="DAC_OUT" pad="P$12"/>
</signal>
<signal name="OUT8">
<contactref element="BRD1" pad="JP2-60"/>
<contactref element="LS_OUT" pad="P14"/>
</signal>
<signal name="OUT7">
<contactref element="BRD1" pad="JP2-58"/>
<contactref element="LS_OUT" pad="P15"/>
</signal>
<signal name="OUT6">
<contactref element="BRD1" pad="JP2-54"/>
<contactref element="LS_OUT" pad="P16"/>
</signal>
<signal name="OUT5">
<contactref element="BRD1" pad="JP2-52"/>
<contactref element="LS_OUT" pad="P17"/>
</signal>
<signal name="OUT4">
<contactref element="BRD1" pad="JP2-50"/>
<contactref element="LS_OUT" pad="P18"/>
</signal>
<signal name="OUT3">
<contactref element="BRD1" pad="JP2-48"/>
<contactref element="LS_OUT" pad="P19"/>
</signal>
<signal name="OUT2">
<contactref element="BRD1" pad="JP2-46"/>
<contactref element="LS_OUT" pad="P20"/>
</signal>
<signal name="OUT1">
<contactref element="BRD1" pad="JP2-44"/>
<contactref element="LS_OUT" pad="P21"/>
</signal>
<signal name="N$67">
<contactref element="R3" pad="2"/>
<contactref element="DAC1" pad="P3"/>
<contactref element="DAC1" pad="P4"/>
</signal>
<signal name="N$109">
<contactref element="C37" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="OPAMP_A" pad="3"/>
</signal>
<signal name="N$44">
<contactref element="OPAMP_A" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="DAC1_OUT">
<contactref element="OPAMP_A" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$113">
<contactref element="R29" pad="1"/>
<contactref element="DAC_OUT" pad="P$1"/>
</signal>
<signal name="N$114">
<contactref element="R4" pad="2"/>
<contactref element="DAC2" pad="P3"/>
<contactref element="DAC2" pad="P4"/>
</signal>
<signal name="N$111">
<contactref element="R5" pad="2"/>
<contactref element="DAC3" pad="P3"/>
<contactref element="DAC3" pad="P4"/>
</signal>
<signal name="N$112">
<contactref element="R6" pad="2"/>
<contactref element="DAC4" pad="P3"/>
<contactref element="DAC4" pad="P4"/>
</signal>
<signal name="N$115">
<contactref element="R7" pad="2"/>
<contactref element="DAC5" pad="P3"/>
<contactref element="DAC5" pad="P4"/>
</signal>
<signal name="N$116">
<contactref element="R8" pad="2"/>
<contactref element="DAC6" pad="P3"/>
<contactref element="DAC6" pad="P4"/>
</signal>
<signal name="N$117">
<contactref element="R9" pad="2"/>
<contactref element="DAC7" pad="P3"/>
<contactref element="DAC7" pad="P4"/>
</signal>
<signal name="N$118">
<contactref element="R10" pad="2"/>
<contactref element="DAC8" pad="P3"/>
<contactref element="DAC8" pad="P4"/>
</signal>
<signal name="N$120">
<contactref element="C38" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="OPAMP_A" pad="5"/>
</signal>
<signal name="N$122">
<contactref element="C39" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="OPAMP_A" pad="10"/>
</signal>
<signal name="N$124">
<contactref element="C40" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="OPAMP_A" pad="12"/>
</signal>
<signal name="N$126">
<contactref element="C41" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="OPAMP_B" pad="3"/>
</signal>
<signal name="N$128">
<contactref element="C42" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="OPAMP_B" pad="5"/>
</signal>
<signal name="N$130">
<contactref element="C43" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="OPAMP_B" pad="10"/>
</signal>
<signal name="N$132">
<contactref element="C44" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="OPAMP_B" pad="12"/>
</signal>
<signal name="N$119">
<contactref element="OPAMP_A" pad="6"/>
<contactref element="R22" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="DAC2_OUT">
<contactref element="R30" pad="2"/>
<contactref element="OPAMP_A" pad="7"/>
<contactref element="R38" pad="1"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$123">
<contactref element="OPAMP_A" pad="9"/>
<contactref element="R23" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$125">
<contactref element="R31" pad="2"/>
<contactref element="OPAMP_A" pad="8"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$129">
<contactref element="R32" pad="2"/>
<contactref element="OPAMP_A" pad="14"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$131">
<contactref element="OPAMP_B" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$133">
<contactref element="R33" pad="2"/>
<contactref element="OPAMP_B" pad="1"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$134">
<contactref element="OPAMP_B" pad="6"/>
<contactref element="R26" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$135">
<contactref element="R34" pad="2"/>
<contactref element="OPAMP_B" pad="7"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$136">
<contactref element="OPAMP_B" pad="9"/>
<contactref element="R27" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$137">
<contactref element="R35" pad="2"/>
<contactref element="OPAMP_B" pad="8"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$138">
<contactref element="OPAMP_B" pad="13"/>
<contactref element="R28" pad="2"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$139">
<contactref element="R36" pad="2"/>
<contactref element="OPAMP_B" pad="14"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$142">
<contactref element="R24" pad="2"/>
<contactref element="OPAMP_A" pad="13"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$172">
<contactref element="BRD1" pad="JP2-42"/>
<contactref element="U20-L51P" pad="1"/>
</signal>
<signal name="-5VA">
<contactref element="OPAMP_B" pad="11"/>
<contactref element="C48" pad="2"/>
<contactref element="OPAMP_A" pad="11"/>
<contactref element="-5V_REG" pad="5"/>
<contactref element="R11" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="-5VA" pad="1"/>
<contactref element="C78" pad="2"/>
<contactref element="C79" pad="2"/>
<contactref element="OPAMP_C" pad="11"/>
<contactref element="OPAMP_D" pad="11"/>
<contactref element="C47" pad="2"/>
</signal>
<signal name="DAC_SCLK">
<contactref element="BRD1" pad="JP2-18"/>
<contactref element="LS_CLK" pad="P19"/>
</signal>
<signal name="DAC_!SYNC!">
<contactref element="BRD1" pad="JP2-16"/>
<contactref element="LS_CLK" pad="P18"/>
</signal>
<signal name="N$41">
<contactref element="BRD1" pad="JP2-34"/>
<contactref element="LS_DAC" pad="P14"/>
</signal>
<signal name="N$42">
<contactref element="BRD1" pad="JP2-32"/>
<contactref element="LS_DAC" pad="P15"/>
</signal>
<signal name="N$68">
<contactref element="BRD1" pad="JP2-30"/>
<contactref element="LS_DAC" pad="P16"/>
</signal>
<signal name="N$69">
<contactref element="BRD1" pad="JP2-28"/>
<contactref element="LS_DAC" pad="P17"/>
</signal>
<signal name="N$70">
<contactref element="BRD1" pad="JP2-26"/>
<contactref element="LS_DAC" pad="P18"/>
</signal>
<signal name="N$71">
<contactref element="BRD1" pad="JP2-24"/>
<contactref element="LS_DAC" pad="P19"/>
</signal>
<signal name="N$72">
<contactref element="LS_DAC" pad="P4"/>
<contactref element="DAC2" pad="P7"/>
</signal>
<signal name="N$73">
<contactref element="BRD1" pad="JP2-20"/>
<contactref element="LS_DAC" pad="P21"/>
</signal>
<signal name="OUT9">
<contactref element="BRD1" pad="JP2-62"/>
<contactref element="DIGITAL_OUT_9" pad="1"/>
</signal>
<signal name="OUT10">
<contactref element="BRD1" pad="JP2-64"/>
<contactref element="DIGITAL_OUT_10" pad="1"/>
</signal>
<signal name="OUT11">
<contactref element="BRD1" pad="JP2-66"/>
<contactref element="DIGITAL_OUT_11" pad="1"/>
</signal>
<signal name="OUT12">
<contactref element="BRD1" pad="JP2-68"/>
<contactref element="DIGITAL_OUT_12" pad="1"/>
</signal>
<signal name="OUT13">
<contactref element="BRD1" pad="JP2-70"/>
<contactref element="DIGITAL_OUT_13" pad="1"/>
</signal>
<signal name="OUT14">
<contactref element="BRD1" pad="JP2-72"/>
<contactref element="DIGITAL_OUT_14" pad="1"/>
</signal>
<signal name="OUT15">
<contactref element="BRD1" pad="JP2-74"/>
<contactref element="DIGITAL_OUT_15" pad="1"/>
</signal>
<signal name="N$110">
<contactref element="R37" pad="2"/>
<contactref element="C49" pad="1"/>
</signal>
<signal name="N$121">
<contactref element="R38" pad="2"/>
<contactref element="C50" pad="1"/>
</signal>
<signal name="N$127">
<contactref element="R40" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$140">
<contactref element="R39" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$145">
<contactref element="INVERTER" pad="5"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="N$146">
<contactref element="INVERTER" pad="3"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="-5.5V_UNREG">
<contactref element="-5V_REG" pad="2"/>
<contactref element="-5V_REG" pad="3"/>
<contactref element="L1" pad="2"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="N$150">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="-5V_REG" pad="4"/>
</signal>
<signal name="N$164">
<contactref element="C26" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="INVERTER" pad="1"/>
</signal>
<signal name="N$147">
<contactref element="LS_OUT" pad="P10"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$148">
<contactref element="R48" pad="1"/>
<contactref element="TTL_OUT" pad="P$12"/>
</signal>
<signal name="N$149">
<contactref element="TTL_OUT" pad="P$10"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$151">
<contactref element="R47" pad="2"/>
<contactref element="LS_OUT" pad="P9"/>
</signal>
<signal name="N$152">
<contactref element="LS_OUT" pad="P8"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="N$153">
<contactref element="R46" pad="1"/>
<contactref element="TTL_OUT" pad="P$9"/>
</signal>
<signal name="N$154">
<contactref element="TTL_OUT" pad="P$7"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$155">
<contactref element="R45" pad="2"/>
<contactref element="LS_OUT" pad="P7"/>
</signal>
<signal name="N$203">
<contactref element="LS_OUT" pad="P6"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="N$204">
<contactref element="R44" pad="1"/>
<contactref element="TTL_OUT" pad="P$6"/>
</signal>
<signal name="N$205">
<contactref element="TTL_OUT" pad="P$4"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="N$206">
<contactref element="R43" pad="2"/>
<contactref element="LS_OUT" pad="P5"/>
</signal>
<signal name="N$207">
<contactref element="LS_OUT" pad="P4"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="N$208">
<contactref element="R42" pad="1"/>
<contactref element="TTL_OUT" pad="P$3"/>
</signal>
<signal name="N$209">
<contactref element="TTL_OUT" pad="P$1"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$210">
<contactref element="R41" pad="2"/>
<contactref element="LS_OUT" pad="P3"/>
</signal>
<signal name="N$276">
<contactref element="5.5V_BOOST" pad="3"/>
<contactref element="R69" pad="2"/>
<contactref element="R68" pad="1"/>
</signal>
<signal name="N$278">
<contactref element="D1" pad="POS"/>
<contactref element="L2" pad="2"/>
<contactref element="5.5V_BOOST" pad="1"/>
</signal>
<signal name="N$97">
<contactref element="5VD" pad="4"/>
<contactref element="C52" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="5VD" pad="5"/>
<contactref element="R73" pad="1"/>
<contactref element="C53" pad="2"/>
<contactref element="R72" pad="1"/>
</signal>
<signal name="N$211">
<contactref element="5VA" pad="4"/>
<contactref element="C56" pad="1"/>
</signal>
<signal name="N$213">
<contactref element="5VA" pad="5"/>
<contactref element="R75" pad="1"/>
<contactref element="C57" pad="2"/>
<contactref element="R74" pad="1"/>
</signal>
<signal name="N$99">
<contactref element="BNC" pad="P$SIG"/>
<contactref element="R76" pad="1"/>
</signal>
<signal name="CLOCK_5V">
<contactref element="R76" pad="2"/>
<contactref element="LS_CLK" pad="P7"/>
</signal>
<signal name="N$163">
<contactref element="ADC_IN" pad="P$3"/>
<contactref element="JP_AIN_2" pad="3"/>
<contactref element="OPAMP_C" pad="5"/>
</signal>
<signal name="N$214">
<contactref element="ADC_IN" pad="P$4"/>
<contactref element="JP_AIN_3" pad="3"/>
<contactref element="OPAMP_C" pad="10"/>
</signal>
<signal name="N$216">
<contactref element="ADC_IN" pad="P$7"/>
<contactref element="JP_AIN_5" pad="3"/>
<contactref element="OPAMP_D" pad="3"/>
</signal>
<signal name="N$217">
<contactref element="ADC_IN" pad="P$9"/>
<contactref element="JP_AIN_6" pad="3"/>
<contactref element="OPAMP_D" pad="5"/>
</signal>
<signal name="N$218">
<contactref element="ADC_IN" pad="P$10"/>
<contactref element="JP_AIN_7" pad="3"/>
<contactref element="OPAMP_D" pad="10"/>
</signal>
<signal name="N$219">
<contactref element="ADC_IN" pad="P$12"/>
<contactref element="JP_AIN_8" pad="3"/>
<contactref element="OPAMP_D" pad="12"/>
</signal>
<signal name="N$224">
<contactref element="R49" pad="1"/>
<contactref element="OPAMP_C" pad="1"/>
<contactref element="OPAMP_C" pad="2"/>
</signal>
<signal name="N$223">
<contactref element="R50" pad="1"/>
<contactref element="JP_AIN_1" pad="1"/>
</signal>
<signal name="N$225">
<contactref element="JP_AIN_1" pad="3"/>
<contactref element="ADC_IN" pad="P$1"/>
<contactref element="OPAMP_C" pad="3"/>
</signal>
<signal name="N$227">
<contactref element="R51" pad="1"/>
<contactref element="OPAMP_C" pad="7"/>
<contactref element="OPAMP_C" pad="6"/>
</signal>
<signal name="N$228">
<contactref element="R52" pad="1"/>
<contactref element="JP_AIN_2" pad="1"/>
</signal>
<signal name="N$231">
<contactref element="R53" pad="1"/>
<contactref element="OPAMP_C" pad="8"/>
<contactref element="OPAMP_C" pad="9"/>
</signal>
<signal name="N$232">
<contactref element="R54" pad="1"/>
<contactref element="JP_AIN_3" pad="1"/>
</signal>
<signal name="N$235">
<contactref element="R55" pad="1"/>
<contactref element="OPAMP_C" pad="14"/>
<contactref element="OPAMP_C" pad="13"/>
</signal>
<signal name="N$236">
<contactref element="R56" pad="1"/>
<contactref element="JP_AIN_4" pad="1"/>
</signal>
<signal name="N$238">
<contactref element="JP_AIN_4" pad="3"/>
<contactref element="ADC_IN" pad="P$6"/>
<contactref element="OPAMP_C" pad="12"/>
</signal>
<signal name="N$239">
<contactref element="R57" pad="1"/>
<contactref element="OPAMP_D" pad="1"/>
<contactref element="OPAMP_D" pad="2"/>
</signal>
<signal name="N$240">
<contactref element="R58" pad="1"/>
<contactref element="JP_AIN_5" pad="1"/>
</signal>
<signal name="N$243">
<contactref element="R59" pad="1"/>
<contactref element="OPAMP_D" pad="7"/>
<contactref element="OPAMP_D" pad="6"/>
</signal>
<signal name="N$244">
<contactref element="R60" pad="1"/>
<contactref element="JP_AIN_6" pad="1"/>
</signal>
<signal name="N$247">
<contactref element="R61" pad="1"/>
<contactref element="OPAMP_D" pad="8"/>
<contactref element="OPAMP_D" pad="9"/>
</signal>
<signal name="N$248">
<contactref element="R62" pad="1"/>
<contactref element="JP_AIN_7" pad="1"/>
</signal>
<signal name="N$251">
<contactref element="R63" pad="1"/>
<contactref element="OPAMP_D" pad="14"/>
<contactref element="OPAMP_D" pad="13"/>
</signal>
<signal name="N$252">
<contactref element="R64" pad="1"/>
<contactref element="JP_AIN_8" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="DI"/>
<contactref element="LED1" pad="DO"/>
</signal>
<signal name="N$2">
<contactref element="LED3" pad="DI"/>
<contactref element="LED2" pad="DO"/>
</signal>
<signal name="OUT16">
<contactref element="BRD1" pad="JP2-76"/>
<contactref element="DIGITAL_OUT_16" pad="1"/>
</signal>
<signal name="SR_IN_A">
<contactref element="BRD1" pad="JP3-74"/>
<contactref element="A16-L63N" pad="1"/>
</signal>
<signal name="SR_IN_B">
<contactref element="BRD1" pad="JP3-72"/>
<contactref element="B16-L63P" pad="1"/>
</signal>
<signal name="LED_DAT">
<contactref element="BRD1" pad="JP3-68"/>
<contactref element="LED_DAT" pad="1"/>
<contactref element="LS_LED" pad="P21"/>
</signal>
<signal name="SR_CLR">
<contactref element="BRD1" pad="JP3-70"/>
<contactref element="A14-L50N" pad="1"/>
</signal>
<signal name="ADC_REF">
<contactref element="ADC_REF" pad="P6"/>
<contactref element="C61" pad="1"/>
<contactref element="C59" pad="+"/>
<contactref element="ADC8" pad="P1"/>
<contactref element="ADC7" pad="P1"/>
<contactref element="ADC6" pad="P1"/>
<contactref element="ADC5" pad="P1"/>
<contactref element="ADC4" pad="P1"/>
<contactref element="ADC3" pad="P1"/>
<contactref element="ADC2" pad="P1"/>
<contactref element="ADC1" pad="P1"/>
</signal>
<signal name="+5VA">
<contactref element="5VA" pad="6"/>
<contactref element="C57" pad="1"/>
<contactref element="C58" pad="1"/>
<contactref element="R75" pad="2"/>
<contactref element="ADC_REF" pad="P2"/>
<contactref element="C60" pad="1"/>
<contactref element="OPAMP_A" pad="4"/>
<contactref element="C46" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="OPAMP_B" pad="4"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="DAC_OUT" pad="P$18"/>
<contactref element="+5VA" pad="1"/>
<contactref element="C76" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="OPAMP_C" pad="4"/>
<contactref element="OPAMP_D" pad="4"/>
<contactref element="ADC_IN" pad="P$18"/>
<contactref element="R50" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R56" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R62" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="DAC_REF" pad="P2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="+5VD">
<contactref element="ADC8" pad="P8"/>
<contactref element="ADC7" pad="P8"/>
<contactref element="ADC6" pad="P8"/>
<contactref element="ADC5" pad="P8"/>
<contactref element="ADC4" pad="P8"/>
<contactref element="ADC3" pad="P8"/>
<contactref element="ADC2" pad="P8"/>
<contactref element="ADC1" pad="P8"/>
<contactref element="C20" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="LS_IN" pad="P1"/>
<contactref element="LS_ADC" pad="P1"/>
<contactref element="LS_ADC" pad="P2"/>
<contactref element="LS_IN" pad="P2"/>
<contactref element="LS_DAC" pad="P1"/>
<contactref element="5VD" pad="6"/>
<contactref element="C53" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="R73" pad="2"/>
<contactref element="TTL_OUT" pad="P$18"/>
<contactref element="LS_OUT" pad="P1"/>
<contactref element="LS_CLK" pad="P1"/>
<contactref element="LS_I2C" pad="P7"/>
<contactref element="C71" pad="1"/>
<contactref element="C70" pad="1"/>
<contactref element="C72" pad="1"/>
<contactref element="C75" pad="1"/>
<contactref element="C73" pad="1"/>
<contactref element="+5VD_1" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="DAC1" pad="P1"/>
<contactref element="DAC2" pad="P1"/>
<contactref element="DAC3" pad="P1"/>
<contactref element="DAC4" pad="P1"/>
<contactref element="DAC5" pad="P1"/>
<contactref element="DAC6" pad="P1"/>
<contactref element="DAC7" pad="P1"/>
<contactref element="DAC8" pad="P1"/>
<contactref element="+5VD" pad="1"/>
<contactref element="LS_LED" pad="P1"/>
<contactref element="C88" pad="1"/>
<contactref element="TTL_IN" pad="P$18"/>
</signal>
<signal name="DAC_REF">
<contactref element="DAC_REF" pad="P6"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="+"/>
<contactref element="DAC8" pad="P2"/>
<contactref element="DAC7" pad="P2"/>
<contactref element="DAC6" pad="P2"/>
<contactref element="DAC5" pad="P2"/>
<contactref element="DAC4" pad="P2"/>
<contactref element="DAC3" pad="P2"/>
<contactref element="DAC2" pad="P2"/>
<contactref element="DAC1" pad="P2"/>
</signal>
<signal name="LED_DAT_OUT">
<contactref element="LED8" pad="DO"/>
</signal>
<signal name="N$13">
<contactref element="R86" pad="2"/>
<contactref element="R85" pad="1"/>
<contactref element="C97" pad="2"/>
<contactref element="3.5VREG2" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="C94" pad="1"/>
<contactref element="3.5VREG2" pad="4"/>
</signal>
<signal name="N$1115">
<contactref element="R88" pad="2"/>
<contactref element="R87" pad="1"/>
<contactref element="C101" pad="2"/>
<contactref element="3.5VREG3" pad="5"/>
</signal>
<signal name="PROTO_GRID">
</signal>
<signal name="N$197">
</signal>
<signal name="N$198">
</signal>
<signal name="N$5">
<contactref element="LED5" pad="DO"/>
<contactref element="LED6" pad="DI"/>
</signal>
<signal name="N$6">
<contactref element="LED6" pad="DO"/>
<contactref element="LED7" pad="DI"/>
</signal>
<signal name="N$7">
<contactref element="LED7" pad="DO"/>
<contactref element="LED8" pad="DI"/>
</signal>
<signal name="N$9">
<contactref element="R67" pad="1"/>
<contactref element="LED1" pad="DI"/>
</signal>
<signal name="N$3">
<contactref element="LED4" pad="DI"/>
<contactref element="LED3" pad="DO"/>
</signal>
<signal name="N$4">
<contactref element="LED5" pad="DI"/>
<contactref element="LED4" pad="DO"/>
</signal>
<signal name="N$10">
<contactref element="C23" pad="1"/>
<contactref element="3.5VREG1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="R71" pad="2"/>
<contactref element="R70" pad="1"/>
<contactref element="C93" pad="2"/>
<contactref element="3.5VREG1" pad="5"/>
</signal>
<signal name="DAISYCHAIN_IN">
<contactref element="DAISY_CHAIN_CONNECTOR" pad="7"/>
<contactref element="R65" pad="1"/>
<contactref element="BRD1" pad="JP3-34"/>
</signal>
<signal name="N$24">
<contactref element="DAISY_CHAIN_CONNECTOR" pad="4"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="+3V5B">
<contactref element="C92" pad="1"/>
<contactref element="3.5VREG1" pad="6"/>
<contactref element="C93" pad="1"/>
<contactref element="R70" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="B" pad="B6"/>
</signal>
<signal name="+3V5A">
<contactref element="+3V5_1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="3.5VREG" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="A" pad="B6"/>
</signal>
<signal name="N$14">
<contactref element="C98" pad="1"/>
<contactref element="3.5VREG3" pad="4"/>
</signal>
<signal name="+3V5C">
<contactref element="C96" pad="1"/>
<contactref element="3.5VREG2" pad="6"/>
<contactref element="C97" pad="1"/>
<contactref element="R85" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C" pad="B6"/>
</signal>
<signal name="+3V5D">
<contactref element="C100" pad="1"/>
<contactref element="3.5VREG3" pad="6"/>
<contactref element="C101" pad="1"/>
<contactref element="R87" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="D" pad="B6"/>
</signal>
<signal name="N$8">
</signal>
<signal name="PROTO_GRID1">
</signal>
<signal name="PROTO_GRID2">
</signal>
<signal name="N$25">
<contactref element="J2" pad="1"/>
<contactref element="POLYFUSE" pad="1"/>
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$86">
<contactref element="LS_LED" pad="P3"/>
<contactref element="R67" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
