(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)")
  (general
    (thickness 1.6)
    (drawings 163)
    (tracks 991)
    (zones 0)
    (modules 66)
    (nets 204)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.4572)
    (uvia_drill 0.2032)
    (uvias_allowed no)
    (uvia_min_size 0.4572)
    (uvia_min_drill 0.2032)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0254)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 84.582 56.1848)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U2-Pad9)")
  (net 2 "Net-(U2-Pad11)")
  (net 3 GND)
  (net 4 "Net-(U1-PadA4)")
  (net 5 "Net-(U1-PadA9)")
  (net 6 "Net-(U1-PadA10)")
  (net 7 "Net-(U1-PadA11)")
  (net 8 "Net-(U1-PadA12)")
  (net 9 "Net-(U1-PadA13)")
  (net 10 "Net-(U1-PadA15)")
  (net 11 "Net-(U1-PadA17)")
  (net 12 "Net-(U1-PadA19)")
  (net 13 "Net-(U1-PadB9)")
  (net 14 "Net-(U1-PadB10)")
  (net 15 "Net-(U1-PadB11)")
  (net 16 "Net-(U1-PadB12)")
  (net 17 "Net-(U1-PadB13)")
  (net 18 "Net-(U1-PadB14)")
  (net 19 "Net-(U1-PadB15)")
  (net 20 "Net-(U1-PadB16)")
  (net 21 "Net-(U1-PadC9)")
  (net 22 "Net-(U1-PadC10)")
  (net 23 "Net-(U1-PadC11)")
  (net 24 "Net-(U1-PadC12)")
  (net 25 "Net-(U1-PadC14)")
  (net 26 "Net-(U1-PadC15)")
  (net 27 "Net-(U1-PadC16)")
  (net 28 "Net-(U1-PadD10)")
  (net 29 "Net-(U1-PadD11)")
  (net 30 "Net-(U1-PadD13)")
  (net 31 "Net-(U1-PadF18)")
  (net 32 "Net-(U1-PadF19)")
  (net 33 "Net-(U1-PadG17)")
  (net 34 "Net-(U1-PadJ3)")
  (net 35 "Net-(U1-PadJ17)")
  (net 36 "Net-(U1-PadK3)")
  (net 37 "Net-(U1-PadK18)")
  (net 38 "Net-(U1-PadK19)")
  (net 39 "Net-(U1-PadK20)")
  (net 40 "Net-(U1-PadL3)")
  (net 41 LCD_D15)
  (net 42 "Net-(U1-PadL19)")
  (net 43 "Net-(U1-PadL20)")
  (net 44 "Net-(U1-PadM3)")
  (net 45 "Net-(U1-PadM1)")
  (net 46 "Net-(U1-PadM6)")
  (net 47 LCD_D12)
  (net 48 LCD_D13)
  (net 49 LCD_D14)
  (net 50 "Net-(U1-PadN3)")
  (net 51 "Net-(U1-PadN1)")
  (net 52 "Net-(U1-PadN2)")
  (net 53 LCD_D9)
  (net 54 LCD_D10)
  (net 55 LCD_D11)
  (net 56 "Net-(U1-PadP3)")
  (net 57 "Net-(U1-PadP1)")
  (net 58 "Net-(U1-PadP2)")
  (net 59 LCD_D6)
  (net 60 LCD_D7)
  (net 61 LCD_D8)
  (net 62 "Net-(U1-PadR13)")
  (net 63 "Net-(U1-PadR3)")
  (net 64 "Net-(U1-PadR1)")
  (net 65 "Net-(U1-PadR2)")
  (net 66 LCD_D3)
  (net 67 LCD_D4)
  (net 68 LCD_D5)
  (net 69 "Net-(U1-PadT3)")
  (net 70 "Net-(U1-PadT1)")
  (net 71 "Net-(U1-PadT2)")
  (net 72 LCD_D0)
  (net 73 LCD_D1)
  (net 74 LCD_D2)
  (net 75 "Net-(U1-PadU13)")
  (net 76 "Net-(U1-PadU12)")
  (net 77 "Net-(U1-PadU10)")
  (net 78 "Net-(U1-PadU8)")
  (net 79 "Net-(U1-PadU9)")
  (net 80 "Net-(U1-PadU7)")
  (net 81 "Net-(U1-PadU3)")
  (net 82 "Net-(U1-PadU1)")
  (net 83 "Net-(U1-PadU2)")
  (net 84 "Net-(U1-PadU6)")
  (net 85 "Net-(U1-PadU14)")
  (net 86 "Net-(U1-PadU18)")
  (net 87 "Net-(U1-PadU19)")
  (net 88 "Net-(U1-PadV13)")
  (net 89 "Net-(U1-PadV11)")
  (net 90 "Net-(U1-PadV12)")
  (net 91 "Net-(U1-PadV10)")
  (net 92 "Net-(U1-PadV9)")
  (net 93 "Net-(U1-PadV1)")
  (net 94 "Net-(U1-PadV5)")
  (net 95 "Net-(U1-PadV6)")
  (net 96 "Net-(U1-PadV15)")
  (net 97 "Net-(U1-PadV14)")
  (net 98 "Net-(U1-PadV17)")
  (net 99 "Net-(U1-PadV20)")
  (net 100 "Net-(U1-PadW10)")
  (net 101 "Net-(U1-PadW9)")
  (net 102 "Net-(U1-PadW8)")
  (net 103 "Net-(U1-PadW1)")
  (net 104 "Net-(U1-PadW5)")
  (net 105 "Net-(U1-PadW16)")
  (net 106 "Net-(U1-PadW15)")
  (net 107 "Net-(U1-PadW13)")
  (net 108 "Net-(U1-PadW14)")
  (net 109 "Net-(U1-PadW12)")
  (net 110 "Net-(U1-PadW11)")
  (net 111 "Net-(U1-PadW17)")
  (net 112 "Net-(U1-PadY10)")
  (net 113 "Net-(U1-PadY8)")
  (net 114 "Net-(U1-PadY15)")
  (net 115 "Net-(U1-PadY13)")
  (net 116 "Net-(U1-PadY14)")
  (net 117 "Net-(U1-PadY11)")
  (net 118 "Net-(U1-PadY17)")
  (net 119 SYS_VDD1_3P3V)
  (net 120 "Net-(RN4-Pad1)")
  (net 121 "Net-(RN4-Pad2)")
  (net 122 "Net-(RN4-Pad7)")
  (net 123 "Net-(RN4-Pad8)")
  (net 124 MMC0_DAT2)
  (net 125 MMC0_DAT3)
  (net 126 MMC0_CMD)
  (net 127 MMC0_CLK)
  (net 128 MMC0_DAT0)
  (net 129 MMC0_DAT1)
  (net 130 GNDPWR)
  (net 131 "Net-(FB2-Pad1)")
  (net 132 "Net-(SW1-Pad2)")
  (net 133 USB0_VBUS)
  (net 134 VIN_AC)
  (net 135 VBAT)
  (net 136 "Net-(R1-Pad1)")
  (net 137 SYS_VDD2_3P3V)
  (net 138 SYS_VOUT)
  (net 139 USB1_DRVVBUS)
  (net 140 USB1_VBUS)
  (net 141 SYS_VDD3_3P3V)
  (net 142 SYS_VDD_1P8V)
  (net 143 USB0_ID)
  (net 144 "Net-(J4-Pad1)")
  (net 145 MMC0_CD)
  (net 146 I2C1_SCL)
  (net 147 UART0_TXD)
  (net 148 I2C1_SDA)
  (net 149 UART0_RXD)
  (net 150 "Net-(C5-Pad1)")
  (net 151 "Net-(FB1-Pad1)")
  (net 152 "Net-(SW2-Pad2)")
  (net 153 USB1_ID)
  (net 154 "Net-(IC1-Pad5)")
  (net 155 "Net-(IC2-Pad5)")
  (net 156 VBOOST)
  (net 157 "Net-(U5-Pad3)")
  (net 158 "Net-(U4-Pad6)")
  (net 159 "Net-(R3-Pad2)")
  (net 160 "Net-(R2-Pad2)")
  (net 161 "Net-(L1-Pad2)")
  (net 162 "Net-(R7-Pad1)")
  (net 163 "Net-(D1-Pad3)")
  (net 164 "Net-(D1-Pad4)")
  (net 165 "Net-(D1-Pad1)")
  (net 166 "Net-(D2-Pad3)")
  (net 167 "Net-(D2-Pad4)")
  (net 168 "Net-(D2-Pad1)")
  (net 169 USB1_D-)
  (net 170 USB1_D+)
  (net 171 USB0_D-)
  (net 172 USB0_D+)
  (net 173 "Net-(U1-PadV18)")
  (net 174 "Net-(U1-PadV19)")
  (net 175 "Net-(U1-PadW19)")
  (net 176 "Net-(U1-PadW18)")
  (net 177 "Net-(U1-PadW20)")
  (net 178 "Net-(U1-PadY19)")
  (net 179 "Net-(U1-PadY18)")
  (net 180 "Net-(X1-Pad14)")
  (net 181 "Net-(X1-Pad1)")
  (net 182 SPI0_MOSI)
  (net 183 SPI0_nCS0)
  (net 184 SPI0_SCLK)
  (net 185 LCD_PWM)
  (net 186 "Net-(Q1-Pad1)")
  (net 187 "Net-(Q1-Pad3)")
  (net 188 "Net-(R16-Pad1)")
  (net 189 LCD_RS)
  (net 190 LCD_RESET)
  (net 191 "Net-(Q2-Pad3)")
  (net 192 "Net-(Q2-Pad1)")
  (net 193 "Net-(Q3-Pad3)")
  (net 194 "Net-(Q3-Pad1)")
  (net 195 "Net-(Q4-Pad3)")
  (net 196 "Net-(Q4-Pad1)")
  (net 197 PWM_RED)
  (net 198 PWM_GREEN)
  (net 199 PWM_BLUE)
  (net 200 "Net-(RN5-Pad8)")
  (net 201 "Net-(RN5-Pad1)")
  (net 202 "Net-(RN6-Pad8)")
  (net 203 "Net-(RN6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.2032)
    (add_net GND)
    (add_net GNDPWR)
    (add_net I2C1_SCL)
    (add_net I2C1_SDA)
    (add_net LCD_D0)
    (add_net LCD_D1)
    (add_net LCD_D10)
    (add_net LCD_D11)
    (add_net LCD_D12)
    (add_net LCD_D13)
    (add_net LCD_D14)
    (add_net LCD_D15)
    (add_net LCD_D2)
    (add_net LCD_D3)
    (add_net LCD_D4)
    (add_net LCD_D5)
    (add_net LCD_D6)
    (add_net LCD_D7)
    (add_net LCD_D8)
    (add_net LCD_D9)
    (add_net LCD_PWM)
    (add_net LCD_RESET)
    (add_net LCD_RS)
    (add_net MMC0_CD)
    (add_net MMC0_CLK)
    (add_net MMC0_CMD)
    (add_net MMC0_DAT0)
    (add_net MMC0_DAT1)
    (add_net MMC0_DAT2)
    (add_net MMC0_DAT3)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(FB1-Pad1)")
    (add_net "Net-(FB2-Pad1)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC2-Pad5)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(RN4-Pad1)")
    (add_net "Net-(RN4-Pad2)")
    (add_net "Net-(RN4-Pad7)")
    (add_net "Net-(RN4-Pad8)")
    (add_net "Net-(RN5-Pad1)")
    (add_net "Net-(RN5-Pad8)")
    (add_net "Net-(RN6-Pad1)")
    (add_net "Net-(RN6-Pad8)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(U1-PadA10)")
    (add_net "Net-(U1-PadA11)")
    (add_net "Net-(U1-PadA12)")
    (add_net "Net-(U1-PadA13)")
    (add_net "Net-(U1-PadA15)")
    (add_net "Net-(U1-PadA17)")
    (add_net "Net-(U1-PadA19)")
    (add_net "Net-(U1-PadA4)")
    (add_net "Net-(U1-PadA9)")
    (add_net "Net-(U1-PadB10)")
    (add_net "Net-(U1-PadB11)")
    (add_net "Net-(U1-PadB12)")
    (add_net "Net-(U1-PadB13)")
    (add_net "Net-(U1-PadB14)")
    (add_net "Net-(U1-PadB15)")
    (add_net "Net-(U1-PadB16)")
    (add_net "Net-(U1-PadB9)")
    (add_net "Net-(U1-PadC10)")
    (add_net "Net-(U1-PadC11)")
    (add_net "Net-(U1-PadC12)")
    (add_net "Net-(U1-PadC14)")
    (add_net "Net-(U1-PadC15)")
    (add_net "Net-(U1-PadC16)")
    (add_net "Net-(U1-PadC9)")
    (add_net "Net-(U1-PadD10)")
    (add_net "Net-(U1-PadD11)")
    (add_net "Net-(U1-PadD13)")
    (add_net "Net-(U1-PadF18)")
    (add_net "Net-(U1-PadF19)")
    (add_net "Net-(U1-PadG17)")
    (add_net "Net-(U1-PadJ17)")
    (add_net "Net-(U1-PadJ3)")
    (add_net "Net-(U1-PadK18)")
    (add_net "Net-(U1-PadK19)")
    (add_net "Net-(U1-PadK20)")
    (add_net "Net-(U1-PadK3)")
    (add_net "Net-(U1-PadL19)")
    (add_net "Net-(U1-PadL20)")
    (add_net "Net-(U1-PadL3)")
    (add_net "Net-(U1-PadM1)")
    (add_net "Net-(U1-PadM3)")
    (add_net "Net-(U1-PadM6)")
    (add_net "Net-(U1-PadN1)")
    (add_net "Net-(U1-PadN2)")
    (add_net "Net-(U1-PadN3)")
    (add_net "Net-(U1-PadP1)")
    (add_net "Net-(U1-PadP2)")
    (add_net "Net-(U1-PadP3)")
    (add_net "Net-(U1-PadR1)")
    (add_net "Net-(U1-PadR13)")
    (add_net "Net-(U1-PadR2)")
    (add_net "Net-(U1-PadR3)")
    (add_net "Net-(U1-PadT1)")
    (add_net "Net-(U1-PadT2)")
    (add_net "Net-(U1-PadT3)")
    (add_net "Net-(U1-PadU1)")
    (add_net "Net-(U1-PadU10)")
    (add_net "Net-(U1-PadU12)")
    (add_net "Net-(U1-PadU13)")
    (add_net "Net-(U1-PadU14)")
    (add_net "Net-(U1-PadU18)")
    (add_net "Net-(U1-PadU19)")
    (add_net "Net-(U1-PadU2)")
    (add_net "Net-(U1-PadU3)")
    (add_net "Net-(U1-PadU6)")
    (add_net "Net-(U1-PadU7)")
    (add_net "Net-(U1-PadU8)")
    (add_net "Net-(U1-PadU9)")
    (add_net "Net-(U1-PadV1)")
    (add_net "Net-(U1-PadV10)")
    (add_net "Net-(U1-PadV11)")
    (add_net "Net-(U1-PadV12)")
    (add_net "Net-(U1-PadV13)")
    (add_net "Net-(U1-PadV14)")
    (add_net "Net-(U1-PadV15)")
    (add_net "Net-(U1-PadV17)")
    (add_net "Net-(U1-PadV18)")
    (add_net "Net-(U1-PadV19)")
    (add_net "Net-(U1-PadV20)")
    (add_net "Net-(U1-PadV5)")
    (add_net "Net-(U1-PadV6)")
    (add_net "Net-(U1-PadV9)")
    (add_net "Net-(U1-PadW1)")
    (add_net "Net-(U1-PadW10)")
    (add_net "Net-(U1-PadW11)")
    (add_net "Net-(U1-PadW12)")
    (add_net "Net-(U1-PadW13)")
    (add_net "Net-(U1-PadW14)")
    (add_net "Net-(U1-PadW15)")
    (add_net "Net-(U1-PadW16)")
    (add_net "Net-(U1-PadW17)")
    (add_net "Net-(U1-PadW18)")
    (add_net "Net-(U1-PadW19)")
    (add_net "Net-(U1-PadW20)")
    (add_net "Net-(U1-PadW5)")
    (add_net "Net-(U1-PadW8)")
    (add_net "Net-(U1-PadW9)")
    (add_net "Net-(U1-PadY10)")
    (add_net "Net-(U1-PadY11)")
    (add_net "Net-(U1-PadY13)")
    (add_net "Net-(U1-PadY14)")
    (add_net "Net-(U1-PadY15)")
    (add_net "Net-(U1-PadY17)")
    (add_net "Net-(U1-PadY18)")
    (add_net "Net-(U1-PadY19)")
    (add_net "Net-(U1-PadY8)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(X1-Pad1)")
    (add_net "Net-(X1-Pad14)")
    (add_net PWM_BLUE)
    (add_net PWM_GREEN)
    (add_net PWM_RED)
    (add_net SPI0_MOSI)
    (add_net SPI0_SCLK)
    (add_net SPI0_nCS0)
    (add_net SYS_VDD1_3P3V)
    (add_net SYS_VDD2_3P3V)
    (add_net SYS_VDD3_3P3V)
    (add_net SYS_VDD_1P8V)
    (add_net SYS_VOUT)
    (add_net UART0_RXD)
    (add_net UART0_TXD)
    (add_net USB0_D+)
    (add_net USB0_D-)
    (add_net USB0_ID)
    (add_net USB0_VBUS)
    (add_net USB1_D+)
    (add_net USB1_D-)
    (add_net USB1_DRVVBUS)
    (add_net USB1_ID)
    (add_net USB1_VBUS)
    (add_net VBAT)
    (add_net VBOOST)
    (add_net VIN_AC)
  )
  (module lichen-badge:LED_SubLED_PLCC4_3.2x2.8mm_Reverse_Mount (layer F.Cu) (tedit 5D3F3257)
    (at 109.4994 83.312)
    (descr "3.2mm x 2.8mm PLCC4 LED, http://www.cree.com/led-components/media/documents/CLV1AFKB(874).pdf")
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference D2 (at 0 -2.65) (layer F.SilkS))
    (fp_text value LED_RABG (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -2.6 -0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 138 SYS_VOUT))
    (pad 1 smd rect (at 2.6 -0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(D2-Pad1)"))
    (pad 4 smd rect (at 2.6 0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(D2-Pad4)"))
    (pad 3 smd rect (at -2.6 0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(D2-Pad3)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-PLCC4_3.2x2.8mm_CCW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lichen-badge:LED_SubLED_PLCC4_3.2x2.8mm_Reverse_Mount (layer F.Cu) (tedit 5D3F3257)
    (at 95.1484 83.8708)
    (descr "3.2mm x 2.8mm PLCC4 LED, http://www.cree.com/led-components/media/documents/CLV1AFKB(874).pdf")
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference D1 (at 0 -2.65) (layer F.SilkS))
    (fp_text value LED_RABG (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -2.6 -0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 138 SYS_VOUT))
    (pad 1 smd rect (at 2.6 -0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at 2.6 0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -2.6 0.725) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-PLCC4_3.2x2.8mm_CCW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_6.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 100.076 65.6844)
    (descr "Mounting Hole 6.5mm, no annular")
    (tags "mounting hole 6.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -7.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.5 6.5) (drill 6.5) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_Array_Convex_4x0402 (layer F.Cu) (tedit 58E0A8A8)
    (at 109.3724 77.0128 90)
    (descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN6 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(Q2-Pad3)"))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(Q3-Pad3)"))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(RN6-Pad8)"))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(Q4-Pad3)"))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(D2-Pad3)"))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(D2-Pad4)"))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(RN6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0402 (layer F.Cu) (tedit 58E0A8A8)
    (at 95.25 77.0128 90)
    (descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN5 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(Q2-Pad3)"))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(Q3-Pad3)"))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(RN5-Pad8)"))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(Q4-Pad3)"))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(D1-Pad3)"))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(RN5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.852 81.98358)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 2.9718 0.05842) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 196 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.852 89.7128)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 3.1496 -0.0254) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 194 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.852 97.3328)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 3.175 0.0254) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 192 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.852 80.53578 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -2.921 -0.00762) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 199 PWM_BLUE))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 196 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.852 88.4428 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -3.048 0.1016) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 198 PWM_GREEN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 194 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.852 95.87738 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -3.1242 0.06858) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 197 PWM_RED))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 192 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 85.344 77.411579 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.9464 -0.007621) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(Q4-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 85.344 85.6488 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -3.175 -0.0254) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 85.344 92.7608 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -3.2512 -0.0254) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_EVQP2 (layer F.Cu) (tedit 5A02FC95)
    (at 108.03636 104.08412 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW3 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value BOOT0 (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 2 smd rect (at 2.58 1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -2.58 1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.58 -1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(R7-Pad1)"))
    (pad 1 smd rect (at 2.58 -1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_EVQP2 (layer F.Cu) (tedit 5A02FC95)
    (at 97.26676 104.08412 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value RESET (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 2 smd rect (at 2.58 1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(SW2-Pad2)"))
    (pad 2 smd rect (at -2.58 1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at -2.58 -1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 2.58 -1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_EVQP2 (layer F.Cu) (tedit 5A02FC95)
    (at 87.10676 104.08412 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value POWER (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 2 smd rect (at 2.58 1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at -2.58 1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -2.58 -1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 2.58 -1 90) (size 1.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 123.03252 140.07592 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.8499 142.07998)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 22 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 187 "Net-(Q1-Pad3)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 188 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.22276 141.03096)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 470 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 186 "Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 185 LCD_PWM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "lichen-badge:LCD-(1.8IN)" (layer B.Cu) (tedit 0)
    (at 97.6884 140.462 270)
    (fp_text reference X1 (at 15.748 -19.812 180) (layer B.SilkS) hide)
    (fp_text value "SPI-LCD-(1.8IN)" (at -3.0648 5.5768 90) (layer B.Fab))
    (fp_text user 1 (at 4.9992 -14.532 90) (layer B.SilkS))
    (pad 1 smd rect (at 5.2 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 181 "Net-(X1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 4.4 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 3.6 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 188 "Net-(R16-Pad1)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 2.8 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 119 SYS_VDD1_3P3V) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 2 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 1.2 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 190 LCD_RESET) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at 0.4 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 189 LCD_RS) (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -0.4 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 182 SPI0_MOSI) (solder_mask_margin 0.1016))
    (pad 9 smd rect (at -1.2 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 184 SPI0_SCLK) (solder_mask_margin 0.1016))
    (pad 10 smd rect (at -2 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 119 SYS_VDD1_3P3V) (solder_mask_margin 0.1016))
    (pad 11 smd rect (at -2.8 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 119 SYS_VDD1_3P3V) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at -3.6 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 183 SPI0_nCS0) (solder_mask_margin 0.1016))
    (pad 13 smd rect (at -4.4 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 14 smd rect (at -5.2 -12.532) (size 1.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 180 "Net-(X1-Pad14)") (solder_mask_margin 0.1016))
    (pad "" np_thru_hole circle (at -12.8 -16.532 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.65 -16.532 270) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.808 142.2908 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.35966 -0.254) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 MMC0_DAT2))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Card:microSD_HC_Hirose_DM3AT-SF-PEJM5 (layer F.Cu) (tedit 5A1DBFB5)
    (at 122.41022 162.97656 20)
    (descr "Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J1 (at -8.02 -7.366 290) (layer F.SilkS))
    (fp_text value Micro_SD_Card_Det (at -0.075 9.575 20) (layer F.Fab))
    (fp_text user KEEPOUT (at -5.775 2.375 110) (layer Cmts.User))
    (fp_text user KEEPOUT (at -6.85 -3.25 110) (layer Cmts.User))
    (fp_text user KEEPOUT (at 4.2 7.65 20) (layer Cmts.User))
    (fp_text user %R (at -0.075 0.375 20) (layer F.Fab))
    (fp_text user KEEPOUT (at -1.075 -1.925 20) (layer Cmts.User))
    (pad 11 smd rect (at 6.675 7.375 20) (size 1.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 11 smd rect (at -6.825 6.925 20) (size 1 2.8) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 10 smd rect (at -6.825 2.775 20) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 145 MMC0_CD))
    (pad 11 smd rect (at -6.825 -3.425 20) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 11 smd rect (at 4.325 -7.725 20) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 7 smd rect (at -3.825 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 128 MMC0_DAT0))
    (pad 6 smd rect (at -2.725 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at -1.625 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 127 MMC0_CLK))
    (pad 4 smd rect (at -0.525 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad 3 smd rect (at 0.575 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 126 MMC0_CMD))
    (pad 2 smd rect (at 1.675 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 125 MMC0_DAT3))
    (pad 1 smd rect (at 2.775 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 124 MMC0_DAT2))
    (pad 8 smd rect (at -4.925 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 129 MMC0_DAT1))
    (pad 9 smd rect (at -5.875 -7.725 20) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3AT-SF-PEJM5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 105.9688 150.749)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J7 (at 1.26238 1.3462) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 GND))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 103.4288 150.749)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J4 (at -1.48082 1.15316) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 144 "Net-(J4-Pad1)"))
  )
  (module Connector_Molex:Molex_PicoBlade_53261-0471_1x04-1MP_P1.25mm_Horizontal (layer F.Cu) (tedit 5B78AD89)
    (at 128.9304 129.4384 114)
    (descr "Molex PicoBlade series connector, 53261-0471 (http://www.molex.com/pdm_docs/sd/532610271_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (attr smd)
    (fp_text reference J6 (at 0 -4.4 114) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 3.8 114) (layer F.Fab))
    (fp_text user %R (at 0 1.9 114) (layer F.Fab))
    (pad 1 smd roundrect (at -1.875 -2.4 114) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at -0.625 -2.4 114) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 149 UART0_RXD))
    (pad 3 smd roundrect (at 0.625 -2.4 114) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 UART0_TXD))
    (pad 4 smd roundrect (at 1.875 -2.4 114) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 VIN_AC))
    (pad MP smd roundrect (at -4.425 0.5 114) (size 2.1 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.119048))
    (pad MP smd roundrect (at 4.425 0.5 114) (size 2.1 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.119048))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53261-0471_1x04-1MP_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 92.8624 120.2182 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.34442 0.02286 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 94.488 119.8118 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference C9 (at 2.794 0.0508 90) (layer F.SilkS))
    (fp_text value 47uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 SYS_VOUT))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 92.6592 160.8836 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB4 (at -0.1778 1.4986 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 GNDPWR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 106.3498 160.8836 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB3 (at -0.1016 1.6764 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 GNDPWR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.7062 160.8836 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 USB1_VBUS))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(FB2-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101.3968 160.8836 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 USB0_VBUS))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 151 "Net-(FB1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.02976 111.04626 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.01792 1.51638 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 LCD_D2))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 162 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.808 151.6888 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.14376 -0.0254) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 114.808 149.9108 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.06756 -0.00508) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 108.458 150.6958 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -3.20026 0.0254 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 MMC0_CD))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.728 150.6958 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -3.22566 0.07366 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 MMC0_DAT1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.808 143.8148 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -2.77622 -0.09398) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 MMC0_DAT0))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 110.998 150.6958 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -3.22566 0.17272 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 MMC0_CLK))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.808 146.8628 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -2.79146 0.10414) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 MMC0_CMD))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.808 145.3388 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.32918 0.00508) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 MMC0_DAT3))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.183 138.01852 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.1082 0.1778 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 159 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 68.4022 138.01852 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.1336 0 90) (layer F.SilkS))
    (fp_text value 750K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 159 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 156 VBOOST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 70.46722 129.58572)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.0828 0.0254) (layer F.SilkS))
    (fp_text value 750K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 160 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Taiyo-Yuden_MD-4040 (layer F.Cu) (tedit 5990349C)
    (at 70.61962 126.56312)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-4040, 4.0mmx4.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L1 (at 3.28422 -0.01778) (layer F.SilkS))
    (fp_text value 2.2uH (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0) (size 1.2 3.7) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(L1-Pad2)"))
    (pad 1 smd rect (at -1.4 0) (size 1.2 3.7) (layers F.Cu F.Paste F.Mask)
      (net 135 VBAT))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_MD-4040.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 71.73722 140.60932)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.8448 0.0762) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 156 VBOOST))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 71.73722 138.24712)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.8194 0.127) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 156 VBOOST))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 70.17004 123.07316)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 3.10134 0.0762) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.9736 137.16 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 4.7K (at -0.0254 -1.1684) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 I2C1_SDA))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 115.6208 137.16)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 1.2192) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 I2C1_SCL))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.9604 133.1214 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.17) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 150 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 119.4816 129.7432 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 SYS_VDD1_3P3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0402 (layer F.Cu) (tedit 58E0A8A8)
    (at 101.14896 118.0672 90)
    (descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at -0.627 -1.88576 90) (layer F.SilkS))
    (fp_text value 100K (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(RN4-Pad8)"))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(RN4-Pad7)"))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 LCD_D12))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(RN4-Pad2)"))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 LCD_D13))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(RN4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0402 (layer F.Cu) (tedit 58E0A8A8)
    (at 103.62438 115.57508 90)
    (descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0.66548 -2.02438 90) (layer F.SilkS))
    (fp_text value 100K (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 61 LCD_D8))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 LCD_D10))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 LCD_D9))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 55 LCD_D11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0402 (layer F.Cu) (tedit 58E0A8A8)
    (at 106.0062 118.14086 90)
    (descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at -0.70574 -2.044 90) (layer F.SilkS))
    (fp_text value 100K (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 67 LCD_D4))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 LCD_D6))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 LCD_D5))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 LCD_D7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0402 (layer F.Cu) (tedit 58E0A8A8)
    (at 108.35894 115.43284 90)
    (descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0.57404 -1.93294 90) (layer F.SilkS))
    (fp_text value 100K (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 LCD_D0))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 LCD_D2))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 LCD_D1))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 66 LCD_D3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 70.46722 133.82752 270)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at 0 -2.6 90) (layer F.SilkS))
    (fp_text value PAM2401SCADJ (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.2 -0.975 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 2.2 -0.325 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 156 VBOOST))
    (pad 6 smd rect (at 2.2 0.325 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U4-Pad6)"))
    (pad 5 smd rect (at 2.2 0.975 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -2.2 0.975 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -2.2 0.325 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 135 VBAT))
    (pad 2 smd rect (at -2.2 -0.325 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R2-Pad2)"))
    (pad 1 smd rect (at -2.2 -0.975 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 75.7174 116.967 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J5 (at 0 -5.8 90) (layer F.SilkS))
    (fp_text value JST (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 VBAT))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lichen-badge:SOT-23-5 (layer F.Cu) (tedit 58A20C20)
    (at 86.3346 157.099 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at -1.2446 2.0574) (layer F.SilkS))
    (fp_text value TPS2051C (at -0.05 2.54) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 156 VBOOST))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 139 USB1_DRVVBUS))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U5-Pad3)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 140 USB1_VBUS))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module "lichen-badge:SON-6(TI)-DRY" (layer F.Cu) (tedit 200000)
    (at 103.8098 160.7312)
    (attr smd)
    (fp_text reference IC2 (at 0.1016 -1.6256) (layer F.SilkS))
    (fp_text value TPD4S012DRYR (at 2.16662 1.34112) (layer F.SilkS) hide)
    (pad 6 smd rect (at -0.49784 -0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 133 USB0_VBUS))
    (pad 5 smd rect (at 0 -0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(IC2-Pad5)"))
    (pad 4 smd rect (at 0.49784 -0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0.49784 0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 143 USB0_ID))
    (pad 2 smd rect (at 0 0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 172 USB0_D+))
    (pad 1 smd rect (at -0.49784 0.37846) (size 0.29972 0.51816) (layers F.Cu F.Paste F.Mask)
      (net 171 USB0_D-))
  )
  (module "lichen-badge:SON-6(TI)-DRY" (layer F.Cu) (tedit 200000)
    (at 90.0938 160.7566)
    (attr smd)
    (fp_text reference IC1 (at -0.0508 -1.4478) (layer F.SilkS))
    (fp_text value TPD4S012DRYR (at -0.0254 3.3528) (layer F.SilkS) hide)
    (pad 6 smd rect (at -0.49784 -0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 140 USB1_VBUS))
    (pad 5 smd rect (at 0 -0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(IC1-Pad5)"))
    (pad 4 smd rect (at 0.49784 -0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0.49784 0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 153 USB1_ID))
    (pad 2 smd rect (at 0 0.37338) (size 0.29972 0.48768) (layers F.Cu F.Paste F.Mask)
      (net 170 USB1_D+))
    (pad 1 smd rect (at -0.49784 0.37846) (size 0.29972 0.51816) (layers F.Cu F.Paste F.Mask)
      (net 169 USB1_D-))
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 5A1DC0BD)
    (at 90.17 165.1508)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J2 (at -5.5626 1.0414 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 4.6 180) (layer F.Fab))
    (fp_text user %R (at 0 1.2) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 180) (layer Dwgs.User))
    (pad 6 smd rect (at 0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at -0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at 2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at -2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at 2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at -2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 5 smd rect (at 1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 153 USB1_ID))
    (pad 3 smd rect (at 0 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 170 USB1_D+))
    (pad 2 smd rect (at -0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 169 USB1_D-))
    (pad 1 smd rect (at -1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(FB2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 5A1DC0BD)
    (at 103.886 165.1508)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J3 (at 5.6642 1.7018 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 4.6 180) (layer F.Fab))
    (fp_text user %R (at 0 1.2) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 180) (layer Dwgs.User))
    (pad 6 smd rect (at 0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at -0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at 2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at -2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at 2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 6 smd rect (at -2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 130 GNDPWR))
    (pad 5 smd rect (at 1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 143 USB0_ID))
    (pad 3 smd rect (at 0 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 172 USB0_D+))
    (pad 2 smd rect (at -0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 171 USB0_D-))
    (pad 1 smd rect (at -1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(FB1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lichen-badge:tux-ghost (layer B.Cu) (tedit 0)
    (at 98.975904 118.891199 180)
    (fp_text reference LOGO1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module lichen-badge:BGA-400-1-27mm (layer F.Cu) (tedit 57362471)
    (at 99.568 135.636)
    (fp_text reference U1 (at -14.2748 14.11224) (layer F.SilkS))
    (fp_text value OSD335x-CSIP (at 0 -14.478) (layer F.Fab))
    (pad Y20 smd circle (at 12.065 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad Y17 smd circle (at 12.065 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U1-PadY17)"))
    (pad Y18 smd circle (at 12.065 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U1-PadY18)"))
    (pad Y19 smd circle (at 12.065 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U1-PadY19)"))
    (pad Y11 smd circle (at 12.065 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U1-PadY11)"))
    (pad Y12 smd circle (at 12.065 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U1-PadW12)"))
    (pad Y14 smd circle (at 12.065 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(U1-PadY14)"))
    (pad Y13 smd circle (at 12.065 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(U1-PadY13)"))
    (pad Y15 smd circle (at 12.065 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U1-PadY15)"))
    (pad Y16 smd circle (at 12.065 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 198 PWM_GREEN))
    (pad Y6 smd circle (at 12.065 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 UART0_RXD))
    (pad Y7 smd circle (at 12.065 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 I2C1_SDA))
    (pad Y5 smd circle (at 12.065 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 184 SPI0_SCLK))
    (pad Y3 smd circle (at 12.065 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 MMC0_DAT0))
    (pad Y4 smd circle (at 12.065 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 SPI0_nCS0))
    (pad Y2 smd circle (at 12.065 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 125 MMC0_DAT3))
    (pad Y1 smd circle (at 12.065 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad Y8 smd circle (at 12.065 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(U1-PadY8)"))
    (pad Y9 smd circle (at 12.065 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U1-PadW9)"))
    (pad Y10 smd circle (at 12.065 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U1-PadY10)"))
    (pad W20 smd circle (at 10.795 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U1-PadW20)"))
    (pad W17 smd circle (at 10.795 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U1-PadW17)"))
    (pad W18 smd circle (at 10.795 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U1-PadW18)"))
    (pad W19 smd circle (at 10.795 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U1-PadW19)"))
    (pad W11 smd circle (at 10.795 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U1-PadW11)"))
    (pad W12 smd circle (at 10.795 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U1-PadW12)"))
    (pad W14 smd circle (at 10.795 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U1-PadW14)"))
    (pad W13 smd circle (at 10.795 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U1-PadW13)"))
    (pad W15 smd circle (at 10.795 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U1-PadW15)"))
    (pad W16 smd circle (at 10.795 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U1-PadW16)"))
    (pad W6 smd circle (at 10.795 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 UART0_TXD))
    (pad W7 smd circle (at 10.795 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 I2C1_SCL))
    (pad W5 smd circle (at 10.795 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U1-PadW5)"))
    (pad W3 smd circle (at 10.795 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 127 MMC0_CLK))
    (pad W4 smd circle (at 10.795 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 SPI0_MOSI))
    (pad W2 smd circle (at 10.795 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 126 MMC0_CMD))
    (pad W1 smd circle (at 10.795 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U1-PadW1)"))
    (pad W8 smd circle (at 10.795 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U1-PadW8)"))
    (pad W9 smd circle (at 10.795 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U1-PadW9)"))
    (pad W10 smd circle (at 10.795 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U1-PadW10)"))
    (pad V20 smd circle (at 9.525 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U1-PadV20)"))
    (pad V19 smd circle (at 9.525 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U1-PadV19)"))
    (pad V18 smd circle (at 9.525 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U1-PadV18)"))
    (pad V17 smd circle (at 9.525 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U1-PadV17)"))
    (pad V14 smd circle (at 9.525 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U1-PadV14)"))
    (pad V16 smd circle (at 9.525 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 197 PWM_RED))
    (pad V15 smd circle (at 9.525 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U1-PadV15)"))
    (pad V6 smd circle (at 9.525 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U1-PadV6)"))
    (pad V5 smd circle (at 9.525 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U1-PadV5)"))
    (pad V4 smd circle (at 9.525 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 MMC0_CD))
    (pad V2 smd circle (at 9.525 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 124 MMC0_DAT2))
    (pad V1 smd circle (at 9.525 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U1-PadV1)"))
    (pad V3 smd circle (at 9.525 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 MMC0_DAT1))
    (pad V7 smd circle (at 9.525 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-PadU7)"))
    (pad V9 smd circle (at 9.525 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U1-PadV9)"))
    (pad V8 smd circle (at 9.525 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-PadU8)"))
    (pad V10 smd circle (at 9.525 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U1-PadV10)"))
    (pad V12 smd circle (at 9.525 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U1-PadV12)"))
    (pad V11 smd circle (at 9.525 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U1-PadV11)"))
    (pad V13 smd circle (at 9.525 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U1-PadV13)"))
    (pad U20 smd circle (at 8.255 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 185 LCD_PWM))
    (pad U19 smd circle (at 8.255 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U1-PadU19)"))
    (pad U18 smd circle (at 8.255 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U1-PadU18)"))
    (pad U17 smd circle (at 8.255 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad U14 smd circle (at 8.255 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U1-PadU14)"))
    (pad U16 smd circle (at 8.255 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad U15 smd circle (at 8.255 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad U6 smd circle (at 8.255 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U1-PadU6)"))
    (pad U5 smd circle (at 8.255 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad U4 smd circle (at 8.255 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad U2 smd circle (at 8.255 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U1-PadU2)"))
    (pad U1 smd circle (at 8.255 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U1-PadU1)"))
    (pad U3 smd circle (at 8.255 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-PadU3)"))
    (pad U7 smd circle (at 8.255 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-PadU7)"))
    (pad U9 smd circle (at 8.255 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1-PadU9)"))
    (pad U8 smd circle (at 8.255 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-PadU8)"))
    (pad U10 smd circle (at 8.255 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-PadU10)"))
    (pad U12 smd circle (at 8.255 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-PadU12)"))
    (pad U11 smd circle (at 8.255 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad U13 smd circle (at 8.255 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U1-PadU13)"))
    (pad T20 smd circle (at 6.985 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 LCD_D2))
    (pad T19 smd circle (at 6.985 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 LCD_D1))
    (pad T18 smd circle (at 6.985 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 LCD_D0))
    (pad T17 smd circle (at 6.985 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T14 smd circle (at 6.985 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T16 smd circle (at 6.985 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T15 smd circle (at 6.985 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T6 smd circle (at 6.985 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T5 smd circle (at 6.985 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T4 smd circle (at 6.985 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T2 smd circle (at 6.985 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U1-PadT2)"))
    (pad T1 smd circle (at 6.985 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-PadT1)"))
    (pad T3 smd circle (at 6.985 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-PadT3)"))
    (pad T7 smd circle (at 6.985 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T9 smd circle (at 6.985 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T8 smd circle (at 6.985 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T10 smd circle (at 6.985 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T12 smd circle (at 6.985 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T11 smd circle (at 6.985 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad T13 smd circle (at 6.985 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R20 smd circle (at 5.715 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 LCD_D5))
    (pad R19 smd circle (at 5.715 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 LCD_D4))
    (pad R18 smd circle (at 5.715 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 LCD_D3))
    (pad R17 smd circle (at 5.715 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R14 smd circle (at 5.715 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R16 smd circle (at 5.715 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R15 smd circle (at 5.715 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R6 smd circle (at 5.715 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R5 smd circle (at 5.715 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R4 smd circle (at 5.715 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R2 smd circle (at 5.715 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-PadR2)"))
    (pad R1 smd circle (at 5.715 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-PadR1)"))
    (pad R3 smd circle (at 5.715 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-PadR3)"))
    (pad R7 smd circle (at 5.715 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R9 smd circle (at 5.715 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R8 smd circle (at 5.715 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad R10 smd circle (at 5.715 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R12 smd circle (at 5.715 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R11 smd circle (at 5.715 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad R13 smd circle (at 5.715 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U1-PadR13)"))
    (pad P20 smd circle (at 4.445 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 LCD_D8))
    (pad P19 smd circle (at 4.445 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 LCD_D7))
    (pad P18 smd circle (at 4.445 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 LCD_D6))
    (pad P17 smd circle (at 4.445 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad P14 smd circle (at 4.445 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P16 smd circle (at 4.445 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P15 smd circle (at 4.445 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P6 smd circle (at 4.445 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P5 smd circle (at 4.445 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P4 smd circle (at 4.445 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad P2 smd circle (at 4.445 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-PadP2)"))
    (pad P1 smd circle (at 4.445 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-PadP1)"))
    (pad P3 smd circle (at 4.445 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-PadP3)"))
    (pad P7 smd circle (at 4.445 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P9 smd circle (at 4.445 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P8 smd circle (at 4.445 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P10 smd circle (at 4.445 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad P12 smd circle (at 4.445 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad P11 smd circle (at 4.445 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad P13 smd circle (at 4.445 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad N20 smd circle (at 3.175 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 LCD_D11))
    (pad N19 smd circle (at 3.175 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 LCD_D10))
    (pad N18 smd circle (at 3.175 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 LCD_D9))
    (pad N17 smd circle (at 3.175 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad N14 smd circle (at 3.175 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N16 smd circle (at 3.175 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad N15 smd circle (at 3.175 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad N6 smd circle (at 3.175 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad N5 smd circle (at 3.175 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad N4 smd circle (at 3.175 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad N2 smd circle (at 3.175 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-PadN2)"))
    (pad N1 smd circle (at 3.175 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-PadN1)"))
    (pad N3 smd circle (at 3.175 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-PadN3)"))
    (pad N7 smd circle (at 3.175 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N9 smd circle (at 3.175 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N8 smd circle (at 3.175 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N10 smd circle (at 3.175 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N12 smd circle (at 3.175 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N11 smd circle (at 3.175 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad N13 smd circle (at 3.175 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad M20 smd circle (at 1.905 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 LCD_D14))
    (pad M19 smd circle (at 1.905 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 LCD_D13))
    (pad M18 smd circle (at 1.905 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 LCD_D12))
    (pad M17 smd circle (at 1.905 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad M14 smd circle (at 1.905 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad M16 smd circle (at 1.905 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad M15 smd circle (at 1.905 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad M6 smd circle (at 1.905 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-PadM6)"))
    (pad M5 smd circle (at 1.905 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad M4 smd circle (at 1.905 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd circle (at 1.905 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(J4-Pad1)"))
    (pad M1 smd circle (at 1.905 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-PadM1)"))
    (pad M3 smd circle (at 1.905 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-PadM3)"))
    (pad M7 smd circle (at 1.905 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad M9 smd circle (at 1.905 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad M8 smd circle (at 1.905 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad M10 smd circle (at 1.905 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad M12 smd circle (at 1.905 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad M11 smd circle (at 1.905 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad M13 smd circle (at 1.905 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad L20 smd circle (at 0.635 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-PadL20)"))
    (pad L19 smd circle (at 0.635 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-PadL19)"))
    (pad L18 smd circle (at 0.635 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 LCD_D15))
    (pad L17 smd circle (at 0.635 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad L14 smd circle (at 0.635 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad L16 smd circle (at 0.635 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad L15 smd circle (at 0.635 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad L6 smd circle (at 0.635 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad L5 smd circle (at 0.635 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad L4 smd circle (at 0.635 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad L2 smd circle (at 0.635 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 USB0_D+))
    (pad L1 smd circle (at 0.635 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 143 USB0_ID))
    (pad L3 smd circle (at 0.635 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-PadL3)"))
    (pad L7 smd circle (at 0.635 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad L9 smd circle (at 0.635 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad L8 smd circle (at 0.635 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad L10 smd circle (at 0.635 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad L12 smd circle (at 0.635 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad L11 smd circle (at 0.635 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad L13 smd circle (at 0.635 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad K20 smd circle (at -0.635 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-PadK20)"))
    (pad K19 smd circle (at -0.635 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-PadK19)"))
    (pad K18 smd circle (at -0.635 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-PadK18)"))
    (pad K17 smd circle (at -0.635 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-PadJ17)"))
    (pad K16 smd circle (at -0.635 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K15 smd circle (at -0.635 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K14 smd circle (at -0.635 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad K13 smd circle (at -0.635 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SYS_VDD_1P8V))
    (pad K12 smd circle (at -0.635 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K11 smd circle (at -0.635 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad K10 smd circle (at -0.635 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 SYS_VDD3_3P3V))
    (pad K9 smd circle (at -0.635 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K8 smd circle (at -0.635 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K7 smd circle (at -0.635 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K6 smd circle (at -0.635 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K1 smd circle (at -0.635 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 USB0_VBUS))
    (pad K4 smd circle (at -0.635 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad K3 smd circle (at -0.635 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-PadK3)"))
    (pad K5 smd circle (at -0.635 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad K2 smd circle (at -0.635 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 USB0_D-))
    (pad J20 smd circle (at -1.905 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad J19 smd circle (at -1.905 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad J18 smd circle (at -1.905 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad J17 smd circle (at -1.905 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-PadJ17)"))
    (pad J16 smd circle (at -1.905 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J15 smd circle (at -1.905 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad J14 smd circle (at -1.905 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad J13 smd circle (at -1.905 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J12 smd circle (at -1.905 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J11 smd circle (at -1.905 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J10 smd circle (at -1.905 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J9 smd circle (at -1.905 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J8 smd circle (at -1.905 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad J7 smd circle (at -1.905 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad J6 smd circle (at -1.905 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad J1 smd circle (at -1.905 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 USB1_ID))
    (pad J4 smd circle (at -1.905 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad J3 smd circle (at -1.905 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-PadJ3)"))
    (pad J5 smd circle (at -1.905 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad J2 smd circle (at -1.905 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 USB1_D+))
    (pad H20 smd circle (at -3.175 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H19 smd circle (at -3.175 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H18 smd circle (at -3.175 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H17 smd circle (at -3.175 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-PadG17)"))
    (pad H16 smd circle (at -3.175 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad H15 smd circle (at -3.175 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad H14 smd circle (at -3.175 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad H13 smd circle (at -3.175 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H12 smd circle (at -3.175 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H11 smd circle (at -3.175 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H10 smd circle (at -3.175 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H9 smd circle (at -3.175 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H8 smd circle (at -3.175 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad H7 smd circle (at -3.175 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad H6 smd circle (at -3.175 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H1 smd circle (at -3.175 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 140 USB1_VBUS))
    (pad H4 smd circle (at -3.175 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad H3 smd circle (at -3.175 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 139 USB1_DRVVBUS))
    (pad H5 smd circle (at -3.175 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad H2 smd circle (at -3.175 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 169 USB1_D-))
    (pad G20 smd circle (at -4.445 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G19 smd circle (at -4.445 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G18 smd circle (at -4.445 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G17 smd circle (at -4.445 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-PadG17)"))
    (pad G16 smd circle (at -4.445 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad G15 smd circle (at -4.445 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 SYS_VOUT))
    (pad G14 smd circle (at -4.445 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 SYS_VOUT))
    (pad G13 smd circle (at -4.445 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 SYS_VDD2_3P3V))
    (pad G12 smd circle (at -4.445 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 SYS_VDD2_3P3V))
    (pad G11 smd circle (at -4.445 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G10 smd circle (at -4.445 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G9 smd circle (at -4.445 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad G8 smd circle (at -4.445 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad G7 smd circle (at -4.445 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G6 smd circle (at -4.445 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G1 smd circle (at -4.445 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G4 smd circle (at -4.445 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G3 smd circle (at -4.445 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad G5 smd circle (at -4.445 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad G2 smd circle (at -4.445 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F20 smd circle (at -5.715 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F19 smd circle (at -5.715 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-PadF19)"))
    (pad F18 smd circle (at -5.715 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-PadF18)"))
    (pad F17 smd circle (at -5.715 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad F16 smd circle (at -5.715 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad F15 smd circle (at -5.715 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 SYS_VOUT))
    (pad F14 smd circle (at -5.715 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 SYS_VOUT))
    (pad F13 smd circle (at -5.715 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 SYS_VDD2_3P3V))
    (pad F12 smd circle (at -5.715 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 SYS_VDD2_3P3V))
    (pad F11 smd circle (at -5.715 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad F10 smd circle (at -5.715 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad F9 smd circle (at -5.715 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad F8 smd circle (at -5.715 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad F7 smd circle (at -5.715 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F6 smd circle (at -5.715 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F1 smd circle (at -5.715 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F4 smd circle (at -5.715 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F3 smd circle (at -5.715 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad F5 smd circle (at -5.715 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad F2 smd circle (at -5.715 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad E20 smd circle (at -6.985 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(R1-Pad1)"))
    (pad E19 smd circle (at -6.985 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 VBAT))
    (pad E18 smd circle (at -6.985 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad E17 smd circle (at -6.985 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E16 smd circle (at -6.985 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E15 smd circle (at -6.985 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E14 smd circle (at -6.985 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E13 smd circle (at -6.985 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E12 smd circle (at -6.985 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E11 smd circle (at -6.985 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E10 smd circle (at -6.985 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E9 smd circle (at -6.985 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E8 smd circle (at -6.985 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E7 smd circle (at -6.985 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E6 smd circle (at -6.985 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E1 smd circle (at -6.985 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad E4 smd circle (at -6.985 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E3 smd circle (at -6.985 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad E5 smd circle (at -6.985 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E2 smd circle (at -6.985 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad D20 smd circle (at -8.255 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 VBAT))
    (pad D19 smd circle (at -8.255 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 VBAT))
    (pad D18 smd circle (at -8.255 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 VBAT))
    (pad D17 smd circle (at -8.255 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D16 smd circle (at -8.255 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D15 smd circle (at -8.255 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D14 smd circle (at -8.255 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-PadD13)"))
    (pad D13 smd circle (at -8.255 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-PadD13)"))
    (pad D12 smd circle (at -8.255 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-PadD11)"))
    (pad D11 smd circle (at -8.255 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-PadD11)"))
    (pad D10 smd circle (at -8.255 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-PadD10)"))
    (pad D9 smd circle (at -8.255 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-PadD10)"))
    (pad D8 smd circle (at -8.255 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad D7 smd circle (at -8.255 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad D6 smd circle (at -8.255 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad D1 smd circle (at -8.255 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad D4 smd circle (at -8.255 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D3 smd circle (at -8.255 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad D5 smd circle (at -8.255 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D2 smd circle (at -8.255 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C20 smd circle (at -9.525 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 VIN_AC))
    (pad C19 smd circle (at -9.525 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 VIN_AC))
    (pad C18 smd circle (at -9.525 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 VIN_AC))
    (pad C17 smd circle (at -9.525 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(SW2-Pad2)"))
    (pad C16 smd circle (at -9.525 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-PadC16)"))
    (pad C15 smd circle (at -9.525 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-PadC15)"))
    (pad C14 smd circle (at -9.525 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-PadC14)"))
    (pad C13 smd circle (at -9.525 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 PWM_BLUE))
    (pad C12 smd circle (at -9.525 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-PadC12)"))
    (pad C11 smd circle (at -9.525 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-PadC11)"))
    (pad C10 smd circle (at -9.525 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-PadC10)"))
    (pad C9 smd circle (at -9.525 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-PadC9)"))
    (pad C8 smd circle (at -9.525 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C7 smd circle (at -9.525 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C6 smd circle (at -9.525 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C1 smd circle (at -9.525 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C4 smd circle (at -9.525 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at -9.525 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C5 smd circle (at -9.525 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad C2 smd circle (at -9.525 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B20 smd circle (at -10.795 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 USB0_VBUS))
    (pad B19 smd circle (at -10.795 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 USB0_VBUS))
    (pad B18 smd circle (at -10.795 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 USB0_VBUS))
    (pad B17 smd circle (at -10.795 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(SW2-Pad2)"))
    (pad B16 smd circle (at -10.795 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-PadB16)"))
    (pad B15 smd circle (at -10.795 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-PadB15)"))
    (pad B14 smd circle (at -10.795 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-PadB14)"))
    (pad B13 smd circle (at -10.795 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-PadB13)"))
    (pad B12 smd circle (at -10.795 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-PadB12)"))
    (pad B11 smd circle (at -10.795 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-PadB11)"))
    (pad B10 smd circle (at -10.795 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-PadB10)"))
    (pad B9 smd circle (at -10.795 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-PadB9)"))
    (pad B8 smd circle (at -10.795 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B7 smd circle (at -10.795 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd circle (at -10.795 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B1 smd circle (at -10.795 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B4 smd circle (at -10.795 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at -10.795 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd circle (at -10.795 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd circle (at -10.795 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A20 smd circle (at -12.065 -12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A19 smd circle (at -12.065 -10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-PadA19)"))
    (pad A18 smd circle (at -12.065 -9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(SW1-Pad2)"))
    (pad A17 smd circle (at -12.065 -8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-PadA17)"))
    (pad A16 smd circle (at -12.065 -6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 190 LCD_RESET))
    (pad A15 smd circle (at -12.065 -5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-PadA15)"))
    (pad A14 smd circle (at -12.065 -4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 189 LCD_RS))
    (pad A13 smd circle (at -12.065 -3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-PadA13)"))
    (pad A12 smd circle (at -12.065 -1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-PadA12)"))
    (pad A11 smd circle (at -12.065 -0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-PadA11)"))
    (pad A10 smd circle (at -12.065 0.635 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-PadA10)"))
    (pad A9 smd circle (at -12.065 1.905 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-PadA9)"))
    (pad A8 smd circle (at -12.065 3.175 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd circle (at -12.065 4.445 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd circle (at -12.065 5.715 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd circle (at -12.065 6.985 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A4 smd circle (at -12.065 8.255 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-PadA4)"))
    (pad A3 smd circle (at -12.065 9.525 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd circle (at -12.065 10.795 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask))
    (pad A1 smd circle (at -12.065 12.065 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module lichen-badge:MMA8452QR1 (layer F.Cu) (tedit 5A7401D7)
    (at 118.98122 133.62432)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U2 (at -2.85242 -2.61112 180) (layer F.SilkS))
    (fp_text value MMA8452QR1 (at 0 2.85) (layer F.Fab) hide)
    (pad 16 smd rect (at -0.5 -1.275 90) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 0 -1.275 90) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0.5 -1.275 90) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (pad 13 smd rect (at 1.275 -1) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 1.275 -0.5) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 11 smd rect (at 1.275 0) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at 1.275 0.5) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd rect (at 1.275 1) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at 0.5 1.275 90) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0 1.275 90) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at -0.5 1.275 90) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 148 I2C1_SDA))
    (pad 5 smd rect (at -1.275 1) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -1.275 0.5) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 146 I2C1_SCL))
    (pad 3 smd rect (at -1.275 0) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.275 -0.5) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.275 -1) (size 0.813 0.305) (layers F.Cu F.Paste F.Mask)
      (net 119 SYS_VDD1_3P3V))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text EEP (at 104.56418 152.49398) (layer F.SilkS))
  (gr_line (start 118.3132 173.5836) (end 117.7036 173.5328) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.842004 173.168459) (end 118.3132 173.5836) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.489704 172.983039) (end 119.842004 173.168459) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.196064 170.163639) (end 120.489704 172.983039) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.159484 169.490539) (end 128.196064 170.163639) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.646144 168.756479) (end 130.159484 169.490539) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.267424 168.096079) (end 132.646144 168.756479) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.226004 165.990419) (end 135.267424 168.096079) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.470604 165.543379) (end 144.226004 165.990419) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.288484 165.035379) (end 145.470604 165.543379) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.842204 164.474039) (end 146.288484 165.035379) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.141924 163.722199) (end 146.842204 164.474039) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.169864 162.909399) (end 147.141924 163.722199) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.068264 162.066119) (end 147.169864 162.909399) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.164024 158.906359) (end 147.068264 162.066119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.897324 157.422999) (end 146.164024 158.906359) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.823664 156.277459) (end 145.897324 157.422999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.950664 155.002379) (end 145.823664 156.277459) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.661864 151.512419) (end 145.950664 155.002379) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.699964 149.853799) (end 146.661864 151.512419) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.491684 148.461879) (end 146.699964 149.853799) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.902404 147.532239) (end 146.491684 148.461879) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.115004 146.932799) (end 145.902404 147.532239) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.200604 146.607679) (end 145.115004 146.932799) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.130504 146.483219) (end 144.200604 146.607679) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.489664 146.445119) (end 142.130504 146.483219) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.143464 146.246999) (end 140.489664 146.445119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.089364 145.855839) (end 139.143464 146.246999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.340064 145.220839) (end 138.089364 145.855839) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.007324 144.728079) (end 137.340064 145.220839) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.486624 143.902579) (end 137.007324 144.728079) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.879564 142.602099) (end 136.486624 143.902579) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.120104 141.100959) (end 135.879564 142.602099) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.840704 140.747899) (end 135.120104 141.100959) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.972024 137.946279) (end 134.840704 140.747899) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.172684 137.108079) (end 133.972024 137.946279) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.281904 136.043819) (end 134.172684 137.108079) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.274284 134.270899) (end 134.281904 136.043819) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.104104 133.148219) (end 134.274284 134.270899) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.707864 132.022999) (end 134.104104 133.148219) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.741904 127.669439) (end 133.707864 132.022999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.771624 125.579019) (end 131.741904 127.669439) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.473684 122.647859) (end 130.771624 125.579019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.741404 118.362879) (end 129.473684 122.647859) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.938764 116.361359) (end 127.741404 118.362879) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.950704 114.245539) (end 126.938764 116.361359) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.104884 112.769799) (end 125.950704 114.245539) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.358124 111.614099) (end 125.104884 112.769799) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.282184 107.329119) (end 124.358124 111.614099) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.709164 103.663899) (end 121.282184 107.329119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.197864 101.454099) (end 118.709164 103.663899) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.960884 99.620219) (end 117.197864 101.454099) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.970284 98.172419) (end 115.960884 99.620219) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.033784 96.828759) (end 114.970284 98.172419) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.229364 92.500599) (end 115.033784 96.828759) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.714504 79.150359) (end 115.229364 92.500599) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.717044 76.650999) (end 115.714504 79.150359) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.691644 75.365759) (end 115.717044 76.650999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.346204 72.244099) (end 115.691644 75.365759) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.624844 69.399299) (end 115.346204 72.244099) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.611384 67.037099) (end 114.624844 69.399299) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.161044 64.870479) (end 113.611384 67.037099) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.403364 63.181379) (end 112.161044 64.870479) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.391684 61.911379) (end 110.403364 63.181379) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.986304 60.976659) (end 108.391684 61.911379) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.506244 60.852199) (end 105.986304 60.976659) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.873024 60.570259) (end 105.506244 60.852199) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.258604 60.379759) (end 103.873024 60.570259) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.490764 60.435639) (end 100.258604 60.379759) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.555284 60.582959) (end 98.490764 60.435639) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.563924 60.930939) (end 96.555284 60.582959) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.884224 61.809779) (end 94.563924 60.930939) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.369624 63.061999) (end 91.884224 61.809779) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.243644 64.580919) (end 89.369624 63.061999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.397064 66.450359) (end 87.243644 64.580919) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.035624 68.403619) (end 85.397064 66.450359) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.034864 70.588019) (end 84.035624 68.403619) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.392244 73.194059) (end 83.034864 70.588019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.194124 74.585979) (end 82.392244 73.194059) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.564204 80.806439) (end 82.194124 74.585979) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.855544 88.139419) (end 81.564204 80.806439) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.555824 90.107919) (end 80.855544 88.139419) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.162124 91.520159) (end 80.555824 90.107919) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.602564 95.241259) (end 80.162124 91.520159) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.538304 97.372319) (end 78.602564 95.241259) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.762844 100.552399) (end 77.538304 97.372319) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.789264 103.808679) (end 75.762844 100.552399) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.118964 108.883599) (end 73.789264 103.808679) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.900784 113.559739) (end 70.118964 108.883599) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.186284 116.638219) (end 66.900784 113.559739) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.260964 121.405799) (end 65.186284 116.638219) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 62.692004 123.066959) (end 63.260964 121.405799) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.449944 128.134259) (end 62.692004 123.066959) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.071484 130.519319) (end 61.449944 128.134259) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.751444 133.226959) (end 61.071484 130.519319) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.705724 135.523119) (end 60.751444 133.226959) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.985124 137.255399) (end 60.705724 135.523119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.493124 138.787019) (end 60.985124 137.255399) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.058024 143.506339) (end 61.493124 138.787019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.941184 143.734939) (end 60.058024 143.506339) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.801484 144.248019) (end 59.941184 143.734939) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.555104 145.830439) (end 59.801484 144.248019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.331584 146.965819) (end 59.555104 145.830439) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.904864 148.210419) (end 59.331584 146.965819) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.891404 149.579479) (end 58.904864 148.210419) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56.456304 151.012039) (end 57.891404 149.579479) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.178684 152.081379) (end 56.456304 151.012039) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.760604 153.818739) (end 55.178684 152.081379) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.724284 154.733139) (end 52.760604 153.818739) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.109604 155.571339) (end 51.724284 154.733139) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.837824 156.371439) (end 51.109604 155.571339) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.911484 157.245199) (end 50.837824 156.371439) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.157864 157.809079) (end 50.911484 157.245199) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.783464 159.391499) (end 51.157864 157.809079) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.322704 160.529419) (end 52.783464 159.391499) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56.992244 162.119459) (end 54.322704 160.529419) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.066664 162.708739) (end 56.992244 162.119459) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.450964 163.386919) (end 58.066664 162.708739) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.761604 164.075259) (end 59.450964 163.386919) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 62.031604 164.748359) (end 60.761604 164.075259) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.664824 165.779599) (end 62.031604 164.748359) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.503024 166.300299) (end 63.664824 165.779599) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.765404 167.288359) (end 64.503024 166.300299) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.545184 167.877639) (end 65.765404 167.288359) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.119224 168.378019) (end 66.545184 167.877639) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.820264 168.985079) (end 67.119224 168.378019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.861664 169.886779) (end 67.820264 168.985079) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.104484 171.837499) (end 68.861664 169.886779) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.858864 172.375979) (end 71.104484 171.837499) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.742784 172.769679) (end 71.858864 172.375979) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.593684 172.927159) (end 72.742784 172.769679) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.520784 173.031299) (end 73.593684 172.927159) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.990424 173.031299) (end 74.520784 173.031299) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.389964 172.957639) (end 77.990424 173.031299) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.558364 172.739199) (end 79.389964 172.957639) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.858844 172.022919) (end 80.558364 172.739199) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.156784 170.846899) (end 81.858844 172.022919) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.777304 168.670119) (end 83.156784 170.846899) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.351344 168.098619) (end 84.777304 168.670119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.704404 167.844619) (end 85.351344 168.098619) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.136204 167.793819) (end 85.704404 167.844619) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.667824 167.715079) (end 86.136204 167.793819) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.017324 167.656659) (end 87.667824 167.715079) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.193344 167.633799) (end 90.017324 167.656659) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.592624 167.628719) (end 91.193344 167.633799) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.666784 167.649039) (end 95.592624 167.628719) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.770664 167.699839) (end 99.666784 167.649039) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.584224 167.765879) (end 102.770664 167.699839) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.189504 167.870019) (end 104.584224 167.765879) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.478044 168.342459) (end 106.189504 167.870019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.454164 169.119699) (end 108.478044 168.342459) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.130564 170.194119) (end 110.454164 169.119699) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.725684 171.372679) (end 112.130564 170.194119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.628144 172.746819) (end 113.725684 171.372679) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.057404 172.980499) (end 115.628144 172.746819) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.674624 173.204019) (end 116.057404 172.980499) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.1956 173.3804) (end 116.674624 173.204019) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.7036 173.5328) (end 117.1956 173.3804) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.259376 84.987497) (xy 107.068876 84.898597) (xy 106.649776 84.799537) (xy 105.641396 84.657297) (xy 105.245156 84.631897)
        (xy 101.252276 84.987497) (xy 100.805236 85.050997) (xy 98.709736 85.396437) (xy 98.013776 85.630117) (xy 97.726756 85.838397)
        (xy 97.058736 86.564837) (xy 96.870776 86.689297) (xy 96.116396 87.184597) (xy 94.754956 87.789117) (xy 91.452956 88.987997)
        (xy 90.431876 89.531557) (xy 89.809576 90.151317) (xy 89.537796 90.992057) (xy 89.626696 92.071557) (xy 90.076276 93.877497)
        (xy 90.495376 94.520117) (xy 90.873836 94.807137) (xy 92.964256 95.558977) (xy 97.414336 97.596057) (xy 98.780856 98.210737)
        (xy 102.474016 99.584877) (xy 103.667816 99.816017) (xy 104.798116 99.882057) (xy 105.679496 99.856657) (xy 106.357676 99.699177)
        (xy 106.852976 99.445177) (xy 106.987596 99.376597) (xy 107.800396 98.802557) (xy 108.354116 98.365677) (xy 108.526836 98.231057)
        (xy 108.839256 97.956737) (xy 108.999276 97.811957) (xy 109.039916 97.776397) (xy 109.232956 97.532557) (xy 109.243116 97.486837)
        (xy 109.222796 97.441117) (xy 108.999276 97.349677) (xy 108.374436 97.283637) (xy 107.434636 97.248077) (xy 106.261156 97.227757)
        (xy 105.280716 97.227757) (xy 103.756716 97.161717) (xy 102.451156 96.953437) (xy 101.303076 96.633397) (xy 98.158556 95.251637)
        (xy 94.500956 93.834317) (xy 92.656916 92.980877) (xy 92.067636 92.559237) (xy 91.803476 92.183317) (xy 91.813636 91.807397)
        (xy 91.864436 91.741357) (xy 92.245436 91.522917) (xy 92.778836 91.614357) (xy 93.368116 92.178237) (xy 94.028516 92.589717)
        (xy 94.856556 93.006277) (xy 95.532196 93.290757) (xy 96.558356 93.712397) (xy 99.748596 94.789357) (xy 102.654356 95.531037)
        (xy 103.970076 95.820597) (xy 106.118916 96.033957) (xy 106.992676 96.023797) (xy 107.526076 95.952677) (xy 108.450636 95.673277)
        (xy 109.390436 95.119557) (xy 111.879636 92.792917) (xy 112.565436 92.137597) (xy 112.946436 91.563557) (xy 112.961676 90.979357)
        (xy 112.758476 90.420557) (xy 112.413036 89.856677) (xy 111.874556 89.267397) (xy 110.904276 88.413957) (xy 109.365036 87.098237)
        (xy 108.232196 86.107637) (xy 107.602276 85.472637)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.307104 86.465559) (xy 107.154704 86.282679) (xy 106.606064 85.977879) (xy 105.996464 85.825479) (xy 105.524024 85.855959)
        (xy 105.351304 86.074399) (xy 105.559584 86.302999) (xy 105.727224 86.333479) (xy 106.128544 86.531599) (xy 106.372384 86.841479)
        (xy 106.788944 87.268199) (xy 107.261384 87.298679) (xy 107.545864 87.049759) (xy 107.505224 86.689079)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.973104 85.962639) (xy 101.485424 85.830559) (xy 101.043464 85.815319) (xy 100.372904 85.855959) (xy 100.073184 86.028679)
        (xy 100.017304 86.328399) (xy 100.200184 86.734799) (xy 100.723424 86.795759) (xy 101.485424 86.526519) (xy 101.973104 86.206479)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.235984 84.966959) (xy 107.058184 84.883139) (xy 106.634004 84.781539) (xy 106.159024 84.720579) (xy 105.630704 84.639299)
        (xy 105.229384 84.613899) (xy 103.588544 84.751059) (xy 102.806224 84.824719) (xy 102.021364 84.898379) (xy 101.228884 84.969499)
        (xy 100.286544 85.114279) (xy 98.709204 85.373359) (xy 98.000544 85.614659) (xy 97.716064 85.817859) (xy 97.045504 86.551919)
        (xy 96.118404 87.158979) (xy 94.746804 87.771119) (xy 91.434644 88.969999) (xy 90.421184 89.513559) (xy 89.793804 90.135859)
        (xy 89.524564 90.979139) (xy 89.613464 92.056099) (xy 89.923344 93.265139) (xy 90.009704 93.633439) (xy 90.068124 93.862039)
        (xy 90.426264 94.415759) (xy 90.482144 94.502119) (xy 90.637084 94.621499) (xy 90.855524 94.786599) (xy 91.696264 95.088859)
        (xy 92.859584 95.510499) (xy 94.261664 96.102319) (xy 95.590084 96.719539) (xy 98.815884 98.223219) (xy 99.727744 98.609299)
        (xy 101.277144 99.206199) (xy 102.430304 99.559259) (xy 103.679984 99.808179) (xy 104.955064 99.861519) (xy 105.706904 99.848819)
        (xy 106.344444 99.683719) (xy 107.213124 99.198579) (xy 108.015764 98.599139) (xy 109.016524 97.768559) (xy 109.156224 97.600919)
        (xy 109.229884 97.501859) (xy 109.219724 97.430739) (xy 109.191784 97.410419) (xy 108.991124 97.334219) (xy 108.765064 97.308819)
        (xy 108.363744 97.265639) (xy 105.325904 97.212299) (xy 103.740944 97.133559) (xy 102.445544 96.937979) (xy 101.282224 96.612859)
        (xy 97.830364 95.116799) (xy 94.546144 93.831559) (xy 93.652064 93.473419) (xy 92.630984 92.962879) (xy 92.039164 92.546319)
        (xy 91.792784 92.193259) (xy 91.785164 91.832579) (xy 91.843584 91.728439) (xy 92.237284 91.504919) (xy 92.763064 91.591279)
        (xy 93.352344 92.160239) (xy 94.020364 92.579339) (xy 96.443524 93.676619) (xy 98.071664 94.240499) (xy 99.689644 94.776439)
        (xy 101.145064 95.177759) (xy 103.911124 95.794979) (xy 106.367304 96.033739) (xy 107.512844 95.949919) (xy 108.500904 95.652739)
        (xy 109.384824 95.099019) (xy 110.771664 93.834099) (xy 111.556524 93.082259) (xy 112.255024 92.398999) (xy 112.580144 92.134839)
        (xy 112.950984 91.563339) (xy 112.933204 90.974059) (xy 112.737624 90.412719) (xy 112.389644 89.851379) (xy 111.896884 89.287499)
        (xy 110.921524 88.403579) (xy 109.986804 87.613639) (xy 108.991124 86.788139) (xy 108.287544 86.168379) (xy 107.561104 85.429239)
        (xy 107.248684 84.977119)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.798144 168.941899) (xy 77.472264 169.513399) (xy 75.854284 169.734379) (xy 75.493604 169.739459) (xy 74.668104 169.714059)
        (xy 73.949284 169.617539) (xy 73.260944 169.414339) (xy 72.519264 169.058739) (xy 72.204304 168.860619) (xy 71.952844 168.703139)
        (xy 71.772504 168.588839) (xy 71.648044 168.515179) (xy 71.406744 168.342459) (xy 71.193384 168.190059) (xy 70.969864 168.032579)
        (xy 70.929224 168.004639) (xy 70.870804 167.963999) (xy 70.522824 167.715079) (xy 70.215484 167.483939) (xy 69.369664 166.848939)
        (xy 67.426564 165.408759) (xy 66.027024 164.443559) (xy 65.315824 163.999059) (xy 64.701144 163.618059) (xy 62.392284 162.515699)
        (xy 61.627744 162.223599) (xy 60.329804 161.768939) (xy 59.242684 161.382859) (xy 58.633084 161.177119) (xy 57.670424 160.801199)
        (xy 56.507104 160.336379) (xy 55.107564 159.673439) (xy 54.111884 159.066379) (xy 53.332104 158.329779) (xy 52.697104 157.473799)
        (xy 52.336424 156.686399) (xy 52.275464 156.353659) (xy 52.519304 155.662779) (xy 53.238124 154.979519) (xy 54.383664 154.336899)
        (xy 55.900044 153.765399) (xy 57.302124 153.259939) (xy 57.538344 153.171039) (xy 58.676264 152.546199) (xy 59.532244 151.761339)
        (xy 60.200264 150.737719) (xy 60.406004 150.298299) (xy 60.789544 149.170539) (xy 61.018144 147.928479) (xy 61.132444 146.744839)
        (xy 61.122284 145.911719) (xy 61.119744 145.561199) (xy 61.002904 144.573139) (xy 61.0362 143.73098) (xy 61.475344 142.942459)
        (xy 62.455784 142.436999) (xy 63.405744 142.467479) (xy 64.383644 142.774819) (xy 65.211684 143.125339) (xy 66.192124 143.922899)
        (xy 66.941424 144.535039) (xy 67.584044 144.931279) (xy 68.655924 145.591679) (xy 69.481424 146.079359) (xy 70.461864 146.462899)
        (xy 71.472784 146.754999) (xy 72.651344 146.754999) (xy 73.570824 146.564499) (xy 74.993224 145.832979) (xy 76.265764 144.740779)
        (xy 77.360504 143.282819) (xy 78.422224 141.131439) (xy 78.965784 140.603119) (xy 79.633804 140.504059) (xy 80.299284 140.686939)
        (xy 80.959684 141.164459) (xy 81.503244 142.152519) (xy 81.833444 143.437759) (xy 81.996004 145.149719) (xy 81.988384 145.726299)
        (xy 81.980764 146.907399) (xy 81.889324 148.093579) (xy 81.775024 149.221339) (xy 81.444824 151.281279) (xy 81.165424 152.937359)
        (xy 81.091764 153.727299) (xy 81.033344 154.733139) (xy 81.033344 155.683099) (xy 81.066364 157.313779) (xy 81.157804 159.449919)
        (xy 81.462604 164.486739) (xy 81.338144 165.261439) (xy 81.231464 165.952319) (xy 81.099384 166.419679) (xy 80.687904 167.163899)
        (xy 79.971624 168.004639) (xy 78.909904 168.852999)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.602684 162.751919) (xy 145.523944 162.388699) (xy 145.191204 161.807039) (xy 145.036264 161.553039) (xy 144.754324 161.083139)
        (xy 144.683204 160.966299) (xy 144.642564 160.900259) (xy 144.030424 159.815679) (xy 143.923744 159.592159) (xy 143.824684 159.376259)
        (xy 143.748484 159.200999) (xy 143.565604 158.814919) (xy 143.509724 158.629499) (xy 143.466544 158.492339) (xy 143.329384 157.999579)
        (xy 143.245564 157.181699) (xy 143.273504 156.259679) (xy 143.349704 155.578959) (xy 143.684984 154.032099) (xy 144.109164 152.850999)
        (xy 144.553664 151.680059) (xy 144.665424 151.360019) (xy 144.840684 150.857099) (xy 144.899104 150.684379) (xy 145.054044 150.163679)
        (xy 145.132784 149.894439) (xy 145.165804 149.706479) (xy 145.226764 149.373739) (xy 145.216604 149.053699) (xy 145.148024 148.596499)
        (xy 144.939744 148.286619) (xy 144.513024 148.085959) (xy 143.855164 147.986899) (xy 142.727404 147.933559) (xy 140.741124 147.933559)
        (xy 139.128224 147.887839) (xy 137.929344 147.755759) (xy 137.004784 147.509379) (xy 136.400264 147.161399) (xy 135.874484 146.589899)
        (xy 135.404584 145.805039) (xy 135.082004 145.088759) (xy 134.754344 144.100699) (xy 134.655284 143.681599) (xy 134.586704 143.381879)
        (xy 134.507964 143.046599) (xy 134.474944 142.797679) (xy 134.441924 142.543679) (xy 134.419064 142.365879) (xy 134.388584 142.134739)
        (xy 134.380964 142.081399) (xy 134.251424 141.357499) (xy 134.124424 140.844419) (xy 133.984724 140.450719) (xy 133.692624 139.937639)
        (xy 133.296384 139.378839) (xy 132.889984 138.936879) (xy 132.508984 138.599059) (xy 131.907004 138.205359) (xy 131.033244 137.837059)
        (xy 130.136624 137.798959) (xy 129.062204 138.190119) (xy 127.736324 139.104519) (xy 126.791444 140.034159) (xy 126.197084 140.692019)
        (xy 125.450324 141.596259) (xy 124.751824 142.464939) (xy 123.677404 143.869559) (xy 120.888484 147.814179) (xy 116.997204 153.623159)
        (xy 115.887224 155.342739) (xy 114.998224 156.772759) (xy 114.378464 157.826859) (xy 113.753624 159.091779) (xy 113.337064 160.130639)
        (xy 112.905264 161.690199) (xy 112.788424 163.501219) (xy 112.920504 164.509599) (xy 112.981464 165.119199) (xy 113.471684 166.699079)
        (xy 114.256544 168.108779) (xy 115.163324 169.043499) (xy 116.275844 169.665799) (xy 117.375664 169.929959) (xy 118.935224 169.929959)
        (xy 121.099304 169.574359) (xy 127.157204 168.238319) (xy 134.855944 166.335859) (xy 140.515064 164.910919) (xy 143.545284 164.065099)
        (xy 144.716224 163.663779) (xy 145.137864 163.404699) (xy 145.424884 163.092279)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.602684 162.751919) (xy 145.523944 162.388699) (xy 145.191204 161.807039) (xy 145.036264 161.553039) (xy 144.754324 161.083139)
        (xy 144.683204 160.966299) (xy 144.642564 160.900259) (xy 144.030424 159.815679) (xy 143.923744 159.592159) (xy 143.824684 159.376259)
        (xy 143.748484 159.200999) (xy 143.565604 158.814919) (xy 143.509724 158.629499) (xy 143.466544 158.492339) (xy 143.329384 157.999579)
        (xy 143.245564 157.181699) (xy 143.273504 156.259679) (xy 143.349704 155.578959) (xy 143.684984 154.032099) (xy 144.109164 152.850999)
        (xy 144.553664 151.680059) (xy 144.665424 151.360019) (xy 144.840684 150.857099) (xy 144.899104 150.684379) (xy 145.054044 150.163679)
        (xy 145.132784 149.894439) (xy 145.165804 149.706479) (xy 145.226764 149.373739) (xy 145.216604 149.053699) (xy 145.148024 148.596499)
        (xy 144.939744 148.286619) (xy 144.513024 148.085959) (xy 143.855164 147.986899) (xy 142.727404 147.933559) (xy 140.741124 147.933559)
        (xy 139.128224 147.887839) (xy 137.929344 147.755759) (xy 137.004784 147.509379) (xy 136.400264 147.161399) (xy 135.874484 146.589899)
        (xy 135.404584 145.805039) (xy 135.082004 145.088759) (xy 134.754344 144.100699) (xy 134.655284 143.681599) (xy 134.586704 143.381879)
        (xy 134.507964 143.046599) (xy 134.474944 142.797679) (xy 134.441924 142.543679) (xy 134.419064 142.365879) (xy 134.388584 142.134739)
        (xy 134.380964 142.081399) (xy 134.251424 141.357499) (xy 134.124424 140.844419) (xy 133.984724 140.450719) (xy 133.692624 139.937639)
        (xy 133.296384 139.378839) (xy 132.889984 138.936879) (xy 132.508984 138.599059) (xy 131.907004 138.205359) (xy 131.033244 137.837059)
        (xy 130.136624 137.798959) (xy 129.062204 138.190119) (xy 127.736324 139.104519) (xy 126.791444 140.034159) (xy 126.197084 140.692019)
        (xy 125.450324 141.596259) (xy 124.751824 142.464939) (xy 123.677404 143.869559) (xy 120.888484 147.814179) (xy 116.997204 153.623159)
        (xy 115.887224 155.342739) (xy 114.998224 156.772759) (xy 114.378464 157.826859) (xy 113.753624 159.091779) (xy 113.337064 160.130639)
        (xy 112.905264 161.690199) (xy 112.788424 163.501219) (xy 112.920504 164.509599) (xy 112.981464 165.119199) (xy 113.471684 166.699079)
        (xy 114.256544 168.108779) (xy 115.163324 169.043499) (xy 116.275844 169.665799) (xy 117.375664 169.929959) (xy 118.935224 169.929959)
        (xy 121.099304 169.574359) (xy 127.157204 168.238319) (xy 134.855944 166.335859) (xy 140.515064 164.910919) (xy 143.545284 164.065099)
        (xy 144.716224 163.663779) (xy 145.137864 163.404699) (xy 145.424884 163.092279)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.798144 168.941899) (xy 77.472264 169.513399) (xy 75.854284 169.734379) (xy 75.493604 169.739459) (xy 74.668104 169.714059)
        (xy 73.949284 169.617539) (xy 73.260944 169.414339) (xy 72.519264 169.058739) (xy 72.204304 168.860619) (xy 71.952844 168.703139)
        (xy 71.772504 168.588839) (xy 71.648044 168.515179) (xy 71.406744 168.342459) (xy 71.193384 168.190059) (xy 70.969864 168.032579)
        (xy 70.929224 168.004639) (xy 70.870804 167.963999) (xy 70.522824 167.715079) (xy 70.215484 167.483939) (xy 69.369664 166.848939)
        (xy 67.426564 165.408759) (xy 66.027024 164.443559) (xy 65.315824 163.999059) (xy 64.701144 163.618059) (xy 62.392284 162.515699)
        (xy 61.627744 162.223599) (xy 60.329804 161.768939) (xy 59.242684 161.382859) (xy 58.633084 161.177119) (xy 57.670424 160.801199)
        (xy 56.507104 160.336379) (xy 55.107564 159.673439) (xy 54.111884 159.066379) (xy 53.332104 158.329779) (xy 52.697104 157.473799)
        (xy 52.336424 156.686399) (xy 52.275464 156.353659) (xy 52.519304 155.662779) (xy 53.238124 154.979519) (xy 54.383664 154.336899)
        (xy 55.900044 153.765399) (xy 57.302124 153.259939) (xy 57.538344 153.171039) (xy 58.676264 152.546199) (xy 59.532244 151.761339)
        (xy 60.200264 150.737719) (xy 60.406004 150.298299) (xy 60.789544 149.170539) (xy 61.018144 147.928479) (xy 61.132444 146.744839)
        (xy 61.122284 145.911719) (xy 61.119744 145.561199) (xy 61.002904 144.573139) (xy 61.0362 143.73098) (xy 61.475344 142.942459)
        (xy 62.455784 142.436999) (xy 63.405744 142.467479) (xy 64.383644 142.774819) (xy 65.211684 143.125339) (xy 66.192124 143.922899)
        (xy 66.941424 144.535039) (xy 67.584044 144.931279) (xy 68.655924 145.591679) (xy 69.481424 146.079359) (xy 70.461864 146.462899)
        (xy 71.472784 146.754999) (xy 72.651344 146.754999) (xy 73.570824 146.564499) (xy 74.993224 145.832979) (xy 76.265764 144.740779)
        (xy 77.360504 143.282819) (xy 78.422224 141.131439) (xy 78.965784 140.603119) (xy 79.633804 140.504059) (xy 80.299284 140.686939)
        (xy 80.959684 141.164459) (xy 81.503244 142.152519) (xy 81.833444 143.437759) (xy 81.996004 145.149719) (xy 81.988384 145.726299)
        (xy 81.980764 146.907399) (xy 81.889324 148.093579) (xy 81.775024 149.221339) (xy 81.444824 151.281279) (xy 81.165424 152.937359)
        (xy 81.091764 153.727299) (xy 81.033344 154.733139) (xy 81.033344 155.683099) (xy 81.066364 157.313779) (xy 81.157804 159.449919)
        (xy 81.462604 164.486739) (xy 81.338144 165.261439) (xy 81.231464 165.952319) (xy 81.099384 166.419679) (xy 80.687904 167.163899)
        (xy 79.971624 168.004639) (xy 78.909904 168.852999)
      )
    )
  )
  (zone (net 119) (net_name SYS_VDD1_3P3V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 49.022 58.7248) (xy 148.082 58.7248) (xy 148.082 175.5648) (xy 49.022 175.5648)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 49.022 58.7248) (xy 148.082 58.7248) (xy 148.082 175.5648) (xy 49.022 175.5648)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.678 144.1704) (xy 90.678 141.986) (xy 91.9734 141.986) (xy 91.9734 130.5814) (xy 90.7034 130.5814)
        (xy 90.7034 126.746) (xy 94.488 126.746) (xy 94.488 127.9652) (xy 105.918 127.9652) (xy 105.918 126.746)
        (xy 108.458 126.746) (xy 108.458 130.556) (xy 107.188 130.556) (xy 107.188 141.9606) (xy 108.4326 141.9606)
        (xy 108.4326 144.1196) (xy 105.8926 144.1196) (xy 105.918 143.256) (xy 93.218 143.256) (xy 93.218 144.1704)
      )
    )
  )
  (zone (net 119) (net_name SYS_VDD1_3P3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.4184 138.811) (xy 97.663 138.811) (xy 97.663 140.1064) (xy 96.4184 140.1064)
      )
    )
  )
  (zone (net 119) (net_name SYS_VDD1_3P3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.8784 137.4902) (xy 95.123 137.4902) (xy 95.123 138.7856) (xy 93.8784 138.7856)
      )
    )
  )
  (zone (net 119) (net_name SYS_VDD1_3P3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.393 129.921) (xy 97.6376 129.921) (xy 97.6376 131.2164) (xy 96.393 131.2164)
      )
    )
  )
  (zone (net 134) (net_name VIN_AC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.4412 128.0922) (xy 126.7206 128.7272) (xy 125.5776 129.3114) (xy 124.1806 129.794) (xy 124.0282 129.3114)
        (xy 125.2474 128.6002)
      )
    )
  )
  (zone (net 138) (net_name SYS_VOUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.853 129.921) (xy 95.0976 129.921) (xy 95.0976 131.2164) (xy 93.853 131.2164)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.69952 132.48386) (xy 127.91186 131.507707) (xy 128.24968 132.22732) (xy 125.99416 133.2484)
      )
    )
  )
  (zone (net 138) (net_name SYS_VOUT) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.599 131.191) (xy 95.377 131.191) (xy 95.38716 86.98738) (xy 91.99626 86.96706) (xy 91.986418 88.062753)
        (xy 93.555503 88.065928)
      )
    )
  )
  (zone (net 133) (net_name USB0_VBUS) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.646 126.0348) (xy 90.17 126.0348) (xy 90.17 148.1328) (xy 102.362 148.1328) (xy 102.362 160.0708)
        (xy 100.33 160.0708) (xy 100.33 150.1648) (xy 88.646 150.1648)
      )
    )
  )
  (zone (net 130) (net_name GNDPWR) (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.868 162.6108) (xy 88.392 162.6108) (xy 88.392 165.4048) (xy 91.948 165.4048) (xy 91.948 162.6108)
        (xy 93.472 162.6108) (xy 93.472 165.4048) (xy 100.584 165.4048) (xy 100.584 162.6108) (xy 102.108 162.6108)
        (xy 102.108 165.4048) (xy 105.664 165.4048) (xy 105.664 162.6108) (xy 109.22 162.6108) (xy 109.22 166.4208)
        (xy 117.22862 170.68038) (xy 133.001385 165.216205) (xy 137.198735 175.570515) (xy 84.582 175.5648) (xy 84.582 165.4048)
        (xy 84.582 163.8808) (xy 84.582 162.6108)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.33022 155.96616) (xy 117.7417 157.09392) (xy 117.08384 157.33268) (xy 116.67998 156.21) (xy 114.97818 154.48534)
        (xy 115.50142 154.11958)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.37112 157.04312) (xy 114.7826 158.17088) (xy 114.12474 158.40964) (xy 113.72088 157.28696) (xy 112.01908 155.5623)
        (xy 112.54232 155.19654)
      )
    )
  )
  (zone (net 119) (net_name SYS_VDD1_3P3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.1514 156.58084) (xy 119.80672 156.34208) (xy 119.39778 155.21432) (xy 116.2304 149.4282) (xy 115.26012 149.4282)
        (xy 115.25758 150.39594) (xy 114.9985 151.50592) (xy 114.9985 151.87168) (xy 115.44554 152.00884) (xy 116.68252 152.01138)
        (xy 118.73992 155.45308)
      )
    )
  )
  (zone (net 130) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.15014 161.69894) (xy 115.09502 161.35858) (xy 124.46 157.95752) (xy 123.15952 153.84272) (xy 124.09932 153.4922)
        (xy 128.63703 166.757985) (xy 132.42925 165.40988) (xy 133.48716 168.18864) (xy 131.019233 168.913175) (xy 130.40868 167.17264)
        (xy 127.85598 168.08704) (xy 124.79528 158.87192) (xy 114.48796 162.64382)
      )
    )
  )
  (zone (net 130) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.35384 170.32986) (xy 116.03482 171.11091) (xy 116.70792 172.86478) (xy 118.364 173.3296) (xy 119.31396 172.96384)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.2388 84.7852) (xy 107.1372 84.3788) (xy 107.0864 83.566) (xy 107.3404 82.4484) (xy 107.8992 81.3816)
        (xy 108.7628 80.6196) (xy 109.5248 80.3656) (xy 110.0328 80.4164) (xy 110.5408 80.6196) (xy 110.998 80.9244)
        (xy 111.4552 81.7372) (xy 111.6076 82.7024) (xy 111.4552 83.82) (xy 111.0996 84.7852) (xy 110.6424 85.2424)
        (xy 109.982 85.5472) (xy 109.0168 85.5472) (xy 108.1024 85.3948) (xy 107.6452 85.1916)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.7392 85.598) (xy 97.8916 85.1916) (xy 98.044 84.1756) (xy 97.9424 83.058) (xy 97.6884 82.042)
        (xy 97.282 81.28) (xy 96.7232 80.772) (xy 96.2152 80.5688) (xy 95.3516 80.5688) (xy 94.2848 80.7212)
        (xy 92.8624 81.534) (xy 92.3036 82.3976) (xy 92.1512 83.3628) (xy 92.3544 84.7344) (xy 92.6084 85.4964)
        (xy 93.0656 86.36) (xy 93.8276 86.7664) (xy 95.3008 86.9696) (xy 96.1644 86.8172) (xy 96.9264 86.4108)
      )
    )
  )
  (zone (net 119) (net_name SYS_VDD1_3P3V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.97006 137.41146) (xy 110.97006 138.71194) (xy 107.94746 138.71194) (xy 107.94492 137.40638)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 84.1502) (xy 93.599 83.9724) (xy 93.6498 83.4644) (xy 93.853 82.9564) (xy 94.4372 82.2706)
        (xy 94.869 81.8134) (xy 95.2754 81.3816) (xy 95.4786 80.9752) (xy 95.3008 80.8482) (xy 94.8944 80.772)
        (xy 94.2594 80.9752) (xy 93.726 81.3816) (xy 93.345 81.8642) (xy 93.1418 82.1436) (xy 92.8878 82.6516)
        (xy 92.7608 83.1342) (xy 92.7608 83.4644) (xy 92.7862 83.7692) (xy 92.8878 83.9978) (xy 93.0402 84.0994)
        (xy 93.345 84.2264) (xy 93.4466 84.1756)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.1024 84.6074) (xy 108.4072 84.4042) (xy 108.585 83.9978) (xy 108.6866 83.7184) (xy 109.1946 82.5754)
        (xy 109.4994 81.915) (xy 109.6264 81.5086) (xy 109.474 81.3054) (xy 109.0422 81.3308) (xy 108.6358 81.5848)
        (xy 108.4326 81.8134) (xy 108.204 82.3722) (xy 108.1024 82.7278) (xy 108.0516 82.9056) (xy 107.9246 83.6676)
        (xy 107.9246 84.0232) (xy 107.9246 84.3534) (xy 108.0262 84.582)
      )
    )
  )
)
