(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 306)
    (zones 0)
    (modules 53)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.6 0.8)
    (user_via 2.5 2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.75)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(C12-Pad2)")
  (net 8 "Net-(C15-Pad1)")
  (net 9 /SRC)
  (net 10 "Net-(C12-Pad1)")
  (net 11 "Net-(C16-Pad1)")
  (net 12 "Net-(C17-Pad1)")
  (net 13 /VCC)
  (net 14 /POL)
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(D5-Pad1)")
  (net 17 "Net-(L1-Pad2)")
  (net 18 /SGNL)
  (net 19 "Net-(R14-Pad2)")
  (net 20 "Net-(R1-Pad1)")
  (net 21 "Net-(R12-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /POL)
    (add_net /SGNL)
    (add_net /SRC)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R14-Pad2)")
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5F1B87EF)
    (at 107.27436 106.8578 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 4.572 0.127) (layer F.SilkS))
    (fp_text value 1N5239B (at 1.651 -2.159 90) (layer F.Fab))
    (fp_text user K (at -1.651 0.127) (layer F.Fab))
    (fp_text user K (at -1.651 0.127) (layer F.Fab))
    (fp_text user %R (at 4.445 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5F1B8C79)
    (at 111.76 129.286 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at -1.651 0.127) (layer F.SilkS))
    (fp_text value 1N4148 (at 1.651 -1.905 90) (layer F.Fab))
    (fp_text user K (at -1.651 -1.397) (layer F.Fab))
    (fp_text user K (at -1.651 -1.397) (layer F.Fab))
    (fp_text user %R (at -1.778 0.381) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5F1B8C52)
    (at 108.712 129.286 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at -1.651 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 1.397 1.778 90) (layer F.Fab))
    (fp_text user K (at -1.778 -1.016) (layer F.Fab))
    (fp_text user K (at -1.778 -1.016) (layer F.Fab))
    (fp_text user %R (at -1.778 0.508) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5F1B8A5F)
    (at 123.952 113.792 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D4 (at 4.953 0) (layer F.SilkS))
    (fp_text value 1N5240B (at -5.842 0) (layer F.Fab))
    (fp_text user K (at -1.524 1.016) (layer F.Fab))
    (fp_text user K (at -1.524 1.016) (layer F.Fab))
    (fp_text user %R (at 4.826 0.762) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5F1B8C9F)
    (at 115.824 124.968 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 1.27 -2.032) (layer F.SilkS))
    (fp_text value 1N5240B (at 1.778 -1.905) (layer F.Fab))
    (fp_text user K (at -0.635 -1.905) (layer F.Fab))
    (fp_text user K (at -0.635 -1.905) (layer F.Fab))
    (fp_text user %R (at 1.143 -1.905) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5F1052BE)
    (at 127.762 73.025)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference FET (at 2.794 -1.27) (layer F.SilkS))
    (fp_text value "FET float" (at 5.08 0.127) (layer F.Fab) hide)
    (fp_text user %R (at 2.159 -1.905) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.67 1.67) (drill 1.67) (layers *.Cu *.Mask))
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5F1B8CCC)
    (at 98.298 71.12)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference POL_T1 (at -2.032 0.889 90) (layer F.SilkS))
    (fp_text value 0 (at -2.286 0.254) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(C16-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5F1B8719)
    (at 127.762 79.248)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference SRC_T1 (at 1.524 3.302 90) (layer F.SilkS))
    (fp_text value SRC_T (at 3.81 0) (layer F.Fab))
    (fp_text user %R (at 0.406 2.364) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 /SRC))
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 5F1B8726)
    (at 127.889 76.708)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference VCC_T1 (at 2.032 -0.508 90) (layer F.SilkS))
    (fp_text value VCC_T (at 3.556 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 /VCC))
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 5F1CAEF6)
    (at 124.079 77.851 90)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value J305 (at 1.143 1.905 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.127 0.381 135) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 3 thru_hole circle (at 2.794 0.381 180) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 /SGNL))
    (pad 2 thru_hole circle (at 1.27 -1.651 180) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /SRC))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 5F1CB0AF)
    (at 107.188 113.665 90)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference T1 (at 4.191 -1.778 90) (layer F.SilkS))
    (fp_text value 2N5551 (at 1.143 2.667 90) (layer F.Fab))
    (fp_text user %R (at 4.191 -1.778 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.127 0.381 135) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad2)"))
    (pad 3 thru_hole circle (at 2.794 0.381 180) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -1.651 180) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 5F1CAF60)
    (at 125.73 117.348 270)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value 2N5087 (at 1.27 2.54 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.127 0.381 315) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 3 thru_hole circle (at 2.794 0.381) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -1.651) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 5F1CB001)
    (at 120.904 119.888 90)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.016 -3.429 90) (layer F.SilkS))
    (fp_text value 2N5087 (at 1.27 2.54 90) (layer F.Fab))
    (fp_text user %R (at 1.016 -3.429 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.127 0.254 135) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (pad 3 thru_hole circle (at 2.794 0.254 180) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -1.651 180) (size 1.75 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 5F1B87D1)
    (at 114.10696 107.69346 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C2 (at 0.127 2.032 180) (layer F.SilkS))
    (fp_text value 330u (at 1.143 -2.032) (layer F.Fab))
    (fp_text user %R (at 0.127 2.032 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 5F1B7823)
    (at 114.046 98.806 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C18 (at 0 2.032 270) (layer F.SilkS))
    (fp_text value 220u (at 1.143 -2.032) (layer F.Fab))
    (fp_text user %R (at 0 2.032 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 5F1B884A)
    (at 115.57 115.316 180)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C8 (at 0.127 1.778 180) (layer F.SilkS))
    (fp_text value 100u (at -0.127 -1.651 180) (layer F.Fab))
    (fp_text user %R (at 0.127 1.778 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B8AB0)
    (at 105.029 121.666 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 8.2p (at 2.667 2.159 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 124.968 131.318)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference XLR3 (at 0 2.159) (layer F.SilkS))
    (fp_text value XLR (at -0.508 2.159) (layer F.Fab))
    (fp_text user %R (at 0 2.159) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 "Net-(R14-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 120.904 131.318)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference XLR2 (at 0 2.159) (layer F.SilkS))
    (fp_text value XLR (at -0.508 2.159) (layer F.Fab))
    (fp_text user %R (at 0 2.159) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 20 "Net-(R1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 116.84 131.318)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference XLR1 (at 0.127 2.159) (layer F.SilkS))
    (fp_text value XLR (at -0.381 2.159) (layer F.Fab))
    (fp_text user %R (at 0.127 2.159) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 116.713 71.374)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference SGNL1 (at 2.413 0.127 90) (layer F.SilkS))
    (fp_text value 0 (at 2.159 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.286) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 /SGNL))
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5F1B76B3)
    (at 114.808 76.327)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV1 (at -2.54 -1.524) (layer F.SilkS))
    (fp_text value 1M (at -2.286 1.778) (layer F.Fab))
    (fp_text user %R (at -2.54 -1.524) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /SRC))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8BCB)
    (at 126.82474 127.03048 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 1.016 -2.159) (layer F.SilkS))
    (fp_text value 82k (at -1.143 -2.159) (layer F.Fab))
    (fp_text user %R (at 1.905 -2.159) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R14-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8C8B)
    (at 118.90248 127.03048)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 1.143 2.159) (layer F.SilkS))
    (fp_text value 82k (at 2.921 2.159) (layer F.Fab))
    (fp_text user %R (at -0.254 2.159) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8622)
    (at 121.666 71.628)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 4.953 -0.889) (layer F.SilkS))
    (fp_text value 1G (at 4.445 -0.635) (layer F.Fab))
    (fp_text user %R (at 4.953 -1.778) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /SGNL))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B86FF)
    (at 123.952 82.042)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 1.143 2.286) (layer F.SilkS))
    (fp_text value 2.2k (at 5.08 1.016) (layer F.Fab))
    (fp_text user %R (at 5.08 -0.762) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B86E4)
    (at 120.65 83.566 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 4.191 -0.254) (layer F.SilkS))
    (fp_text value 2.2k (at -1.016 3.048) (layer F.Fab))
    (fp_text user %R (at 4.064 -0.254) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /SRC))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8764)
    (at 124.714 87.122 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 4.318 -0.127) (layer F.SilkS))
    (fp_text value 750R (at 1.016 -2.159 90) (layer F.Fab))
    (fp_text user %R (at 4.318 -0.127) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B774A)
    (at 101.854 83.82 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 4.826 1.016) (layer F.SilkS))
    (fp_text value 1.5M (at 5.207 -0.889) (layer F.Fab))
    (fp_text user %R (at 4.826 1.016) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /POL))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8745)
    (at 120.904 89.154 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -2.286 0.254) (layer F.SilkS))
    (fp_text value 8k2 (at 2.032 1.778 90) (layer F.Fab))
    (fp_text user %R (at -2.286 0.254) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B77D3)
    (at 101.092 91.186)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -2.794 0) (layer F.SilkS))
    (fp_text value 1.5k (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at -2.794 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8A13)
    (at 123.698 107.442 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at -2.54 0.762) (layer F.SilkS))
    (fp_text value 100k (at -3.302 -0.762) (layer F.Fab))
    (fp_text user %R (at -2.54 0.762) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8A37)
    (at 121.666 110.49)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 4.826 0) (layer F.SilkS))
    (fp_text value 100k (at 5.588 1.016) (layer F.Fab))
    (fp_text user %R (at 4.826 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B879B)
    (at 103.124 98.806 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 1.524 2.159 90) (layer F.SilkS))
    (fp_text value 750k (at -0.508 2.286 90) (layer F.Fab))
    (fp_text user %R (at 2.794 2.032 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8B81)
    (at 124.73178 123.698)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 4.318 0 90) (layer F.SilkS))
    (fp_text value 47R (at 4.953 -1.397) (layer F.Fab))
    (fp_text user %R (at 4.318 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5F1B8B5D)
    (at 121.02338 123.64974 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.175 2.032) (layer F.SilkS))
    (fp_text value 47R (at 0.381 2.032) (layer F.Fab))
    (fp_text user %R (at 3.175 2.032) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 103.124 71.374)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference POL1 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 0 (at -2.159 1.397) (layer F.Fab))
    (fp_text user %R (at 0 -2.286) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 /POL))
  )
  (module Inductor_THT:L_Axial_L7.0mm_D3.3mm_P12.70mm_Horizontal_Fastron_MICC (layer F.Cu) (tedit 5F1B8C06)
    (at 101.6 132.08 90)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 12.7mm  length 7mm diameter 3.3mm Fastron MICC")
    (fp_text reference L2 (at 6.35 -0.508 90) (layer F.SilkS))
    (fp_text value 150uH (at 6.35 0.889 90) (layer F.Fab))
    (fp_text user %R (at 6.35 -0.508 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P12.70mm_Horizontal_Fastron_MICC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L7.0mm_D3.3mm_P12.70mm_Horizontal_Fastron_MICC (layer F.Cu) (tedit 5F1B8A7E)
    (at 101.6 104.14 270)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 12.7mm  length 7mm diameter 3.3mm Fastron MICC")
    (fp_text reference L1 (at 6.35 0.508 90) (layer F.SilkS))
    (fp_text value 100uH (at 6.35 -0.889 90) (layer F.Fab))
    (fp_text user %R (at 6.35 0.508 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P12.70mm_Horizontal_Fastron_MICC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 109.728 71.374)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference GND1 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 0 (at -2.159 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.286) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B8963)
    (at 124.57176 94.30258 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C21 (at 2.5 0) (layer F.SilkS))
    (fp_text value 1u (at -2.286 0) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B77F0)
    (at 107.188 99.568 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C20 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 0.01u (at 4.064 -2.032 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B76E2)
    (at 103.124 76.708 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C19 (at 2.5 0) (layer F.SilkS))
    (fp_text value "0.1u 100V" (at 2.54 2.032) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /POL))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B897F)
    (at 119.57812 97.6249)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C17 (at 2.5 0) (layer F.SilkS))
    (fp_text value 8.2n (at 7.874 0) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B7709)
    (at 98.5012 80.26908)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C16 (at 2.5 0) (layer F.SilkS))
    (fp_text value "0.01u 100V" (at -5.588 0) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B8AE4)
    (at 115.57 121.666 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C15 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1u (at 4.826 2.159) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4 (layer F.Cu) (tedit 5F1B77AA)
    (at 107.2134 82.57794)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor")
    (fp_text reference C12 (at 5 0) (layer F.SilkS))
    (fp_text value 0.1u (at 5.334 1.524) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4 (layer F.Cu) (tedit 5F1B877F)
    (at 107.188 89.408)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor")
    (fp_text reference C9 (at 4.953 0) (layer F.SilkS))
    (fp_text value 0.1u (at 5.08 1.524) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SRC))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B8B37)
    (at 104.73944 124.5616)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 2.5 0) (layer F.SilkS))
    (fp_text value 27p (at 3.048 -2.413) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B89C5)
    (at 119.57812 100.67798)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.5 0) (layer F.SilkS))
    (fp_text value 470p (at 7.874 -0.254) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B89E7)
    (at 124.968 103.886 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 2.54 0) (layer F.SilkS))
    (fp_text value 470p (at -3.048 -0.254) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B8C18)
    (at 105.41 132.334 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value "1n 100V" (at 2.667 -1.651 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5F1B7776)
    (at 99.10826 87.58428)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 0.1u (at -2.54 -0.127) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Pimped Alice v56" (at 98.14306 118.5418 90) (layer F.SilkS))
  (gr_line (start 96.774 134.112) (end 94.234 69.088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.794 134.112) (end 96.774 134.112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.334 69.088) (end 129.794 134.112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.234 69.088) (end 132.334 69.088) (layer Edge.Cuts) (width 0.1))
)
