(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 136.8552 104.4194)
    (grid_origin 136.8552 104.4194)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GNDREF")
  (net 3 "/7_SDA")
  (net 4 "/8_SCL")
  (net 5 "/2_INT")
  (net 6 "/3_LDR")
  (net 7 "/4_LDK")
  (net 8 "/5_LEDA")
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 142.5934 94.8946 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -1.9558 -0.0508 180) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/8_SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 149.3012 95.5294 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/2_INT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 142.5934 98.3742 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.2352 0.0762 180) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/7_SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 152.0952 93.9419)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -1.9304 9.1694) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/2_INT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/3_LDR") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/4_LDK") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 144.7038 102.2096 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 142.3162 102.2096 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 2.6416 0 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 8 "/5_LEDA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "OptoDevice:Broadcom_APDS-9160-003" (layer "F.Cu")
    (at 145.7452 97.7519 -90)
    (descr "Broadcom DFN, 8 Pin (https://docs.broadcom.com/docs/APDS-9160-003-DS)")
    (tags "proximity sensor avago")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Proximity Sensor, I2C interface, 1.7-3.6V, LGA-8")
    (property "ki_keywords" "opto proximity sensor avago broadcom")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.54) (layer "F.SilkS") hide)
    (fp_text value "APDS-9160-003" (at 0 2.65 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.915 -0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.305 -0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/2_INT") (pinfunction "INT") (pintype "open_collector"))
    (pad "3" smd roundrect (at 0.305 -0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/3_LDR") (pinfunction "LDR") (pintype "input"))
    (pad "4" smd roundrect (at 0.915 -0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/4_LDK") (pinfunction "LEDK") (pintype "output"))
    (pad "5" smd roundrect (at 0.915 0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/5_LEDA") (pinfunction "LEDA") (pintype "input"))
    (pad "6" smd roundrect (at 0.305 0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "7" smd roundrect (at -0.305 0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/7_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -0.915 0.69 270) (size 0.4 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/8_SCL") (pinfunction "SCL") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/OptoDevice.3dshapes/Broadcom_APDS-9160-003.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 139.3952 101.5619 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "SBoB1_APDS-9160-003.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at -2.1082 -1.4732) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/5_LEDA") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/7_SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/8_SCL") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 136.8552 91.0844) (end 154.6352 104.4194)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "(SBoB1)" (at 148.1836 93.726) (layer "B.SilkS"))
  (gr_text "Sensor Breakout Board 1" (at 145.7198 92.329) (layer "B.SilkS"))
  (gr_text "W" (at 153.5684 103.8606) (layer "B.SilkS"))
  (gr_text "K" (at 154.2034 103.378) (layer "B.SilkS"))
  (gr_text "Made with KiCad 7" (at 151.4856 103.886) (layer "B.SilkS"))
  (gr_text "Rev 1 02042024" (at 137.2616 104.0384 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.4922 92.6084 -90) (layer "F.SilkS"))
  (gr_text "LDA" (at 137.922 102.6922 90) (layer "F.SilkS"))
  (gr_text "VDD" (at 137.9474 100.2284 90) (layer "F.SilkS"))
  (gr_text "I²C Addr:0x53" (at 146.2024 104.1654) (layer "F.SilkS"))
  (gr_text "LDR" (at 153.4922 97.663 270) (layer "F.SilkS"))
  (gr_text "SDA" (at 137.9982 97.6884 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 137.9982 95.0214 90) (layer "F.SilkS"))
  (gr_text "Broadcom APDS-9160-003" (at 137.2362 92.1766) (layer "F.SilkS"))
  (gr_text "INT" (at 153.4922 95.5294 270) (layer "F.SilkS"))
  (gr_text "LDK" (at 153.5176 100.4316 270) (layer "F.SilkS"))
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.481142 98.681801)
        (xy 143.198299 98.398958)
        (xy 142.409149 98.7992)
        (xy 142.592693 99.287407)
        (xy 143.0684 99.483452)
      )
    )
  )
  (zone (net 4) (net_name "/8_SCL") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.198299 96.694842)
        (xy 143.481142 96.411999)
        (xy 143.0684 95.610348)
        (xy 142.592693 95.806393)
        (xy 142.409148 96.2946)
      )
    )
  )
  (zone (net 2) (net_name "GNDREF") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 136.8552 104.4194)
        (xy 154.6352 104.4194)
        (xy 154.6352 91.0844)
        (xy 136.8552 91.0844)
      )
    )
  )
  (zone (net 6) (net_name "/3_LDR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.964915 97.8569)
        (xy 150.964915 98.2569)
        (xy 151.309902 99.347181)
        (xy 152.0962 99.0219)
        (xy 152.420481 98.236602)
      )
    )
  )
  (zone (net 4) (net_name "/8_SCL") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.335652 95.165194)
        (xy 140.618494 94.882352)
        (xy 140.180498 93.616619)
        (xy 139.394493 93.941193)
        (xy 139.069919 94.727198)
      )
    )
  )
  (zone (net 3) (net_name "/7_SDA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.6434 97.2617)
        (xy 141.6434 97.6617)
        (xy 142.265013 97.931121)
        (xy 142.5944 97.4617)
        (xy 142.265013 96.992279)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.949529 93.152686)
        (xy 141.666686 93.435529)
        (xy 142.1184 94.197531)
        (xy 142.594107 93.982807)
        (xy 142.757694 93.4946)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.6434 99.0867)
        (xy 141.6434 99.4867)
        (xy 142.265013 99.756121)
        (xy 142.5944 99.2867)
        (xy 142.265013 98.817279)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.829481 100.329262)
        (xy 145.546638 100.046419)
        (xy 144.46045 100.5846)
        (xy 144.703093 101.172807)
        (xy 145.4288 101.277951)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.757938 95.136305)
        (xy 148.475095 94.853462)
        (xy 147.954327 95.134448)
        (xy 148.106693 95.504707)
        (xy 148.476952 95.657073)
      )
    )
  )
  (zone (net 4) (net_name "/8_SCL") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.6434 95.6071)
        (xy 141.6434 96.0071)
        (xy 142.265013 96.276521)
        (xy 142.5944 95.8071)
        (xy 142.265013 95.337679)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.820295 93.589138)
        (xy 142.103138 93.306295)
        (xy 141.822152 92.785527)
        (xy 141.451893 92.937893)
        (xy 141.299527 93.308152)
      )
    )
  )
  (zone (net 3) (net_name "/7_SDA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.5434 97.6469)
        (xy 143.5434 97.2469)
        (xy 142.921787 96.992279)
        (xy 142.5924 97.4617)
        (xy 142.921787 97.931121)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.9252 99.2219)
        (xy 140.9252 98.8219)
        (xy 139.720481 98.236602)
        (xy 139.3942 99.0219)
        (xy 139.720481 99.807198)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.384788 100.208269)
        (xy 145.667631 100.491112)
        (xy 146.028043 100.003243)
        (xy 145.745907 99.719693)
        (xy 145.3452 99.7204)
      )
    )
  )
  (zone (net 5) (net_name "/2_INT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.969057 97.2569)
        (xy 150.969057 97.6569)
        (xy 152.420481 97.267198)
        (xy 152.0962 96.4819)
        (xy 151.309902 96.156619)
      )
    )
  )
  (zone (net 8) (net_name "/5_LEDA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.0037 100.9721)
        (xy 141.0037 101.3721)
        (xy 141.745529 101.74057)
        (xy 142.3172 101.1721)
        (xy 141.745529 100.60363)
      )
    )
  )
  (zone (net 5) (net_name "/2_INT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.5652 96.2819)
        (xy 150.5652 96.6819)
        (xy 151.769919 97.267198)
        (xy 152.0962 96.4819)
        (xy 151.769919 95.696602)
      )
    )
  )
  (zone (net 8) (net_name "/5_LEDA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.441881 100.329262)
        (xy 143.159038 100.046419)
        (xy 142.07285 100.5846)
        (xy 142.315493 101.172807)
        (xy 143.0412 101.277951)
      )
    )
  )
  (zone (net 8) (net_name "/5_LEDA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.904321 101.313522)
        (xy 140.621478 101.030679)
        (xy 140.2452 100.7119)
        (xy 139.394493 101.562607)
        (xy 140.2452 102.203772)
      )
    )
  )
  (zone (net 7) (net_name "/4_LDK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 151.154748 100.338606)
        (xy 150.871906 100.621448)
        (xy 151.309902 101.887181)
        (xy 152.095907 101.562607)
        (xy 152.420481 100.776602)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.348903 94.979654)
        (xy 148.631746 95.262497)
        (xy 149.416368 95.1044)
        (xy 149.301907 94.616193)
        (xy 148.829419 94.350712)
      )
    )
  )
  (zone (net 3) (net_name "/7_SDA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.519354 97.6617)
        (xy 140.519354 97.2617)
        (xy 140.180498 96.156619)
        (xy 139.3942 96.4819)
        (xy 139.069919 97.267198)
      )
    )
  )
  (zone (net 5) (net_name "/2_INT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.2512 96.6819)
        (xy 150.2512 96.2819)
        (xy 149.642133 95.980862)
        (xy 149.3002 96.4419)
        (xy 149.629587 96.911321)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 136.8552 104.4194)
        (xy 154.6352 104.4194)
        (xy 154.6352 91.0844)
        (xy 136.8552 91.0844)
      )
    )
  )
)
