(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 140)
    (zones 0)
    (modules 2)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad16)")
  (net 2 "Net-(U1-Pad1)")
  (net 3 "Net-(U2-Pad39)")
  (net 4 GND)
  (net 5 +5V)
  (net 6 /PRGA14R)
  (net 7 /PRGA16R)
  (net 8 /PRGA14N)
  (net 9 /PRGA13R)
  (net 10 /PRGA15R)
  (net 11 /PRGRWN)
  (net 12 /CHRA16R)
  (net 13 /CHRA11R)
  (net 14 /WRAMWE)
  (net 15 /WRAMCE)
  (net 16 /PRGD3S)
  (net 17 /PRGD2S)
  (net 18 /PRGD4S)
  (net 19 /PRGD1S)
  (net 20 /PRGD5S)
  (net 21 /PRGD0S)
  (net 22 /PRGD6S)
  (net 23 /PRGA0S)
  (net 24 /PRGD7S)
  (net 25 /WRAM-CE)
  (net 26 /M2)
  (net 27 /PRG-CER)
  (net 28 /PRGA17R)
  (net 29 /PRGA13N)
  (net 30 /PRGA18R)
  (net 31 /PRGCEN)
  (net 32 /IRQ)
  (net 33 /CHRA17R)
  (net 34 /CHRA15R)
  (net 35 /CIRAM)
  (net 36 /CHRA12R)
  (net 37 /CHRA14R)
  (net 38 /CHRA13R)
  (net 39 /CHRA10N)
  (net 40 /CHRA11N)
  (net 41 /CHRA12N)
  (net 42 /CHRA10R)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /CHRA10N)
    (add_net /CHRA10R)
    (add_net /CHRA11N)
    (add_net /CHRA11R)
    (add_net /CHRA12N)
    (add_net /CHRA12R)
    (add_net /CHRA13R)
    (add_net /CHRA14R)
    (add_net /CHRA15R)
    (add_net /CHRA16R)
    (add_net /CHRA17R)
    (add_net /CIRAM)
    (add_net /IRQ)
    (add_net /M2)
    (add_net /PRG-CER)
    (add_net /PRGA0S)
    (add_net /PRGA13N)
    (add_net /PRGA13R)
    (add_net /PRGA14N)
    (add_net /PRGA14R)
    (add_net /PRGA15R)
    (add_net /PRGA16R)
    (add_net /PRGA17R)
    (add_net /PRGA18R)
    (add_net /PRGCEN)
    (add_net /PRGD0S)
    (add_net /PRGD1S)
    (add_net /PRGD2S)
    (add_net /PRGD3S)
    (add_net /PRGD4S)
    (add_net /PRGD5S)
    (add_net /PRGD6S)
    (add_net /PRGD7S)
    (add_net /PRGRWN)
    (add_net /WRAM-CE)
    (add_net /WRAMCE)
    (add_net /WRAMWE)
    (add_net GND)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U2-Pad39)")
  )
  (module Package_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5A02E8C5)
    (at 114.3 97.02752)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U2 (at 7.62 -2.33) (layer F.SilkS) hide)
    (fp_text value AX5202P (at 7.62 50.59) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 24.13) (layer F.Fab) hide)
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U2-Pad39)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /CHRA10N))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /PRG-CER))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /CHRA11N))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /PRGA17R))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /CHRA12N))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /PRGA13N))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /CHRA10R))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /PRGA18R))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /CHRA16R))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /PRGA14R))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /CHRA11R))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /PRGA16R))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /WRAMWE))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /PRGA14N))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /WRAMCE))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /PRGA13R))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /PRGD3S))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /PRGA15R))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /PRGD2S))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /PRGRWN))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /PRGD4S))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /PRGCEN))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /PRGD1S))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /IRQ))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /PRGD5S))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /CHRA17R))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /PRGD0S))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /CHRA15R))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /PRGD6S))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /CIRAM))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /PRGA0S))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /CHRA12R))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /PRGD7S))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /CHRA14R))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /WRAM-CE))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /CHRA13R))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /M2))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5D9F72AF)
    (at 121.92 121.412 90)
    (descr "LQFP, 44 Pin (https://www.nxp.com/files-static/shared/doc/package_info/98ASS23225W.pdf?&fsrch=1), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference U1 (at 0.17272 0.09144 180) (layer F.SilkS))
    (fp_text value MMC3 (at -1.35128 0.09144 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 44 smd roundrect (at -4 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /CHRA16R))
    (pad 43 smd roundrect (at -3.2 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /CHRA11R))
    (pad 42 smd roundrect (at -2.4 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /WRAMWE))
    (pad 41 smd roundrect (at -1.6 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /WRAMCE))
    (pad 40 smd roundrect (at -0.8 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 39 smd roundrect (at 0 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /PRGD3S))
    (pad 38 smd roundrect (at 0.8 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /PRGD2S))
    (pad 37 smd roundrect (at 1.6 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /PRGD4S))
    (pad 36 smd roundrect (at 2.4 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /PRGD1S))
    (pad 35 smd roundrect (at 3.2 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /PRGD5S))
    (pad 34 smd roundrect (at 4 -5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /PRGD0S))
    (pad 33 smd roundrect (at 5.6625 -4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /PRGD6S))
    (pad 32 smd roundrect (at 5.6625 -3.2 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /PRGA0S))
    (pad 31 smd roundrect (at 5.6625 -2.4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /PRGD7S))
    (pad 30 smd roundrect (at 5.6625 -1.6 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /WRAM-CE))
    (pad 29 smd roundrect (at 5.6625 -0.8 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /M2))
    (pad 28 smd roundrect (at 5.6625 0 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 27 smd roundrect (at 5.6625 0.8 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 26 smd roundrect (at 5.6625 1.6 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /PRG-CER))
    (pad 25 smd roundrect (at 5.6625 2.4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /PRGA17R))
    (pad 24 smd roundrect (at 5.6625 3.2 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /PRGA13N))
    (pad 23 smd roundrect (at 5.6625 4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /PRGA18R))
    (pad 22 smd roundrect (at 4 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /PRGA14R))
    (pad 21 smd roundrect (at 3.2 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /PRGA16R))
    (pad 20 smd roundrect (at 2.4 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /PRGA14N))
    (pad 19 smd roundrect (at 1.6 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /PRGA13R))
    (pad 18 smd roundrect (at 0.8 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /PRGA15R))
    (pad 17 smd roundrect (at 0 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /PRGRWN))
    (pad 16 smd roundrect (at -0.8 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad16)"))
    (pad 15 smd roundrect (at -1.6 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 14 smd roundrect (at -2.4 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /PRGCEN))
    (pad 13 smd roundrect (at -3.2 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /IRQ))
    (pad 12 smd roundrect (at -4 5.6625 90) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /CHRA17R))
    (pad 11 smd roundrect (at -5.6625 4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /CHRA15R))
    (pad 10 smd roundrect (at -5.6625 3.2 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /CIRAM))
    (pad 9 smd roundrect (at -5.6625 2.4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /CHRA12R))
    (pad 8 smd roundrect (at -5.6625 1.6 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /CHRA14R))
    (pad 7 smd roundrect (at -5.6625 0.8 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /CHRA13R))
    (pad 6 smd roundrect (at -5.6625 0 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 5 smd roundrect (at -5.6625 -0.8 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /CHRA10N))
    (pad 4 smd roundrect (at -5.6625 -1.6 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /CHRA11N))
    (pad 3 smd roundrect (at -5.6625 -2.4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /CHRA12N))
    (pad 2 smd roundrect (at -5.6625 -3.2 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /CHRA10R))
    (pad 1 smd roundrect (at -5.6625 -4 90) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text www.github.com/winddrake/MMC3toAX5202P (at 121.9835 119.253 90) (layer B.SilkS))
  (gr_line (start 129.54 146.87804) (end 114.3 146.8755) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.3 95.4278) (end 114.3 146.8755) (layer Edge.Cuts) (width 0.05))
  (gr_text "AX5202P to MMC3\nBy WindDrake" (at 121.92 106.2355 90) (layer F.SilkS))
  (gr_line (start 129.54 95.4278) (end 129.54 146.87804) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.3 95.4278) (end 129.54 95.4278) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.54 95.4405) (xy 129.54 146.8755) (xy 114.3 146.8755) (xy 114.3 95.4278)
      )
    )
  )
)
