<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="45" y1="35" x2="10" y2="35" width="0" layer="20"/>
<wire x1="10" y1="35" x2="0" y2="25" width="0" layer="20" curve="90"/>
<wire x1="0" y1="25" x2="0" y2="10" width="0" layer="20"/>
<wire x1="0" y1="10" x2="10" y2="0" width="0" layer="20" curve="90"/>
<wire x1="10" y1="0" x2="45" y2="0" width="0" layer="20"/>
<wire x1="45" y1="0" x2="55" y2="10" width="0" layer="20" curve="90"/>
<wire x1="55" y1="10" x2="55" y2="25" width="0" layer="20"/>
<wire x1="55" y1="25" x2="45" y2="35" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="Strawson_Eagle_Lib">
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
<package name="0402-RES">
<description>&lt;b&gt; Resistor 0402&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="BeagleBone_Blue">
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="Seeed-OPL-Inductor">
<packages>
<package name="L0603">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-1101NE">
<description>SparkFun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="pocketbone">
<description>Generated from &lt;b&gt;pocketbone.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="OSD3358">
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="USB-AB-MICRO-SMD">
<description>micro USB AB connector for OTG support. 5-pins: USBVCC, GND, D+, D-, USBID. Can act as host or device</description>
</package>
<package name="SOT95P290X145-5N">
</package>
<package name="DCK5">
</package>
<package name="CM200C-32.768KAZF-UT">
</package>
<package name="445C33D24M00000">
</package>
<package name="P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C8" library="Strawson_Eagle_Lib" package="0402-CAP" value="0.1uF"/>
<element name="C1" library="Strawson_Eagle_Lib" package="0402-CAP" value="0.1uF"/>
<element name="C5" library="Strawson_Eagle_Lib" package="0402-CAP" value="20pF"/>
<element name="C7" library="Strawson_Eagle_Lib" package="0402-CAP" value="20pF"/>
<element name="C6" library="Strawson_Eagle_Lib" package="0402-CAP" value="20pF"/>
<element name="C4" library="Strawson_Eagle_Lib" package="0402-CAP" value="20pF"/>
<element name="C9" library="Strawson_Eagle_Lib" package="0402-CAP" value="1uF"/>
<element name="C2" library="Strawson_Eagle_Lib" package="0805" value="10uF"/>
<element name="C3" library="Strawson_Eagle_Lib" package="0402-CAP" value="0.1uF"/>
<element name="C11" library="Strawson_Eagle_Lib" package="0402-CAP" value="0.1uF"/>
<element name="C10" library="Strawson_Eagle_Lib" package="0805" value="10uF"/>
<element name="USR0" library="BeagleBone_Blue" package="LED-0603" value="BLUE"/>
<element name="USR1" library="BeagleBone_Blue" package="LED-0603" value="BLUE"/>
<element name="USR2" library="BeagleBone_Blue" package="LED-0603" value="BLUE"/>
<element name="USR3" library="BeagleBone_Blue" package="LED-0603" value="BLUE"/>
<element name="PWR" library="BeagleBone_Blue" package="LED-0603" value="BLUE"/>
<element name="J1" library="pocketbone" package="MICRO-SD-SOCKET-PP" value="USD_CONNECTOR">
<attribute name="PROD_ID" value="CONN-07820"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Seeed-OPL-Inductor" package="L0603" value="120"/>
<element name="R27" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R13" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R14" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R15" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R16" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R17" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R18" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R19" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R20" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R21" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R22" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R24" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R25" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R26" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R11" library="Strawson_Eagle_Lib" package="0402-RES" value="0"/>
<element name="R12" library="Strawson_Eagle_Lib" package="0402-RES" value="0,DNI"/>
<element name="R29" library="Strawson_Eagle_Lib" package="0402-RES" value="10K,1%"/>
<element name="R5" library="Strawson_Eagle_Lib" package="0402-RES" value="1.5K,1%"/>
<element name="R6" library="Strawson_Eagle_Lib" package="0402-RES" value="1.5K,1%"/>
<element name="R9" library="Strawson_Eagle_Lib" package="0402-RES" value="4.87k"/>
<element name="R28" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R23" library="Strawson_Eagle_Lib" package="0402-RES" value="100K,1%"/>
<element name="R7" library="Strawson_Eagle_Lib" package="0402-RES" value="1.5K,1%"/>
<element name="R8" library="Strawson_Eagle_Lib" package="0402-RES" value="4.87k"/>
<element name="R10" library="Strawson_Eagle_Lib" package="0402-RES" value="10K,1%"/>
<element name="R1" library="Strawson_Eagle_Lib" package="0402-RES" value="240"/>
<element name="R2" library="Strawson_Eagle_Lib" package="0402-RES" value="240"/>
<element name="R3" library="Strawson_Eagle_Lib" package="0402-RES" value="240"/>
<element name="R4" library="Strawson_Eagle_Lib" package="0402-RES" value="240"/>
<element name="U2" library="pocketbone" package="OSD3358" value="OSD3358"/>
<element name="TP1" library="pocketbone" package="P1-17" value="TPSQPAD1-17">
<attribute name="TP_SIGNAL_NAME" value="SYS_5V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="pocketbone" package="P1-17" value="TPSQPAD1-17">
<attribute name="TP_SIGNAL_NAME" value="WP"/>
</element>
<element name="TP2" library="pocketbone" package="P1-17" value="TPSQPAD1-17">
<attribute name="TP_SIGNAL_NAME" value="5.0V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="pocketbone" package="SOT95P290X145-5N" value="24LC_32AT-I/OT">
<attribute name="OC_NEWARK" value="08P0113"/>
<attribute name="OC_FARNELL" value="1700993  "/>
<attribute name="SUPPLIER" value="MICROCHIP"/>
<attribute name="PACKAGE" value="SOT-23-5 "/>
<attribute name="MPN" value="24LC32AT-I/OT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="pocketbone" package="DCK5" value="SN74LVC1G07_DCK_5">
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/gpn/SN74LVC1G07"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SC70"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="PACKAGE_DESIGNATOR" value="DCK"/>
<attribute name="FAMILY_NAME" value="LL BUFFER AND DRIVER WITH OPEN-DRAIN OUTPUT"/>
<attribute name="GENERIC_PART_NUMBER" value="SN74LVC1G07"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="sn74lvc1g07_dck_5"/>
<attribute name="PIN_COUNT" value="5"/>
<attribute name="DESCRIPTION" value="Single Buffer/Driver With Open-Drain Output"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB0" library="pocketbone" package="USB-AB-MICRO-SMD" value="USB-MICRO-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="pocketbone" package="USB-AB-MICRO-SMD" value="USB-MICRO-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="pocketbone" package="CM200C-32.768KAZF-UT" value="CM200C-32.768KAZF-UT"/>
<element name="Y2" library="pocketbone" package="445C33D24M00000" value="445C33D24M00000"/>
<element name="TP3" library="pocketbone" package="P1-17" value="TPSQPAD1-17">
<attribute name="TP_SIGNAL_NAME" value="GND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="SWITCH-MOMENTARY-2SMD-1101NE">
<attribute name="PROD_ID" value="SWCH-00815"/>
</element>
<element name="RESET" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="SWITCH-MOMENTARY-2SMD-1101NE">
<attribute name="PROD_ID" value="SWCH-00815"/>
</element>
</elements>
<signals>
<signal name="VIN_BAT_0">
<contactref element="U2" pad="Y2"/>
</signal>
<signal name="VIN_BAT_1">
<contactref element="U2" pad="Y3"/>
</signal>
<signal name="5.0V">
<contactref element="U2" pad="Y5"/>
<contactref element="U2" pad="Y6"/>
<contactref element="TP2" pad="TP"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="SYS_5V">
<contactref element="U2" pad="Y4"/>
<contactref element="U2" pad="W4"/>
<contactref element="TP1" pad="TP"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="USB_DC">
<contactref element="U2" pad="Y8"/>
<contactref element="U2" pad="Y9"/>
<contactref element="USB0" pad="VBUS"/>
<contactref element="U2" pad="P15"/>
</signal>
<signal name="N$12">
<contactref element="U2" pad="D19"/>
<contactref element="U2" pad="C6"/>
</signal>
<signal name="PWR">
<contactref element="U2" pad="D20"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="I2C0_SCL">
<contactref element="U2" pad="C16"/>
<contactref element="U2" pad="C20"/>
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="I2C0_SDA">
<contactref element="U2" pad="C19"/>
<contactref element="U2" pad="C17"/>
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="U20"/>
<contactref element="U2" pad="V20"/>
<contactref element="C8" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="VDD_3V3AUX">
<contactref element="U2" pad="Y11"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="PWR_LEDR">
<contactref element="PWR" pad="C"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="GND1"/>
<contactref element="J1" pad="GND3"/>
<contactref element="J1" pad="GND"/>
<contactref element="C9" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="USB0" pad="GND"/>
<contactref element="USB0" pad="SHIELD1"/>
<contactref element="USB0" pad="SHIELD2"/>
<contactref element="USB0" pad="SHIELD3"/>
<contactref element="USB0" pad="SHIELD4"/>
<contactref element="U2" pad="A1"/>
<contactref element="U2" pad="J6"/>
<contactref element="U2" pad="L19"/>
<contactref element="U2" pad="M10"/>
<contactref element="U2" pad="M19"/>
<contactref element="U2" pad="N7"/>
<contactref element="U2" pad="V1"/>
<contactref element="U2" pad="V19"/>
<contactref element="U2" pad="W2"/>
<contactref element="U2" pad="W11"/>
<contactref element="U2" pad="W20"/>
<contactref element="U2" pad="Y18"/>
<contactref element="R29" pad="2"/>
<contactref element="TP3" pad="TP"/>
<contactref element="RESET" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="USB1" pad="GND"/>
<contactref element="USB1" pad="SHIELD3"/>
<contactref element="USB1" pad="SHIELD4"/>
<contactref element="USB1" pad="SHIELD1"/>
<contactref element="USB1" pad="SHIELD2"/>
</signal>
<signal name="VDD_1V8">
<contactref element="U2" pad="N16"/>
<contactref element="U2" pad="R16"/>
<contactref element="U2" pad="E9"/>
<contactref element="U2" pad="D10"/>
</signal>
<signal name="PMIC_PGOOD">
<contactref element="U2" pad="A20"/>
<contactref element="U2" pad="B15"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="PMIC_NWAKEUP">
<contactref element="U2" pad="A19"/>
<contactref element="U2" pad="C5"/>
</signal>
<signal name="LDO_PGOOD">
<contactref element="U2" pad="B20"/>
<contactref element="U2" pad="B5"/>
</signal>
<signal name="PMIC_INT">
<contactref element="U2" pad="B19"/>
<contactref element="U2" pad="B18"/>
</signal>
<signal name="N$26">
<contactref element="Y1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U2" pad="M20"/>
</signal>
<signal name="N$27">
<contactref element="U2" pad="K20"/>
<contactref element="Y1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$31">
<contactref element="U2" pad="L20"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="U2" pad="H20"/>
<contactref element="C6" pad="1"/>
<contactref element="Y2" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="U2" pad="F20"/>
<contactref element="C4" pad="2"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="G20"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="U2" pad="B10"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="U2" pad="A10"/>
<contactref element="R10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="VDD_RTC">
<contactref element="U3" pad="5"/>
<contactref element="U2" pad="E14"/>
</signal>
<signal name="N$43">
<contactref element="U2" pad="V16"/>
<contactref element="USR3" pad="A"/>
</signal>
<signal name="N$44">
<contactref element="U2" pad="T15"/>
<contactref element="USR2" pad="A"/>
</signal>
<signal name="N$45">
<contactref element="U2" pad="U15"/>
<contactref element="USR1" pad="A"/>
</signal>
<signal name="N$46">
<contactref element="U2" pad="V15"/>
<contactref element="USR0" pad="A"/>
</signal>
<signal name="N$47">
<contactref element="USR0" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="USR1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="USR2" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$59">
<contactref element="USR3" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="U2" pad="G18"/>
<contactref element="J1" pad="CMD"/>
</signal>
<signal name="VCC_3V3B">
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="VCC"/>
</signal>
<signal name="NTE">
<contactref element="U2" pad="F18"/>
<contactref element="J1" pad="DAT2"/>
</signal>
<signal name="N$77">
<contactref element="U2" pad="G16"/>
<contactref element="J1" pad="DAT0"/>
</signal>
<signal name="N$70">
<contactref element="U2" pad="G15"/>
<contactref element="J1" pad="DAT1"/>
</signal>
<signal name="N$75">
<contactref element="U2" pad="C15"/>
<contactref element="J1" pad="CD1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="CLK"/>
<contactref element="U2" pad="G17"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="CD/DAT3"/>
<contactref element="U2" pad="F17"/>
</signal>
<signal name="MDIR_4A">
<contactref element="R13" pad="2"/>
<contactref element="U2" pad="R1"/>
</signal>
<signal name="MDIR_4B">
<contactref element="R14" pad="2"/>
<contactref element="U2" pad="R2"/>
</signal>
<signal name="MDIR_3B">
<contactref element="U2" pad="R3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="MDIR_3A">
<contactref element="R16" pad="1"/>
<contactref element="U2" pad="R4"/>
</signal>
<signal name="SVO7">
<contactref element="R17" pad="1"/>
<contactref element="U2" pad="T1"/>
</signal>
<signal name="SVO8">
<contactref element="R18" pad="1"/>
<contactref element="U2" pad="T2"/>
</signal>
<signal name="SVO5">
<contactref element="R19" pad="2"/>
<contactref element="U2" pad="T3"/>
</signal>
<signal name="SVO6">
<contactref element="R20" pad="2"/>
<contactref element="U2" pad="T4"/>
</signal>
<signal name="SERVO_EN">
<contactref element="U2" pad="U3"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="MDIR_2B">
<contactref element="U2" pad="U4"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="BATT_LED_2">
<contactref element="R26" pad="2"/>
<contactref element="U2" pad="T5"/>
</signal>
<signal name="UART5_TX">
<contactref element="R21" pad="2"/>
<contactref element="U2" pad="U1"/>
</signal>
<signal name="UART5_RX">
<contactref element="R22" pad="2"/>
<contactref element="U2" pad="U2"/>
</signal>
<signal name="USB0_DP">
<contactref element="U2" pad="N17"/>
<contactref element="USB0" pad="D+"/>
</signal>
<signal name="USB0_DM">
<contactref element="U2" pad="N18"/>
<contactref element="USB0" pad="D-"/>
</signal>
<signal name="USB0_ID">
<contactref element="U2" pad="P16"/>
<contactref element="USB0" pad="ID"/>
</signal>
<signal name="USB1_DP">
<contactref element="U2" pad="R17"/>
<contactref element="USB1" pad="D+"/>
</signal>
<signal name="USB1_DM">
<contactref element="U2" pad="R18"/>
<contactref element="USB1" pad="D-"/>
</signal>
<signal name="N$129">
<contactref element="U2" pad="T18"/>
<contactref element="L1" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="EQEP_1A">
<contactref element="U2" pad="V2"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="EQEP_1B">
<contactref element="U2" pad="V3"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="LCD_DATA_14">
<contactref element="R25" pad="1"/>
<contactref element="U2" pad="V4"/>
</signal>
<signal name="N$131">
<contactref element="U2" pad="B4"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="USB1_ID">
<contactref element="U2" pad="P17"/>
<contactref element="USB1" pad="ID"/>
</signal>
<signal name="N$1">
<contactref element="L1" pad="2"/>
<contactref element="USB1" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
