<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>OUT</text>
<text>IN</text>
<text>R</text>
<text>L</text>
<text>TDA7266 Audio Amp</text>
<text>L</text>
<text>R</text>
<text>DC IN</text>
<wire x1="3.81" y1="0" x2="40.64" y2="0" width="0.254" layer="20"/>
<wire x1="40.64" y1="0" x2="44.45" y2="3.81" width="0.254" layer="20" curve="90"/>
<wire x1="44.45" y1="3.81" x2="44.45" y2="27.94" width="0.254" layer="20"/>
<wire x1="44.45" y1="27.94" x2="40.64" y2="31.75" width="0.254" layer="20" curve="90"/>
<wire x1="40.64" y1="31.75" x2="3.81" y2="31.75" width="0.254" layer="20"/>
<wire x1="3.81" y1="31.75" x2="0" y2="27.94" width="0.254" layer="20" curve="90"/>
<wire x1="0" y1="27.94" x2="0" y2="3.81" width="0.254" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0.254" layer="20" curve="90"/>
<text>-</text>
<text>+</text>
<text>3-16V</text>
<text>KD0GLS 2017</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="CAPACITOR_ELECTROLYTIC_3.5MM">
</package>
<package name="CAPACITOR_FILM_2.5MM">
</package>
<package name="EIA3216">
<description>Kemet size A</description>
</package>
<package name="0805">
</package>
<package name="MULTIWATT15">
</package>
<package name="CONN_PHOENIX_TERM_BLOCK_3PIN_100">
</package>
<package name="CONN_PHOENIX_TERM_BLOCK_2PIN_100">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="kd0gls" package="CAPACITOR_ELECTROLYTIC_3.5MM" value="470uF"/>
<element name="C3" library="kd0gls" package="EIA3216" value="10uF"/>
<element name="C4" library="kd0gls" package="CAPACITOR_FILM_2.5MM" value="0.1uF"/>
<element name="C5" library="kd0gls" package="CAPACITOR_FILM_2.5MM" value="0.22uF"/>
<element name="C6" library="kd0gls" package="CAPACITOR_FILM_2.5MM" value="0.22uF"/>
<element name="U1" library="kd0gls" package="MULTIWATT15" value="TDA7266"/>
<element name="R1" library="kd0gls" package="0805" value="47K"/>
<element name="R2" library="kd0gls" package="0805" value="47K"/>
<element name="J1" library="kd0gls" package="CONN_PHOENIX_TERM_BLOCK_3PIN_100" value="CONN_PHOENIX_TERM_BLOCK_3PIN_100"/>
<element name="J2" library="kd0gls" package="CONN_PHOENIX_TERM_BLOCK_2PIN_100" value="CONN_PHOENIX_TERM_BLOCK_2PIN_100"/>
<element name="J3" library="kd0gls" package="CONN_PHOENIX_TERM_BLOCK_2PIN_100" value="CONN_PHOENIX_TERM_BLOCK_2PIN_100"/>
<element name="R3" library="kd0gls" package="0805" value="1MEG"/>
<element name="R4" library="kd0gls" package="0805" value="1MEG"/>
<element name="J4" library="kd0gls" package="CONN_PHOENIX_TERM_BLOCK_2PIN_100" value="CONN_PHOENIX_TERM_BLOCK_2PIN_100"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="C1" pad="+"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="13"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="-"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="9"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="RIN">
<contactref element="J1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="LIN">
<contactref element="J1" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="STANDBY_MUTE">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="LOUT-">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="LOUT+">
<contactref element="U1" pad="15"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="ROUT+">
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="ROUT-">
<contactref element="U1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="LIN2">
<contactref element="C6" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="RIN2">
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
