(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 98)
    (zones 0)
    (modules 4)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J2-Pad5)")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "Net-(J2-Pad3)")
  (net 9 "Net-(J2-Pad2)")
  (net 10 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_gap 0.1524)
    (diff_pair_width 0.1524)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5BBFA2DB)
    (at 132.08 101.6)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value LEFT (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5BBFA2DD)
    (at 149.86 111.76 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value RIGHT (at 0 12.49 180) (layer F.Fab))
    (fp_text user %R (at 0 5.08 270) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:Molex_52892-1033_1x10-1MP_P0.5mm_Horizontal (layer B.Cu) (tedit 5BBF9966)
    (at 140.97 102.235)
    (descr "0.50mm Pitch Easy-On FFC/FPC Connector, Right-Angle, Surface Mount, ZIF, Bottom Contact Style, Cable Retention Guide, 10 Circuits (https://www.molex.com/webdocs/datasheets/pdf/en-us/0528921033_FFC_FPC_CONNECTORS.pdf)")
    (tags "molex FFC/FPC connector Pitch 0.5mm right angle")
    (attr smd)
    (fp_text reference J3 (at 0 3.57) (layer B.SilkS))
    (fp_text value FFC_10 (at 0 -4.9) (layer B.Fab))
    (fp_text user %R (at 0.02 -1.28) (layer B.Fab))
    (pad MP smd rect (at -4.9 -1.37) (size 1.6 2.2) (layers B.Cu B.Paste B.Mask))
    (pad MP smd rect (at 4.9 -1.37) (size 1.6 2.2) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -2.25 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -1.75 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -1.25 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -0.75 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -0.25 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0.25 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 7 smd rect (at 0.75 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 8 smd rect (at 1.25 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 9 smd rect (at 1.75 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 10 smd rect (at 2.25 1.77) (size 0.3 1.4) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Molex_502244-1530_1x15-1MP_P0.5mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:Molex_52892-1033_1x10-1MP_P0.5mm_Horizontal (layer F.Cu) (tedit 5BBF9966)
    (at 140.97 111.125)
    (descr "0.50mm Pitch Easy-On FFC/FPC Connector, Right-Angle, Surface Mount, ZIF, Bottom Contact Style, Cable Retention Guide, 10 Circuits (https://www.molex.com/webdocs/datasheets/pdf/en-us/0528921033_FFC_FPC_CONNECTORS.pdf)")
    (tags "molex FFC/FPC connector Pitch 0.5mm right angle")
    (attr smd)
    (fp_text reference J4 (at 0 -3.57) (layer F.SilkS))
    (fp_text value FFC_10 (at 0 4.9) (layer F.Fab))
    (fp_text user %R (at 0.02 1.28 180) (layer F.Fab))
    (pad MP smd rect (at -4.9 1.37) (size 1.6 2.2) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at 4.9 1.37) (size 1.6 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -1.75 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -1.25 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -0.75 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -0.25 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0.25 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 7 smd rect (at 0.75 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 8 smd rect (at 1.25 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 9 smd rect (at 1.75 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 10 smd rect (at 2.25 -1.77) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Molex_502244-1530_1x15-1MP_P0.5mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 6 (at 149.86 114.3) (layer F.SilkS))
  (gr_text 5 (at 132.08 114.3) (layer F.SilkS))
  (gr_text 10 (at 149.86 99.06) (layer F.SilkS))
  (gr_text 1 (at 132.08 99.06) (layer F.SilkS))
  (gr_line (start 129.54 97.79) (end 152.4 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 115.57) (end 129.54 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 115.57) (end 129.54 115.57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 97.79) (end 152.4 115.57) (layer Edge.Cuts) (width 0.15))
)
