(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 59)
    (no_connects 0)
    (area 93.887857 67.189999 165.175001 107.390001)
    (thickness 1.6)
    (drawings 44)
    (tracks 119)
    (zones 0)
    (modules 32)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDA)
  (net 2 GND)
  (net 3 "Net-(R5-Pad2)")
  (net 4 "Net-(R6-Pad2)")
  (net 5 "Net-(R7-Pad2)")
  (net 6 "Net-(R8-Pad2)")
  (net 7 "Net-(C18-Pad1)")
  (net 8 "Net-(C18-Pad2)")
  (net 9 "Net-(P1-Pad1)")
  (net 10 "Net-(P1-Pad2)")
  (net 11 "Net-(P2-Pad1)")
  (net 12 "Net-(P2-Pad2)")
  (net 13 "Net-(P3-Pad1)")
  (net 14 "Net-(P3-Pad2)")
  (net 15 "Net-(P4-Pad1)")
  (net 16 "Net-(P4-Pad2)")
  (net 17 "Net-(C1-Pad1)")
  (net 18 "Net-(C2-Pad2)")
  (net 19 +12V)
  (net 20 "Net-(RV1-Pad2)")
  (net 21 "Net-(RV3-Pad2)")
  (net 22 "Net-(RV4-Pad2)")
  (net 23 "Net-(RV2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(RV2-Pad2)")
    (add_net "Net-(RV3-Pad2)")
    (add_net "Net-(RV4-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(C1-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58FECD4C)
    (at 111.125 71.12)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at -4.445 -1.27) (layer F.SilkS))
    (fp_text value Input1 (at -10.795 5.715) (layer F.Fab))
    (fp_text user %R (at -3.81 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58FECD4A)
    (at 111.125 78.74)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at -5.08 -0.635) (layer F.SilkS))
    (fp_text value Input1 (at -12.065 4.445) (layer F.Fab))
    (fp_text user %R (at -3.81 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58FECD4D)
    (at 111.125 86.36)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at -5.08 -2.54) (layer F.SilkS))
    (fp_text value Input1 (at -14.605 3.81) (layer F.Fab))
    (fp_text user %R (at -4.445 -3.175) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58FECD4F)
    (at 111.125 93.98)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P4 (at -5.08 -5.08) (layer F.SilkS))
    (fp_text value Input1 (at -12.7 4.445) (layer F.Fab))
    (fp_text user %R (at -4.445 -3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P4-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5ADB97DF)
    (at 149.225 69.215 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P6 (at 13.97 43.18 270) (layer F.SilkS))
    (fp_text value MixOut (at 5.08 44.45 270) (layer F.Fab))
    (fp_text user %R (at 2.54 42.545 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Libraries:AudioTransformer-4pin (layer F.Cu) (tedit 5ADB97E8)
    (at 122.555 100.33 180)
    (fp_text reference T3 (at 19.05 13.335 180) (layer F.SilkS))
    (fp_text value TRANSFO-AUDIO (at 19.685 31.75 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(RV3-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDA))
    (pad 4 thru_hole circle (at -2.54 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(R7-Pad2)"))
  )
  (module Libraries:AudioTransformer-4pin (layer F.Cu) (tedit 5ADB97EB)
    (at 135.89 94.615)
    (fp_text reference T4 (at -27.94 7.62) (layer F.SilkS))
    (fp_text value TRANSFO-AUDIO (at -33.02 -24.765) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(RV4-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(R8-Pad2)"))
    (pad 4 thru_hole circle (at -2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDA))
  )
  (module Libraries:C_1206_MTS (layer F.Cu) (tedit 5ADB9350)
    (at 151.13 80.645 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at 0 3.175 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADB9598)
    (at 114.935 80.01 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 2.3 270) (layer B.Fab))
    (fp_text value 47 (at 0 -1.905 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(P2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADB9646)
    (at 114.935 87.63 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 6.35 270) (layer B.Fab))
    (fp_text value 47 (at 0 -1.905 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADB95A0)
    (at 114.935 95.25 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 2.3 270) (layer B.Fab))
    (fp_text value 47 (at 0 -1.905 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(P4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB8EFB)
    (at 143.51 85.09 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10k (at -3.81 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB8EFE)
    (at 143.51 82.55 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10k (at -3.81 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB8EF5)
    (at 143.51 90.17 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10k (at -3.81 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB8EF7)
    (at 143.51 87.63 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10k (at -3.81 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB9103)
    (at 153.035 100.965)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -2.3) (layer F.Fab))
    (fp_text value 10k (at 3.81 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 +12V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB9315)
    (at 147.955 76.835)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -2.3) (layer F.Fab))
    (fp_text value 10k (at 3.81 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 5ADB97D4)
    (at 147.955 100.965 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -14.605 43.815 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.905 40.64 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Libraries:C_1206_MTS (layer F.Cu) (tedit 5ADB9700)
    (at 153.035 88.265 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 680pF (at -5.08 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:C_1206_MTS (layer B.Cu) (tedit 5ADB97DC)
    (at 153.035 94.615 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 47.625 6.985 180) (layer B.Fab))
    (fp_text value 1uF (at 0 -1.905 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 +12V))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 5ADB97D8)
    (at 159.385 94.615)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at -53.975 -6.985) (layer F.SilkS))
    (fp_text value 100uF (at -53.975 1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5ADB97E5)
    (at 156.21 69.215 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -11.43 -48.26 90) (layer F.SilkS))
    (fp_text value Power (at -3.81 -50.165 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADB959B)
    (at 114.935 72.39 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 2.3 270) (layer B.Fab))
    (fp_text value 47 (at 0 -1.905 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(P1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB9107)
    (at 153.035 103.505 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10k (at -3.81 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5ADB9710)
    (at 153.035 85.725 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10k (at -3.81 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:AudioTransformer-4pin (layer F.Cu) (tedit 5ADB97F0)
    (at 122.555 80.01 180)
    (fp_text reference T1 (at 17.78 2.54 180) (layer F.SilkS))
    (fp_text value TRANSFO-AUDIO (at 19.685 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDA))
    (pad 4 thru_hole circle (at -2.54 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(R5-Pad2)"))
  )
  (module Libraries:AudioTransformer-4pin (layer F.Cu) (tedit 5ADB97F3)
    (at 135.89 74.295)
    (fp_text reference T2 (at -27.94 5.715) (layer F.SilkS))
    (fp_text value TRANSFO-AUDIO (at -33.02 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(RV2-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(R6-Pad2)"))
    (pad 4 thru_hole circle (at -2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDA))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5ADB97DA)
    (at 153.035 94.615 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 46.99 4.445 180) (layer F.SilkS))
    (fp_text value TL072 (at 48.895 2.54 180) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 +12V))
    (pad 7 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 6 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 5 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 2 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 5ADB97F2)
    (at 120.015 70.485 270)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at 6.35 15.875 270) (layer F.SilkS))
    (fp_text value 1k (at 1.27 13.97 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 5ADB9656)
    (at 133.35 83.82 270)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV2 (at -1.27 24.765 270) (layer F.SilkS))
    (fp_text value 1k (at 0 28.575 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(RV2-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 5ADB963B)
    (at 120.015 90.805 270)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV3 (at 5.715 12.065 270) (layer F.SilkS))
    (fp_text value 1k (at 1.905 13.335 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(RV3-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P3-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 5ADB97EE)
    (at 133.35 104.14 270)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV4 (at -3.81 25.4 270) (layer F.SilkS))
    (fp_text value 1k (at -29.845 30.48 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(RV4-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P4-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 117.475 70.485) (layer F.SilkS))
  (gr_text 3 (at 117.475 90.805) (layer F.SilkS))
  (gr_text 100uF (at 147.955 106.045) (layer F.SilkS))
  (gr_text 100uF (at 160.655 98.425) (layer F.SilkS))
  (gr_text O (at 142.875 93.98) (layer B.Mask))
  (gr_text o (at 143.51 96.52) (layer B.Mask))
  (gr_text o (at 144.78 95.25) (layer B.Mask))
  (gr_text <>< (at 146.05 97.155) (layer B.Mask))
  (gr_text ><> (at 142.875 98.425) (layer B.Mask))
  (gr_text GND (at 158.75 71.755) (layer F.SilkS))
  (gr_text Out (at 149.86 71.755) (layer F.SilkS))
  (gr_text GND (at 146.05 71.755) (layer F.SilkS))
  (gr_text +V (at 155.575 71.755) (layer F.SilkS))
  (gr_text MixOut (at 147.955 73.66) (layer F.SilkS))
  (gr_text Power (at 157.48 73.66) (layer F.SilkS))
  (gr_text 4 (at 140.97 104.14) (layer F.SilkS))
  (gr_text 3 (at 113.03 87.63) (layer F.SilkS))
  (gr_text 2 (at 141.605 80.01) (layer F.SilkS))
  (gr_text 1 (at 113.03 72.39) (layer F.SilkS))
  (gr_text 4 (at 113.03 95.25) (layer F.SilkS))
  (gr_text 2 (at 113.03 80.01) (layer F.SilkS))
  (gr_line (start 165.1 67.31) (end 165.1 74.295) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 67.31) (end 165.1 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 74.295) (end 109.22 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 107.315) (end 165.1 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "by @SmittyHalibut" (at 152.4 74.295) (layer B.SilkS))
  (gr_text 10k (at 101.6 96.52) (layer F.SilkS))
  (gr_text "Mix Out" (at 99.695 94.615) (layer F.SilkS))
  (gr_text GND (at 100.33 100.33) (layer F.SilkS))
  (gr_text SLM-v1.2a (at 152.4 76.835) (layer B.SilkS))
  (gr_text "Speaker Level Mixer" (at 152.4 71.755) (layer B.SilkS))
  (gr_text 10k (at 97.155 78.105) (layer F.SilkS))
  (gr_text 10k (at 97.155 84.455) (layer F.SilkS))
  (gr_text 10k (at 97.155 90.805) (layer F.SilkS))
  (gr_text +12v (at 97.79 96.52) (layer F.SilkS))
  (gr_text 10k (at 104.14 95.25) (layer F.SilkS))
  (gr_text 10k (at 104.14 88.9) (layer F.SilkS))
  (gr_text 10k (at 104.14 82.55) (layer F.SilkS))
  (gr_text 10k (at 97.79 75.565) (layer F.SilkS))
  (gr_line (start 138.43 107.315) (end 109.22 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 74.295) (end 165.1 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 106.045) (end 109.22 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 74.295) (end 109.22 74.93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 74.93) (end 109.22 106.045) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 80.645) (xy 155.575 80.645) (xy 155.575 99.06) (xy 146.05 99.06) (xy 146.05 107.315)
        (xy 116.84 107.315) (xy 116.84 67.31) (xy 142.24 67.31) (xy 142.24 80.645)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.685 107.315) (xy 146.685 99.695) (xy 156.21 99.695) (xy 156.21 80.01) (xy 142.875 80.01)
        (xy 142.875 67.31) (xy 165.1 67.31) (xy 165.1 107.315)
      )
    )
  )
)
