(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 164)
    (tracks 146)
    (zones 0)
    (modules 185)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.999999 2.999999)
    (pad_drill 2.999999)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 113.665 120.015)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 TH0)
  (net 9 +5V)
  (net 10 TH1)
  (net 11 THB)
  (net 12 D6)
  (net 13 D5)
  (net 14 D4)
  (net 15 D3)
  (net 16 D2)
  (net 17 RST)
  (net 18 RxI)
  (net 19 TxO)
  (net 20 SS)
  (net 21 MOSI)
  (net 22 IO13)
  (net 23 +3V3)
  (net 24 AREF)
  (net 25 A3)
  (net 26 A4)
  (net 27 A5)
  (net 28 "Net-(J5-Pad8)")
  (net 29 "Net-(J5-Pad7)")
  (net 30 +12V)
  (net 31 MISO)
  (net 32 SCK)
  (net 33 Lim_X+)
  (net 34 Lim_Y+)
  (net 35 Lim_Z+)
  (net 36 Lim_X-)
  (net 37 Lim_Y-)
  (net 38 Lim_Z-)
  (net 39 "Net-(J4-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net AREF)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net GND)
    (add_net IO13)
    (add_net Lim_X+)
    (add_net Lim_X-)
    (add_net Lim_Y+)
    (add_net Lim_Y-)
    (add_net Lim_Z+)
    (add_net Lim_Z-)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net RST)
    (add_net RxI)
    (add_net SCK)
    (add_net SS)
    (add_net TH0)
    (add_net TH1)
    (add_net THB)
    (add_net TxO)
  )
  (net_class 12V ""
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
  )
  (net_class 5V ""
    (clearance 0.2032)
    (trace_width 0.889)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A42B)
    (at 136.892 69.723 90)
    (descr "Through hole straight socket strip, 1x17, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x17 2.54mm single row")
    (fp_text reference J5 (at 0 43.321 180) (layer F.SilkS))
    (fp_text value Conn_01x17 (at 0 43.41 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 IO13))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 AREF))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 THB))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 TH1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 TH0))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 A3))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 A4))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 A5))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J5-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 RST))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 MISO))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 SCK))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A42B)
    (at 136.892 84.963 90)
    (descr "Through hole straight socket strip, 1x17, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x17 2.54mm single row")
    (fp_text reference J4 (at 0 43.448 180) (layer F.SilkS))
    (fp_text value Conn_01x17 (at 0 43.41 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 Lim_Z-))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 Lim_Z+))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 Lim_Y-))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 Lim_Y+))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 Lim_X-))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 Lim_X+))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 D6))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 D4))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 D3))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 D2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 RxI))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 TxO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 SS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 MOSI))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90227B)
    (at 177.546 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 IO13))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902261)
    (at 172.466 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 AREF))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902253)
    (at 162.306 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 A3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90224C)
    (at 159.766 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 A4))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902246)
    (at 157.226 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 A5))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90222B)
    (at 147.066 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 RST))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902203)
    (at 141.986 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 +12V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9021F9)
    (at 139.446 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 MISO))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9021F1)
    (at 136.906 72.263)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 SCK))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90228C)
    (at 136.906 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 MOSI))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902295)
    (at 139.446 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 SS))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90229D)
    (at 141.986 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 TxO))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9022A5)
    (at 144.526 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 RxI))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9022AF)
    (at 152.146 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 D2))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9022B7)
    (at 154.686 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 D3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9022BE)
    (at 157.226 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 D4))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9022C4)
    (at 159.766 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 D5))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9022CB)
    (at 162.306 82.423)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 D6))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902086)
    (at 112.522 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 114.681)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902080)
    (at 112.522 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 112.141)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902077)
    (at 112.522 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 109.601)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902071)
    (at 112.522 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 107.061)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902069)
    (at 112.522 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 104.521)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902062)
    (at 112.522 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 101.981)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90205B)
    (at 112.522 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 99.441)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902053)
    (at 112.522 96.901)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902049)
    (at 112.522 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 94.361)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902043)
    (at 112.522 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 91.821)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90203A)
    (at 112.522 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 89.281)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902032)
    (at 112.522 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 86.741)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90202B)
    (at 112.522 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 84.201)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902024)
    (at 112.522 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 81.661)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90201A)
    (at 112.522 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 79.121)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902013)
    (at 112.522 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 76.581)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 115.062 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90200A)
    (at 112.522 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 125.222 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 122.682 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 117.602 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 120.142 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901E21)
    (at 127.762 74.041)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902152)
    (at 122.682 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +3V3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902130)
    (at 115.062 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90214D)
    (at 125.222 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +3V3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902001)
    (at 112.522 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902146)
    (at 127.762 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +3V3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90213C)
    (at 120.142 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902136)
    (at 117.602 71.501)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D901FC1)
    (at 112.522 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902116)
    (at 120.142 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D90210C)
    (at 117.602 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D902106)
    (at 115.062 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9020FE)
    (at 127.762 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +3V3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9020F7)
    (at 125.222 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +3V3))
  )
  (module myPads:Single_PTH (layer F.Cu) (tedit 5D9020F1)
    (at 122.682 68.961)
    (fp_text reference REF** (at 0 1.524) (layer F.SilkS) hide)
    (fp_text value Single_PTH (at 0 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +3V3))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5D9039BB)
    (at 113.665 120.015)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H4 (at -1.905 -3.81) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.999999 2.999999) (drill 2.999999) (layers *.Cu *.Mask)
      (clearance 1.905))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5D9039B1)
    (at 179.705 120.015)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 2.54 -3.175) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.999999 2.999999) (drill 2.999999) (layers *.Cu *.Mask)
      (clearance 1.905))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5D9039CA)
    (at 179.705 59.055)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H2 (at -3.175 -2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.999999 2.999999) (drill 2.999999) (layers *.Cu *.Mask)
      (clearance 1.905))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5D9039C3)
    (at 113.665 59.055)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 3.81 -2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.999999 2.999999) (drill 2.999999) (layers *.Cu *.Mask)
      (clearance 1.905))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 175.26 109.22 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 1.016 2.032) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 Lim_Z-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 159.512 109.22 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 1.016 2.032) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 Lim_Y-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 143.764 109.22 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 1.016 2.032) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 Lim_X-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 162.306 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 146.558 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.81 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 175.26 92.964 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 1.524 2.032) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 Lim_Z+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 159.512 92.964 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 1.524 2.032) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 Lim_Y+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 143.764 92.964 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 1.524 2.032) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 Lim_X+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 162.306 103.124 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 146.558 103.124 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.81 103.124 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 59FF03AB)
    (at 135.255 60.706 180)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J12 (at 9.144 0) (layer F.SilkS))
    (fp_text value "Power In" (at 2.54 5.08) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 30 +12V))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 172.72 118.11 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J11 (at 6.858 -3.55) (layer F.SilkS))
    (fp_text value Lim_Z- (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 156.972 118.11 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J10 (at 6.858 -3.556) (layer F.SilkS))
    (fp_text value Lim_Y- (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 141.478 118.11 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J9 (at 7.366 -3.55) (layer F.SilkS))
    (fp_text value Lim_X- (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 172.72 101.854 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J8 (at 7.366 -3.55) (layer F.SilkS))
    (fp_text value Lim_Z+ (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 156.972 101.854 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J7 (at 7.366 -3.55) (layer F.SilkS))
    (fp_text value Lim_Y+ (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 141.478 101.854 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J6 (at 7.366 -3.55) (layer F.SilkS))
    (fp_text value Lim_X+ (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 167.513 59.69)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J3 (at -2.286 4.572) (layer F.SilkS))
    (fp_text value THB (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 THB))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 155.829 59.69)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J2 (at -2.286 4.572) (layer F.SilkS))
    (fp_text value TH1 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 TH1))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 144.145 59.69)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J1 (at -2.286 4.572) (layer F.SilkS))
    (fp_text value TH0 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 TH0))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 167.64 112.522)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C6 (at 7.112 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 151.892 112.522)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C5 (at 7.112 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 136.525 112.522)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C4 (at 7.112 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 167.64 96.266)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C3 (at 7.112 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 152.019 96.266)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C2 (at 7.112 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 136.398 96.266)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C1 (at 7.112 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text D12 (at 177.546 87.1855) (layer F.SilkS))
  (gr_text D11 (at 175.006 87.1855) (layer F.SilkS))
  (gr_text D10 (at 172.466 87.1855) (layer F.SilkS))
  (gr_text D9 (at 169.926 87.1855) (layer F.SilkS))
  (gr_text D8 (at 167.386 87.1855) (layer F.SilkS))
  (gr_text D7 (at 164.846 87.1855) (layer F.SilkS))
  (gr_text D12 (at 177.546 86.741) (layer B.SilkS))
  (gr_text D11 (at 175.006 86.741) (layer B.SilkS))
  (gr_text D10 (at 172.466 86.741) (layer B.SilkS))
  (gr_text D9 (at 169.926 86.741) (layer B.SilkS))
  (gr_text D8 (at 167.386 86.741) (layer B.SilkS))
  (gr_text D7 (at 164.846 86.741) (layer B.SilkS))
  (gr_text A2 (at 164.7825 67.6275) (layer F.SilkS))
  (gr_text AREF (at 172.466 67.6275) (layer F.SilkS))
  (gr_text D13 (at 177.546 67.6275) (layer F.SilkS))
  (gr_text A4 (at 159.766 67.6275) (layer F.SilkS))
  (gr_text RST (at 147.066 67.6275) (layer F.SilkS))
  (gr_text A3 (at 162.306 67.6275) (layer F.SilkS))
  (gr_text A5 (at 157.226 67.6275) (layer F.SilkS))
  (gr_text GND (at 144.526 67.6275) (layer F.SilkS))
  (gr_text A1 (at 167.386 67.6275) (layer F.SilkS))
  (gr_text A0 (at 169.926 67.6275) (layer F.SilkS))
  (gr_text 3.3V (at 175.006 67.6275) (layer F.SilkS))
  (gr_text 5V (at 149.606 67.6275) (layer F.SilkS))
  (gr_text MISO (at 139.446 67.6275) (layer F.SilkS))
  (gr_text SCK (at 136.906 67.6275) (layer F.SilkS))
  (gr_text 12V (at 141.986 67.6275) (layer F.SilkS))
  (gr_text D2 (at 152.146 87.1982) (layer F.SilkS))
  (gr_text D3 (at 154.686 87.1982) (layer F.SilkS))
  (gr_text D5 (at 159.766 87.1855) (layer F.SilkS))
  (gr_text RxI (at 144.526 87.1982) (layer F.SilkS))
  (gr_text TxO (at 141.986 87.1982) (layer F.SilkS))
  (gr_text MOSI (at 136.906 87.1982) (layer F.SilkS))
  (gr_text D4 (at 157.226 87.1982) (layer F.SilkS))
  (gr_text D6 (at 162.306 87.1855) (layer F.SilkS))
  (gr_text SS (at 139.446 87.1982) (layer F.SilkS))
  (gr_text GND (at 149.606 87.1982) (layer F.SilkS))
  (gr_text "HW v0.1" (at 120.523 121.666) (layer F.SilkS))
  (gr_text GND (at 149.606 86.741) (layer B.SilkS))
  (gr_text GND (at 144.526 68.072) (layer B.SilkS))
  (gr_text 5V (at 149.606 68.072) (layer B.SilkS))
  (gr_text 3.3V (at 175.006 68.072) (layer B.SilkS))
  (gr_text A0 (at 169.926 68.072) (layer B.SilkS))
  (gr_text A1 (at 167.386 68.072) (layer B.SilkS))
  (gr_text A2 (at 164.7825 68.072) (layer B.SilkS))
  (gr_text "Proto Area" (at 122.555 117.094) (layer F.SilkS))
  (gr_text "Arduino Micro Atmega 32U4" (at 157.353 77.216) (layer F.SilkS))
  (gr_text USB (at 177.165 77.47 270) (layer F.SilkS))
  (gr_text 3.3V (at 124.46 66.04) (layer B.SilkS))
  (gr_text 5V (at 117.475 66.167) (layer B.SilkS))
  (gr_text G (at 112.522 66.167) (layer B.SilkS))
  (gr_text MOSI (at 136.906 86.741) (layer B.SilkS))
  (gr_text SS (at 139.446 86.741) (layer B.SilkS))
  (gr_text TxO (at 141.986 86.741) (layer B.SilkS))
  (gr_text RxI (at 144.526 86.741) (layer B.SilkS))
  (gr_text D2 (at 152.146 86.741) (layer B.SilkS))
  (gr_text D3 (at 154.686 86.741) (layer B.SilkS))
  (gr_text D4 (at 157.226 86.741) (layer B.SilkS))
  (gr_text D5 (at 159.766 86.741) (layer B.SilkS))
  (gr_text D6 (at 162.306 86.741) (layer B.SilkS))
  (gr_text D13 (at 177.546 68.072) (layer B.SilkS))
  (gr_text AREF (at 172.466 68.072) (layer B.SilkS))
  (gr_text A3 (at 162.306 68.072) (layer B.SilkS))
  (gr_text A4 (at 159.766 68.072) (layer B.SilkS))
  (gr_text A5 (at 157.226 68.072) (layer B.SilkS))
  (gr_text RST (at 147.066 68.072) (layer B.SilkS))
  (gr_text 12V (at 141.986 68.072) (layer B.SilkS))
  (gr_text MISO (at 139.446 68.072) (layer B.SilkS))
  (gr_text SCK (at 136.906 68.072) (layer B.SilkS))
  (gr_text 3.3V (at 124.46 66.04) (layer F.SilkS))
  (gr_text 5V (at 117.475 66.167) (layer F.SilkS))
  (gr_text G (at 112.522 66.167) (layer F.SilkS))
  (gr_text GND (at 130.175 65.786) (layer F.SilkS))
  (gr_text +12V (at 135.255 65.786) (layer F.SilkS))
  (gr_text 5V (at 172.72 120.015) (layer B.SilkS))
  (gr_text S (at 170.18 120.015) (layer B.SilkS))
  (gr_text GND (at 167.64 120.015) (layer B.SilkS))
  (gr_text GND (at 151.892 120.015) (layer B.SilkS))
  (gr_text 5V (at 156.972 120.015) (layer B.SilkS))
  (gr_text S (at 154.432 120.015) (layer B.SilkS))
  (gr_text S (at 138.938 120.015) (layer B.SilkS))
  (gr_text GND (at 136.398 120.015) (layer B.SilkS))
  (gr_text 5V (at 141.478 120.015) (layer B.SilkS))
  (gr_text GND (at 136.398 103.759) (layer B.SilkS))
  (gr_text S (at 138.938 103.759) (layer B.SilkS))
  (gr_text 5V (at 141.478 103.759) (layer B.SilkS))
  (gr_text 5V (at 156.972 103.759) (layer B.SilkS))
  (gr_text GND (at 151.892 103.759) (layer B.SilkS))
  (gr_text S (at 154.432 103.759) (layer B.SilkS))
  (gr_text GND (at 167.64 103.759) (layer B.SilkS))
  (gr_text 5V (at 172.72 103.759) (layer B.SilkS))
  (gr_text S (at 170.18 103.759) (layer B.SilkS))
  (gr_text GND (at 172.593 61.595) (layer B.SilkS))
  (gr_text 5V (at 167.513 61.595) (layer B.SilkS))
  (gr_text S (at 170.053 61.595) (layer B.SilkS))
  (gr_text S (at 158.369 61.595) (layer B.SilkS))
  (gr_text GND (at 160.909 61.595) (layer B.SilkS))
  (gr_text 5V (at 155.829 61.595) (layer B.SilkS))
  (gr_text GND (at 149.225 61.595) (layer B.SilkS))
  (gr_text S (at 146.685 61.595) (layer B.SilkS))
  (gr_text 5V (at 144.145 61.595) (layer B.SilkS))
  (gr_text A2 (at 146.685 64.516) (layer F.SilkS))
  (gr_text A1 (at 158.369 64.516) (layer F.SilkS))
  (gr_text A0 (at 170.053 64.516) (layer F.SilkS))
  (gr_text D11 (at 170.307 105.537) (layer F.SilkS))
  (gr_text D9 (at 154.559 105.537) (layer F.SilkS))
  (gr_text D7 (at 138.938 105.537) (layer F.SilkS))
  (gr_text D12 (at 170.307 121.793) (layer F.SilkS))
  (gr_text D10 (at 154.559 121.793) (layer F.SilkS))
  (gr_text D8 (at 139.065 121.793) (layer F.SilkS))
  (gr_arc (start 180.34 120.65) (end 180.34 123.19) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.03 120.65) (end 110.49 120.65) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.03 58.42) (end 113.03 55.88) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 180.34 58.42) (end 182.88 58.42) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.03 55.88) (end 180.34 55.88) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 120.65) (end 110.49 58.42) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.34 123.19) (end 113.03 123.19) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.88 58.42) (end 182.88 120.65) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.889) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 110.49 55.88) (xy 182.88 55.88) (xy 182.88 123.19) (xy 110.49 123.19)
      )
    )
  )
  (zone (net 9) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.889) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 110.49 55.88) (xy 182.88 55.88) (xy 182.88 123.19) (xy 110.49 123.19)
      )
    )
  )
  (zone (net 23) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.889) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 121.412 67.366922) (xy 129.413 67.366922) (xy 129.413 72.891422) (xy 121.412 72.891422)
      )
    )
  )
  (zone (net 23) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.889) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 121.412 67.366922) (xy 129.413 67.366922) (xy 129.413 72.891422) (xy 121.412 72.891422)
      )
    )
  )
)
