(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 31)
    (no_connects 0)
    (area 135.49412 62.144 165.053334 96.631)
    (thickness 1.6)
    (drawings 13)
    (tracks 127)
    (zones 0)
    (modules 15)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 149.86 82.296)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 PB5)
  (net 5 "Net-(IC1-Pad2)")
  (net 6 "Net-(IC1-Pad3)")
  (net 7 PB0)
  (net 8 PB1)
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(M0-Pad1)")
  (net 11 "Net-(M1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(M0-Pad1)")
    (add_net "Net-(M1-Pad1)")
    (add_net PB0)
    (add_net PB1)
    (add_net PB5)
  )
  (net_class Large ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Medium ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer B.Cu) (tedit 586B3F77)
    (at 156.21 73.406 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 2.5 360) (layer B.SilkS))
    (fp_text value 10uf (at 1.25 -2.5 270) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 586B3ECA)
    (at 149.86 67.056)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value "Red LED" (at 1.524 -3.937) (layer F.Fab) hide)
    (fp_text user K (at -1.905 1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 586AB911)
    (at 147.32 79.756)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 3.81 10.16) (layer F.SilkS) hide)
    (fp_text value ATTINY85-P (at 0 -3.72) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 PB5))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PB0))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 586403B1)
    (at 143.51 79.756 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference ISP1 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 PB0))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 PB5))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 586B3F1F)
    (at 160.02 84.836)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference M0 (at -2.54 -1.905) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(M0-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 586B3F16)
    (at 140.97 84.836)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference M1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(M1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 586404B8)
    (at 152.4 92.456 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1.27 -2.286 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 586B3F6C)
    (at 147.32 69.596 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference Q1 (at 1.27 3.175 180) (layer F.SilkS))
    (fp_text value Photo_NPN (at 1.3 -2.9 180) (layer F.Fab) hide)
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 586B3F68)
    (at 154.94 69.596)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference Q2 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value Photo_NPN (at 1.3 -2.9) (layer F.Fab) hide)
    (fp_text user K (at -1.69 1.74) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 586B3F5C)
    (at 151.13 87.376)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.54) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 PB0))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(M0-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 586B3F57)
    (at 151.13 82.296 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 2.54 0 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 PB1))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(M1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 586B3EE4)
    (at 151.13 72.136 90)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R1 (at 0.635 1.27 180) (layer F.SilkS))
    (fp_text value 330 (at 0 4.50088 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.49936 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole circle (at 2.5019 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 586B3ED4)
    (at 140.97 69.596 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R2 (at 0.635 1.27 360) (layer F.SilkS))
    (fp_text value 10k (at 0 4.50088 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 586B3EB1)
    (at 160.02 78.486 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R3 (at 0.635 1.905 360) (layer F.SilkS))
    (fp_text value 10k (at 0 4.50088 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 586B3EEB)
    (at 160.02 69.596 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R4 (at 0.635 -1.27 360) (layer F.SilkS))
    (fp_text value 10K (at 0 4.50088 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 PB5))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3V3))
  )
  (gr_line (start 138.43 64.516) (end 162.56 64.516) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 89.916) (end 138.43 64.516) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 89.916) (end 138.43 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 91.186) (end 144.78 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 91.186) (end 146.05 91.186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 92.456) (end 147.32 91.186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 94.996) (end 147.32 92.456) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 94.996) (end 147.32 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 91.186) (end 154.94 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 91.186) (end 154.94 91.186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 89.916) (end 156.21 91.186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 89.916) (end 157.48 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 64.516) (end 162.56 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
)
