<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="66.02" y2="0" width="0" layer="20"/>
<wire x1="66.02" y1="0" x2="66.04" y2="36.83" width="0" layer="20"/>
<wire x1="66.04" y1="36.83" x2="10.16" y2="36.83" width="0" layer="20"/>
<wire x1="10.16" y1="36.83" x2="10.16" y2="17.78" width="0" layer="20"/>
<wire x1="10.16" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<text>3 = Bank 0 (00000-7FFFF)
2 = Bank 1 (80000-FFFFF)
1 = Bank 2 (100000-17FFFF)
0 = Bank 3 (180000-1FFFFF)</text>
<text>A4000 KickSwitch for 27C160
(C) Abweichler 2018</text>
<text>A4000 KickSwitch for 27C160
(C) Abweichler 2018</text>
<text>Turn Amiga off
before switching!</text>
<text>Turn Amiga off
before switching!</text>
</plain>
<libraries>
<library name="Switches_rev16a">
<description>&lt;BR&gt;Wurth Elektronik - Switches&lt;br&gt;&lt;Hr&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="428527320911">
<description>WS-RAT-10x10 mm washable THT Rotary Switch,6 pins,10 positions</description>
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
</description>
<packages>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="Amiga_xxl">
<packages>
<package name="DIL42-WIDE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW1" library="Switches_rev16a" package="428527320911" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="Amiga_xxl" package="DIL42-WIDE" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="M1206" value="">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="Amiga_xxl" package="DIL42-WIDE" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="M1206" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="22"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="42"/>
<contactref element="R2" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="IC2" pad="42"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="SW1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="12"/>
<contactref element="IC1" pad="31"/>
<contactref element="SW1" pad="C1"/>
<contactref element="SW1" pad="C2"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC2" pad="31"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
