(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 0.8)
    (drawings 17)
    (tracks 41)
    (zones 0)
    (modules 2)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x3ffff_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U0-Pad20)")
  (net 3 "Net-(U0-Pad5)")
  (net 4 "Net-(C1-Pad2)")
  (net 5 "Net-(M1-Pad2)")
  (net 6 "Net-(M1-Pad3)")
  (net 7 "Net-(M1-Pad4)")
  (net 8 "Net-(M1-Pad5)")
  (net 9 "Net-(M1-Pad6)")
  (net 10 "Net-(M1-Pad7)")
  (net 11 "Net-(M1-Pad8)")
  (net 12 "Net-(M1-Pad9)")
  (net 13 "Net-(M1-Pad11)")
  (net 14 "Net-(M1-Pad12)")
  (net 15 "Net-(M1-Pad13)")
  (net 16 "Net-(M1-Pad15)")
  (net 17 "Net-(M1-Pad16)")
  (net 18 "Net-(M1-Pad17)")
  (net 19 "Net-(M1-Pad18)")
  (net 20 "Net-(M1-Pad19)")
  (net 21 "Net-(M1-Pad21)")
  (net 22 "Net-(M1-Pad22)")
  (net 23 "Net-(M1-Pad23)")
  (net 24 "Net-(M1-Pad24)")
  (net 25 "Net-(M1-Pad25)")
  (net 26 "Net-(M1-Pad27)")
  (net 27 "Net-(U0-Pad19)")
  (net 28 "Net-(U0-Pad21)")
  (net 29 "Net-(U0-Pad30)")
  (net 30 "Net-(M1-Pad10)")
  (net 31 "Net-(U0-Pad31)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(M1-Pad10)")
    (add_net "Net-(M1-Pad11)")
    (add_net "Net-(M1-Pad12)")
    (add_net "Net-(M1-Pad13)")
    (add_net "Net-(M1-Pad15)")
    (add_net "Net-(M1-Pad16)")
    (add_net "Net-(M1-Pad17)")
    (add_net "Net-(M1-Pad18)")
    (add_net "Net-(M1-Pad19)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad21)")
    (add_net "Net-(M1-Pad22)")
    (add_net "Net-(M1-Pad23)")
    (add_net "Net-(M1-Pad24)")
    (add_net "Net-(M1-Pad25)")
    (add_net "Net-(M1-Pad27)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M1-Pad5)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(M1-Pad7)")
    (add_net "Net-(M1-Pad8)")
    (add_net "Net-(M1-Pad9)")
    (add_net "Net-(U0-Pad19)")
    (add_net "Net-(U0-Pad20)")
    (add_net "Net-(U0-Pad21)")
    (add_net "Net-(U0-Pad30)")
    (add_net "Net-(U0-Pad31)")
    (add_net "Net-(U0-Pad5)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal (layer F.Cu) (tedit 5E28CE3A)
    (at 123.04014 115.12804 90)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (fp_text reference CP2102 (at 1.397 -2.76352 90) (layer F.SilkS))
    (fp_text value PinHeader_1x05_P2.54mm_Horizontal (at 4.385 12.43 90) (layer F.Fab))
    (fp_text user %R (at 2.77 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(M1-Pad16)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(M1-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(M1-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:GBBus (layer F.Cu) (tedit 5E28CE4E)
    (at 118.46 123.42)
    (descr "Connector Pads for Gameboy Cartridges")
    (fp_text reference U0 (at 23.12 -2.565) (layer F.SilkS) hide)
    (fp_text value CartBus (at 24.49 -7.525) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.7 3 180) (size 1.4 6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad2)") (solder_mask_margin 0.0508))
    (pad 2 smd rect (at 2.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 5.4 3 180) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(M1-Pad22)") (solder_mask_margin 0.0508))
    (pad 5 smd rect (at 6.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U0-Pad5)") (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 8.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(M1-Pad10)") (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 9.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M1-Pad9)") (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 11.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(M1-Pad8)") (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 12.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(M1-Pad7)") (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 14.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M1-Pad6)") (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 15.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-Pad5)") (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 17.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad4)") (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 18.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-Pad3)") (solder_mask_margin 0.0508))
    (pad 14 smd rect (at 20.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(M1-Pad25)") (solder_mask_margin 0.0508))
    (pad 15 smd rect (at 21.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(M1-Pad24)") (solder_mask_margin 0.0508))
    (pad 16 smd rect (at 23.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(M1-Pad21)") (solder_mask_margin 0.0508))
    (pad 17 smd rect (at 24.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(M1-Pad23)") (solder_mask_margin 0.0508))
    (pad 18 smd rect (at 26.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(M1-Pad2)") (solder_mask_margin 0.0508))
    (pad 19 smd rect (at 27.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U0-Pad19)") (solder_mask_margin 0.0508))
    (pad 20 smd rect (at 29.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U0-Pad20)") (solder_mask_margin 0.0508))
    (pad 21 smd rect (at 30.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U0-Pad21)") (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 3.9 3 180) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(M1-Pad27)") (solder_mask_margin 0.0508))
    (pad 22 smd rect (at 32.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M1-Pad11)") (solder_mask_margin 0.0508))
    (pad 23 smd rect (at 33.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M1-Pad12)") (solder_mask_margin 0.0508))
    (pad 24 smd rect (at 35.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(M1-Pad13)") (solder_mask_margin 0.0508))
    (pad 25 smd rect (at 36.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(M1-Pad15)") (solder_mask_margin 0.0508))
    (pad 26 smd rect (at 38.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(M1-Pad16)") (solder_mask_margin 0.0508))
    (pad 27 smd rect (at 39.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(M1-Pad17)") (solder_mask_margin 0.0508))
    (pad 28 smd rect (at 41.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(M1-Pad18)") (solder_mask_margin 0.0508))
    (pad 29 smd rect (at 42.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(M1-Pad19)") (solder_mask_margin 0.0508))
    (pad 30 smd rect (at 44.4 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U0-Pad30)") (solder_mask_margin 0.0508))
    (pad 31 smd rect (at 45.9 3) (size 1 6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U0-Pad31)") (solder_mask_margin 0.0508))
    (pad 32 smd rect (at 47.6 3 180) (size 1.4 6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (gr_text 3V3 (at 133.20014 117.8337 90) (layer F.SilkS))
  (gr_text TXD (at 130.66014 117.8337 90) (layer F.SilkS))
  (gr_text RXD (at 128.12014 117.8337 90) (layer F.SilkS))
  (gr_text GND (at 125.58014 117.8337 90) (layer F.SilkS))
  (gr_text +5V (at 123.04014 118.0337 90) (layer F.SilkS))
  (gr_line (start 168.17 121.402) (end 168.17 110.3884) (layer Edge.Cuts) (width 0.0254))
  (gr_circle (center 142.62 114.652) (end 146.12 114.652) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 117.07 121.402) (end 117.82 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 117.07 110.3884) (end 117.07 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 119.36 130.002) (end 165.99 130.002) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 168.17 110.3884) (end 117.07 110.3884) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 167.42 128.362) (end 167.42 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 117.82 121.402) (end 117.82 128.442) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 167.42 121.402) (end 168.17 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 165.83913 128.427) (end 167.42 128.362) (angle 86.88278645) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 119.345 128.47668) (end 119.36 130.002) (angle 91.86616649) (layer Edge.Cuts) (width 0.0254))
)
