(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 40)
    (zones 0)
    (modules 5)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad3)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad3)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J3-Pad1)")
  (net 9 "Net-(J4-Pad3)")
  (net 10 G)
  (net 11 B)
  (net 12 C)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net B)
    (add_net C)
    (add_net G)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad3)")
  )
  (module LTC2644IMS-L8_PBF:SOP65P490X110-12N_LTC2644IMS-L8#PBF (layer F.Cu) (tedit 5F88A167)
    (at 109.6 59.365)
    (fp_text reference U1 (at -0.968 -2.8064) (layer F.SilkS))
    (fp_text value LTC2644IMS-L8#PBF (at 11.224 2.8064) (layer F.Fab))
    (pad 12 smd rect (at 2.16 -1.625) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 10 G))
    (pad 11 smd rect (at 2.16 -0.975) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad3)"))
    (pad 10 smd rect (at 2.16 -0.325) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 9 smd rect (at 2.16 0.325) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 8 smd rect (at 2.16 0.975) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 12 C))
    (pad 7 smd rect (at 2.16 1.625) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 11 B))
    (pad 6 smd rect (at -2.16 1.625) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 10 G))
    (pad 5 smd rect (at -2.16 0.975) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -2.16 0.325) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -2.16 -0.325) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -2.16 -0.975) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 1 smd rect (at -2.16 -1.625) (size 1.45 0.48) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad3)"))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm (layer F.Cu) (tedit 5A4528F9)
    (at 127 59.69 270)
    (fp_text reference J4 (at 2.85 -2.28 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.71 2.7 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 B))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 C))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm (layer F.Cu) (tedit 5A4528F9)
    (at 92.71 57.15 90)
    (fp_text reference J3 (at 2.85 -2.28 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.71 2.7 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad1)"))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm (layer F.Cu) (tedit 5A4528F9)
    (at 127 57.15 90)
    (fp_text reference J2 (at 2.286 2.032 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.71 2.7 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm (layer F.Cu) (tedit 5A4528F9)
    (at 92.71 59.69 270)
    (fp_text reference J1 (at 2.85 2.286 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.71 2.7 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 G))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (gr_text "Breakout_LTC2644 " (at 109.22 67.056) (layer F.SilkS))
  (gr_text _PD (at 120.904 61.976) (layer F.SilkS))
  (gr_text IN_B (at 120.904 59.436) (layer F.SilkS))
  (gr_text IN_A (at 120.904 56.388) (layer F.SilkS))
  (gr_text REF (at 121.412 53.848) (layer F.SilkS))
  (gr_text REFSEL (at 121.412 51.308) (layer F.SilkS))
  (gr_text GND (at 99.568 65.024) (layer F.SilkS))
  (gr_text IOVcc (at 99.568 61.468) (layer F.SilkS))
  (gr_text IDLSEL (at 99.06 59.436) (layer F.SilkS))
  (gr_text VoutB (at 99.06 56.388) (layer F.SilkS))
  (gr_text VoutA (at 99.06 53.848) (layer F.SilkS))
  (gr_text Vcc (at 98.044 51.308) (layer F.SilkS))
  (gr_line (start 88.9 76.2) (end 88.9 46.99) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.81 76.2) (end 88.9 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.81 46.99) (end 130.81 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 46.99) (end 130.81 46.99) (layer Edge.Cuts) (width 0.05))
  (zone (net 10) (net_name G) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 72.136) (xy 89.916 72.136) (xy 89.916 48.768) (xy 129.032 48.768)
      )
    )
  )
)
