(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 28)
    (no_connects 0)
    (area 144.704999 72.314999 184.225001 135.965001)
    (thickness 1.6)
    (drawings 14)
    (tracks 102)
    (zones 0)
    (modules 6)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (user_trace_width 3.81)
    (user_trace_width 5.08)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(RV1-Pad2)")
  (net 4 "Net-(RV1-Pad1)")
  (net 5 "Net-(U1-Pad9)")
  (net 6 "Net-(U1-Pad10)")
  (net 7 "Net-(U1-Pad11)")
  (net 8 "Net-(U1-Pad12)")
  (net 9 "Net-(U1-Pad13)")
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J3-Pad6)")
  (net 13 "Net-(J2-Pad8)")
  (net 14 "Net-(J3-Pad5)")
  (net 15 "Net-(J2-Pad3)")
  (net 16 "Net-(J2-Pad5)")
  (net 17 "Net-(J3-Pad8)")
  (net 18 "Net-(J3-Pad7)")
  (net 19 "Net-(J3-Pad4)")
  (net 20 "Net-(J3-Pad3)")
  (net 21 "Net-(J2-Pad4)")
  (net 22 "Net-(J2-Pad6)")
  (net 23 "Net-(J2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad9)")
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5934AE29)
    (at 158.115 85.725)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -8.45 5.75 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at -6.2 -5.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -6 0) (size 4.5 4.5) (drill oval 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -3 4.7) (size 4.5 4.5) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Potentiometers:Potentiometer_Trimmer_VishaySpectrol_Econtrim-Type36X (layer F.Cu) (tedit 594A9ADC)
    (at 177.165 133.35)
    (descr "Potentiometer, Trimmer, Spectrol Type 36X, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer Trimmer Spectrol Type 36X Econtrim Rev A 02 Aug 2010 ")
    (fp_text reference RV1 (at 4.445 -5.715) (layer F.SilkS))
    (fp_text value POT (at 0 -4.445) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(RV1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 5931C4C5)
    (at 147.32 76.2 90)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference U1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value ILI9341_LCD_Breakout (at 2.54 16.51 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad8)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad5)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(RV1-Pad2)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 -0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module wemos_d1_mini:D1_mini_board (layer F.Cu) (tedit 5931C4D1)
    (at 164.465 111.125 180)
    (fp_text reference U2 (at 1.27 18.81 180) (layer F.SilkS))
    (fp_text value WeMos_mini (at 0 1.27 180) (layer F.Fab))
    (fp_text user WeMos (at 0 -15.24 180) (layer F.SilkS))
    (pad 8 thru_hole circle (at -11.43 -10.16 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J3-Pad8)"))
    (pad 7 thru_hole circle (at -11.43 -7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J3-Pad7)"))
    (pad 6 thru_hole circle (at -11.43 -5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at -11.43 -2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J3-Pad5)"))
    (pad 4 thru_hole circle (at -11.43 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at -11.43 2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at -11.43 5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -11.43 7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad1)"))
    (pad 16 thru_hole circle (at 11.43 7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad1)"))
    (pad 15 thru_hole circle (at 11.43 5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad2)"))
    (pad 14 thru_hole circle (at 11.43 2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad3)"))
    (pad 13 thru_hole circle (at 11.43 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J2-Pad4)"))
    (pad 12 thru_hole circle (at 11.43 -2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J2-Pad5)"))
    (pad 11 thru_hole circle (at 11.43 -5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J2-Pad6)"))
    (pad 10 thru_hole circle (at 11.43 -7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J2-Pad7)"))
    (pad 9 thru_hole circle (at 11.43 -10.16 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J2-Pad8)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 594A9C65)
    (at 148.59 103.505)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 1.905 20.955) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 594A9C71)
    (at 179.705 103.505)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X08 (at -1.27 20.955) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text LED (at 165.1 79.375 90) (layer F.SilkS))
  (gr_text SCK (at 162.56 78.74 90) (layer F.SilkS))
  (gr_text MOSI (at 160.02 78.74 90) (layer F.SilkS))
  (gr_text D/C (at 157.48 78.74 90) (layer F.SilkS))
  (gr_text RST (at 154.94 78.74 90) (layer F.SilkS))
  (gr_text CS (at 152.4 78.74 90) (layer F.SilkS))
  (gr_text "GND\n" (at 149.86 78.74 90) (layer F.SilkS))
  (gr_text "3.3V\n" (at 147.32 78.74 90) (layer F.SilkS))
  (gr_text "WEMOS-ILI9341 ADAPTER BOARD REV2" (at 160.02 133.985) (layer F.SilkS))
  (gr_text "shitty board design" (at 156.845 131.445) (layer F.SilkS))
  (gr_line (start 144.78 135.89) (end 184.15 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.15 72.39) (end 144.78 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.15 135.89) (end 184.15 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 72.39) (end 144.78 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
)
