(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 1373)
    (zones 0)
    (modules 102)
    (nets 93)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.01)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.001 0.001)
    (mod_text_width 0.00025)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 110.001429 39.998355)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad29)")
  (net 2 "Net-(U1-Pad28)")
  (net 3 "Net-(U1-Pad23)")
  (net 4 "Net-(U1-Pad22)")
  (net 5 "Net-(J2-Pad16)")
  (net 6 "Net-(J2-Pad14)")
  (net 7 "Net-(J2-Pad12)")
  (net 8 "Net-(J2-Pad11)")
  (net 9 "Net-(J2-Pad10)")
  (net 10 "Net-(J2-Pad9)")
  (net 11 "Net-(J2-Pad8)")
  (net 12 "Net-(J2-Pad7)")
  (net 13 "Net-(J2-Pad3)")
  (net 14 "Net-(J2-Pad2)")
  (net 15 "Net-(J2-Pad1)")
  (net 16 "Net-(J3-Pad12)")
  (net 17 "Net-(J3-Pad11)")
  (net 18 "Net-(J3-Pad9)")
  (net 19 "Net-(J3-Pad8)")
  (net 20 "Net-(J3-Pad7)")
  (net 21 "Net-(J3-Pad4)")
  (net 22 "Net-(J3-Pad3)")
  (net 23 UA)
  (net 24 UB)
  (net 25 UC)
  (net 26 "Net-(U2-Pad4)")
  (net 27 "Net-(C1-Pad1)")
  (net 28 "Net-(C2-Pad1)")
  (net 29 "Net-(D4-Pad2)")
  (net 30 /V9203/IAP)
  (net 31 /V9203/IAN)
  (net 32 "Net-(C14-Pad2)")
  (net 33 GND)
  (net 34 /V9203/IAP_IN)
  (net 35 /V9203/IAN_IN)
  (net 36 /V9203/IBN_IN)
  (net 37 /V9203/IBP_IN)
  (net 38 /V9203/ICN_IN)
  (net 39 /V9203/ICP_IN)
  (net 40 /V9203/INN_IN)
  (net 41 /V9203/INP_IN)
  (net 42 "Net-(JP1-Pad1)")
  (net 43 "Net-(C21-Pad1)")
  (net 44 "Net-(C20-Pad2)")
  (net 45 /V9203/UAP)
  (net 46 /V9203/UBP)
  (net 47 /V9203/UCP)
  (net 48 MISO)
  (net 49 MOSI)
  (net 50 SCK)
  (net 51 +3V3)
  (net 52 USB)
  (net 53 SCL)
  (net 54 SDA)
  (net 55 /V9203/INN)
  (net 56 /V9203/ICP)
  (net 57 /V9203/ICN)
  (net 58 /V9203/IBN)
  (net 59 /V9203/INP)
  (net 60 /V9203/IBP)
  (net 61 CS)
  (net 62 "Net-(J6-Pad1)")
  (net 63 "Net-(C22-Pad2)")
  (net 64 "Net-(D6-Pad2)")
  (net 65 "Net-(D7-Pad2)")
  (net 66 "Net-(R27-Pad2)")
  (net 67 "Net-(R28-Pad2)")
  (net 68 "Net-(J8-Pad2)")
  (net 69 "Net-(J7-Pad2)")
  (net 70 "Net-(J6-Pad5)")
  (net 71 "Net-(J6-Pad4)")
  (net 72 "Net-(J6-Pad3)")
  (net 73 "Net-(J6-Pad2)")
  (net 74 /V9203/V_MISO)
  (net 75 /V9203/V_MOSI)
  (net 76 /V9203/V_CS)
  (net 77 /V9203/V_CLK)
  (net 78 "Net-(R37-Pad1)")
  (net 79 "Net-(R36-Pad1)")
  (net 80 "Net-(J6-Pad8)")
  (net 81 "Net-(J6-Pad7)")
  (net 82 "Net-(R35-Pad1)")
  (net 83 "Net-(R34-Pad1)")
  (net 84 "Net-(R33-Pad1)")
  (net 85 "Net-(R38-Pad1)")
  (net 86 "Net-(J6-Pad6)")
  (net 87 /V9203/DS)
  (net 88 "Net-(J10-Pad2)")
  (net 89 "Net-(J11-Pad1)")
  (net 90 "Net-(J11-Pad3)")
  (net 91 PM0)
  (net 92 PM1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /V9203/DS)
    (add_net /V9203/IAN)
    (add_net /V9203/IAN_IN)
    (add_net /V9203/IAP)
    (add_net /V9203/IAP_IN)
    (add_net /V9203/IBN)
    (add_net /V9203/IBN_IN)
    (add_net /V9203/IBP)
    (add_net /V9203/IBP_IN)
    (add_net /V9203/ICN)
    (add_net /V9203/ICN_IN)
    (add_net /V9203/ICP)
    (add_net /V9203/ICP_IN)
    (add_net /V9203/INN)
    (add_net /V9203/INN_IN)
    (add_net /V9203/INP)
    (add_net /V9203/INP_IN)
    (add_net /V9203/UAP)
    (add_net /V9203/UBP)
    (add_net /V9203/UCP)
    (add_net /V9203/V_CLK)
    (add_net /V9203/V_CS)
    (add_net /V9203/V_MISO)
    (add_net /V9203/V_MOSI)
    (add_net CS)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J11-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(J6-Pad7)")
    (add_net "Net-(J6-Pad8)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R33-Pad1)")
    (add_net "Net-(R34-Pad1)")
    (add_net "Net-(R35-Pad1)")
    (add_net "Net-(R36-Pad1)")
    (add_net "Net-(R37-Pad1)")
    (add_net "Net-(R38-Pad1)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U2-Pad4)")
    (add_net PM0)
    (add_net PM1)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net UA)
    (add_net UB)
    (add_net UC)
    (add_net USB)
  )
  (module Connector_Molex:Molex_Nano-Fit_105314-xx08_2x04_P2.50mm_Horizontal (layer F.Cu) (tedit 5B782416)
    (at 146.831 51.4284)
    (descr "Molex Nano-Fit Power Connectors, 105314-xx08, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053141208_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit top entry")
    (fp_text reference J1 (at 8.65 -2.92) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 8.65 10.42) (layer F.Fab))
    (fp_text user %R (at 8.65 8.52) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9.68 7.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 9.68 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.5 7.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 /V9203/INP_IN))
    (pad 7 thru_hole circle (at 2.5 5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 40 /V9203/INN_IN))
    (pad 6 thru_hole circle (at 2.5 2.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 /V9203/ICP_IN))
    (pad 5 thru_hole circle (at 2.5 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 /V9203/ICN_IN))
    (pad 4 thru_hole circle (at 0 7.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 /V9203/IBP_IN))
    (pad 3 thru_hole circle (at 0 5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 /V9203/IBN_IN))
    (pad 2 thru_hole circle (at 0 2.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 /V9203/IAP_IN))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 35 /V9203/IAN_IN))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Nano-Fit_105314-xx08_2x04_P2.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 142.64 70.4022 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J11 (at -1.7 0 180) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 180) (layer B.Fab))
    (pad 3 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(J11-Pad3)"))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 61 CS))
    (pad 1 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(J11-Pad1)"))
  )
  (module Whatnick_logo:Whatnick_logo (layer B.Cu) (tedit 0)
    (at 132.150229 53.257155 180)
    (fp_text reference LOGO2 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Connectors_JST:JST_SH_SM06B-SRSS-TB_06x1.00mm_Angled locked (layer F.Cu) (tedit 56B07436)
    (at 124.707 43.75 180)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J9 (at -2.5 -4 180) (layer F.SilkS))
    (fp_text value JST6 (at 0 4.5 180) (layer F.Fab))
    (pad "" smd rect (at 3.8 1.9375 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.8 1.9375 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 5 smd rect (at 1.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 4 smd rect (at 0.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 50 SCK))
    (pad 3 smd rect (at -0.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 49 MOSI))
    (pad 2 smd rect (at -1.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 48 MISO))
    (pad 1 smd rect (at -2.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 61 CS))
    (model ${KIPRJMOD}/JST_PH.3dshapes/SM06B-SRSS-TB.STEP
      (offset (xyz 0 1.199999981977808 -0.3999999939926029))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 128.324 59.4802 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C29 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 91 PM0))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 123.244 59.4802 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C28 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 92 PM1))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 133.395 59.4802 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C30 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 87 /V9203/DS))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 133.522 62.5536)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J10 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(J10-Pad2)"))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 51 +3V3))
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 125.191 61.3852 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R40 (at 0 1.35 90) (layer B.SilkS))
    (fp_text value 20K (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 91 PM0))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(J8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 135.409 63.6204 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R43 (at 0.224258 1.731388 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 130.271 61.5448 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R39 (at 0 1.35 90) (layer B.SilkS))
    (fp_text value 20K (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 92 PM1))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 125.191 63.5188 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R44 (at 0 1.35 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(J8-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 130.296 63.6784 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R42 (at 0 1.35 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 135.325 61.4796 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R41 (at 0 1.35 270) (layer B.SilkS))
    (fp_text value 20K (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 /V9203/DS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_SM09B-SRSS-TB_09x1.00mm_Angled locked (layer F.Cu) (tedit 56B07436)
    (at 143.178 43.75 180)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J6 (at -4 -4 180) (layer F.SilkS))
    (fp_text value JST9 (at 0 4.5 180) (layer F.Fab))
    (pad "" smd rect (at 5.3 1.9375 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -5.3 1.9375 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 8 smd rect (at 3 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(J6-Pad8)"))
    (pad 7 smd rect (at 2 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(J6-Pad7)"))
    (pad 6 smd rect (at 1 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(J6-Pad6)"))
    (pad 5 smd rect (at 0 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J6-Pad5)"))
    (pad 4 smd rect (at -1 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J6-Pad4)"))
    (pad 3 smd rect (at -2 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at -3 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J6-Pad2)"))
    (pad 1 smd rect (at -4 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J6-Pad1)"))
    (model ${KIPRJMOD}/JST_PH.3dshapes/SM09B-SRSS-TB.STEP
      (offset (xyz 0 1.099999983479657 -0.2999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 138.162 50.3028 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C27 (at 0 -1.27 135) (layer F.SilkS))
    (fp_text value 1u (at 0 1.27 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.270001 135) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 125.082 61.7916 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R38 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R38-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(J6-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 138.512 60.559 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 0 -1.35 315) (layer F.SilkS))
    (fp_text value 10K (at 0 1.45 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 315) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R33-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 127.774 64.3316 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R34-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J6-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 123.572 60.5216 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R35 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(J6-Pad7)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R35-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 122.201 59.3024 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R36 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R36-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(J6-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 126.453 63.0616 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R37 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J6-Pad5)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R37-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 157.118 43.1734)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference MK1 (at 0 -3.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 157.626 67.0494)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference MK2 (at 0 -3.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 113.049 65.5889)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference MK3 (at 0 -3.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 112.986 43.0464)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference MK4 (at 0 -3.2) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 134.385429 70.986355 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value OPEN_HARDWARE_1 (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Capacitors_SMD:C_0402 locked (layer F.Cu) (tedit 58AA841A)
    (at 142.513 63.9164 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 /V9203/V_MOSI))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer F.Cu) (tedit 58AA841A)
    (at 138.602 63.9164 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C25 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 /V9203/V_CLK))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer F.Cu) (tedit 58AA841A)
    (at 136.722 63.8744 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C24 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 76 /V9203/V_CS))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer F.Cu) (tedit 58AA841A)
    (at 140.532 63.9164 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C23 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 48 MISO))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer F.Cu) (tedit 58E0A804)
    (at 139.001 62.1472)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at 0 -1.35) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 /V9203/V_CLK))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer F.Cu) (tedit 58E0A804)
    (at 137.085 62.1472)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at 0 -1.35) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 CS))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 /V9203/V_CS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer F.Cu) (tedit 58E0A804)
    (at 142.862 62.1472)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R29 (at 0 -1.35) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 /V9203/V_MOSI))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer F.Cu) (tedit 58E0A804)
    (at 140.931 62.1472 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R30 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 MISO))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 /V9203/V_MISO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 154.451 57.1434 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 36 /V9203/IBN_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 152.546 57.1434 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 /V9203/INN_IN))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 147.466 61.5884)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 /V9203/IBP_IN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 152.546 53.3334 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 /V9203/ICP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 150.641 48.8884)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 /V9203/ICN_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 147.466 48.8884 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 /V9203/IAN_IN))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 150.641 61.5884 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 /V9203/INP_IN))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 154.451 53.3334 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 2.4R/10ppm (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 /V9203/IAP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer F.Cu) (tedit 58AA841A)
    (at 126.511 48.2788 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer B.Cu) (tedit 58AA841A)
    (at 125.038 55.89 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 47 /V9203/UCP))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer B.Cu) (tedit 58AA841A)
    (at 125.038 52.4024 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 46 /V9203/UBP))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer B.Cu) (tedit 58AA841A)
    (at 125.038 48.8972 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 45 /V9203/UAP))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 142.793 60.2676 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 0 -1.27 225) (layer F.SilkS))
    (fp_text value 1u (at 0 1.27 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 225) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 140.464 52.4015 315)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 0 -1.27 315) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 315) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 315) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -0.55 0 315) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 122.87 48.2788 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C22-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.711 50.7426)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 59 /V9203/INP))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.703 49.3964 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 55 /V9203/INN))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.796 55.3654)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 60 /V9203/IBP))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.787 56.6354 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 /V9203/IBN))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.754 52.3936)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 56 /V9203/ICP))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.761 53.689 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 /V9203/ICN))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.83 58.5912)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 30 /V9203/IAP))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 139.83 59.8104 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 31 /V9203/IAN))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 locked (layer F.Cu) (tedit 58AA841A)
    (at 124.632 48.8972 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C20-Pad2)"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 locked (layer F.Cu) (tedit 58AA844E)
    (at 123.197 69.2084 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 1u/50V (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 148.621 82.7339)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1u/16V (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:GS2 locked (layer F.Cu) (tedit 586134A1)
    (at 147.979 70.194 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP1 (at 1.78 0 270) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at -1.8 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP1-Pad1)"))
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 123.362 62.5536)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 51 +3V3))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(J8-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 128.391 62.5536)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(J7-Pad2)"))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 51 +3V3))
  )
  (module Resistors_SMD:R_0402 locked (layer F.Cu) (tedit 58E0A804)
    (at 126.41 49.5488 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 100R (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.1 49.3456)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 40 /V9203/INN_IN))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 55 /V9203/INN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 124.639 50.9204 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 43K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 122.759 49.5996)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R25 (at 0 -1.35) (layer F.SilkS))
    (fp_text value 75K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer B.Cu) (tedit 58E0A804)
    (at 123.565 52.4008 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 0 1.35 270) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 /V9203/UBP))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.125 53.7398)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 38 /V9203/ICN_IN))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 /V9203/ICN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.1 50.768)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 /V9203/INP))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 /V9203/INP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.1 52.3428)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 39 /V9203/ICP_IN))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 56 /V9203/ICP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.151 56.6862)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 /V9203/IBN))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 /V9203/IBN_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.151 55.3654)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 37 /V9203/IBP_IN))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 60 /V9203/IBP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.176 58.6166)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /V9203/IAP))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 /V9203/IAP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 142.19 59.785)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.35) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 35 /V9203/IAN_IN))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 /V9203/IAN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer B.Cu) (tedit 58E0A804)
    (at 123.514 48.8956 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 1.35 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 /V9203/UAP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 locked (layer B.Cu) (tedit 58E0A804)
    (at 123.667 55.9424 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0 1.35 270) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 /V9203/UCP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 121.304 64.5094)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R28-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 121.325 66.7319)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R27-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 117.52 66.6049)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 117.456 64.5729)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering locked (layer F.Cu) (tedit 58E0A804)
    (at 146.946 72.7644 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering locked (layer B.Cu) (tedit 58AAD9E8)
    (at 120.568 48.8884 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 UA))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 /V9203/UAP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering locked (layer B.Cu) (tedit 58AAD9E8)
    (at 120.568 52.4112 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 /V9203/UBP))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 UB))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering locked (layer B.Cu) (tedit 58AAD9E8)
    (at 120.542 55.8734 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 UC))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 /V9203/UCP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer F.Cu) (tedit 57B6E980)
    (at 141.389 58.4712 225)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C14 (at 0 -2.55 225) (layer F.SilkS))
    (fp_text value 10u (at 0 2.55 225) (layer F.Fab))
    (pad 2 smd rect (at 1.375 0 225) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -1.375 0 225) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer F.Cu) (tedit 57B6E980)
    (at 140.819 49.8606 315)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C13 (at 0 -2.55 315) (layer F.SilkS))
    (fp_text value 10u (at 0 2.55 315) (layer F.Fab))
    (pad 2 smd rect (at 1.375 0 315) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 1 smd rect (at -1.375 0 315) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Crystals:Crystal_SMD_Abracon_ABM8G-4pin_3.2x2.5mm locked (layer F.Cu) (tedit 58CD2E9C)
    (at 121.177 55.594 90)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM8G http://www.abracon.com/Resonators/ABM8G.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.45 90) (layer F.SilkS))
    (fp_text value Crystal_GND24 (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 3 smd rect (at 1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad22)"))
    (pad 2 smd rect (at 1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad23)"))
    (model ${KIPRJMOD}/Crystal.3dshapes/NDK_NX3225GD-8MHZ-STD-CRA-3.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module GROVE-CONNECTOR-SMD:HW4-SMD-2.0-90D locked (layer F.Cu) (tedit 59088D75)
    (at 150.741 76.0184 270)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference J5 (at -0.127 -9.3345 270) (layer F.SilkS))
    (fp_text value "GROVE-CONNECTOR-SMD-90D(4+2P-2.0)" (at 0.860755 -4.650229 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3 0.1) (size 2.74 1.01) (layers F.Cu F.Paste F.Mask)
      (net 53 SCL) (solder_mask_margin 0.2))
    (pad 2 smd rect (at -1 0.1) (size 2.74 1.01) (layers F.Cu F.Paste F.Mask)
      (net 54 SDA) (solder_mask_margin 0.2))
    (pad 3 smd rect (at 1 0.1) (size 2.74 1.01) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3) (solder_mask_margin 0.2))
    (pad 4 smd rect (at 3 0.1) (size 2.74 1.01) (layers F.Cu F.Paste F.Mask)
      (net 33 GND) (solder_mask_margin 0.2))
    (pad SS1 smd rect (at -5.4 -7.4) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND) (solder_mask_margin 0.2))
    (pad SS2 smd rect (at 5.4 -7.4) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND) (solder_mask_margin 0.2))
    (model "${KIPRJMOD}/SeeedStudio.3dshapes/Grove Connecteur.wrl"
      (offset (xyz 0 10.59999984080397 -0.7999999879852057))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 90))
    )
  )
  (module Diodes_SMD:D_SMA_Standard locked (layer F.Cu) (tedit 586432E5)
    (at 114.827 80.0034 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.3 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 UB))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad1)"))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SMA_Standard locked (layer F.Cu) (tedit 586432E5)
    (at 114.827 75.7489 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 UA))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SMA_Standard locked (layer F.Cu) (tedit 586432E5)
    (at 114.827 71.5579 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D3 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.3 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 25 UC))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad1)"))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SOD-123 locked (layer F.Cu) (tedit 58645DC7)
    (at 143.911 69.5894)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D5 (at 0 -2) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 52 USB))
    (model ${KIPRJMOD}/Diodes.3dshapes/SOD-123FL.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 locked (layer F.Cu) (tedit 57FE93A5)
    (at 143.237 72.7644)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.8 locked (layer F.Cu) (tedit 58AA8B00)
    (at 144.545 79.0284 90)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.8")
    (attr smd)
    (fp_text reference C2 (at 0 3.92 90) (layer F.SilkS))
    (fp_text value 100u/16V (at 0 -3.92 90) (layer F.Fab))
    (fp_text user %R (at 0 3.92 90) (layer F.Fab))
    (fp_text user + (at -3.38 2.35 90) (layer F.SilkS))
    (fp_text user + (at -1.38 -0.06 90) (layer F.Fab))
    (pad 2 smd rect (at 2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x10 locked (layer F.Cu) (tedit 58AA9153)
    (at 123.463 75.8144 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C1 (at 0 5.45 90) (layer F.SilkS))
    (fp_text value 220u/50V (at 0 -5.45 90) (layer F.Fab))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab))
    (fp_text user + (at -4.78 3.9 90) (layer F.SilkS))
    (fp_text user + (at -2.31 -0.08 90) (layer F.Fab))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ROF-78E:SMD-4 locked (layer F.Cu) (tedit 59088D64)
    (at 128.305 82.6134)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value ROF-78E (at 6.182029 -1.848045) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1 -11.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad1)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at 11.5 -11.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 33 GND) (solder_mask_margin 0.2))
    (pad 3 smd rect (at 11.5 -1) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C2-Pad1)") (solder_mask_margin 0.2))
    (pad 4 smd rect (at 1 -1) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad4)") (solder_mask_margin 0.2))
    (model ${KIPRJMOD}/RECOM_ROF-78E.3dshapes/RECOM_ROF-78E.step
      (offset (xyz 6.299999905383492 6.299999905383492 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_4pol locked (layer F.Cu) (tedit 56301633)
    (at 114.7 48.8884 270)
    (descr "4-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J4 (at 5.25 -4.3 270) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x04 (at 5.25 6 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 UA))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 UB))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 UC))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm locked (layer F.Cu) (tedit 58CD5446)
    (at 153.943 66.5226 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 0 30.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 USB))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(J11-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(J11-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 SCL))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 SDA))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (offset (xyz 0 -13.96999979019165 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x16_Pitch2.54mm locked (layer F.Cu) (tedit 58CD5446)
    (at 153.958 86.8426 270)
    (descr "Through hole straight socket strip, 1x16, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x16 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 40.43 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 +3V3))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 SCK))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 MOSI))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 MISO))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x16_Pitch2.54mm.wrl
      (offset (xyz 0 -19.04999971389771 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm locked (layer F.Cu) (tedit 58CC9A48)
    (at 132.607 55.4924 225)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 -7.45 225) (layer F.SilkS))
    (fp_text value V9203 (at 0 7.45 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at -5.7 -3.2 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 3 smd rect (at -5.7 -2.4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 4 smd rect (at -5.7 -1.6 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /V9203/IAN))
    (pad 5 smd rect (at -5.7 -0.8 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /V9203/IAP))
    (pad 6 smd rect (at -5.7 0 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 /V9203/IBN))
    (pad 7 smd rect (at -5.7 0.8 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 /V9203/IBP))
    (pad 8 smd rect (at -5.7 1.6 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 57 /V9203/ICN))
    (pad 9 smd rect (at -5.7 2.4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 56 /V9203/ICP))
    (pad 10 smd rect (at -5.7 3.2 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 55 /V9203/INN))
    (pad 11 smd rect (at -5.7 4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 59 /V9203/INP))
    (pad 12 smd rect (at -4 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C20-Pad2)"))
    (pad 13 smd rect (at -3.2 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /V9203/UAP))
    (pad 14 smd rect (at -2.4 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /V9203/UBP))
    (pad 15 smd rect (at -1.6 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /V9203/UCP))
    (pad 16 smd rect (at -0.8 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C21-Pad1)"))
    (pad 17 smd rect (at 0 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C22-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 19 smd rect (at 1.6 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 87 /V9203/DS))
    (pad 20 smd rect (at 2.4 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 21 smd rect (at 3.2 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (pad 22 smd rect (at 4 5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 5.7 4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 5.7 3.2 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 91 PM0))
    (pad 25 smd rect (at 5.7 2.4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 92 PM1))
    (pad 26 smd rect (at 5.7 1.6 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R28-Pad2)"))
    (pad 27 smd rect (at 5.7 0.8 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R27-Pad2)"))
    (pad 28 smd rect (at 5.7 0 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 5.7 -0.8 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 5.7 -1.6 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R36-Pad1)"))
    (pad 31 smd rect (at 5.7 -2.4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R35-Pad1)"))
    (pad 32 smd rect (at 5.7 -3.2 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R38-Pad1)"))
    (pad 33 smd rect (at 5.7 -4 225) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R37-Pad1)"))
    (pad 34 smd rect (at 4 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R34-Pad1)"))
    (pad 35 smd rect (at 3.2 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J6-Pad3)"))
    (pad 36 smd rect (at 2.4 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J6-Pad2)"))
    (pad 37 smd rect (at 1.6 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J6-Pad1)"))
    (pad 38 smd rect (at 0.8 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 76 /V9203/V_CS))
    (pad 39 smd rect (at 0 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 77 /V9203/V_CLK))
    (pad 40 smd rect (at -0.8 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 74 /V9203/V_MISO))
    (pad 41 smd rect (at -1.6 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 75 /V9203/V_MOSI))
    (pad 42 smd rect (at -2.4 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R33-Pad1)"))
    (pad 43 smd rect (at -3.2 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 GND))
    (pad 44 smd rect (at -4 -5.7 315) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 +3V3))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text TAPR (at 134.385429 74.415355) (layer B.SilkS))
  (gr_text CS (at 140.837029 68.725755) (layer F.SilkS))
  (gr_text SCL (at 151.403429 68.725755) (layer F.SilkS))
  (gr_text SDA (at 154.019629 68.725755) (layer F.SilkS))
  (gr_text VUSB (at 131.108829 68.725755) (layer F.SilkS))
  (gr_text GND (at 123.387229 84.5) (layer F.SilkS))
  (gr_text 3V3 (at 118.434229 84.5) (layer F.SilkS))
  (gr_text CK (at 141.218029 84.5) (layer F.SilkS))
  (gr_text SI (at 143.8 84.5) (layer F.SilkS))
  (gr_text SO (at 146.2 84.5) (layer F.SilkS))
  (gr_text "SCK,MOSI,MISO used\nCS on pin 9 or 10. \n(0 or 15 for Huzzah)" (at 120.034429 71.214955) (layer B.SilkS))
  (gr_text DSLEEP (at 132 62.5 90) (layer B.SilkS))
  (gr_text PM0 (at 126.5 62.5 90) (layer B.SilkS))
  (gr_text PM1 (at 121.5 62.5 90) (layer B.SilkS))
  (gr_text CSMUX (at 142.767429 72.383355) (layer B.SilkS))
  (gr_text "V9203 3-phase low voltage\nEnergy Monitor Featherwing\nv1.2 14-05-2020\nhttp://whatnick.com" (at 134.995029 79.876355) (layer B.SilkS))
  (gr_arc (start 115 85) (end 110 85) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 155 45) (end 160 45) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 115 45) (end 115 40) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 155 85) (end 155 90) (angle -90) (layer Edge.Cuts) (width 0.01))
  (dimension 50.000049 (width 0.3) (layer F.Fab)
    (gr_text "50.000 mm" (at 134.999466 38.127815 -0.08021403891) (layer F.Fab))
    (feature1 (pts (xy 110.002 36.283) (xy 109.997576 39.442814)))
    (feature2 (pts (xy 160.002 36.353) (xy 159.997576 39.512814)))
    (crossbar (pts (xy 160.001356 36.812817) (xy 110.001356 36.742817)))
    (arrow1a (pts (xy 110.001356 36.742817) (xy 111.12868 36.157974)))
    (arrow1b (pts (xy 110.001356 36.742817) (xy 111.127038 37.330814)))
    (arrow2a (pts (xy 160.001356 36.812817) (xy 158.875674 36.22482)))
    (arrow2b (pts (xy 160.001356 36.812817) (xy 158.874032 37.39766)))
  )
  (dimension 50.000025 (width 0.3) (layer F.Fab)
    (gr_text "50.000 mm" (at 162.904548 64.87889 89.94270424) (layer F.Fab))
    (feature1 (pts (xy 165.194447 89.881205) (xy 161.529549 89.87754)))
    (feature2 (pts (xy 165.244447 39.881205) (xy 161.579549 39.87754)))
    (crossbar (pts (xy 164.279548 39.88024) (xy 164.229548 89.88024)))
    (arrow1a (pts (xy 164.229548 89.88024) (xy 163.644254 88.75315)))
    (arrow1b (pts (xy 164.229548 89.88024) (xy 164.817095 88.754323)))
    (arrow2a (pts (xy 164.279548 39.88024) (xy 163.692001 41.006157)))
    (arrow2b (pts (xy 164.279548 39.88024) (xy 164.864842 41.00733)))
  )
  (gr_line (start 110 85) (end 110 45) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 155 90) (end 115 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 160 45) (end 160 85) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 115 40) (end 155 40) (layer Edge.Cuts) (width 0.01))
  (zone (net 33) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.801429 90.798355) (xy 110.001429 90.798355) (xy 110.001429 39.998355) (xy 160.801429 39.998355)
      )
    )
  )
  (zone (net 33) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.801429 90.798355) (xy 110.001429 90.798355) (xy 110.001429 39.998355) (xy 160.801429 39.998355)
      )
    )
  )
)
