(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 100)
    (no_connects 0)
    (area 128.448999 87.681999 166.699001 113.232001)
    (thickness 1.6)
    (drawings 16)
    (tracks 361)
    (zones 0)
    (modules 52)
    (nets 41)
  )
  (page USLetter)
  (title_block
    (title "Analog Frontend PCB")
    (date 2017-07-31)
    (rev v2.1b)
    (company "Columbia University Creative Machines Lab")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.508)
    (uvia_drill 0.4064)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.1016)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEEFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/vfinal/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 Vfiltered)
  (net 4 V_VGA)
  (net 5 "Net-(C11-Pad1)")
  (net 6 "Net-(C12-Pad1)")
  (net 7 "Net-(C12-Pad2)")
  (net 8 "Net-(C13-Pad1)")
  (net 9 "Net-(C13-Pad2)")
  (net 10 "Net-(C14-Pad1)")
  (net 11 "Net-(C14-Pad2)")
  (net 12 "Net-(C15-Pad1)")
  (net 13 "Net-(C15-Pad2)")
  (net 14 "Net-(C17-Pad1)")
  (net 15 GAIN)
  (net 16 /VCM)
  (net 17 "Net-(CFB1-Pad1)")
  (net 18 "Net-(CFB1-Pad2)")
  (net 19 "Net-(CINH1-Pad1)")
  (net 20 "Net-(CLMD1-Pad2)")
  (net 21 "Net-(D1-Pad3)")
  (net 22 "Net-(R6-Pad2)")
  (net 23 "Net-(R10-Pad2)")
  (net 24 "Net-(U2-Pad2)")
  (net 25 /VGA_PWR)
  (net 26 /VGA-)
  (net 27 /VGA+)
  (net 28 "Net-(R11-Pad1)")
  (net 29 /PULSE)
  (net 30 /RFin)
  (net 31 /PCAP)
  (net 32 "Net-(J2-Pad1)")
  (net 33 "Net-(J4-Pad1)")
  (net 34 "Net-(J6-Pad1)")
  (net 35 "Net-(C26-Pad2)")
  (net 36 "Net-(D3-Pad1)")
  (net 37 20V)
  (net 38 /V_ENVLP)
  (net 39 /Vpiezo)
  (net 40 "Net-(C26-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.4064)
    (add_net +5V)
    (add_net /PCAP)
    (add_net /PULSE)
    (add_net /RFin)
    (add_net /VCM)
    (add_net /VGA+)
    (add_net /VGA-)
    (add_net /VGA_PWR)
    (add_net /V_ENVLP)
    (add_net /Vpiezo)
    (add_net 20V)
    (add_net GAIN)
    (add_net GND)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(CFB1-Pad1)")
    (add_net "Net-(CFB1-Pad2)")
    (add_net "Net-(CINH1-Pad1)")
    (add_net "Net-(CLMD1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad2)")
    (add_net V_VGA)
    (add_net Vfiltered)
  )
  (net_class Power ""
    (clearance 0.381)
    (trace_width 0.762)
    (via_dia 1.524)
    (via_drill 0.889)
    (uvia_dia 0.508)
    (uvia_drill 0.4064)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 134.62 107.696 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C26 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value .01u (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C26-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 594428EE)
    (at 154.559 100.33 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 1.905 -0.127 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /VGA-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:QSOP-20_3.9x8.6mm_Pitch0.64mm (layer F.Cu) (tedit 58B201A7)
    (at 147.828 103.886)
    (descr "20 Lead Quarter Size Outline Plastic Package (QSOP) (https://www.intersil.com/content/dam/Intersil/documents/m20_/m20.15.pdf)")
    (tags "QSOP-20 ")
    (attr smd)
    (fp_text reference U5 (at -2.54 -3.81) (layer F.SilkS))
    (fp_text value AD8331 (at 0 6) (layer F.Fab))
    (pad 1 smd rect (at -2.795 -2.8575) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CLMD1-Pad2)"))
    (pad 20 smd rect (at 2.795 -2.8575) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.795 -2.2175) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CFB1-Pad1)"))
    (pad 19 smd rect (at 2.795 -2.2175) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -2.795 -1.5775) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 18 smd rect (at 2.795 -1.5775) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at -2.795 -0.9375) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C13-Pad1)"))
    (pad 17 smd rect (at 2.795 -0.9375) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.795 -0.2975) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C14-Pad1)"))
    (pad 16 smd rect (at 2.795 -0.2975) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 26 /VGA-))
    (pad 6 smd rect (at -2.795 0.3425) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.795 0.3425) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 27 /VGA+))
    (pad 7 smd rect (at -2.795 0.9825) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C14-Pad2)"))
    (pad 14 smd rect (at 2.795 0.9825) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 25 /VGA_PWR))
    (pad 8 smd rect (at -2.795 1.6225) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C13-Pad2)"))
    (pad 13 smd rect (at 2.795 1.6225) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 25 /VGA_PWR))
    (pad 9 smd rect (at -2.795 2.2625) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.795 2.2625) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 10 smd rect (at -2.795 2.9025) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 15 GAIN))
    (pad 11 smd rect (at 2.795 2.9025) (size 1.524 0.38) (layers F.Cu F.Paste F.Mask)
      (net 16 /VCM))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 59CA903C)
    (at 135.128 92.71 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.524 360) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 Vfiltered))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D197B3)
    (at 140.2715 93.9165 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.7145 0.4445 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 Vfiltered))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing_Handsoldering (layer F.Cu) (tedit 59D197B7)
    (at 131.064 91.948)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3, Housing, Handsoldering,")
    (attr smd)
    (fp_text reference U2 (at 1.778 -2.032) (layer F.SilkS))
    (fp_text value MD0100N8 (at -0.14986 5.30098) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 2.35204) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 39 /Vpiezo))
    (pad 2 smd rect (at 0 2.35204) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at 1.50114 2.35204) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 0 -1.6002) (size 1.99898 4.0005) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad2)"))
    (pad 2 smd trapezoid (at 0 0.7493 180) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:SOT-523 (layer F.Cu) (tedit 591D3A70)
    (at 135.6995 95.3135 90)
    (attr smd)
    (fp_text reference D1 (at 0.3175 -1.5875 180) (layer F.SilkS))
    (fp_text value BAV99T (at 0 1.905 90) (layer F.Fab))
    (pad 1 smd rect (at -0.65 -0.5 270) (size 0.51 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.65 0.5 270) (size 0.51 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 0 270) (size 0.51 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad3)"))
    (model smd_trans/sot323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.75 0.6 0.6))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5944278A)
    (at 141.617 101.854 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -0.115 -1.143 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442973)
    (at 157.226 101.346 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0.127 -1.397 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442C60)
    (at 138.938 104.521 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 1.524 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442C69)
    (at 141.224 104.521 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 2.032 0.127 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C14-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442938)
    (at 157.226 104.394 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -0.762 -1.397 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594428AF)
    (at 153.162 107.442 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 1.778 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 /VGA_PWR))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442C32)
    (at 151.638 109.855 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 1.778 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 597A4F3D)
    (at 146.558 110.236 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 1.651 0.127 360) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 GAIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442C3E)
    (at 149.86 109.855 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 1.778 0 360) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /VCM))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 150.368 96.774 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0.508 -1.524 180) (layer F.SilkS))
    (fp_text value 6.8nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 V_VGA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 /RFin))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 150.368 93.853 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0.127 -1.524 180) (layer F.SilkS))
    (fp_text value 2.2nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 /PCAP))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 160.2105 93.7895 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 /V_ENVLP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 154.051 91.821)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0.127 -1.397 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D1C9B7)
    (at 141.605 98.171 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference CFB1 (at 1.27 0.762 180) (layer F.SilkS))
    (fp_text value 18nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CFB1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(CFB1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594425B8)
    (at 141.478 96.52)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference CINH1 (at 0.254 -1.143) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(CINH1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CFB1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442640)
    (at 147.447 98.298 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference CLMD1 (at 0.127 1.27 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CLMD1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59442615)
    (at 144.399 98.171)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference CSH1 (at -0.127 -1.143 180) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CFB1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 138.557 97.409 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at -1.651 0.127 360) (layer F.SilkS))
    (fp_text value "120nH FB" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 Vfiltered))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(CINH1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5944276A)
    (at 141.617 99.949)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at 1.778 0) (layer F.SilkS))
    (fp_text value "120nH FB" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5944290D)
    (at 154.559 98.552)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L4 (at -1.917 0) (layer F.SilkS))
    (fp_text value "120nH FB" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /VGA-))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59442900)
    (at 154.686 103.886)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L5 (at -1.917 0.127) (layer F.SilkS))
    (fp_text value "120nH FB" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /VGA+))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59442C23)
    (at 154.813 106.68 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L6 (at 1.651 0 360) (layer F.SilkS))
    (fp_text value "120nH FB" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /VGA_PWR))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5944299E)
    (at 159.004 101.219 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.524 0 360) (layer F.SilkS))
    (fp_text value 237 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 594428DE)
    (at 154.559 102.108 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.917 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /VGA+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59442966)
    (at 159.004 104.267 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 1.778 0 360) (layer F.SilkS))
    (fp_text value 237 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 158.242 97.409)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 68 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /V_ENVLP))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5944270E)
    (at 138.43 100.584 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RFB1 (at 1.524 0 360) (layer F.SilkS))
    (fp_text value 274 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(CFB1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:TSOT-23-6_MK06A (layer F.Cu) (tedit 58CE4E80)
    (at 153.924 94.615 180)
    (descr "6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf")
    (tags "TSOT-23-6 MK06A TSOT-6")
    (attr smd)
    (fp_text reference U6 (at -0.127 -2.032 180) (layer F.SilkS))
    (fp_text value LTC5507 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -1.31 0 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (pad 4 smd rect (at 1.31 0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at 1.31 0 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 /PCAP))
    (pad 6 smd rect (at 1.31 -0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 /RFin))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-6_MK06A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:CX2041NLT (layer F.Cu) (tedit 5942FFBC)
    (at 158.75 109.22 180)
    (fp_text reference T1 (at -0.127 -2.794 360) (layer F.SilkS))
    (fp_text value CX2041NLT (at 0 3.81 180) (layer F.Fab))
    (pad 5 smd rect (at -1.27 -1.5875 180) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.27 1.5875 180) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 0 1.5875 180) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.27 -1.5875 180) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 4 V_VGA))
    (pad 3 smd rect (at 1.27 1.5875 180) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 58307A47)
    (at 138.176 93.853 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 1.651 -0.254 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 Vfiltered))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Inductors_SMD.3dshapes\L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:SCREWM3 (layer F.Cu) (tedit 59D1C7DE)
    (at 139.0015 90.3605)
    (fp_text reference J2 (at -0.0635 -0.1905) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_1x01 (at 0.0762 3.3608) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.0254 -0.381) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
  )
  (module custom:SCREWM3 (layer F.Cu) (tedit 59D1C7DB)
    (at 130.81 111.1885)
    (fp_text reference J4 (at -0.254 -0.4445) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_1x01 (at 0.0762 3.3608) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.0254 -0.381) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad1)"))
  )
  (module custom:SCREWM3 (layer F.Cu) (tedit 59D1C7E0)
    (at 159.512 90.297)
    (fp_text reference J6 (at -0.254 -0.381) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_1x01 (at 0.0762 3.3608) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.0254 -0.381) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 34 "Net-(J6-Pad1)"))
  )
  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3)
    (at 140.1445 109.6645 180)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D3 (at 0 -3 180) (layer F.SilkS))
    (fp_text value BZX84C6V2L (at 0 3.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 180) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2.15 0 180) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 59D190C4)
    (at 135.3185 100.9015 90)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D4 (at -4.2545 0.0635 180) (layer F.SilkS))
    (fp_text value BZX84C6V2L (at 0 3.1 90) (layer F.Fab))
    (fp_text user %R (at 0.5715 1.4605 90) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A011EC8)
    (at 133.858 111.506 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -1.143 -0.889 180) (layer F.SilkS))
    (fp_text value 4.02 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 20V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C26-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 164.5285 111.9505)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.0635 -1.2065) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 20V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 161.0995 97.4725 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 1.7145 -0.0635 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A011ECD)
    (at 135.382 111.506 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.889 1.143 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 20V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x04_Pitch2.54mm (layer B.Cu) (tedit 5862ED53)
    (at 162.306 108.331)
    (descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at 1.27 -8.763) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.585 -9.89) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 20V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PULSE))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GAIN))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 129.9845 101.6 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference LS1 (at -0.8255 -1.778 180) (layer F.SilkS))
    (fp_text value Piezo (at 4.315 4.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /Vpiezo))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59D1CD84)
    (at 132.334 100.838 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Rdamp1 (at 1.524 -0.381 180) (layer F.SilkS))
    (fp_text value 200 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:SAM8857-ND (layer F.Cu) (tedit 59D28DFC)
    (at 166.438 93.782 90)
    (fp_text reference J7 (at -4.699 -1.397 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 5.08 90) (layer F.Fab))
    (pad 2 connect rect (at 3.5 -2.1 90) (size 1.35 4.2) (layers *.Mask F.Cu)
      (net 1 GND))
    (pad 2 connect rect (at -3.5 -2.1 90) (size 1.35 4.2) (layers *.Mask F.Cu)
      (net 1 GND))
    (pad 1 connect rect (at 0 -1.9 90) (size 1.27 3.6) (layers F.Cu F.Mask)
      (net 38 /V_ENVLP))
    (pad 2 connect rect (at -3.5 -2.1 90) (size 1.35 4.2) (layers *.Mask B.Cu)
      (net 1 GND))
    (pad 2 connect rect (at 3.5 -2.1 90) (size 1.35 4.2) (layers *.Mask B.Cu)
      (net 1 GND))
  )
  (module custom:SOT-23 (layer F.Cu) (tedit 5A00BE14)
    (at 130.429 105.791)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value Q_NMOS_SDG (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 /PULSE))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C26-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 5A01201C)
    (at 135.89 105.41 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L7 (at -2.032 -0.762 180) (layer F.SilkS))
    (fp_text value .35u (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /Vpiezo))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 129.413 97.79) (layer F.SilkS))
  (gr_text + (at 129.413 102.997) (layer F.SilkS))
  (gr_text GND (at 165.481 109.982 90) (layer F.SilkS))
  (gr_text 20V (at 161.163 108.331 90) (layer F.SilkS))
  (gr_text Pulse (at 160.782 105.791 90) (layer F.SilkS))
  (gr_text Gain (at 160.782 103.251 90) (layer F.SilkS))
  (gr_text 5V (at 160.782 100.711 90) (layer F.SilkS))
  (gr_line (start 166.624 87.757) (end 128.524 87.757) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.624 113.157) (end 166.624 87.757) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 113.157) (end 166.624 113.157) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 87.757) (end 128.524 113.157) (layer Edge.Cuts) (width 0.15))
  (gr_text V_ENVLP (at 163.957 88.773) (layer F.SilkS))
  (gr_text Piezo (at 133.223 101.6) (layer B.SilkS))
  (gr_text GND (at 132.461 98.298) (layer B.SilkS))
  (gr_text "Analog Frontend v2.1b\n" (at 147.574 103.759) (layer B.SilkS))
  (gr_text "Columbia University \nCreative Machines Lab\nOct 2, 2017" (at 147.955 98.425) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.624 113.157) (xy 128.524 113.157) (xy 128.524 87.757) (xy 166.624 87.757)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.524 87.63) (xy 128.524 113.157) (xy 166.624 113.157) (xy 166.624 87.63) (xy 166.497 87.63)
      )
    )
  )
)
