(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3.3V")
  (net 2 "GND")
  (net 3 "/SCL")
  (net 4 "/SDA")
  (net 5 "+5V")
  (net 6 "/PM_RX")
  (net 7 "/PM_TX")
  (net 8 "/LED_DATA")
  (net 9 "/D_CS")
  (net 10 "/D_DCRS")
  (net 11 "/D_RST")
  (net 12 "/SCK")
  (net 13 "/DI")
  (net 14 "/DO")
  (net 15 "unconnected-(U2-NC-Pad1)")
  (net 16 "Net-(J5-Pin_2)")
  (net 17 "unconnected-(J3-SET-Pad3)")
  (net 18 "unconnected-(J3-RESET-Pad6)")
  (net 19 "unconnected-(J3-Pad7)")
  (net 20 "unconnected-(J3-Pad8)")
  (net 21 "unconnected-(J4-Pin_14-Pad14)")
  (net 22 "unconnected-(J4-Pin_15-Pad15)")
  (net 23 "unconnected-(J4-Pin_18-Pad18)")
  (net 24 "unconnected-(J4-Pin_19-Pad19)")
  (net 25 "unconnected-(J4-Pin_20-Pad20)")
  (net 26 "Net-(D1-K)")
  (net 27 "Net-(D1-A)")
  (footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 41.148 41.656 -90)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 3.048 0.254) (layer "F.SilkS"))
    (fp_text value "LED" (at 0.0365 2.032 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 26 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 27 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_LGA:Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering" (layer "F.Cu")
    (at 48.33 41.8275)
    (descr "Bosch  LGA, 8 Pin (https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BME680-DS001-00.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "Bosch LGA NoLead")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "4-in-1 sensor, gas, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8")
    (property "ki_keywords" "Bosch gas pressure humidity temperature environment environmental measurement digital")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.45) (layer "F.SilkS"))
    (fp_text value "BME680" (at 0.438 2.45) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.2 -1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.4 -1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "CSB") (pintype "input"))
    (pad "3" smd roundrect (at 0.4 -1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "SDI") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 1.2 -1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "SCK") (pintype "input"))
    (pad "5" smd roundrect (at 1.2 1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "SDO") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 0.4 1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "7" smd roundrect (at -0.4 1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd roundrect (at -1.2 1.1875) (size 0.5 0.525) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1myFootprints:Xiao ESP32S3" (layer "F.Cu")
    (at 82.55 60.86)
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -3.81 -24.03 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "GND" (at 12.7 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "3V3" (at 12.7 -15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "MOSI" (at 12.7 -12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "SeeedStudio Xiao" (at 2.54 -12.7 270 unlocked) (layer "F.SilkS"))
    (fp_text user "D0" (at -7.62 -20.32 unlocked) (layer "F.SilkS"))
    (fp_text user "SCL" (at -7.62 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "D3" (at -7.62 -12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "RX" (at 12.7 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "MISO" (at 12.7 -10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "SCK" (at 12.7 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "SDA" (at -7.62 -10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "D2" (at -7.62 -15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "TX" (at -7.62 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "D1" (at -7.62 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "Adafruit QT PY" (at 0 -12.7 270 unlocked) (layer "F.SilkS"))
    (fp_text user "5V" (at 12.7 -20.32 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole oval (at -5.08 -20.32) (size 2.5 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/LED_DATA") (pinfunction "D0") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at -5.08 -17.78) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/D_CS") (pinfunction "D1") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -5.08 -15.24) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/D_DCRS") (pinfunction "D2") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -5.08 -12.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/D_RST") (pinfunction "D3") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -5.08 -10.16) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/SCL") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at -5.08 -7.62) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/SDA") (pinfunction "SCL") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -5.08 -5.08) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/PM_RX") (pinfunction "TX") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 10.16 -5.08) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/PM_TX") (pinfunction "RX") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 10.16 -7.62) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/SCK") (pinfunction "SCK") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 10.16 -10.16) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/DI") (pinfunction "MISO") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at 10.16 -12.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/DO") (pinfunction "MOSI") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at 10.16 -15.24) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "3v3") (pintype "power_in"))
    (pad "13" thru_hole rect (at 10.16 -17.78) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "14" thru_hole circle (at 10.16 -20.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "+5V") (pinfunction "5V") (pintype "power_out"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 53.34 42.1025 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 3.4675 -0.2925) (layer "F.SilkS"))
    (fp_text value "100nF" (at -3.5175 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1myFootprints:Generic I2C OLED" (layer "F.Cu")
    (at 58.32 29.21 90)
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -1.17 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (fp_text user "SCL" (at -2.54 -10.16 90 unlocked) (layer "F.SilkS"))
    (fp_text user "OLED" (at 2.794 -9.552 unlocked) (layer "F.SilkS"))
    (fp_text user "SDA" (at -2.54 -12.7 90 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -2.54 -7.62 90 unlocked) (layer "F.SilkS"))
    (fp_text user "VCC" (at -2.54 -5.08 90 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole oval (at 0 -12.7 90) (size 2.5 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/SDA") (pinfunction "SDA") (pintype "input"))
    (pad "2" thru_hole circle (at 0 -10.16 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "3" thru_hole rect (at 0 -7.62 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole circle (at 0 -5.08 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
  )
  (footprint "1myFootprints:PMS5003 Connector" (layer "F.Cu")
    (at 53.32 61.13)
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -7.6 -10.33 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "SET" (at -2.5 -10.16 90 unlocked) (layer "F.SilkS"))
    (fp_text user "PMS5003" (at 2.54 -10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "VCC" (at -5 -10.16 90 unlocked) (layer "F.SilkS"))
    (fp_text user "RX" (at -1.25 -10.16 90 unlocked) (layer "F.SilkS"))
    (fp_text user "RESET" (at 1.5 -10.16 90 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -3.75 -10.16 90 unlocked) (layer "F.SilkS"))
    (fp_text user "TX" (at 0.5 -10.16 90 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.98 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5V") (pinfunction "5V") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -3.73 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -2.48 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(J3-SET-Pad3)") (pinfunction "SET") (pintype "input+no_connect") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -1.23 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/PM_RX") (pinfunction "RX") (pintype "input") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at 0.02 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/PM_TX") (pinfunction "TX") (pintype "output") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at 1.27 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(J3-RESET-Pad6)") (pinfunction "RESET") (pintype "input+no_connect") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at 2.52 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(J3-Pad7)") (pinfunction "7") (pintype "no_connect") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at 3.77 -7.79) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(J3-Pad8)") (pinfunction "8") (pintype "no_connect") (solder_mask_margin 0.0762))
    (pad "S1" smd rect (at -7.53 -4.89) (size 2.1 3) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0762))
    (pad "S2" smd rect (at 6.32 -4.89) (size 2.1 3) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0762))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 102.1025 33.97)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Power Supply, Single Buffer GATE, CMOS Logic, Level Shifter, SOT-23-5")
    (property "ki_keywords" "single buffer level shift")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "SN74LV1T34DBV" (at 0 2.4) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(U2-NC-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/LED_DATA") (pinfunction "A") (pintype "input"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J5-Pin_2)") (pinfunction "Y") (pintype "output"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (at 63.5 42.1025 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 2.9865 0.1925) (layer "F.SilkS"))
    (fp_text value "4.7K" (at -3.81 0.1925) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 3 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1210_3225Metric" (layer "F.Cu")
    (at 68.58 42.1025 90)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.9865 0) (layer "F.SilkS"))
    (fp_text value "4.7K" (at -3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 4 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 40.64 28.448)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "1myFootprints:Cuttable Pad 1206" (layer "F.Cu")
    (at 42.97625 44.077)
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.20375 -6.485) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439))
    (pad "1" smd roundrect (at -1 -6.485) (size 2 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 26 "Net-(D1-K)") (pinfunction "1") (pintype "input"))
    (pad "2" smd roundrect (at 1.4075 -6.485) (size 2 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 2 "GND") (pinfunction "2") (pintype "output"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 85.09 33.02 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 1.905 180) (layer "F.SilkS"))
    (fp_text value "100µF" (at -0.635 -1.905 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1myFootprints:AMPHENOL_20021511-00020T4LF" (layer "F.Cu")
    (at 108.585 48.895 -90)
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -8.89 -3.81) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at 7.395 4.435 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at -5.715 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 1 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -5.715 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 9 "/D_CS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -4.445 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 11 "/D_RST") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -4.445 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at -3.175 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -3.175 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 10 "/D_DCRS") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 14 "/DO") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -1.905 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at -0.635 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 1 "+3.3V") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at -0.635 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 13 "/DI") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0.635 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 12 "/SCK") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 0.635 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 1.905 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 1.905 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 21 "unconnected-(J4-Pin_14-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" thru_hole circle (at 3.175 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 22 "unconnected-(J4-Pin_15-Pad15)") (pinfunction "Pin_15") (pintype "passive+no_connect"))
    (pad "16" thru_hole circle (at 3.175 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 4.445 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 2 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 4.445 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 23 "unconnected-(J4-Pin_18-Pad18)") (pinfunction "Pin_18") (pintype "passive+no_connect"))
    (pad "19" thru_hole circle (at 5.715 0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 24 "unconnected-(J4-Pin_19-Pad19)") (pinfunction "Pin_19") (pintype "passive+no_connect"))
    (pad "20" thru_hole circle (at 5.715 -0.635 270) (size 1.1 1.1) (drill 0.7) (layers "*.Cu")
      (net 25 "unconnected-(J4-Pin_20-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 115.57 57.404)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 44.45 41.656 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 27 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 40.64 57.15)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 115.57 28.448)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 109.88 29.225)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.85) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J5-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal" (layer "F.Cu")
    (at 64.77 29.875 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (property "Sheetfile" "printer monitor.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -5.08 0.665) (layer "F.SilkS"))
    (fp_text value "~" (at 0 3.98) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "MP" smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (pad "MP" smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1myFootprints:OSHW-Logo2_7.3x6mm_SilkScreen" (layer "B.Cu")
    (at 65.278 49.276 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Logo2_7.3x6mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (footprint "Symbol:KiCad-Logo2_5mm_SilkScreen" (layer "B.Cu")
    (at 51.816 49.022 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 5.08) (layer "B.SilkS") hide)
    (fp_text value "KiCad-Logo2_5mm_SilkScreen" (at 0 -5.08) (layer "B.Fab") hide)
  )
  (footprint "1myFootprints:CTRLH Logo" (layer "B.Cu")
    (at 86.995 49.53 180)
    (attr board_only)
    (fp_text reference "REF**" (at 4.173109 2.895837 unlocked) (layer "B.SilkS") hide)
    (fp_text value "CTRLH Logo" (at 4.173109 1.395837 unlocked) (layer "B.Fab") hide)
  )
  (gr_rect (start 37.465 25.4) (end 118.491 60.325)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "github.com/romkey/printer-monitor-pcb\nv0.02\n2/7/2024" (at 90.805 41.91) (layer "B.SilkS"))
  (gr_text "SPI TFT" (at 108.585 60.325) (layer "F.SilkS"))
  (gr_text "5V" (at 107.975 29.225) (layer "F.SilkS"))
  (gr_text "LEDs" (at 107.34 38.115) (layer "F.SilkS"))
  (gr_text "GND" (at 107.975 34.305) (layer "F.SilkS"))
  (gr_text "D" (at 107.975 31.765) (layer "F.SilkS"))
  (gr_text "STEMMAQT/Qwiic" (at 64.77 27.19) (layer "F.SilkS"))
)
