(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 68)
    (tracks 121)
    (zones 0)
    (modules 21)
    (nets 34)
  )
  (page A4)
  (title_block
    (title arduboy-pmod)
    (date 2020-05-13)
    (rev v0.1)
    (comment 3 "2020 (C) Sonal Pinto, sonalpinto@gmail.com")
    (comment 4 "License: CC-BY-SA V4.0")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad3)")
  (net 4 /RIGHT)
  (net 5 /LEFT)
  (net 6 "Net-(S1-Pad4)")
  (net 7 "Net-(S2-Pad4)")
  (net 8 /CS)
  (net 9 /RST)
  (net 10 /DC)
  (net 11 /SCK)
  (net 12 /MOSI)
  (net 13 "Net-(J2-Pad10)")
  (net 14 "Net-(J2-Pad9)")
  (net 15 "Net-(J2-Pad8)")
  (net 16 /A)
  (net 17 /B)
  (net 18 /UP)
  (net 19 /DOWN)
  (net 20 "Net-(J3-Pad10)")
  (net 21 "Net-(S1-Pad2)")
  (net 22 "Net-(S2-Pad2)")
  (net 23 "Net-(S3-Pad4)")
  (net 24 "Net-(S3-Pad2)")
  (net 25 "Net-(S4-Pad2)")
  (net 26 "Net-(S4-Pad4)")
  (net 27 "Net-(S5-Pad4)")
  (net 28 "Net-(S5-Pad2)")
  (net 29 "Net-(S6-Pad2)")
  (net 30 "Net-(S6-Pad4)")
  (net 31 /SPK)
  (net 32 "Net-(LS1-Pad2)")
  (net 33 "Net-(Q1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net /A)
    (add_net /B)
    (add_net /CS)
    (add_net /DC)
    (add_net /DOWN)
    (add_net /LEFT)
    (add_net /MOSI)
    (add_net /RIGHT)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SPK)
    (add_net /UP)
    (add_net GND)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(LS1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S2-Pad2)")
    (add_net "Net-(S2-Pad4)")
    (add_net "Net-(S3-Pad2)")
    (add_net "Net-(S3-Pad4)")
    (add_net "Net-(S4-Pad2)")
    (add_net "Net-(S4-Pad4)")
    (add_net "Net-(S5-Pad2)")
    (add_net "Net-(S5-Pad4)")
    (add_net "Net-(S6-Pad2)")
    (add_net "Net-(S6-Pad4)")
    (add_net VCC)
  )
  (module arduboy-pmod:ghost (layer B.Cu) (tedit 0)
    (at 134.112 65.024 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module arduboy-pmod:pacman (layer B.Cu) (tedit 0)
    (at 161.29 65.024 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module arduboy-pmod:Adafruit_SSD1306 (layer F.Cu) (tedit 5ECFE102)
    (at 138.43 64.77)
    (descr "Adafruit SSD1306 OLED 1.3 inch 128x64 I2C & SPI https://learn.adafruit.com/monochrome-oled-breakouts/downloads")
    (tags "Adafruit SSD1306 OLED 1.3 inch 128x64 I2C & SPI ")
    (fp_text reference J1 (at 8.89 -5) (layer F.SilkS) hide)
    (fp_text value Conn_01x08 (at 8.89 30) (layer F.Fab))
    (fp_text user GND (at 17.78 2.794 90) (layer F.SilkS))
    (fp_text user 3V3 (at 15.24 2.794 90) (layer F.SilkS))
    (fp_text user CS (at 10.16 2.286 90) (layer F.SilkS))
    (fp_text user RST (at 7.62 2.794 90) (layer F.SilkS))
    (fp_text user DC (at 5.08 2.286 90) (layer F.SilkS))
    (fp_text user SCK (at 2.54 2.794 90) (layer F.SilkS))
    (fp_text user MOSI (at 0 3.048 90) (layer F.SilkS))
    (fp_text user %R (at 8.89 14.732) (layer F.Fab))
    (pad 1 thru_hole rect (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole circle (at 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /CS))
    (pad 5 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 6 thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /DC))
    (pad 7 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCK))
    (pad 8 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (model ${KISYS3DMOD}/Display.3dshapes/Adafruit_SSD1306.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module arduboy-pmod:Switch_Tactile_THT_B3F-1xxx_nosilk (layer F.Cu) (tedit 5ECFE0A7)
    (at 186.69 72.39 270)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S6 (at 3.2512 -2.2094 90) (layer F.SilkS) hide)
    (fp_text value B3F-1020 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(S6-Pad4)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 6.5012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(S6-Pad2)"))
    (pad 1 thru_hole rect (at 0.0012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 /B))
  )
  (module digikey-footprints:Piezo_Transducer_THT_PS1240P02BT (layer F.Cu) (tedit 5ECFE300)
    (at 184.15 90.17)
    (fp_text reference LS1 (at 0.075 -4.75) (layer F.SilkS) hide)
    (fp_text value Speaker (at 0.575 9.825) (layer F.Fab))
    (fp_text user %R (at -0.1 2.75) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 5) (size 1.85 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 32 "Net-(LS1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (module arduboy-pmod:Switch_Tactile_THT_B3F-1xxx_nosilk (layer F.Cu) (tedit 5ECFE0A7)
    (at 175.26 77.47 270)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S5 (at 3.2512 -2.2094 90) (layer F.SilkS) hide)
    (fp_text value B3F-1020 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(S5-Pad4)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 6.5012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(S5-Pad2)"))
    (pad 1 thru_hole rect (at 0.0012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A))
  )
  (module arduboy-pmod:Switch_Tactile_THT_B3F-1xxx_nosilk (layer F.Cu) (tedit 5ECFE0A7)
    (at 116.332 82.55 270)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S4 (at 3.2512 -2.2094 90) (layer F.SilkS) hide)
    (fp_text value B3F-1020 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(S4-Pad4)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 6.5012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(S4-Pad2)"))
    (pad 1 thru_hole rect (at 0.0012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DOWN))
  )
  (module arduboy-pmod:Switch_Tactile_THT_B3F-1xxx_nosilk (layer F.Cu) (tedit 5ECFE0A7)
    (at 116.332 68.58 270)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S3 (at 3.2512 -2.2094 90) (layer F.SilkS) hide)
    (fp_text value B3F-1020 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(S3-Pad4)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 6.5012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(S3-Pad2)"))
    (pad 1 thru_hole rect (at 0.0012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 /UP))
  )
  (module arduboy-pmod:Switch_Tactile_THT_B3F-1xxx_nosilk (layer F.Cu) (tedit 5ECFE0A7)
    (at 123.952 75.692 270)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S2 (at 3.2512 -2.2094 90) (layer F.SilkS) hide)
    (fp_text value B3F-1020 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(S2-Pad4)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 6.5012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(S2-Pad2)"))
    (pad 1 thru_hole rect (at 0.0012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RIGHT))
  )
  (module arduboy-pmod:Switch_Tactile_THT_B3F-1xxx_nosilk (layer F.Cu) (tedit 5ECFE0A7)
    (at 108.712 75.692 270)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S1 (at 3.2512 -2.2094 90) (layer F.SilkS) hide)
    (fp_text value B3F-1020 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(S1-Pad4)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 6.5012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(S1-Pad2)"))
    (pad 1 thru_hole rect (at 0.0012 0.0106 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /LEFT))
  )
  (module digikey-footprints:TO-92-3_Formed_Leads (layer F.Cu) (tedit 5AF4B307)
    (at 187.96 57.15 270)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference Q1 (at 2.6 -3.35 90) (layer F.SilkS) hide)
    (fp_text value Q_NPN_ECB (at 2.6 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.6 -1.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.2 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole circle (at 2.6 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(LS1-Pad2)"))
  )
  (module arduboy-pmod:PMODHeader_2x6_2.54mm_Horizontal_Mirrored (layer F.Cu) (tedit 5EBCE74B)
    (at 142.24 57.15 270)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J2 (at 2.286 1.016 unlocked) (layer F.SilkS) hide)
    (fp_text value PMOD1B (at -5.655 14.97 90) (layer F.Fab))
    (fp_text user 12 (at -2.54 14.732 180) (layer F.SilkS))
    (fp_text user 6 (at 0 14.224 180) (layer F.SilkS))
    (fp_text user GND (at 2.54 10.16 90) (layer F.SilkS))
    (fp_text user 3V3 (at 2.54 12.7 90) (layer F.SilkS))
    (fp_text user 7 (at -2.54 -1.524 180) (layer F.SilkS))
    (fp_text user 1 (at 0 -1.524 180) (layer F.SilkS))
    (fp_text user %R (at -5.31 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCK))
    (pad 7 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 8 thru_hole oval (at -2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /CS))
    (pad 9 thru_hole oval (at -2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /DC))
    (pad 10 thru_hole oval (at -2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at -2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at -2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (offset (xyz 0 -12.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module arduboy-pmod:PMODHeader_2x6_2.54mm_Horizontal_Mirrored (layer F.Cu) (tedit 5EBCE74B)
    (at 165.1 57.15 270)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J3 (at 2.286 1.016 unlocked) (layer F.SilkS) hide)
    (fp_text value PMOD1A (at -5.655 14.97 90) (layer F.Fab))
    (fp_text user 12 (at -2.54 14.732 180) (layer F.SilkS))
    (fp_text user 6 (at 0 14.224 180) (layer F.SilkS))
    (fp_text user GND (at 2.54 10.16 90) (layer F.SilkS))
    (fp_text user 3V3 (at 2.54 12.7 90) (layer F.SilkS))
    (fp_text user 7 (at -2.54 -1.524 180) (layer F.SilkS))
    (fp_text user 1 (at 0 -1.524 180) (layer F.SilkS))
    (fp_text user %R (at -5.31 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /LEFT))
    (pad 7 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RIGHT))
    (pad 8 thru_hole oval (at -2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /B))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /UP))
    (pad 9 thru_hole oval (at -2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SPK))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DOWN))
    (pad 10 thru_hole oval (at -2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad10)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at -2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at -2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (offset (xyz 0 -12.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 110.49 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 /LEFT))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 113.03 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 /RIGHT))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 115.57 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 /UP))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 118.11 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 /DOWN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 /A))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 179.07 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 /B))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 184.15 57.15 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 1K (at 2.54 0 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 /SPK))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 181.61 62.23 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text value 1K (at 2.54 0 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(LS1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1K (at 184.15 59.69 90) (layer F.SilkS))
  (gr_text 1K (at 181.61 59.69 90) (layer F.SilkS))
  (gr_text "Arduboy PMOD v0.1" (at 146.304 61.468) (layer B.SilkS))
  (gr_text SPK (at 184.15 92.71) (layer F.SilkS))
  (gr_text PMOD1A (at 163.322 59.436) (layer F.SilkS))
  (gr_text PMOD1B (at 140.462 59.436) (layer F.SilkS))
  (gr_arc (start 107.95 92.71) (end 99.06 92.71) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 186.69 92.71) (end 186.69 101.6) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 191.77 54.61) (end 195.58 54.61) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 102.87 54.61) (end 102.87 50.8) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (dimension 96.52 (width 0.15) (layer Cmts.User)
    (gr_text "3.8000 in" (at 147.32 39.34) (layer Cmts.User))
    (feature1 (pts (xy 195.58 45.72) (xy 195.58 40.053579)))
    (feature2 (pts (xy 99.06 45.72) (xy 99.06 40.053579)))
    (crossbar (pts (xy 99.06 40.64) (xy 195.58 40.64)))
    (arrow1a (pts (xy 195.58 40.64) (xy 194.453496 41.226421)))
    (arrow1b (pts (xy 195.58 40.64) (xy 194.453496 40.053579)))
    (arrow2a (pts (xy 99.06 40.64) (xy 100.186504 41.226421)))
    (arrow2b (pts (xy 99.06 40.64) (xy 100.186504 40.053579)))
  )
  (dimension 50.8 (width 0.15) (layer Cmts.User)
    (gr_text "2.0000 in" (at 208.31 76.2 270) (layer Cmts.User))
    (feature1 (pts (xy 201.93 101.6) (xy 207.596421 101.6)))
    (feature2 (pts (xy 201.93 50.8) (xy 207.596421 50.8)))
    (crossbar (pts (xy 207.01 50.8) (xy 207.01 101.6)))
    (arrow1a (pts (xy 207.01 101.6) (xy 206.423579 100.473496)))
    (arrow1b (pts (xy 207.01 101.6) (xy 207.596421 100.473496)))
    (arrow2a (pts (xy 207.01 50.8) (xy 206.423579 51.926504)))
    (arrow2b (pts (xy 207.01 50.8) (xy 207.596421 51.926504)))
  )
  (dimension 22.86 (width 0.15) (layer Cmts.User)
    (gr_text "0.9000 in" (at 147.32 49.56) (layer Cmts.User))
    (feature1 (pts (xy 158.75 48.26) (xy 158.75 48.846421)))
    (feature2 (pts (xy 135.89 48.26) (xy 135.89 48.846421)))
    (crossbar (pts (xy 135.89 48.26) (xy 158.75 48.26)))
    (arrow1a (pts (xy 158.75 48.26) (xy 157.623496 48.846421)))
    (arrow1b (pts (xy 158.75 48.26) (xy 157.623496 47.673579)))
    (arrow2a (pts (xy 135.89 48.26) (xy 137.016504 48.846421)))
    (arrow2b (pts (xy 135.89 48.26) (xy 137.016504 47.673579)))
  )
  (gr_line (start 99.06 92.71) (end 99.06 54.61) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 186.69 101.6) (end 107.95 101.6) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 195.58 54.61) (end 195.58 92.71) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 102.87 50.8) (end 191.77 50.8) (layer Edge.Cuts) (width 0.0254))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 102.87) (xy 97.79 102.87) (xy 97.79 49.53) (xy 196.85 49.53)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 102.87) (xy 97.79 102.87) (xy 97.79 49.53) (xy 196.85 49.53)
      )
    )
  )
)
