(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 13)
    (no_connects 0)
    (area 99.924999 99.924999 133.275001 143.275001)
    (thickness 1.6)
    (drawings 16)
    (tracks 59)
    (zones 0)
    (modules 7)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad5)")
  (net 2 "Net-(J1-Pad4)")
  (net 3 HEAT_+)
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 HEAT_-)
  (net 7 GND)
  (net 8 "Net-(J7-Pad2)")
  (net 9 "Net-(J7-Pad5)")
  (net 10 "Net-(J1-Pad15)")
  (net 11 "Net-(J1-Pad14)")
  (net 12 "Net-(J1-Pad13)")
  (net 13 FAN_CTL_+)
  (net 14 FAN_CTL_-)
  (net 15 "Net-(J1-Pad7)")
  (net 16 "Net-(J1-Pad6)")
  (net 17 E1_2)
  (net 18 E1_1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net E1_1)
    (add_net E1_2)
    (add_net FAN_CTL_+)
    (add_net FAN_CTL_-)
    (add_net GND)
    (add_net HEAT_+)
    (add_net HEAT_-)
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad5)")
  )
  (module custom:VGA_Female (layer F.Cu) (tedit 5A2C73A7)
    (at 116.6 114.5)
    (descr http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10090929.pdf)
    (tags "VGA, HD15")
    (fp_text reference J1 (at 0.508 5.334) (layer F.SilkS) hide)
    (fp_text value DB15_Control (at 0 -5.08) (layer F.Fab) hide)
    (pad 15 thru_hole circle (at -4.83 1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at -2.54 1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at -0.25 1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at 2.04 1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 17 E1_2))
    (pad 11 thru_hole circle (at 4.33 1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 18 E1_1))
    (pad 5 thru_hole circle (at -4.83 -1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at -2.54 -1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 1 thru_hole circle (at 4.33 -1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 3 HEAT_+))
    (pad 2 thru_hole circle (at 2.04 -1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -0.25 -1.98) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 10 thru_hole circle (at -3.68 0) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 6 HEAT_-))
    (pad 9 thru_hole circle (at -1.39 0) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 13 FAN_CTL_+))
    (pad 8 thru_hole circle (at 0.9 0) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 14 FAN_CTL_-))
    (pad 7 thru_hole circle (at 3.19 0) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad7)"))
    (pad 0 thru_hole circle (at -12.5 0) (size 4 4) (drill 3.15) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 0 thru_hole circle (at 12.5 0) (size 4 4) (drill 3.15) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 6 thru_hole circle (at 5.48 0) (size 1.6 1.6) (drill 1.25) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A2C6FA5)
    (at 111.5 126 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J4 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value FAN_CTL (at 1.25 4.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 13 FAN_CTL_+))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 14 FAN_CTL_-))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A2C6F78)
    (at 118.5 126 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J5 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value FAN_AO (at 1.25 4.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 HEAT_+))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A2C6FB1)
    (at 104.5 126 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J6 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value EO (at 1.25 4.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 18 E1_1))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 17 E1_2))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.00mm (layer F.Cu) (tedit 5A2C81F4)
    (at 111.6 101 90)
    (descr "Through hole straight pin header, 1x06, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.00mm single row")
    (fp_text reference J7 (at 0 -2.06 90) (layer F.SilkS) hide)
    (fp_text value Stepper (at 0 12.06 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J7-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J7-Pad5)"))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 5A2C81EB)
    (at 125 127.5)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J8 (at 2.54 -5.08) (layer F.SilkS) hide)
    (fp_text value HEAT (at 2.54 5.08) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 HEAT_+))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 6 HEAT_-))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LOGOS:logo_MLlabs_small (layer B.Cu) (tedit 0)
    (at 108.5 117.5 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "Thanks to Colen Casey" (at 116.5 141) (layer B.SilkS))
  (gr_text "By Maniacal Labs" (at 122.5 120) (layer B.SilkS))
  (gr_text "Formbot T-Rex 2+\nExtruder PCB - Right" (at 117 107.5) (layer B.SilkS))
  (gr_text - (at 130 132.5) (layer F.SilkS))
  (gr_text + (at 125 132.5) (layer F.SilkS))
  (gr_text E1 (at 104.5 132.5) (layer F.SilkS))
  (gr_text "CTL FAN" (at 111 132.5) (layer F.SilkS))
  (gr_text "AO FAN" (at 118 132.5) (layer F.SilkS))
  (gr_circle (center 122.95 136.7) (end 125.45 136.7) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 110.25 136.7) (end 112.75 136.7) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 130.2 140.2) (end 131.7 140.2) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 103 140.2) (end 104.5 140.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 143.2) (end 133.2 143.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.2 100) (end 133.2 143.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 100 143.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 133.2 100) (angle 90) (layer Edge.Cuts) (width 0.15))
)
