<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="28.5625" y2="0" width="0" layer="20"/>
<wire x1="28.5625" y1="0" x2="28.5625" y2="23.485" width="0" layer="20"/>
<wire x1="28.5625" y1="23.485" x2="0" y2="23.485" width="0" layer="20"/>
<wire x1="0" y1="23.485" x2="0" y2="0" width="0" layer="20"/>
<text>otb-8266</text>
<text>v0.1</text>
<text>(c) packom.net
2016</text>
<text>otb-8266
breakout
v0.1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
</package>
</packages>
</library>
<library name="Piers's library">
<packages>
<package name="OTB-8266-V0.1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="VALUE"/>
</element>
<element name="OTB-8266" library="Piers's library" package="OTB-8266-V0.1" value="OTB-8266-V0.1"/>
</elements>
<signals>
<signal name="GPIO4">
<contactref element="J1" pad="4"/>
<contactref element="OTB-8266" pad="GPIO4"/>
</signal>
<signal name="TX">
<contactref element="J2" pad="7"/>
<contactref element="OTB-8266" pad="TX"/>
</signal>
<signal name="GPIO14">
<contactref element="OTB-8266" pad="GPIO14"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="GPIO12">
<contactref element="OTB-8266" pad="GPIO12"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="GPIO15">
<contactref element="OTB-8266" pad="GPIO15"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="OTB-8266" pad="ANT_GND"/>
<contactref element="J2" pad="1"/>
<contactref element="OTB-8266" pad="GND"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GPIO5">
<contactref element="OTB-8266" pad="GPIO5"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="GPIO2">
<contactref element="OTB-8266" pad="GPIO2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="GPIO13">
<contactref element="OTB-8266" pad="GPIO13"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="GPIO16">
<contactref element="OTB-8266" pad="GPIO16"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="TOUT">
<contactref element="J2" pad="5"/>
<contactref element="OTB-8266" pad="TOUT"/>
</signal>
<signal name="GPIO0">
<contactref element="J2" pad="9"/>
<contactref element="OTB-8266" pad="GPIO0"/>
</signal>
<signal name="VCC">
<contactref element="OTB-8266" pad="VCC"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="RX">
<contactref element="OTB-8266" pad="RX"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="RST">
<contactref element="OTB-8266" pad="RST"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="CH_EN">
<contactref element="OTB-8266" pad="CH_EN"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="ANT">
<contactref element="OTB-8266" pad="ANT_+VE"/>
<contactref element="J2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
