(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (footprint "Custom:CONN_112404_AMP" (layer "F.Cu")
    (at 129.2606 69.7992)
    (tags "112404 ")
    (property "Sheetfile" "Empower EC2047 test board v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "112404")
    (attr through_hole)
    (fp_text reference "J2" (at 0.06 7.43 unlocked) (layer "F.SilkS"))
    (fp_text value "112404" (at -0.09 11.49 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.01 9.41 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.8034 1.8034) (drill 1.2954) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -3.175 -3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 3.175 -3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at -3.175 3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 3.175 3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Custom:EC2047 parallel" (layer "F.Cu")
    (at 143.9832 70.612)
    (property "Sheetfile" "Empower EC2047 test board v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0.0348 -3.175 unlocked) (layer "F.SilkS"))
    (fp_text value "C_Polarized" (at 0.02 6.59 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.02 4.31 unlocked) (layer "F.Fab"))
    (pad "1" smd circle (at 1 0) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd circle (at 0.6 0) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "3" smd circle (at 0.2 0) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "4" smd circle (at -0.2 0) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "5" smd circle (at -0.6 0) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "6" smd circle (at -1 0) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "7" smd circle (at 1 -0.4) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "8" smd circle (at 0.6 -0.4) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "9" smd circle (at 0.2 -0.4) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "10" smd circle (at -0.2 -0.4) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "11" smd circle (at -0.6 -0.4) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "12" smd circle (at -1 -0.4) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "13" smd circle (at 1 -0.8) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "14" smd circle (at 0.6 -0.8) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "15" smd circle (at 0.2 -0.8) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "16" smd circle (at -0.2 -0.8) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "17" smd circle (at -0.6 -0.8) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "18" smd circle (at -1 -0.8) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "19" smd circle (at 1 -1.2) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "20" smd circle (at 0.6 -1.2) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "21" smd circle (at 0.2 -1.2) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "22" smd circle (at -0.2 -1.2) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "23" smd circle (at -0.6 -1.2) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "24" smd circle (at -1 -1.2) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "25" smd circle (at 1 -1.6) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "26" smd circle (at 0.6 -1.6) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "27" smd circle (at 0.2 -1.6) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "28" smd circle (at -0.2 -1.6) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "29" smd circle (at -0.6 -1.6) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "30" smd circle (at -1 -1.6) (size 0.3 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)"))
  )
  (footprint "Custom:CONN_112404_AMP" (layer "F.Cu")
    (at 159.4358 69.6722)
    (tags "112404 ")
    (property "Sheetfile" "Empower EC2047 test board v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "112404")
    (attr through_hole)
    (fp_text reference "J1" (at 0.06 7.43 unlocked) (layer "F.SilkS"))
    (fp_text value "112404" (at -0.09 11.49 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.01 9.41 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.8034 1.8034) (drill 1.2954) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -3.175 -3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 3.175 -3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at -3.175 3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 3.175 3.175) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask"))
  )
  (gr_rect (start 120.5484 60.1726) (end 167.9194 79.629)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Note capacitor directionality" (at 134.2644 78.2066) (layer "F.SilkS"))
  (gr_text "E2047 test board v2" (at 137.16 62.3824) (layer "F.SilkS"))
  (gr_text "-" (at 145.8722 68.4784) (layer "F.SilkS"))
  (gr_text "+" (at 139.2682 68.5038) (layer "F.SilkS"))
)
