(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 813)
    (zones 0)
    (modules 75)
    (nets 99)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.7 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 9 9)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VGL)
  (net 4 VGH)
  (net 5 +3V3)
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(C6-Pad2)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C12-Pad1)")
  (net 10 "Net-(C13-Pad1)")
  (net 11 "Net-(C14-Pad1)")
  (net 12 +BATT)
  (net 13 EN)
  (net 14 CHARGE)
  (net 15 "Net-(C21-Pad1)")
  (net 16 "Net-(C22-Pad1)")
  (net 17 "Net-(C23-Pad1)")
  (net 18 XTAL1)
  (net 19 XTAL2)
  (net 20 "Net-(C26-Pad1)")
  (net 21 "Net-(C28-Pad1)")
  (net 22 "Net-(D4-Pad2)")
  (net 23 "Net-(D5-Pad2)")
  (net 24 "Net-(D6-Pad2)")
  (net 25 CHARGE_STATUS)
  (net 26 DISP_CLK)
  (net 27 DISP_DIN)
  (net 28 DISP_CS)
  (net 29 DISP_DC)
  (net 30 DISP_RST)
  (net 31 DISP_BUSY)
  (net 32 "Net-(J1-Pad7)")
  (net 33 "Net-(J1-Pad6)")
  (net 34 RESE)
  (net 35 GDR)
  (net 36 "Net-(J1-Pad1)")
  (net 37 D+)
  (net 38 D-)
  (net 39 "Net-(J3-Pad4)")
  (net 40 "Net-(J3-Pad6)")
  (net 41 SOLAR)
  (net 42 "Net-(J7-Pad5)")
  (net 43 "Net-(J7-Pad4)")
  (net 44 RX)
  (net 45 TX)
  (net 46 BOOT0)
  (net 47 MTMS)
  (net 48 MTCK)
  (net 49 MTDO)
  (net 50 MTDI)
  (net 51 "Net-(JP1-Pad1)")
  (net 52 "Net-(Q2-Pad1)")
  (net 53 "Net-(Q2-Pad5)")
  (net 54 "Net-(Q2-Pad2)")
  (net 55 "Net-(Q2-Pad6)")
  (net 56 SCL)
  (net 57 LED_R)
  (net 58 LED_G)
  (net 59 LED_B)
  (net 60 "Net-(R16-Pad2)")
  (net 61 "Net-(R18-Pad2)")
  (net 62 TOUCH7)
  (net 63 BATT_ALARM)
  (net 64 TOUCH8)
  (net 65 "Net-(R23-Pad2)")
  (net 66 "Net-(R24-Pad2)")
  (net 67 TOUCH9)
  (net 68 ACCEL_IRQ)
  (net 69 "Net-(U1-Pad32)")
  (net 70 "Net-(U2-Pad5)")
  (net 71 "Net-(U3-Pad7)")
  (net 72 "Net-(U6-Pad5)")
  (net 73 "Net-(U6-Pad6)")
  (net 74 "Net-(U7-Pad1)")
  (net 75 "Net-(U7-Pad6)")
  (net 76 "Net-(U7-Pad9)")
  (net 77 "Net-(U7-Pad10)")
  (net 78 "Net-(U7-Pad11)")
  (net 79 "Net-(U7-Pad12)")
  (net 80 "Net-(U7-Pad13)")
  (net 81 "Net-(U7-Pad14)")
  (net 82 "Net-(U7-Pad15)")
  (net 83 "Net-(U7-Pad17)")
  (net 84 "Net-(U7-Pad22)")
  (net 85 "Net-(U7-Pad24)")
  (net 86 "Net-(C29-Pad1)")
  (net 87 AUX_RX)
  (net 88 AUX_TX)
  (net 89 AUX_RTS)
  (net 90 AUX_CTS)
  (net 91 "Net-(U5-Pad3)")
  (net 92 "Net-(U5-Pad5)")
  (net 93 "Net-(U5-Pad7)")
  (net 94 "Net-(U7-Pad23)")
  (net 95 B0)
  (net 96 B3)
  (net 97 B1)
  (net 98 B2)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net ACCEL_IRQ)
    (add_net AUX_CTS)
    (add_net AUX_RTS)
    (add_net AUX_RX)
    (add_net AUX_TX)
    (add_net B0)
    (add_net B1)
    (add_net B2)
    (add_net B3)
    (add_net BATT_ALARM)
    (add_net BOOT0)
    (add_net CHARGE)
    (add_net CHARGE_STATUS)
    (add_net D+)
    (add_net D-)
    (add_net DISP_BUSY)
    (add_net DISP_CLK)
    (add_net DISP_CS)
    (add_net DISP_DC)
    (add_net DISP_DIN)
    (add_net DISP_RST)
    (add_net EN)
    (add_net GDR)
    (add_net GND)
    (add_net LED_B)
    (add_net LED_G)
    (add_net LED_R)
    (add_net MTCK)
    (add_net MTDI)
    (add_net MTDO)
    (add_net MTMS)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(Q2-Pad6)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad10)")
    (add_net "Net-(U7-Pad11)")
    (add_net "Net-(U7-Pad12)")
    (add_net "Net-(U7-Pad13)")
    (add_net "Net-(U7-Pad14)")
    (add_net "Net-(U7-Pad15)")
    (add_net "Net-(U7-Pad17)")
    (add_net "Net-(U7-Pad22)")
    (add_net "Net-(U7-Pad23)")
    (add_net "Net-(U7-Pad24)")
    (add_net "Net-(U7-Pad6)")
    (add_net "Net-(U7-Pad9)")
    (add_net RESE)
    (add_net RX)
    (add_net SCL)
    (add_net SOLAR)
    (add_net TOUCH7)
    (add_net TOUCH8)
    (add_net TOUCH9)
    (add_net TX)
    (add_net VGH)
    (add_net VGL)
    (add_net XTAL1)
    (add_net XTAL2)
  )
  (net_class Touch ""
    (clearance 0.7)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
  )
  (module atag-simple:TOUCH_CIRCLE locked (layer B.Cu) (tedit 5E4C6C41)
    (at 170.2 105.5 270)
    (fp_text reference T1 (at 0 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -9.7 90) (layer B.Fab))
    (fp_text user "5/50 spacing" (at 0 -0.25 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 0 -4 270) (size 0.4 0.4) (drill 0.254) (layers *.Cu *.Mask)
      (net 61 "Net-(R18-Pad2)"))
    (pad 1 smd circle (at 0 0 270) (size 9 9) (layers B.Cu)
      (net 61 "Net-(R18-Pad2)") (clearance 1.27))
  )
  (module atag-simple:TOUCH_CIRCLE locked (layer B.Cu) (tedit 5E4C6C41)
    (at 146.5 105.5 90)
    (fp_text reference T2 (at 0 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -9.7 90) (layer B.Fab))
    (fp_text user "5/50 spacing" (at 0 -0.25 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 0 -4 90) (size 0.4 0.4) (drill 0.254) (layers *.Cu *.Mask)
      (net 65 "Net-(R23-Pad2)"))
    (pad 1 smd circle (at 0 0 90) (size 9 9) (layers B.Cu)
      (net 65 "Net-(R23-Pad2)") (clearance 1.27))
  )
  (module atag-simple:TOUCH_CIRCLE locked (layer B.Cu) (tedit 5E4C6C41)
    (at 122.8 105.5)
    (fp_text reference T3 (at 0 0) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -9.7) (layer B.Fab))
    (fp_text user "5/50 spacing" (at 0 -0.25) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 0 -4) (size 0.4 0.4) (drill 0.254) (layers *.Cu *.Mask)
      (net 66 "Net-(R24-Pad2)"))
    (pad 1 smd circle (at 0 0) (size 9 9) (layers B.Cu)
      (net 66 "Net-(R24-Pad2)") (clearance 1.27))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.8 108.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.1 -0.05) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.4 114.7125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.1125 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VGL))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.6 112.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.1 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VGH))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.6 118.2 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.1 0 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.8 103.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.1 0.05) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 157.9 114.7 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.1 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.8 102.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.1 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.9 117.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.1 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 106.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 2.0125 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.4 117.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 22u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 109.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.3125 -0.05) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 108.05 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 2.3 0.05) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C12-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 111.05 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 2.3125 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 112.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 2.3 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C14-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.1125 94.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 2.3 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.9 117.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 2.2875 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 EN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-1608-10_AVX-L (layer F.Cu) (tedit 5B301BBE)
    (at 146.8 96.7 90)
    (descr "Tantalum Capacitor SMD AVX-L (1608-10 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C18 (at -2.4 0 90) (layer F.SilkS))
    (fp_text value 100u (at 0 1.48 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7125 0 90) (size 1.075 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.238095)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7125 0 90) (size 1.075 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.238095)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-1608-10_AVX-L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.3 100 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -2.3 0) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 CHARGE))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.9 114.7 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 114.7 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.2) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 101.7 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 2.3 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.2 103.2 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 2.3 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.5 117.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 12.5p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 XTAL1))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.3 117.8875 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 2.3125 0 90) (layer F.SilkS))
    (fp_text value 12.5p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 XTAL2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 153 96.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C26-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142 109.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at -2.3 0 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C28-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.8 109.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at -2.3 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 162.75 119.1 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -2.95 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VGL))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 162.75 114.4 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at -2.95 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VGH))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 162.75 116.75 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at -2.95 -0.05) (layer F.SilkS))
    (fp_text value D (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117 93.9)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at -2.1 0) (layer F.SilkS))
    (fp_text value RED (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117 92.4)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at -2.1 0) (layer F.SilkS))
    (fp_text value GRN (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117 90.9)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D6 (at -2.1 0) (layer F.SilkS))
    (fp_text value BLU (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module atag-simple:Amphenol_24pin_0.5mm locked (layer F.Cu) (tedit 5D376555)
    (at 172.5 107 90)
    (fp_text reference J1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value "Flex Display" (at 0 -2 90) (layer F.Fab))
    (pad 13 smd rect (at -0.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 DISP_CLK))
    (pad 14 smd rect (at -0.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 DISP_DIN))
    (pad 16 smd rect (at -1.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 15 smd rect (at -1.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 17 smd rect (at -2.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at -2.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (pad 19 smd rect (at -3.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 20 smd rect (at -3.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 21 smd rect (at -4.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 VGH))
    (pad 22 smd rect (at -4.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C14-Pad1)"))
    (pad 23 smd rect (at -5.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VGL))
    (pad 24 smd rect (at -5.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (pad 12 smd rect (at 0.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 DISP_CS))
    (pad 11 smd rect (at 0.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 DISP_DC))
    (pad 10 smd rect (at 1.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 DISP_RST))
    (pad 9 smd rect (at 1.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 DISP_BUSY))
    (pad 8 smd rect (at 2.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at 3.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 3.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C23-Pad1)"))
    (pad 4 smd rect (at 4.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C22-Pad1)"))
    (pad 3 smd rect (at 4.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 RESE))
    (pad 2 smd rect (at 5.25 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 GDR))
    (pad 1 smd rect (at 5.75 -0.5 90) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1-Pad1)"))
    (pad "" smd rect (at -7.4 1.85 90) (size 2 3) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 7.4 1.85 90) (size 2 3) (layers F.Cu F.Paste F.Mask))
  )
  (module atag-simple:BATT_PAD locked (layer F.Cu) (tedit 5D1820F0)
    (at 159.5 93)
    (fp_text reference J2 (at -5.2 -2.25 90) (layer F.SilkS))
    (fp_text value BATT (at 0 -0.5) (layer F.Fab))
    (fp_text user "(+)" (at -2.4 0.9) (layer F.SilkS))
    (fp_text user "(-)" (at 2.6 0.9) (layer F.SilkS))
    (fp_text user GND (at 5.3 -2.25 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.5 -2.25) (size 4 4) (layers F.Cu F.Mask)
      (net 12 +BATT))
    (pad 2 smd rect (at 2.5 -2.25) (size 4 4) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 locked (layer F.Cu) (tedit 5D8620A7)
    (at 153.3 105.5 90)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J3 (at 0 -3.1 270) (layer F.SilkS))
    (fp_text value USB_B_MICRO (at 0 4.6 270) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 270) (layer Dwgs.User))
    (fp_text user %R (at 0 1.2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.46 90) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 14 CHARGE))
    (pad 2 smd rect (at -0.65 -1.46 90) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 37 D+))
    (pad 3 smd rect (at 0 -1.46 90) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 38 D-))
    (pad 4 smd rect (at 0.65 -1.46 90) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.46 90) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.4875 -1.375 90) (size 1.425 1.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 2.4875 -1.375 90) (size 1.425 1.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at -3.375 1.2 90) (size 1.65 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 3.375 1.2 90) (size 1.65 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at -1.15 1.2 90) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 1.55 1.2 90) (size 1 1.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad6)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module atag-simple:SOIC_clipProgSmall locked (layer F.Cu) (tedit 5C59A3E2)
    (at 115.3 123.6)
    (fp_text reference J7 (at 3.3 -0.6 90) (layer F.SilkS))
    (fp_text value "Prog Bite" (at 0.127 1.397) (layer F.Fab))
    (pad 5 smd oval (at -1.905 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 42 "Net-(J7-Pad5)"))
    (pad 4 smd oval (at -1.905 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 43 "Net-(J7-Pad4)"))
    (pad 3 smd oval (at -0.635 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 44 RX))
    (pad 2 smd oval (at 0.635 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 45 TX))
    (pad 1 smd oval (at 1.905 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 13 EN))
    (pad 6 smd oval (at -0.635 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 46 BOOT0))
    (pad 7 smd oval (at 0.635 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 8 smd oval (at 1.905 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 5 +3V3))
    (pad "" np_thru_hole circle (at -2.54 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
  )
  (module atag-simple:SOIC_clipProgSmall locked (layer F.Cu) (tedit 5C59A3E2)
    (at 128.3 123.6)
    (fp_text reference J8 (at -3.065 -0.6 90) (layer F.SilkS))
    (fp_text value "JTag Bite" (at 0.127 1.397) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.54 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 -1.905) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad 8 smd oval (at 1.905 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 47 MTMS))
    (pad 7 smd oval (at 0.635 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 48 MTCK))
    (pad 6 smd oval (at -0.635 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 49 MTDO))
    (pad 1 smd oval (at 1.905 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 5 +3V3))
    (pad 2 smd oval (at 0.635 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd oval (at -0.635 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 4 smd oval (at -1.905 -0.75) (size 0.8 1.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 5 smd oval (at -1.905 -0.75) (size 0.8 1.5) (layers B.Cu B.Mask)
      (net 50 MTDI))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 148.85 96.75 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 2.35 0 180) (layer F.SilkS))
    (fp_text value Jumper_2_Bridged (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 51 "Net-(JP1-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Inductor_SMD:L_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.5 113.9 90)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 2.7 0 180) (layer F.SilkS))
    (fp_text value 68uH (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer F.Cu) (tedit 5A02FF57)
    (at 164.8 99.4 270)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q1 (at 0 1.7 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at -0.05 2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at -1 0.65 180) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 34 RESE))
    (pad 1 smd rect (at -1 -0.65 180) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 35 GDR))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5A02FF57)
    (at 175.95 90.8 270)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference Q2 (at 2.3 0 270) (layer F.SilkS))
    (fp_text value FDG6304P (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Q2-Pad1)"))
    (pad 3 smd rect (at -0.95 0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 SOLAR))
    (pad 5 smd rect (at 0.95 0 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q2-Pad5)"))
    (pad 2 smd rect (at -0.95 0 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q2-Pad2)"))
    (pad 4 smd rect (at 0.95 0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +BATT))
    (pad 6 smd rect (at 0.95 -0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q2-Pad6)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer F.Cu) (tedit 5A02FF57)
    (at 180.8 93.8)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q5 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value SI2102 (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q2-Pad6)"))
    (pad 2 smd rect (at -1 0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 168.2 99.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2 0) (layer F.SilkS))
    (fp_text value 0.47 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 RESE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120 93.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 LED_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120 92.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 LED_G))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120 90.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 LED_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.5 96.6125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.0875 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C26-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 CHARGE_STATUS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 117.4 117.9 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 EN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 168.2 98.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -2.3 0) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 GDR))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.5 96.6125 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -1.9125 0) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 135.9 121.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 2.3 0) (layer F.SilkS))
    (fp_text value 510 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(R18-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 TOUCH7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.4125 89.45 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 2.3125 0.05) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 BATT_ALARM))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 178.25 90.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.3 0 90) (layer F.SilkS))
    (fp_text value 2.2M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SOLAR))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 179.75 90.8 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -1.9 -0.05 180) (layer F.SilkS))
    (fp_text value 2.2M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(Q2-Pad6)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 181.25 90.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 1.25 90) (layer F.SilkS))
    (fp_text value 6.8M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(Q2-Pad6)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.8 113.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 2.3 0) (layer F.SilkS))
    (fp_text value 510 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 TOUCH8))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.8 100.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 2.3 0) (layer F.SilkS))
    (fp_text value 510 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R24-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 TOUCH9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 172.15 90.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at -2.4 0 90) (layer F.SilkS))
    (fp_text value 30M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(Q2-Pad5)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SOLAR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 173.65 90.8 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 2.3 0.05 90) (layer F.SilkS))
    (fp_text value 3.9M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(Q2-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(Q2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Module:ESP32-WROOM-32 locked (layer F.Cu) (tedit 5B5B4654)
    (at 122.9 105.5 90)
    (descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf")
    (tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
    (attr smd)
    (fp_text reference U1 (at -10.2 -12.5) (layer F.SilkS))
    (fp_text value ESP32-WROOM-32 (at 0 11.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user "KEEP-OUT ZONE" (at 0 -19 90) (layer Cmts.User))
    (fp_text user Antenna (at 0 -13 90) (layer Cmts.User))
    (fp_text user "5 mm" (at 11.8 -14.375 90) (layer Cmts.User))
    (fp_text user "5 mm" (at -11.2 -14.375 90) (layer Cmts.User))
    (fp_text user "5 mm" (at 7.8 -19.075) (layer Cmts.User))
    (pad 39 smd rect (at -1 -0.755 90) (size 5 5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -8.5 -8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -8.5 -6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -8.5 -5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 EN))
    (pad 4 smd rect (at -8.5 -4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 BATT_ALARM))
    (pad 5 smd rect (at -8.5 -3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 CHARGE_STATUS))
    (pad 6 smd rect (at -8.5 -1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 ACCEL_IRQ))
    (pad 7 smd rect (at -8.5 -0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 DISP_BUSY))
    (pad 8 smd rect (at -8.5 0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 XTAL1))
    (pad 9 smd rect (at -8.5 1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 XTAL2))
    (pad 10 smd rect (at -8.5 3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 LED_R))
    (pad 11 smd rect (at -8.5 4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 DISP_CS))
    (pad 12 smd rect (at -8.5 5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 TOUCH7))
    (pad 13 smd rect (at -8.5 6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 MTMS))
    (pad 14 smd rect (at -8.5 8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 MTDI))
    (pad 15 smd rect (at -5.715 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -4.445 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 TOUCH8))
    (pad 17 smd rect (at -3.175 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 AUX_RX))
    (pad 18 smd rect (at -1.905 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 AUX_TX))
    (pad 19 smd rect (at -0.635 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 AUX_RTS))
    (pad 20 smd rect (at 0.635 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 AUX_CTS))
    (pad 21 smd rect (at 1.905 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 B0))
    (pad 22 smd rect (at 3.175 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 B1))
    (pad 23 smd rect (at 4.445 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 MTDO))
    (pad 24 smd rect (at 5.715 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 TOUCH9))
    (pad 25 smd rect (at 8.5 8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 BOOT0))
    (pad 26 smd rect (at 8.5 6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 SCL))
    (pad 27 smd rect (at 8.5 5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 DISP_RST))
    (pad 28 smd rect (at 8.5 4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 DISP_DC))
    (pad 29 smd rect (at 8.5 3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 LED_B))
    (pad 30 smd rect (at 8.5 1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 DISP_CLK))
    (pad 31 smd rect (at 8.5 0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 LED_G))
    (pad 32 smd rect (at 8.5 -0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at 8.5 -1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 B2))
    (pad 34 smd rect (at 8.5 -3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 RX))
    (pad 35 smd rect (at 8.5 -4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 TX))
    (pad 36 smd rect (at 8.5 -5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 B3))
    (pad 37 smd rect (at 8.5 -6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 DISP_DIN))
    (pad 38 smd rect (at 8.5 -8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:DFN-10_2x2mm_P0.4mm (layer F.Cu) (tedit 5A0AA2C0)
    (at 137.75 106)
    (descr "10-Lead Plastic DFN (2mm x 2mm)  0.40mm pitch")
    (tags "DFN 10 0.4mm")
    (attr smd)
    (fp_text reference U2 (at 2.05 0 180) (layer F.SilkS))
    (fp_text value MMA8652FCR1 (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 -0.8) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at -0.8 -0.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 SCL))
    (pad 3 smd rect (at -0.8 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 ACCEL_IRQ))
    (pad 4 smd rect (at -0.8 0.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at -0.8 0.8) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at 0.8 0.8) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.8 0.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0.8 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 9 smd rect (at 0.8 -0.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.8 -0.8) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 BOOT0))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-10_2x2mm_P0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module atag-simple:ST_HLGA-10_2.5x2.5mm_P0.6mm_extended (layer F.Cu) (tedit 5D33DF6F)
    (at 140.2 118.2)
    (descr "ST  HLGA, 10 Pin (https://www.st.com/resource/en/datasheet/lps25hb.pdf#page=46), generated with kicad-footprint-generator ipc_lga_layoutBorder_generator.py")
    (tags "ST HLGA LGA")
    (attr smd)
    (fp_text reference U3 (at -1.15 -2.3) (layer F.SilkS))
    (fp_text value LPS25HB (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.175 -0.3) (size 1.05 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at -1.175 0.3) (size 1.05 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 SCL))
    (pad 3 smd roundrect (at -0.6 1.175) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at 0 1.175) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 BOOT0))
    (pad 5 smd roundrect (at 0.6 1.175) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 6 smd roundrect (at 1.175 0.3) (size 1.05 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 7 smd roundrect (at 1.175 -0.3) (size 1.05 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U3-Pad7)"))
    (pad 8 smd roundrect (at 0.6 -1.175) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 0 -1.175) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 10 smd roundrect (at -0.6 -1.175) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/ST_HLGA-10_2.5x2.5mm_P0.6mm_LayoutBorder3x2y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3 (layer F.Cu) (tedit 5A02FF57)
    (at 149.65 91.9 90)
    (descr SOT-89-3)
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference U4 (at 0.45 -2.95 90) (layer F.SilkS))
    (fp_text value MCP1703A-3302_SOT89 (at 0.45 3.25 90) (layer F.Fab))
    (fp_text user %R (at 0.38 0) (layer F.Fab))
    (pad 2 smd trapezoid (at 2.667 0) (size 1.6 0.85) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask)
      (net 12 +BATT))
    (pad 1 smd rect (at -1.48 -1.5) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.3335 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 +BATT))
    (pad 3 smd rect (at -1.48 1.5) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 1.3335 0) (size 2.2 1.84) (layers F.Cu F.Paste F.Mask)
      (net 12 +BATT))
    (pad 2 smd trapezoid (at -0.0762 0 180) (size 1.5 1) (rect_delta 0 0.7 ) (layers F.Cu F.Paste F.Mask)
      (net 12 +BATT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module atag-simple:LC709203F (layer F.Cu) (tedit 5D1AA39F)
    (at 142.55 91.95 90)
    (fp_text reference U6 (at 0 2.75 90) (layer F.SilkS))
    (fp_text value LC709203F (at 0 -2.75 90) (layer F.Fab))
    (pad 1 smd rect (at -0.975 1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.325 1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.325 1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 +BATT))
    (pad 4 smd rect (at 0.975 1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 63 BATT_ALARM))
    (pad 5 smd rect (at 0.975 -1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U6-Pad5)"))
    (pad 6 smd rect (at 0.325 -1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U6-Pad6)"))
    (pad 7 smd rect (at -0.325 -1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 46 BOOT0))
    (pad 8 smd rect (at -0.975 -1.8 90) (size 0.35 0.7) (layers F.Cu F.Paste F.Mask)
      (net 56 SCL))
    (pad "" smd rect (at 0 0 90) (size 1.96 2.56) (layers F.Cu F.Paste F.Mask))
  )
  (module Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm (layer F.Cu) (tedit 5C1FD453)
    (at 145.4 112.6 180)
    (descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U7 (at -2.1 -3.05) (layer F.SilkS))
    (fp_text value CP2104 (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 25 smd roundrect (at 0 0 180) (size 2.6 2.6) (layers F.Cu F.Mask) (roundrect_rratio 0.096154)
      (net 2 GND))
    (pad "" smd roundrect (at -0.65 -0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad 1 smd roundrect (at -1.9375 -1.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(U7-Pad1)"))
    (pad 2 smd roundrect (at -1.9375 -0.75 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 smd roundrect (at -1.9375 -0.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 D+))
    (pad 4 smd roundrect (at -1.9375 0.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 D-))
    (pad 5 smd roundrect (at -1.9375 0.75 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(C29-Pad1)"))
    (pad 6 smd roundrect (at -1.9375 1.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U7-Pad6)"))
    (pad 7 smd roundrect (at -1.25 1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 CHARGE))
    (pad 8 smd roundrect (at -0.75 1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 CHARGE))
    (pad 9 smd roundrect (at -0.25 1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U7-Pad9)"))
    (pad 10 smd roundrect (at 0.25 1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U7-Pad10)"))
    (pad 11 smd roundrect (at 0.75 1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U7-Pad11)"))
    (pad 12 smd roundrect (at 1.25 1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(U7-Pad12)"))
    (pad 13 smd roundrect (at 1.9375 1.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(U7-Pad13)"))
    (pad 14 smd roundrect (at 1.9375 0.75 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U7-Pad14)"))
    (pad 15 smd roundrect (at 1.9375 0.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U7-Pad15)"))
    (pad 16 smd roundrect (at 1.9375 -0.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C28-Pad1)"))
    (pad 17 smd roundrect (at 1.9375 -0.75 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(U7-Pad17)"))
    (pad 18 smd roundrect (at 1.9375 -1.25 180) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 AUX_RTS))
    (pad 19 smd roundrect (at 1.25 -1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 AUX_CTS))
    (pad 20 smd roundrect (at 0.75 -1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 AUX_TX))
    (pad 21 smd roundrect (at 0.25 -1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 AUX_RX))
    (pad 22 smd roundrect (at -0.25 -1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(U7-Pad22)"))
    (pad 23 smd roundrect (at -0.75 -1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(U7-Pad23)"))
    (pad 24 smd roundrect (at -1.25 -1.9375 180) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(U7-Pad24)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm (layer F.Cu) (tedit 5D24C08C)
    (at 124.4 117.6)
    (descr "SMD Crystal MicroCrystal CC7V-T1A/CM7V-T1A series https://www.microcrystal.com/fileadmin/Media/Products/32kHz/Datasheet/CC7V-T1A.pdf, 3.2x1.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 1.6) (layer F.SilkS))
    (fp_text value "32.768 kHz" (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 XTAL1))
    (pad 2 smd rect (at 1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 19 XTAL2))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module atag-simple:QFN-12-1EP_2x2mm_P0.4mm_EP1.45x1.45mm (layer F.Cu) (tedit 5DE95C31)
    (at 159.1 96.7 90)
    (descr "QFN, 12 Pin (https://ww2.minicircuits.com/case_style/DQ1225.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U5 (at 0 2.2 270) (layer F.SilkS))
    (fp_text value CPC4053QN (at 0 2.82 90) (layer F.Fab))
    (fp_text user %R (at 0 -4 90) (layer F.Fab))
    (pad 13 smd roundrect (at 0 0 90) (size 1.2 1.2) (layers F.Cu F.Mask) (roundrect_rratio 0.172)
      (net 2 GND))
    (pad "" smd roundrect (at -0.3 -0.3 90) (size 0.5 0.5) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.3 0.3 90) (size 0.5 0.5) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.3 -0.3 90) (size 0.5 0.5) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.3 0.3 90) (size 0.5 0.5) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.2 -0.4 90) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C26-Pad1)"))
    (pad 2 smd roundrect (at -1.2 0 90) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 CHARGE))
    (pad 3 smd roundrect (at -1.2 0.4 90) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(U5-Pad3)"))
    (pad 4 smd roundrect (at -0.4 1.2 90) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at 0 1.2 90) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(U5-Pad5)"))
    (pad 6 smd roundrect (at 0.4 1.2 90) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 7 smd roundrect (at 1.2 0.4 90) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(U5-Pad7)"))
    (pad 8 smd roundrect (at 1.2 0 90) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +BATT))
    (pad 9 smd roundrect (at 1.2 -0.4 90) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +BATT))
    (pad 10 smd roundrect (at 0.4 -1.2 90) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 CHARGE_STATUS))
    (pad 11 smd roundrect (at 0 -1.2 90) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at -0.4 -1.2 90) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-12-1EP_3x3mm_P0.51mm_EP1.45x1.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module atag-simple:SOLAR_PAD locked (layer F.Cu) (tedit 5E48AE77)
    (at 168.15 90.8)
    (fp_text reference J4 (at 2.85 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.05) (size 4 4) (layers F.Cu F.Mask)
      (net 41 SOLAR))
  )
  (module atag-simple:SOLAR_PAD locked (layer F.Cu) (tedit 5E48AE77)
    (at 125.4 90.8)
    (fp_text reference J5 (at -2.7 -1 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.05) (size 4 4) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 131.3 92.4 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J6 (at -2.1 2.5 180) (layer F.SilkS))
    (fp_text value Conn_02x03_Counter_Clockwise (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 B0))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 B2))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 B1))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 B3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 134 118 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at -2.3 0 180) (layer F.SilkS))
    (fp_text value Jumper_2_Open (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 64 TOUCH8) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 48 MTCK) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (gr_text "ATag Simple 2" (at 154.2 121.8) (layer F.SilkS))
  (gr_circle (center 142.983095 117.4) (end 143.483095 117.7) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.9 100.4) (end 156.9 99.4) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 160.4 100.4) (end 161.4 100.4) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 160.4 110.6) (end 160.4 111.6) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.9 110.6) (end 155.9 110.6) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.9 111.6) (end 160.4 111.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161.4 100.4) (end 161.4 110.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.9 99.4) (end 160.4 99.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155.9 110.6) (end 155.9 100.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 185 98.5) (end 185 115.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 186 115.5) (end 185 115.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 186 98.5) (end 186 97.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 186 116.5) (end 186 124) (layer Edge.Cuts) (width 0.05))
  (gr_text BATTERY (at 159.5 88.1) (layer F.SilkS))
  (gr_text SOLAR (at 168.2 88.1) (layer F.SilkS))
  (gr_text "(+)" (at 168.1 93.9) (layer F.SilkS))
  (gr_text "(-)" (at 125.4 93.9) (layer F.SilkS))
  (gr_text SOLAR (at 125.4 88.1) (layer F.SilkS))
  (gr_text JTAG (at 132.8 123) (layer F.SilkS))
  (gr_text PROG (at 110.4 122.8) (layer F.SilkS))
  (gr_line (start 113.45 113.85) (end 107 113.85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.45 97.15) (end 113.45 113.85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107 97.15) (end 113.45 97.15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107 97.15) (end 107 87) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107 124) (end 107 113.85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 186 124) (end 107 124) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 186 87) (end 186 97.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107 87) (end 186 87) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 186 124) (xy 107 124) (xy 107 87) (xy 186 87)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 186 124) (xy 107 124) (xy 107 87) (xy 186 87)
      )
    )
  )
  (zone (net 12) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 166 88.4) (xy 159 88.4) (xy 159 93.2) (xy 170.6 93.2) (xy 171.4 92.4)
        (xy 174.4 92.4) (xy 174.4 91.5) (xy 176.4 91.5) (xy 176.4 95.4) (xy 175.7 96.1)
        (xy 155.4 96.1) (xy 155.4 94.9) (xy 151.8 94.9) (xy 151.8 92.5) (xy 147.5 92.5)
        (xy 147.5 94.1) (xy 146.7 94.9) (xy 143.6 94.9) (xy 143.6 94.1) (xy 144.7 94.1)
        (xy 144.7 87) (xy 166 87)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 141.5 95.3) (xy 146 95.3) (xy 146 97) (xy 150.4 97) (xy 150.4 99.1)
        (xy 149.5 100) (xy 141.6 100) (xy 137.4 95.9) (xy 137.4 94.7) (xy 138.2 94.7)
        (xy 139.3 93.6) (xy 141.5 93.6)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 139.7 118) (xy 137.4 118) (xy 137.4 117.7) (xy 136.3 117.7) (xy 136.3 115.1)
        (xy 139.7 115.1)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 143.5 121.1) (xy 140.7 121.1) (xy 140.7 118.3) (xy 143.5 118.3)
      )
    )
  )
  (zone (net 41) (net_name SOLAR) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 176.6 90.1) (xy 174.4 90.1) (xy 174.4 89.2) (xy 172.5 89.2) (xy 172.5 90.3)
        (xy 171.4 90.3) (xy 171.4 91.9) (xy 170.6 92.7) (xy 166.3 92.7) (xy 166.3 87)
        (xy 176.6 87)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 165.7 92.6) (xy 160.1 92.6) (xy 160.1 88.9) (xy 165.7 88.9)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 129.1 92.6) (xy 123.5 92.6) (xy 123.5 88.9) (xy 129.1 88.9)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 186 124) (xy 107 124) (xy 107 87) (xy 186 87)
      )
    )
  )
)
