(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 67)
    (no_connects 0)
    (area 124.03 59.655 176.425 113.525)
    (thickness 1.6)
    (drawings 43)
    (tracks 350)
    (zones 0)
    (modules 29)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.27 4.191)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(JP1-Pad1)")
  (net 4 "Net-(JP2-Pad2)")
  (net 5 RAW)
  (net 6 D2)
  (net 7 "Net-(IC1-Pad28)")
  (net 8 "Net-(IC1-Pad27)")
  (net 9 TX)
  (net 10 RX)
  (net 11 D3)
  (net 12 D5)
  (net 13 D6)
  (net 14 ss)
  (net 15 MOSI)
  (net 16 MISO)
  (net 17 SCK)
  (net 18 A0)
  (net 19 A1)
  (net 20 A4)
  (net 21 A5)
  (net 22 Reset)
  (net 23 "Net-(C3-Pad1)")
  (net 24 "Net-(ANT1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A4)
    (add_net A5)
    (add_net D2)
    (add_net D3)
    (add_net D5)
    (add_net D6)
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net RX)
    (add_net Reset)
    (add_net TX)
  )
  (net_class Big ""
    (clearance 0.3)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad2)")
  )
  (net_class RAW ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net RAW)
  )
  (net_class SPI ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net MISO)
    (add_net MOSI)
    (add_net SCK)
    (add_net ss)
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow_Oval (layer F.Cu) (tedit 59BD6172)
    (at 150.33 75.28)
    (descr "TO-92 leads molded, narrow, oval pads, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "Voltage Reg." (at 1.31 -3.32) (layer F.SilkS))
    (fp_text value "" (at 0 3 180) (layer F.Fab))
    (fp_text user "" (at 0 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -0.28 0.58 45) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole circle (at 2.8 0.59 45) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 591422AC)
    (at 172.31 63.93)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value "" (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 591422AC)
    (at 127.21 108.95)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value "" (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 591422AC)
    (at 155.09 86.33)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value "" (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 59501084)
    (at 143.29 71.51)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 0,1uF (at 1.41 3.53) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 59501087)
    (at 145.8 65.86 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 10uF (at 1.2 3.5 180) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5950107E)
    (at 157.3 72.92)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference "" (at 0 -2.33) (layer F.SilkS))
    (fp_text value "" (at 0 4.87) (layer F.Fab))
    (fp_text user "" (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5950107C)
    (at 160.92 72.91)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference "" (at 0 -2.33) (layer F.SilkS))
    (fp_text value "" (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5914230F)
    (at 127.29 104.17 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference RAW (at 1.95 -0.35 270) (layer F.SilkS))
    (fp_text value "" (at 0 4.87 180) (layer F.Fab))
    (fp_text user "" (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RAW))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:MYSX_2.4 (layer F.Cu) (tedit 591410F1)
    (at 135.9 90.64)
    (descr "Through hole pin header")
    (tags "pin header MYSX 2.4")
    (fp_text reference MysX (at 0 -3.302) (layer F.SilkS))
    (fp_text value MYSX_2.4 (at 7.04 15.11 90) (layer F.SilkS))
    (fp_text user 2.4 (at 3.27 -3.3) (layer F.SilkS))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 A1))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 A0))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 A4))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 A5))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 D6))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 D5))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 D2))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 D3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 RAW))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 TX))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 RX))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 Reset))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 595011C4)
    (at 166.85 67.62 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 595011FA)
    (at 140.09 65.71 270)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference "" (at 1.07 13.97 360) (layer F.SilkS))
    (fp_text value "" (at 2.24 12.29 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.4 2 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 D2))
    (pad 3 smd rect (at -1.4 4 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.4 6 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.4 8 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.4 10 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.4 12 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -1.4 14 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd rect (at 18.3 14 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 18.3 12 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(ANT1-Pad1)"))
    (pad 11 smd rect (at 18.3 10 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 18.3 8 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 SCK))
    (pad 13 smd rect (at 18.3 6 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 MISO))
    (pad 14 smd rect (at 18.3 4 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 MOSI))
    (pad 15 smd rect (at 18.3 2 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 ss))
    (pad 16 smd rect (at 18.3 0 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 59136C00)
    (at 153.78 95.95 270)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference Arduino (at -14.17 -0.2 360) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0 270) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad28)"))
    (pad 27 thru_hole oval (at 7.62 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad27)"))
    (pad 1 thru_hole oval (at -13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 TX))
    (pad 2 thru_hole oval (at -11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 RX))
    (pad 3 thru_hole oval (at -8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 Reset))
    (pad 4 thru_hole oval (at -6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 D2))
    (pad 6 thru_hole oval (at -1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 D3))
    (pad 7 thru_hole oval (at 1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 D5))
    (pad 9 thru_hole oval (at 6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 D6))
    (pad 10 thru_hole oval (at 8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 ss))
    (pad 14 thru_hole oval (at 11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 A0))
    (pad 18 thru_hole oval (at 1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 A1))
    (pad 19 thru_hole oval (at -1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole oval (at -3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole oval (at -6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at -11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at -2.54 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 A4))
    (pad 26 thru_hole oval (at -5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 A5))
    (pad 27 thru_hole oval (at 13.97 -5.08 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 13.97 -2.54 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad28)"))
    (pad 29 thru_hole oval (at 13.97 0 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 591422E5)
    (at 131.56 99.71 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "D3 Resistor" (at 5.1 0.6 270) (layer F.SilkS))
    (fp_text value "" (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 D3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5950104F)
    (at 168.28 73.17)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 0,1uF (at 4.89 0.17 90) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-footprints:SMA_EDGE (layer F.Cu) (tedit 592EF4BD)
    (at 124.58 89.79 270)
    (fp_text reference SMA (at 3.6 -1.2 360) (layer F.SilkS))
    (fp_text value "" (at 0 -6.35 270) (layer F.SilkS))
    (pad 2 smd rect (at -2.1463 -2.0955 270) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 270) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -1.8415 270) (size 1.27 3.683) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(ANT1-Pad1)"))
    (pad 2 smd rect (at -2.1463 -2.0955 270) (size 1.27 4.191) (layers B.Cu F.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 270) (size 1.27 4.191) (layers B.Cu F.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 59501075)
    (at 170.27 87.02 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference 0,1uF (at -2.52 0.03 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.56 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A0))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59501059)
    (at 165.29 93.96 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59501047)
    (at 127.59 89.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference Antenna (at 3.9 0.51 180) (layer F.SilkS))
    (fp_text value "" (at 0 2.33) (layer F.Fab))
    (fp_text user "" (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(ANT1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5950105C)
    (at 165.3 96.87 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5950105E)
    (at 165.29 102.71 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59501061)
    (at 165.28 105.67 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59501069)
    (at 165.3 99.78 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 59501078)
    (at 165.3 79.21)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 1MΩ (at 3.78 3.27) (layer F.SilkS))
    (fp_text value "" (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A0))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 59501070)
    (at 165.3 82.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 470kΩ (at 3.76 -3.17) (layer F.SilkS))
    (fp_text value "" (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(JP2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A0))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module graphicslogo:OpenSourceLogo_1000x1000_neg (layer F.Cu) (tedit 59136AF5)
    (at 152.48 97.46)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 591422A6)
    (at 165.29 108.65 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 591422AC)
    (at 172.12 109.15)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value "" (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module ASKicadLib:3_block_Screw_Terminal (layer F.Cu) (tedit 59BD5C48)
    (at 155.52 66.48)
    (fp_text reference "" (at -5.28 2.86) (layer F.SilkS))
    (fp_text value "" (at 0.18 -5.55) (layer F.Fab))
    (pad 3 thru_hole circle (at 4.81 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 1 thru_hole circle (at -5 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text "Antenna Trace\n9,495mm" (at 128.47 80.83) (layer F.SilkS))
  (gr_text "Out Gnd In" (at 169 69.64) (layer F.SilkS))
  (gr_text GND (at 163.4 96.8 90) (layer F.SilkS))
  (gr_text 3.3V (at 163.39 93.92 90) (layer F.SilkS))
  (gr_text "VOut Gnd VIn" (at 151.24 77.7) (layer F.SilkS))
  (gr_text "REG  BAT" (at 159.27 77.72) (layer F.SilkS))
  (gr_text ">3.3V   Gnd  <=3.3V\n" (at 155.39 63.51) (layer F.SilkS))
  (gr_text "3.3V 8mhz" (at 154.03 84.26) (layer F.SilkS))
  (gr_text "Pro Mini" (at 153.85 83.08) (layer F.SilkS))
  (gr_text openhardware.io (at 133.02 78.49) (layer F.SilkS))
  (gr_text openhardware.io (at 152.48 103.21) (layer F.SilkS))
  (gr_text "by sundberg84" (at 152.49 93.16) (layer F.SilkS))
  (gr_text "Easy PCB" (at 152.62 91.72) (layer F.SilkS))
  (gr_text "Licensed under \nCERN OHL v.1.2" (at 133.17 76.38) (layer F.SilkS))
  (gr_text "RFM69 Edition" (at 132.97 74.13) (layer F.SilkS))
  (gr_text "Rev 9" (at 133.09 72.1) (layer F.SilkS))
  (gr_text "Easy PCB" (at 133.01 69.93) (layer F.SilkS))
  (gr_text "(MysX)" (at 125.25 101.56 90) (layer F.SilkS))
  (gr_text "A1 A4 D6 D2 GND RX GND 3,3" (at 141.58 99.21 90) (layer F.SilkS))
  (gr_text "A0 A5 D5 D3 RST TX VCC Raw" (at 140.47 99.32 90) (layer F.SilkS))
  (gr_text Extra (at 168.98 91.42) (layer F.SilkS))
  (gr_text "Bat. measurer" (at 168.93 76.84) (layer F.SilkS))
  (gr_text Temp/Hum (at 132.1 104.75 90) (layer F.SilkS))
  (gr_text Antenna (at 126.84 94.31) (layer F.SilkS))
  (gr_text " DIY " (at 130.19 89.43) (layer F.SilkS))
  (gr_text Booster (at 167.19 64.8) (layer F.SilkS))
  (gr_line (start 124.64 111.54) (end 124.64 61.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.51 111.54) (end 124.64 111.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.51 61.61) (end 174.51 111.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.55 61.61) (end 174.51 61.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.05 60.97) (xy 141.32 61.02) (xy 141.21 86.39) (xy 124.05 86.39)
      )
    )
  )
)
