(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 13)
    (zones 0)
    (modules 8)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_7fffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative true)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror true)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/Users/ikorin/Desktop/"))
  )
  (net 0 "")
  (net 1 "Net-(Q1-Pad2)")
  (net 2 "Net-(Q1-Pad3)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 108 85)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 80 85)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 108 61)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 80 61)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 92.775068 81.395024 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 330 (at -0.004976 -1.975068 270) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.65 270) (layer B.Fab) hide)
    (fp_text user %R (at -0.5 -2 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Thirdparty:B5B-ZR (layer F.Cu) (tedit 5D213A09)
    (at 94.210001 85)
    (fp_text reference B5B-ZR (at 7.789999 0.2) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 0 5.15) (layer F.Fab) hide)
    (fp_text user %R (at 6.789999 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.95 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -1.45 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 0.05 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 1.55 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 3.05 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad5)"))
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 86 80 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference 2N2222 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sensor:piD-TECH_eVx (layer F.Cu) (tedit 5CFEC1B8)
    (at 94.286302 66.831107 270)
    (fp_text reference eVx (at 0 11.786302 90) (layer F.SilkS))
    (fp_text value Pid-Tech_eVx (at -0.260001 -7.739999 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.38 -2.54 270) (size 4 4) (drill 2.49) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 2 thru_hole circle (at 4.24 0 270) (size 4 4) (drill 2.49) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at -3.38 2.54 270) (size 4 4) (drill 2.49) (layers *.Cu *.Mask)
      (net 2 "Net-(Q1-Pad3)"))
    (model ":Personal 3D Models:piD-TECH eVx.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (gr_text NC (at 95.8 86.3) (layer B.SilkS))
  (gr_text EN (at 92.7 86.3) (layer B.SilkS))
  (gr_text OUT (at 94.3 86.3) (layer B.SilkS))
  (gr_text 5V (at 97.3 86.3) (layer B.SilkS))
  (gr_text GND (at 91.3 86.3) (layer B.SilkS))
  (gr_text "@ikorin\n2019" (at 80 72 90) (layer F.SilkS))
  (gr_text "VOC Sensor\nv0.1" (at 108 73 -90) (layer F.SilkS))
  (gr_line (start 76 89) (end 76 56) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 112 89) (end 76 89) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 112 56) (end 112 89) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 76 56) (end 112 56) (layer Edge.Cuts) (width 0.12))
)
