(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 414)
    (zones 0)
    (modules 107)
    (nets 65)
  )
  (page A4)
  (title_block
    (title "ASPERA GSE")
    (date 2024-05-05)
    (rev 1.0)
    (comment 1 "S/C POWER BUS SIMULATOR")
    (comment 2 ASPERA-UA-DWG-000xx_Power)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Q14-Pad2)")
  (net 2 "Net-(Q14-Pad3)")
  (net 3 GND)
  (net 4 "Net-(Q12-Pad3)")
  (net 5 "Net-(Q12-Pad2)")
  (net 6 "Net-(Q10-Pad2)")
  (net 7 "Net-(Q10-Pad3)")
  (net 8 "Net-(Q8-Pad3)")
  (net 9 "Net-(Q8-Pad2)")
  (net 10 "Net-(Q6-Pad2)")
  (net 11 "Net-(Q6-Pad3)")
  (net 12 "Net-(Q4-Pad3)")
  (net 13 "Net-(Q4-Pad2)")
  (net 14 "Net-(Q2-Pad2)")
  (net 15 "Net-(Q2-Pad3)")
  (net 16 "/Power Box Top/+3.3V")
  (net 17 "/Power Box Top/+12V_BUS")
  (net 18 "Net-(Q16-Pad2)")
  (net 19 "Net-(Q16-Pad3)")
  (net 20 "Net-(C5-Pad2)")
  (net 21 "/Power Box Top/MCP.PWR")
  (net 22 "/Power Box Top/+28V_BUS")
  (net 23 "/Power Box Top/SHTR2.PWR")
  (net 24 "Net-(C10-Pad2)")
  (net 25 "Net-(C6-Pad2)")
  (net 26 "/Power Box Top/HVPS1.PWR")
  (net 27 "/Power Box Top/HVPS2.PWR")
  (net 28 "Net-(C7-Pad2)")
  (net 29 "Net-(C4-Pad2)")
  (net 30 "/Power Box Top/MISC.PWR")
  (net 31 "/Power Box Top/Heater.PWR")
  (net 32 "Net-(C8-Pad2)")
  (net 33 "Net-(C9-Pad2)")
  (net 34 "/Power Box Top/SHTR1.PWR")
  (net 35 "/Power Box Top/POBC.PWR")
  (net 36 "Net-(C3-Pad2)")
  (net 37 "Net-(D8-Pad2)")
  (net 38 "Net-(D2-Pad2)")
  (net 39 "Net-(D3-Pad2)")
  (net 40 "Net-(D1-Pad2)")
  (net 41 "Net-(D4-Pad2)")
  (net 42 "Net-(D5-Pad2)")
  (net 43 "Net-(D6-Pad2)")
  (net 44 "Net-(D7-Pad2)")
  (net 45 "/Power Box Top/Power Switch: HVPS2/Vctl")
  (net 46 "/Power Box Top/HVPS2.CTL")
  (net 47 "/Power Box Top/POBC.CTL")
  (net 48 "/Power Box Top/Power Switch: POBC/Vctl")
  (net 49 "/Power Box Top/Power Switch: HEATER/Vctl")
  (net 50 "/Power Box Top/Heater.CTL")
  (net 51 "/Power Box Top/SHTR1.CTL")
  (net 52 "/Power Box Top/Power Switch: SHTR1/Vctl")
  (net 53 "/Power Box Top/Power Switch: SHTR2/Vctl")
  (net 54 "/Power Box Top/SHTR2.CTL")
  (net 55 "/Power Box Top/HVPS1.CTL")
  (net 56 "/Power Box Top/Power Switch: HVPS1/Vctl")
  (net 57 "/Power Box Top/Power Switch: MCP/Vctl")
  (net 58 "/Power Box Top/MCP.CTL")
  (net 59 "/Power Box Top/MISC.CTL")
  (net 60 "/Power Box Top/Power Switch: MISC/Vctl")
  (net 61 "Net-(J2-Pad0)")
  (net 62 "Net-(J1-Pad0)")
  (net 63 "Net-(X2-Pad1)")
  (net 64 "Net-(X1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/Power Box Top/+3.3V")
    (add_net "/Power Box Top/HVPS1.CTL")
    (add_net "/Power Box Top/HVPS2.CTL")
    (add_net "/Power Box Top/Heater.CTL")
    (add_net "/Power Box Top/MCP.CTL")
    (add_net "/Power Box Top/MISC.CTL")
    (add_net "/Power Box Top/POBC.CTL")
    (add_net "/Power Box Top/Power Switch: HEATER/Vctl")
    (add_net "/Power Box Top/Power Switch: HVPS1/Vctl")
    (add_net "/Power Box Top/Power Switch: HVPS2/Vctl")
    (add_net "/Power Box Top/Power Switch: MCP/Vctl")
    (add_net "/Power Box Top/Power Switch: MISC/Vctl")
    (add_net "/Power Box Top/Power Switch: POBC/Vctl")
    (add_net "/Power Box Top/Power Switch: SHTR1/Vctl")
    (add_net "/Power Box Top/Power Switch: SHTR2/Vctl")
    (add_net "/Power Box Top/SHTR1.CTL")
    (add_net "/Power Box Top/SHTR2.CTL")
    (add_net GND)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J2-Pad0)")
    (add_net "Net-(Q10-Pad2)")
    (add_net "Net-(Q10-Pad3)")
    (add_net "Net-(Q12-Pad2)")
    (add_net "Net-(Q12-Pad3)")
    (add_net "Net-(Q14-Pad2)")
    (add_net "Net-(Q14-Pad3)")
    (add_net "Net-(Q16-Pad2)")
    (add_net "Net-(Q16-Pad3)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(Q6-Pad3)")
    (add_net "Net-(Q8-Pad2)")
    (add_net "Net-(Q8-Pad3)")
    (add_net "Net-(X1-Pad1)")
    (add_net "Net-(X2-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/Power Box Top/+12V_BUS")
    (add_net "/Power Box Top/+28V_BUS")
    (add_net "/Power Box Top/HVPS1.PWR")
    (add_net "/Power Box Top/HVPS2.PWR")
    (add_net "/Power Box Top/Heater.PWR")
    (add_net "/Power Box Top/MCP.PWR")
    (add_net "/Power Box Top/MISC.PWR")
    (add_net "/Power Box Top/POBC.PWR")
    (add_net "/Power Box Top/SHTR1.PWR")
    (add_net "/Power Box Top/SHTR2.PWR")
  )
  (module holes:HOLE_3.5mm_connected (layer F.Cu) (tedit 5A486E14)
    (at 79 131.5)
    (fp_text reference X1 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 64 "Net-(X1-Pad1)"))
  )
  (module holes:HOLE_3.5mm_connected (layer F.Cu) (tedit 5A486E14)
    (at 147.5 131.5)
    (fp_text reference X2 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 63 "Net-(X2-Pad1)"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 52 66)
    (fp_text reference JJ14 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 52 102.8)
    (fp_text reference JJ16 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 52 84.7)
    (fp_text reference JJ13 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 52 81.9)
    (fp_text reference JJ12 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 52 99.5)
    (fp_text reference JJ11 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 100.6 132.5)
    (fp_text reference JJ15 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 168 98.8)
    (fp_text reference JJ2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 168 80.5)
    (fp_text reference JJ1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 168 102.2)
    (fp_text reference JJ3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
  )
  (module Daves_footprints:HOLE_22ga (layer F.Cu) (tedit 6639A643)
    (at 168 116.8)
    (fp_text reference JJ4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Jumper_hole (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 103.71 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at -3.8 0.09 180) (layer B.SilkS))
    (fp_text value YELLOW (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Yellow.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 141.42 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW2 (at 4.9 -0.02 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/Power Box Top/MISC.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/Power Box Top/Power Switch: MISC/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 128.85 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW3 (at 4.9 0.05 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/Power Box Top/MCP.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/Power Box Top/Power Switch: MCP/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 116.28 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW4 (at 4.9 -0.08 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/Power Box Top/HVPS1.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/Power Box Top/Power Switch: HVPS1/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 66 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW8 (at -4.9 -0.1 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/Power Box Top/SHTR2.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/Power Box Top/Power Switch: SHTR2/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 78.57 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW7 (at 4.9 -0.07 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/Power Box Top/SHTR1.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/Power Box Top/Power Switch: SHTR1/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 91.14 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW6 (at 4.9 -0.04 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/Power Box Top/Heater.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/Power Box Top/Power Switch: HEATER/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 153.99 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW1 (at 4.9 0.01 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/Power Box Top/POBC.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/Power Box Top/Power Switch: POBC/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Toggle_Switch_SPST_200MSP3T4B7M2QE (layer B.Cu) (tedit 663887EA)
    (at 103.71 101.5 90)
    (descr http://spec_sheets.e-switch.com/specs/T111597.pdf)
    (fp_text reference SW5 (at 4.9 -0.01 180) (layer B.SilkS))
    (fp_text value SW_SPDT_MSM (at -0.05 -4.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/Power Box Top/HVPS2.CTL"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/Power Box Top/Power Switch: HVPS2/Vctl"))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (model ${KISYS3DMOD}/Dave.3dshapes/200MSPxT4B7M2xE_stp_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 78.57 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D7 (at -3.8 0.03 180) (layer B.SilkS))
    (fp_text value GREEN (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Green.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 66 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D8 (at -3.8 -1.2 180) (layer B.SilkS))
    (fp_text value GREEN (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Green.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 91.14 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at -3.8 -0.04 180) (layer B.SilkS))
    (fp_text value GREEN (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Green.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 116.28 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D4 (at -3.8 0.02 180) (layer B.SilkS))
    (fp_text value YELLOW (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Yellow.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 128.85 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at -3.8 0.05 180) (layer B.SilkS))
    (fp_text value GREEN (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Green.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 141.42 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at -3.8 0.08 180) (layer B.SilkS))
    (fp_text value GREEN (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Green.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:LED_T1_3-4 (layer B.Cu) (tedit 6638ED4D)
    (at 153.99 77 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at -3.8 0.01 180) (layer B.SilkS))
    (fp_text value GREEN (at 0 -3.96 90) (layer B.Fab))
    (fp_text user %R (at -0.02 0 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/LED_T1_3_4_Green.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:5747841-3 (layer F.Cu) (tedit 6638E163)
    (at 86 50)
    (fp_text reference J1 (at 0 14.45) (layer F.SilkS))
    (fp_text value DB15_Male (at -0.3 3.3) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 0 thru_hole circle (at 16.65 9.52) (size 5 5) (drill 3.302) (layers *.Cu *.Mask)
      (net 62 "Net-(J1-Pad0)"))
    (pad 0 thru_hole circle (at -16.65 9.52) (size 5 5) (drill 3.18) (layers *.Cu *.Mask)
      (net 62 "Net-(J1-Pad0)"))
    (pad 9 thru_hole circle (at 8.3058 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole circle (at 5.5372 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole circle (at 2.7686 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 12 thru_hole circle (at 0 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole circle (at -2.7686 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole circle (at -5.5372 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 15 thru_hole circle (at -8.3058 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 9.6901 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 47 "/Power Box Top/POBC.CTL"))
    (pad 2 thru_hole circle (at 6.9215 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 59 "/Power Box Top/MISC.CTL"))
    (pad 3 thru_hole circle (at 4.1529 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 58 "/Power Box Top/MCP.CTL"))
    (pad 4 thru_hole circle (at 1.3843 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 55 "/Power Box Top/HVPS1.CTL"))
    (pad 5 thru_hole circle (at -1.3843 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 46 "/Power Box Top/HVPS2.CTL"))
    (pad 6 thru_hole circle (at -4.1529 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 50 "/Power Box Top/Heater.CTL"))
    (pad 7 thru_hole circle (at -6.9215 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 51 "/Power Box Top/SHTR1.CTL"))
    (pad 8 thru_hole circle (at -9.6901 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 54 "/Power Box Top/SHTR2.CTL"))
    (model ${KISYS3DMOD}/Dave.3dshapes/C-5747841-3.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:5747845-4 (layer F.Cu) (tedit 66388C24)
    (at 134 50)
    (fp_text reference J2 (at 0 14.45) (layer F.SilkS))
    (fp_text value DB15_Female_MountingHoles (at -0.3 3.3) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 0 thru_hole circle (at 16.65 9.52) (size 5 5) (drill 3.302) (layers *.Cu *.Mask)
      (net 61 "Net-(J2-Pad0)"))
    (pad 0 thru_hole circle (at -16.65 9.52) (size 5 5) (drill 3.18) (layers *.Cu *.Mask)
      (net 61 "Net-(J2-Pad0)"))
    (pad 15 thru_hole circle (at 8.3058 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole circle (at 5.5372 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole circle (at 2.7686 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 12 thru_hole circle (at 0 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole circle (at -2.7686 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole circle (at -5.5372 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole circle (at -8.3058 8.1) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole circle (at 9.6901 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 35 "/Power Box Top/POBC.PWR"))
    (pad 7 thru_hole circle (at 6.9215 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 30 "/Power Box Top/MISC.PWR"))
    (pad 6 thru_hole circle (at 4.1529 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 21 "/Power Box Top/MCP.PWR"))
    (pad 5 thru_hole circle (at 1.3843 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 26 "/Power Box Top/HVPS1.PWR"))
    (pad 4 thru_hole circle (at -1.3843 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 27 "/Power Box Top/HVPS2.PWR"))
    (pad 3 thru_hole circle (at -4.1529 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 31 "/Power Box Top/Heater.PWR"))
    (pad 2 thru_hole circle (at -6.9215 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 34 "/Power Box Top/SHTR1.PWR"))
    (pad 1 thru_hole rect (at -9.6901 10.94) (size 1.651 1.651) (drill 1.04) (layers *.Cu *.Mask)
      (net 23 "/Power Box Top/SHTR2.PWR"))
    (model ${KISYS3DMOD}/Dave.3dshapes/C-5747845-4.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:DB9_offBoard (layer F.Cu) (tedit 66384E9A)
    (at 110 132.5)
    (descr "Connecteur DB9 male droit")
    (tags "CONN DB9")
    (fp_text reference J3 (at 0.02 5.89) (layer F.SilkS))
    (fp_text value DB9_Male (at 0.93 -2.79) (layer F.Fab))
    (fp_text user %R (at 0.02 5.86) (layer F.Fab))
    (pad 9 thru_hole circle (at 4.19 2.79) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole circle (at 1.4 2.79) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole circle (at -1.27 2.79) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 6 thru_hole circle (at -4.06 2.79) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 5 thru_hole circle (at 5.46 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 2.8 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 0 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 thru_hole circle (at -2.67 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 1 thru_hole rect (at -5.46 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 113.4 127.8)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C1 (at 5.4 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0 -2.75) (layer F.Fab))
    (pad 1 smd rect (at -2.9 0) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 2.9 0) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 163.5 73.5 90)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C3 (at -5.5 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 2 smd rect (at 2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 163.5 91.5 90)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C4 (at -5.1 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 163.5 110 90)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C5 (at -4.9 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 2 smd rect (at 2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 163.5 128 90)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C6 (at -4.8 0.1 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 2.9 0 90) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 56 128.5 270)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C7 (at -4.9 -0.1) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 270) (layer F.Fab))
    (pad 2 smd rect (at 2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 56 110 270)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C8 (at -5 0.1) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 2 smd rect (at 2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 56 91.5 270)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C9 (at -5 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 270) (layer F.Fab))
    (pad 2 smd rect (at 2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer F.Cu) (tedit 58AA8525)
    (at 56 73.5 270)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C10 (at -5 0.2) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 2 smd rect (at 2.9 0 270) (size 2.2 3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_C_0805_HandSoldering (layer F.Cu) (tedit 5B4CB6B0)
    (at 113 119 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.3 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.1 68 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -3.3 0 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "/Power Box Top/Power Switch: POBC/Vctl"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 57 79)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R38 (at 3.5 0.5) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q16-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 163.5 68)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -3.2 0) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q2-Pad3)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 104.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.5 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(Q6-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 "/Power Box Top/Power Switch: MCP/Vctl"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 156.5 109.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -0.1 -1.5 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 80.9 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0.1 1.5 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(Q4-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 86 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.5 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 "/Power Box Top/Power Switch: MISC/Vctl"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 163.5 86)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -3.3 0) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q4-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 156.5 91.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 63 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -3.4 0 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 156.5 73.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.1 -1.5 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 69.3 71.8 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.5 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 "/Power Box Top/SHTR2.PWR"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 80.4 71.6 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0.1 -1.5 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "/Power Box Top/SHTR1.PWR"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 91.8 72.9)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.3) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 "/Power Box Top/Heater.PWR"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 102.6 72.9)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0.8 -1.5) (layer B.SilkS))
    (fp_text value 4.99K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 27 "/Power Box Top/HVPS2.PWR"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 117.4 72.9 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.1 1.5 180) (layer B.SilkS))
    (fp_text value 4.99K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 26 "/Power Box Top/HVPS1.PWR"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 129.9 72.8 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.9 1.4 180) (layer B.SilkS))
    (fp_text value 4.99K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 "/Power Box Top/MCP.PWR"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 151 71 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.1 1.5 270) (layer B.SilkS))
    (fp_text value 4.99K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 "/Power Box Top/POBC.PWR"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 163.5 104.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at -3.2 0.05) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q6-Pad3)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 63 128.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 -1.6 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 65.9 82.3)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 57 115.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 3.4 0.1) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q12-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 64.6 85.3 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at 0 -1.4 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "/Power Box Top/Power Switch: SHTR2/Vctl"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 140.5 71.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 4.99K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 "/Power Box Top/MISC.PWR"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 63 73.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at -3.5 0 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 56.2 102.7 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at -3.6 -0.1 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(Q14-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 57.9 97)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 0 -1.6) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 52 "/Power Box Top/Power Switch: SHTR1/Vctl"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(Q14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 57 97)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 3.3 0.2) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(Q14-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 63 91.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 3.3 -0.1 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 53.8 117.2 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q12-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 57.8 115.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0.1 -1.5) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "/Power Box Top/Power Switch: HEATER/Vctl"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 63 110 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at -0.1 -1.5 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 53.8 135.4 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0.1 1.5 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 57.8 134)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 -1.5) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q10-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "/Power Box Top/Power Switch: HVPS2/Vctl"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 163.5 122.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -3.2 0.1) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q8-Pad3)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 57 134)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 3.4 0.05) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q10-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 117.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 1.5 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(Q8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 122.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.6 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(Q8-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 56 "/Power Box Top/Power Switch: HVPS1/Vctl"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.2 99.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0.1 1.5 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(Q6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 156.5 127.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 3 0.05 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Steward_Logo (layer F.Cu) (tedit 5F2C1ACD)
    (at 117 110)
    (fp_text reference G1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value STEWARD_LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 159.5 91.5 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D10 (at -5.3 0 180) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 159.5 73.5 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D9 (at -5.3 0.1 180) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 159.5 128 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D12 (at -5.2 0 180) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 159.5 110 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D11 (at -5.1 0.2 180) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 60 110 270)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D14 (at -5.2 -0.1) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 60 128.5 270)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D13 (at -5.1 -0.1) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 60 91.5 270)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D15 (at -5.2 0) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 60 73.5 270)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D16 (at -5.2 0) (layer F.SilkS))
    (fp_text value 12V (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 168 70.9 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at -3.2 0) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "/Power Box Top/POBC.PWR"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 52 94.15 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q13 (at -3.35 0 180) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(C9-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "/Power Box Top/SHTR1.PWR"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 52 112.35 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q11 (at -3.35 0.2 180) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "/Power Box Top/Heater.PWR"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 168 89.07 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at -3.27 0) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "/Power Box Top/MISC.PWR"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 52 130.55 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q9 (at -3.45 0 180) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "/Power Box Top/HVPS2.PWR"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 168 125.47 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q7 (at -3.27 0) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "/Power Box Top/HVPS1.PWR"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 52 76 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q15 (at -3.5 0 180) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "/Power Box Top/+28V_BUS"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "/Power Box Top/SHTR2.PWR"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 168 107.27 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q5 (at -3.17 0) (layer F.SilkS))
    (fp_text value IXTP18P10T (at 2.54 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "/Power Box Top/MCP.PWR"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 55.5 83)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q16 (at 5 0) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 "Net-(Q16-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 "Net-(Q16-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 113 122.5 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 4.8 0 180) (layer F.SilkS))
    (fp_text value LP2950-3.3_TO92 (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 "/Power Box Top/+3.3V"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 "/Power Box Top/+12V_BUS"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 162 65)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at -2.5 0) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 "Net-(Q2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 162 83)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at -2.4 0) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 "Net-(Q4-Pad3)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 162 101.5)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q6 (at -2.4 0) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(Q6-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 "Net-(Q6-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 162 119.5)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q8 (at -2.4 0.1) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(Q8-Pad3)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(Q8-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 55.5 137.5)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q10 (at 5.3 -0.1) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(Q10-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(Q10-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 55.5 119.5)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q12 (at 5.3 -0.1) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(Q12-Pad3)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(Q12-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 55.5 101)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q14 (at 5.1 -0.2) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(Q14-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(Q14-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "PCB: ASPERA-UA-DWG-xxxxx\nVersion 1.0\n2024/05/07 D. Hamara" (at 135.5 122.5) (layer F.SilkS))
  (gr_text "Aspera GSE Power" (at 136 116) (layer F.SilkS))
  (gr_text "STEWARD OBSERVATORY" (at 136.5 112.5) (layer F.SilkS))
  (gr_text "#22 jumper" (at 60.9 72.4) (layer B.SilkS))
  (gr_text "#22 jumper" (at 61.6 91.5) (layer B.SilkS))
  (gr_text "#22 jumper" (at 80.9 118.4 327) (layer B.SilkS))
  (gr_text "#22 jumper" (at 159.6 107.7) (layer B.SilkS))
  (gr_text "#22 jumper" (at 158.6 89.7) (layer B.SilkS))
  (dimension 90 (width 0.3) (layer Dwgs.User)
    (gr_text "90.000 mm" (at 179.1 95 270) (layer Dwgs.User))
    (feature1 (pts (xy 170 140) (xy 177.586421 140)))
    (feature2 (pts (xy 170 50) (xy 177.586421 50)))
    (crossbar (pts (xy 177 50) (xy 177 140)))
    (arrow1a (pts (xy 177 140) (xy 176.413579 138.873496)))
    (arrow1b (pts (xy 177 140) (xy 177.586421 138.873496)))
    (arrow2a (pts (xy 177 50) (xy 176.413579 51.126504)))
    (arrow2b (pts (xy 177 50) (xy 177.586421 51.126504)))
  )
  (dimension 120 (width 0.3) (layer Dwgs.User)
    (gr_text "120.000 mm" (at 110 37.4) (layer Dwgs.User))
    (feature1 (pts (xy 170 51.5) (xy 170 38.913579)))
    (feature2 (pts (xy 50 51.5) (xy 50 38.913579)))
    (crossbar (pts (xy 50 39.5) (xy 170 39.5)))
    (arrow1a (pts (xy 170 39.5) (xy 168.873496 40.086421)))
    (arrow1b (pts (xy 170 39.5) (xy 168.873496 38.913579)))
    (arrow2a (pts (xy 50 39.5) (xy 51.126504 40.086421)))
    (arrow2b (pts (xy 50 39.5) (xy 51.126504 38.913579)))
  )
  (gr_line (start 50 140) (end 50 50) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 140) (end 50 140) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 50) (end 170 140) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 50) (end 170 50) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 169.5 50.5) (xy 50.5 50.5) (xy 50.5 139.5) (xy 169.5 139.5)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 169.5 50.5) (xy 50.5 50.5) (xy 50.5 139.5) (xy 169.5 139.5)
      )
    )
  )
)
