(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 127)
    (zones 0)
    (modules 39)
    (nets 11)
  )
  (page USLetter)
  (title_block
    (title "Heath W5-M Power Supply Capboard")
    (date 2020-03-25)
    (company "SDS Labs")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (user_trace_width 1.905)
    (user_trace_width 2.54)
    (user_trace_width 3.175)
    (user_trace_width 3.81)
    (trace_clearance 0.2)
    (zone_clearance 2.54)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.715 5.715)
    (pad_drill 4.4958)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(C10-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C12-Pad1)")
  (net 10 "Net-(C13-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E7F7243)
    (at 196.215 141.0335)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill2mm (at 0 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.4958) (layers *.Cu *.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E7F723C)
    (at 196.215 77.5335)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill2mm (at 0 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.4958) (layers *.Cu *.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E7F7229)
    (at 75.565 77.343)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill2mm (at 0 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.4958) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F618F)
    (at 90.17 77.0255)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C1 (at -4.699 14.224) (layer F.SilkS))
    (fp_text value "39uf 450V" (at 5.207 -3.556) (layer B.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F60B0)
    (at 121.666 77.089)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C2 (at 13.716 14.351) (layer F.SilkS))
    (fp_text value "39uf 450V" (at 4.953 -3.429) (layer B.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F617A)
    (at 90.17 109.093)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C3 (at -4.445 14.097) (layer F.SilkS))
    (fp_text value "39uf 450V" (at 4.826 -3.302) (layer B.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F60A6)
    (at 121.666 109.093)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C4 (at 13.716 14.097) (layer F.SilkS))
    (fp_text value "39uf 450V" (at 4.953 -3.302) (layer B.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F6159)
    (at 90.17 141.097)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C5 (at -4.699 13.97) (layer F.SilkS))
    (fp_text value "33uf 400V" (at 5.207 -3.429) (layer B.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F6075)
    (at 121.666 141.097)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C6 (at 13.716 13.97) (layer F.SilkS))
    (fp_text value "33uf 400V" (at 5.08 -3.429) (layer B.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F603E)
    (at 163.322 76.962 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C7 (at -3.937 -14.478 180) (layer F.SilkS))
    (fp_text value "33uf 400V" (at 5.588 3.302 180) (layer B.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F6059)
    (at 163.195 141.224 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C8 (at -4.191 -13.843 180) (layer F.SilkS))
    (fp_text value "33uf 400V" (at 5.334 3.556 180) (layer B.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E7F6049)
    (at 163.322 109.22 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C9 (at -3.937 -13.97 180) (layer F.SilkS))
    (fp_text value "33uf 400V" (at 5.461 3.429 180) (layer B.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 5E7F61E6)
    (at 73.152 116.713 90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 8mm Capacitor")
    (fp_text reference C10 (at 18.288 -3.556 90) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 7.239 0.127 90) (layer B.SilkS))
    (fp_text user %R (at 7.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 5E7F5EA9)
    (at 178.562 70.626 270)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 8mm Capacitor")
    (fp_text reference C11 (at 15.099 -5.334 270) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 7.62 0.127 270) (layer B.SilkS))
    (fp_text user %R (at 7.5 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 15 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 5E7F5EB5)
    (at 178.562 134.634 270)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 8mm Capacitor")
    (fp_text reference C12 (at 14.972 -5.334 270) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 7.874 0 270) (layer B.SilkS))
    (fp_text user %R (at 7.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 5E7F5E00)
    (at 178.562 102.094 270)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 8mm Capacitor")
    (fp_text reference C13 (at 18.415 -3.429 270) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 7.366 -0.254 270) (layer B.SilkS))
    (fp_text user %R (at 9.525 -0.127 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 15 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F61B4)
    (at 80.9625 62.738)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Rect (at 4.572 -1.778) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F61B9)
    (at 75.692 62.738)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Inductor (at 0 3.81) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F61CA)
    (at 57.785 62.738)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Inductor (at 5.715 -0.127) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F61D0)
    (at 57.785 68.199)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Output CT" (at 6.858 -0.381) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F60DC)
    (at 145.542 62.738)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value GND (at 4.191 -1.651) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F60E3)
    (at 140.081 62.738)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Red/Yel (at -6.096 -1.778) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F5E2B)
    (at 202.1205 64.77)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Input B+" (at 1.397 6.604 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 8 "Net-(C11-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F5E27)
    (at 194.6275 64.77)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J8 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "2nd Stage B+" (at 3.302 2.667 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F5E2E)
    (at 187.1345 64.77)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J9 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Driver B+" (at 1.27 6.35 270) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 10 "Net-(C13-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E7F5E31)
    (at 181.8005 64.77)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Pre B+" (at -3.429 -0.127 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 10 "Net-(C13-Pad1)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5E7F6107)
    (at 106.426 63.119)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.207 -2.413) (layer F.SilkS))
    (fp_text value "100K 1W" (at 5.207 0.127) (layer B.SilkS))
    (fp_text user %R (at 5.245999 0.139999) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5E7F6117)
    (at 105.9815 90.6145)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value "100K 1W" (at 5.207 0.127) (layer B.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5E7F6132)
    (at 105.918 122.6185)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value "100K 1W" (at 4.953 0.127) (layer B.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5E7F6120)
    (at 105.9815 95.631)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 4.953 2.413) (layer F.SilkS))
    (fp_text value "100K 1W" (at 5.207 0.127) (layer B.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_Power_L48.0mm_W12.5mm_P55.88mm (layer F.Cu) (tedit 5E7F61DE)
    (at 60.325 136.652 90)
    (descr "Resistor, Axial_Power series, Box, pin pitch=55.88mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 55.88mm 15W length 48mm width 12.5mm height 12.5mm")
    (fp_text reference R5 (at 52.07 7.493 90) (layer F.SilkS))
    (fp_text value "100 10w" (at 27.178 -0.127 90) (layer B.SilkS))
    (fp_text user %R (at 27.94 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 55.88 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_Power_L48.0mm_W12.5mm_P55.88mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5E7F613C)
    (at 105.8545 127.5715)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 4.953 2.413) (layer F.SilkS))
    (fp_text value "100K 1W" (at 4.953 -0.127) (layer B.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5E7F614C)
    (at 105.791 154.432)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value "100K 1W" (at 5.08 0) (layer B.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P25.40mm (layer F.Cu) (tedit 5E7F5DCD)
    (at 202.184 97.79 270)
    (descr "Resistor, Axial_Power series, Box, pin pitch=25.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 25.4mm 4W length 20mm width 6.4mm height 6.4mm")
    (fp_text reference R8 (at 28.067 2.921 270) (layer F.SilkS))
    (fp_text value "15K 3W" (at 12.954 0.127 270) (layer B.SilkS))
    (fp_text user %R (at 13.843 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 25.4 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P25.40mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P25.40mm (layer F.Cu) (tedit 5E7F5DA3)
    (at 194.691 97.79 270)
    (descr "Resistor, Axial_Power series, Box, pin pitch=25.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 25.4mm 4W length 20mm width 6.4mm height 6.4mm")
    (fp_text reference R9 (at 28.067 2.794 270) (layer F.SilkS))
    (fp_text value "22K 3W" (at 12.446 0 270) (layer B.SilkS))
    (fp_text user %R (at 13.589 -0.127 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 25.4 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P25.40mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P25.40mm (layer F.Cu) (tedit 5E7F5D99)
    (at 187.198 97.79 270)
    (descr "Resistor, Axial_Power series, Box, pin pitch=25.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Box pin pitch 25.4mm 4W length 20mm width 6.4mm height 6.4mm")
    (fp_text reference R10 (at 28.575 2.667 270) (layer F.SilkS))
    (fp_text value "6800 3W" (at 12.7 0.889 270) (layer B.SilkS))
    (fp_text user %R (at 14.224 0.635 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 2 thru_hole oval (at 25.4 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P25.40mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sdsLogos:sdsLabs-large-fSilk (layer F.Cu) (tedit 5A94A1E6)
    (at 66.929 152.5905)
    (fp_text reference G*** (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08) (layer F.SilkS) hide)
  )
  (module sdsLogos:sdsLabs-large-bSilk (layer F.Cu) (tedit 5A94A1E6)
    (at 66.2305 152.5905)
    (fp_text reference G*** (at 0 -7.62) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08) (layer B.SilkS) hide)
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E7F7231)
    (at 75.565 140.97)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill2mm (at 0 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.4958) (layers *.Cu *.Mask))
  )
  (gr_text "Heath W5-M Capacitor Board" (at 185.7375 155.6385) (layer F.SilkS))
  (gr_circle (center 75.565 77.343) (end 77.597 77.343) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 196.215 77.47) (end 198.247 77.47) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 196.215 140.97) (end 198.247 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 75.565 140.97) (end 77.597 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.74 160.02) (end 53.34 160.02) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.74 58.42) (end 205.74 160.02) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 58.42) (end 205.74 58.42) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 160.02) (end 53.34 58.42) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.54))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.4035 159.9565) (xy 205.74 160.02) (xy 205.74 58.42) (xy 53.34 58.42)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.54))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.2765 160.0835) (xy 205.6765 160.0835) (xy 205.74 58.42) (xy 53.34 58.42) (xy 53.4035 159.9565)
      )
    )
  )
)
