(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 55)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (grid_origin 100 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad1)")
  (net 2 "Net-(J0-Pad2)")
  (net 3 "Net-(J0-Pad3)")
  (net 4 "Net-(J0-Pad4)")
  (net 5 "Net-(J0-Pad5)")
  (net 6 "Net-(J0-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(J0-Pad1)")
    (add_net "Net-(J0-Pad2)")
    (add_net "Net-(J0-Pad3)")
    (add_net "Net-(J0-Pad4)")
    (add_net "Net-(J0-Pad5)")
    (add_net "Net-(J0-Pad6)")
  )
  (module mpms-transport-puck-pcb:mpms-transport-puck-wire-pad (layer F.Cu) (tedit 5CF6F10D)
    (at -1.125 -1.948557 30)
    (fp_text reference 6 (at 0 -0.75 30 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.5 30) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 30) (size 0.5 0.75) (rect_delta 0 -0.25 ) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J0-Pad6)"))
  )
  (module mpms-transport-puck-pcb:mpms-transport-puck-wire-pad (layer F.Cu) (tedit 5CF6F10D)
    (at -2.25 0 90)
    (fp_text reference 5 (at 0 -0.75 90 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.5 90) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 90) (size 0.5 0.75) (rect_delta 0 -0.25 ) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J0-Pad5)"))
  )
  (module mpms-transport-puck-pcb:mpms-transport-puck-wire-pad (layer F.Cu) (tedit 5CF6F10D)
    (at -1.125 1.948557 150)
    (fp_text reference 4 (at 0 -0.75 150 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.5 150) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 150) (size 0.5 0.75) (rect_delta 0 -0.25 ) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J0-Pad4)"))
  )
  (module mpms-transport-puck-pcb:mpms-transport-puck-wire-pad (layer F.Cu) (tedit 5CF6F10D)
    (at 1.125 1.948557 210)
    (fp_text reference 3 (at 0 -0.75 210 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.5 30) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 210) (size 0.5 0.75) (rect_delta 0 -0.25 ) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J0-Pad3)"))
  )
  (module mpms-transport-puck-pcb:mpms-transport-puck-wire-pad (layer F.Cu) (tedit 5CF6F10D)
    (at 2.25 0 270)
    (fp_text reference 2 (at 0 -0.75 270 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.5 90) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 270) (size 0.5 0.75) (rect_delta 0 -0.25 ) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J0-Pad2)"))
  )
  (module mpms-transport-puck-pcb:mpms-transport-puck-wire-pad (layer F.Cu) (tedit 5CF6F10D)
    (at 1.125 -1.948557 330)
    (fp_text reference 1 (at 0 -0.75 330 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.5 150) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 330) (size 0.5 0.75) (rect_delta 0 -0.25 ) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J0-Pad1)"))
  )
  (module mpms-transport-puck-pcb:samtec-cle-106-xx-x-DV-x (layer B.Cu) (tedit 5D2F6107)
    (at 0 0 180)
    (fp_text reference J0 (at -2.159 5.715) (layer B.SilkS) hide)
    (fp_text value Conn_02x06_Counter_Clockwise (at 0 -6.5) (layer B.Fab) hide)
    (fp_text user 7 (at 2.8 1.8) (layer B.SilkS))
    (fp_text user 1 (at -2.8 -1.8) (layer B.SilkS))
    (pad 12 smd rect (at -2 1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -1.2 1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -0.4 1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 0.4 1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 1.2 1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at 2 1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 2 -1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J0-Pad6)"))
    (pad 5 smd rect (at 1.2 -1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J0-Pad5)"))
    (pad 4 smd rect (at 0.4 -1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J0-Pad4)"))
    (pad 3 smd rect (at -0.4 -1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J0-Pad3)"))
    (pad 2 smd rect (at -1.2 -1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J0-Pad2)"))
    (pad 1 smd rect (at -2 -1.98 180) (size 0.508 1.37) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J0-Pad1)"))
  )
  (gr_text "MPMS\ntransport\npuck v2" (at 0 0) (layer B.SilkS))
  (gr_circle (center 0 0) (end 3.7 0) (layer Edge.Cuts) (width 0.05))
)
