<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="21.59" y1="69.85" x2="56.769" y2="69.977" width="0.2032" layer="20"/>
<wire x1="21.59" y1="58.039" x2="21.59" y2="69.85" width="0.2032" layer="20"/>
<wire x1="21.59" y1="58.039" x2="26.289" y2="58.039" width="0.2032" layer="20"/>
<wire x1="26.289" y1="58.039" x2="26.3652" y2="62.103" width="0.2032" layer="20"/>
<wire x1="26.3652" y1="62.103" x2="56.769" y2="62.23" width="0.2032" layer="20"/>
<wire x1="56.769" y1="62.23" x2="56.769" y2="69.977" width="0.2032" layer="20"/>
<hole x="25.019" y="64.262" drill="1.778"/>
<hole x="27.559" y="64.262" drill="1.778"/>
<hole x="30.099" y="64.262" drill="1.778"/>
<hole x="32.639" y="64.262" drill="1.778"/>
<hole x="35.179" y="64.262" drill="1.778"/>
<text>Famicom Disk System Resistor Data Fix  </text>
<text>Frank Strasser</text>
</plain>
<libraries>
<library name="via">
<packages>
<package name="VIA4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="4pinresistorarray">
<packages>
<package name="CAY16472J4LF">
<description>&lt;b&gt;CAY16-472J4LF&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="via" package="VIA4" value="VIA4"/>
<element name="U$2" library="via" package="VIA4" value="VIA4"/>
<element name="U$3" library="via" package="VIA4" value="VIA4"/>
<element name="U$4" library="via" package="VIA4" value="VIA4"/>
<element name="U$5" library="via" package="VIA4" value="VIA4"/>
<element name="U$6" library="via" package="VIA4" value="VIA4"/>
<element name="U$7" library="via" package="VIA4" value="VIA4"/>
<element name="U$8" library="via" package="VIA4" value="VIA4"/>
<element name="U$9" library="via" package="VIA4" value="VIA4"/>
<element name="U$10" library="4pinresistorarray" package="CAY16472J4LF" value="4PINRESISTORARRAY"/>
<element name="U$11" library="4pinresistorarray" package="CAY16472J4LF" value="4PINRESISTORARRAY"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="1"/>
<contactref element="U$10" pad="8"/>
<contactref element="U$10" pad="7"/>
<contactref element="U$10" pad="6"/>
<contactref element="U$10" pad="5"/>
<contactref element="U$11" pad="8"/>
<contactref element="U$11" pad="7"/>
<contactref element="U$11" pad="6"/>
<contactref element="U$11" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="1"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="1"/>
<contactref element="U$10" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$4" pad="1"/>
<contactref element="U$10" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$5" pad="1"/>
<contactref element="U$10" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U$7" pad="1"/>
<contactref element="U$11" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$8" pad="1"/>
<contactref element="U$11" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U$9" pad="1"/>
<contactref element="U$11" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$6" pad="1"/>
<contactref element="U$11" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
