(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 14)
    (no_connects 0)
    (area 141.347429 95.391 155.832572 115.890952)
    (thickness 1.6)
    (drawings 16)
    (tracks 68)
    (zones 0)
    (modules 5)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.01)
    (user_trace_width 0.02)
    (user_trace_width 0.04)
    (user_trace_width 0.05)
    (user_trace_width 0.1)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (trace_clearance 0.25)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.01)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.06 0.88)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x000f8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(IC1-Pad1)")
  (net 4 "Net-(IC1-Pad5)")
  (net 5 "Net-(IC1-Pad6)")
  (net 6 "Net-(IC1-Pad8)")
  (net 7 "Net-(P2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P2-Pad4)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5898D19D)
    (at 145.542 105.156 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 270) (layer Cmts.User))
    (fp_text value 0.1u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_2x2mm_Pitch0.5mm (layer F.Cu) (tedit 5898C4CD)
    (at 148.59 105.156)
    (descr "DFN8 2x2, 0.5P; CASE 506CN (see ON Semiconductor 506CN.PDF)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference IC1 (at 0 -2.075) (layer F.SilkS))
    (fp_text value ATTINY10-MA (at 0 2.075) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -0.9 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.9 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.9 0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.9 0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 0.9 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at 0.9 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 8 smd rect (at 0.9 -0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at 0 0.44) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0 -0.44) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5898CB28)
    (at 152.654 98.806)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39) (layer Cmts.User))
    (fp_text value CONN_4 (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5898CAA1)
    (at 151.13 110.49 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference TPI (at 1.27 -2.39 270) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.47 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad6)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5898CB36)
    (at 144.526 98.806)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.39) (layer Cmts.User))
    (fp_text value CONN_2 (at 0 4.93) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text V- (at 147.32 101.092) (layer F.SilkS))
  (gr_text V+ (at 147.32 98.806) (layer F.SilkS))
  (gr_text PB3 (at 150.622 106.426 90) (layer F.SilkS))
  (gr_text PB2 (at 150.622 103.886 90) (layer F.SilkS))
  (gr_text PB1 (at 150.622 101.346 90) (layer F.SilkS))
  (gr_text PB0 (at 150.622 98.806 90) (layer F.SilkS))
  (gr_line (start 142.24 115.57) (end 142.24 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 115.57) (end 142.24 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 96.52) (end 154.94 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 96.52) (end 154.94 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.432 115.316) (xy 142.748 115.316) (xy 142.748 97.028) (xy 154.432 97.028)
      )
    )
  )
)
