(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 31)
    (no_connects 1)
    (area 14.974999 14.974999 31.025001 29.025001)
    (thickness 1.6)
    (drawings 16)
    (tracks 88)
    (zones 0)
    (modules 10)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (trace_clearance 0.1)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 15 15)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(USB1-Pad2)")
  (net 2 "Net-(USB1-Pad3)")
  (net 3 "Net-(USB1-Pad8)")
  (net 4 "Net-(USB1-Pad10)")
  (net 5 "Net-(USB1-Pad11)")
  (net 6 "Net-(USB1-Pad14)")
  (net 7 "Net-(USB1-Pad25)")
  (net 8 "Net-(USB1-Pad15)")
  (net 9 "Net-(USB1-Pad20)")
  (net 10 "Net-(USB1-Pad22)")
  (net 11 "Net-(USB1-Pad23)")
  (net 12 /GND)
  (net 13 /DN)
  (net 14 /DP)
  (net 15 /VBUS)
  (net 16 /CC1)
  (net 17 /CC2)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CC1)
    (add_net /CC2)
    (add_net /DN)
    (add_net /DP)
    (add_net /GND)
    (add_net /VBUS)
    (add_net "Net-(USB1-Pad10)")
    (add_net "Net-(USB1-Pad11)")
    (add_net "Net-(USB1-Pad14)")
    (add_net "Net-(USB1-Pad15)")
    (add_net "Net-(USB1-Pad2)")
    (add_net "Net-(USB1-Pad20)")
    (add_net "Net-(USB1-Pad22)")
    (add_net "Net-(USB1-Pad23)")
    (add_net "Net-(USB1-Pad25)")
    (add_net "Net-(USB1-Pad3)")
    (add_net "Net-(USB1-Pad8)")
  )
  (module local:Wurth-632723300011 (layer F.Cu) (tedit 5C42C6B8)
    (at 16 22 270)
    (attr smd)
    (fp_text reference USB1 (at 0 -12 270) (layer F.SilkS) hide)
    (fp_text value Wurth-632723300011 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 27 smd rect (at 0 -2.9 270) (size 0.2 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (pad 27 smd rect (at 0 -6 270) (size 0.2 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (pad 26 thru_hole oval (at -4.27 -3.45 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu B.Mask)
      (net 12 /GND))
    (pad 26 thru_hole oval (at -4.27 -8.18 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu B.Mask)
      (net 12 /GND))
    (pad 26 thru_hole oval (at 4.27 -3.45 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu B.Mask)
      (net 12 /GND))
    (pad 26 thru_hole oval (at 4.27 -8.18 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu B.Mask)
      (net 12 /GND))
    (pad 25 thru_hole circle (at -2 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 7 "Net-(USB1-Pad25)"))
    (pad 24 thru_hole circle (at -2.8 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 12 /GND))
    (pad 23 thru_hole circle (at -2.4 -8.63 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 11 "Net-(USB1-Pad23)"))
    (pad 22 thru_hole circle (at -1.6 -8.63 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 10 "Net-(USB1-Pad22)"))
    (pad 21 thru_hole circle (at -1.2 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 15 /VBUS))
    (pad 20 thru_hole circle (at -0.8 -8.62 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 9 "Net-(USB1-Pad20)"))
    (pad 19 thru_hole circle (at -0.4 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 13 /DN))
    (pad 18 thru_hole circle (at 0.4 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 14 /DP))
    (pad 17 thru_hole circle (at 0.8 -8.63 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 17 /CC2))
    (pad 16 thru_hole circle (at 1.2 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 15 /VBUS))
    (pad 15 thru_hole circle (at 1.6 -8.63 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 8 "Net-(USB1-Pad15)"))
    (pad 25 thru_hole circle (at 2 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 7 "Net-(USB1-Pad25)"))
    (pad 14 thru_hole circle (at 2.4 -8.63 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 6 "Net-(USB1-Pad14)"))
    (pad 13 thru_hole circle (at 2.8 -9.33 270) (size 0.65 0.65) (drill 0.4) (layers *.Cu B.Mask)
      (net 12 /GND))
    (pad 12 smd rect (at 2.75 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (pad 11 smd rect (at 2.25 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(USB1-Pad11)"))
    (pad 10 smd rect (at 1.75 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(USB1-Pad10)"))
    (pad 9 smd rect (at 1.25 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS))
    (pad 8 smd rect (at 0.75 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(USB1-Pad8)"))
    (pad 7 smd rect (at 0.25 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 /DN))
    (pad 6 smd rect (at -0.25 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /DP))
    (pad 5 smd rect (at -0.75 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 /CC1))
    (pad 4 smd rect (at -1.25 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS))
    (pad 3 smd rect (at -1.75 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(USB1-Pad3)"))
    (pad 2 smd rect (at -2.25 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(USB1-Pad2)"))
    (pad 1 smd rect (at -2.75 -10.58 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
  )
  (module local:PINS-1.27-1x4 (layer F.Cu) (tedit 566F4375)
    (at 30.25 22 90)
    (fp_text reference P1 (at 0 1.27 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -1.27 90) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at 1.905 0 90) (size 0.8 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 /VBUS))
    (pad 3 thru_hole oval (at 0.635 0 90) (size 0.8 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 /DP))
    (pad 2 thru_hole oval (at -0.635 0 90) (size 0.8 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 /DN))
    (pad 1 thru_hole oval (at -1.905 0 90) (size 0.8 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 /GND))
  )
  (module local:0603_m1608 (layer F.Cu) (tedit 5CA22571)
    (at 29 20 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.75 1 450) (layer F.SilkS))
    (fp_text value RSMALL (at 0 1.27 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /CC1))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:0603_m1608 (layer F.Cu) (tedit 5CA2256F)
    (at 28 20 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.75 1 270) (layer F.SilkS))
    (fp_text value RSMALL (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /CC1))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:0603_m1608 (layer F.Cu) (tedit 5CA2256B)
    (at 28 24 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.75 0 450) (layer F.SilkS))
    (fp_text value RSMALL (at 0 1.27 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /CC2))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /VBUS))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:0603_m1608 (layer F.Cu) (tedit 5CA22569)
    (at 29 24 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.75 0 270) (layer F.SilkS))
    (fp_text value RSMALL (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /CC2))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:HOLE_1.6mm (layer F.Cu) (tedit 5CA20ED7)
    (at 16.25 27.75)
    (fp_text reference J4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PIN (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
  )
  (module local:HOLE_1.6mm (layer F.Cu) (tedit 5CA20ED7)
    (at 29.75 27.75)
    (fp_text reference J1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PIN (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
  )
  (module local:HOLE_1.6mm (layer F.Cu) (tedit 5CA20ED7)
    (at 29.75 16.25)
    (fp_text reference J2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PIN (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
  )
  (module local:HOLE_1.6mm (layer F.Cu) (tedit 5CA20ED7)
    (at 16.25 16.25)
    (fp_text reference J3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PIN (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
  )
  (gr_text "USB-C breakout\n04-2019 F4GRX\nrev 1" (at 19.5 20.25) (layer B.SilkS))
  (dimension 14 (width 0.15) (layer Dwgs.User)
    (gr_text "14 mm" (at 36.8 22 270) (layer Dwgs.User))
    (feature1 (pts (xy 35 29) (xy 36.086421 29)))
    (feature2 (pts (xy 35 15) (xy 36.086421 15)))
    (crossbar (pts (xy 35.5 15) (xy 35.5 29)))
    (arrow1a (pts (xy 35.5 29) (xy 34.913579 27.873496)))
    (arrow1b (pts (xy 35.5 29) (xy 36.086421 27.873496)))
    (arrow2a (pts (xy 35.5 15) (xy 34.913579 16.126504)))
    (arrow2b (pts (xy 35.5 15) (xy 36.086421 16.126504)))
  )
  (dimension 11 (width 0.15) (layer Dwgs.User)
    (gr_text "11 mm" (at 33.8 22 90) (layer Dwgs.User))
    (feature1 (pts (xy 32 16.5) (xy 33.086421 16.5)))
    (feature2 (pts (xy 32 27.5) (xy 33.086421 27.5)))
    (crossbar (pts (xy 32.5 27.5) (xy 32.5 16.5)))
    (arrow1a (pts (xy 32.5 16.5) (xy 33.086421 17.626504)))
    (arrow1b (pts (xy 32.5 16.5) (xy 31.913579 17.626504)))
    (arrow2a (pts (xy 32.5 27.5) (xy 33.086421 26.373496)))
    (arrow2b (pts (xy 32.5 27.5) (xy 31.913579 26.373496)))
  )
  (gr_line (start 31 15) (end 15 15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 31 29) (end 31 15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15 29) (end 31 29) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15 15) (end 15 29) (angle 90) (layer Edge.Cuts) (width 0.05))
  (zone (net 12) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15 15) (xy 31 15) (xy 31 29) (xy 15 29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15 26.5) (xy 31 26.5) (xy 31 29) (xy 15 29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15 15) (xy 31 15) (xy 31 17.5) (xy 15 17.5)
      )
    )
  )
  (zone (net 12) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15 15) (xy 31 15) (xy 31 29) (xy 15 29)
      )
    )
  )
)
