(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 310)
    (tracks 160)
    (zones 0)
    (modules 29)
    (nets 13)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - Constant Current Driver (DMX-DCC)")
    (date 2024-02-09)
    (rev 1.1)
    (company "Sparky Bobo Designs")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 https://creativecommons.org/licenses/by-sa/4.0/)
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0 License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(J5-Pad1)")
  (net 4 "Net-(J6-Pad1)")
  (net 5 +VDC)
  (net 6 /C)
  (net 7 /D)
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(D4-Pad1)")
  (net 10 "Net-(J6-Pad2)")
  (net 11 "Net-(J5-Pad2)")
  (net 12 "Net-(D3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /C)
    (add_net /D)
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
  )
  (net_class 1Amp ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.508)
    (diff_pair_gap 0.1524)
    (add_net +VDC)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 164.9095 94.234)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 5.715 0) (layer F.SilkS))
    (fp_text value 5.1v (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.5 0) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 124.079 94.234 180)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 5.7785 0) (layer F.SilkS))
    (fp_text value 5.1v (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 180) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.5 0 180) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 139.6365 96.941 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D2 (at -5.421 0 180) (layer F.SilkS))
    (fp_text value MBRA140 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 155.7655 96.9645 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at -5.3975 0.0635 180) (layer F.SilkS))
    (fp_text value MBRA140 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-5_Handsoldering (layer F.Cu) (tedit 5C33D69A)
    (at 135.1915 96.3295 270)
    (descr "SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf")
    (tags SOT-89-5)
    (attr smd)
    (fp_text reference U2 (at 3.3655 2.8575) (layer F.SilkS))
    (fp_text value AL8861 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.5 0) (layer F.Fab))
    (pad 2 smd custom (at 0 0 270) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3.6 -0.5) (xy -0.9 -0.5) (xy -0.4 -1) (xy 0.4 -1) (xy 0.9 -0.5)
           (xy 3.6 -0.5) (xy 3.6 0.5) (xy 0.9 0.5) (xy 0.4 1) (xy -0.4 1)
           (xy -0.9 0.5) (xy -3.6 0.5)) (width 0))
      ))
    (pad 3 smd rect (at -2.35 1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at -2.35 -1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at 2.35 1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J6-Pad2)"))
    (pad 5 smd rect (at 2.35 -1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-5_Handsoldering (layer F.Cu) (tedit 5C33D69A)
    (at 151.257 96.3295 270)
    (descr "SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf")
    (tags SOT-89-5)
    (attr smd)
    (fp_text reference U1 (at 3.3655 2.794 180) (layer F.SilkS))
    (fp_text value AL8861 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.5 0) (layer F.Fab))
    (pad 2 smd custom (at 0 0 270) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3.6 -0.5) (xy -0.9 -0.5) (xy -0.4 -1) (xy 0.4 -1) (xy 0.9 -0.5)
           (xy 3.6 -0.5) (xy 3.6 0.5) (xy 0.9 0.5) (xy 0.4 1) (xy -0.4 1)
           (xy -0.9 0.5) (xy -3.6 0.5)) (width 0))
      ))
    (pad 3 smd rect (at -2.35 1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at -2.35 -1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 2.35 1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J5-Pad2)"))
    (pad 5 smd rect (at 2.35 -1.5 270) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:L_BOURNS_SRN6045TA (layer F.Cu) (tedit 65C19DF6)
    (at 136.4615 88.7095 180)
    (descr "Choke, SMD, 6.0x6.0mm 4.2mm height")
    (tags "Choke SMD SRN6045TA")
    (attr smd)
    (fp_text reference L2 (at -0.0127 4.1529) (layer F.SilkS))
    (fp_text value 33uH (at 0 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.35 0 180) (size 1.8 5.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2.35 0 180) (size 1.8 5.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:L_BOURNS_SRN6045TA (layer F.Cu) (tedit 65C19DF6)
    (at 152.5075 88.7095 180)
    (descr "Choke, SMD, 6.0x6.0mm 4.2mm height")
    (tags "Choke SMD SRN6045TA")
    (attr smd)
    (fp_text reference L1 (at 0.0059 4.1529) (layer F.SilkS))
    (fp_text value 33uH (at 0 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.35 0 180) (size 1.8 5.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2.35 0 180) (size 1.8 5.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 126.111 97.282 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 3.683 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 /D))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 162.8775 97.3455)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 3.556 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 /C))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 659CBF62)
    (at 163.1315 103.378)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 2.921 -2.794 -180) (layer F.SilkS))
    (fp_text value Output (at 4.385 7.35) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 -270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /C))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal (layer F.Cu) (tedit 5A00FA1A)
    (at 132.0165 68.707 180)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Angled || order number: 1803277 8A 160V")
    (tags "phoenix_contact connector MC_01x02_G_3.81mm")
    (fp_text reference J6 (at 2.905 -2.8 180) (layer F.SilkS))
    (fp_text value "D Out" (at 1.905 9 180) (layer F.Fab))
    (fp_text user %R (at 2.905 3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 134.747 78.0415 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -3.583 0.0635) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 150.9395 78.0415 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -3.6195 0.0635) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 +VDC))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 659C8E78)
    (at 153.811751 81.660473 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at -0.050273 6.275851) (layer F.SilkS))
    (fp_text value "LED C" (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 659C8E93)
    (at 137.682751 81.660473 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0.025927 -3.744449) (layer F.SilkS))
    (fp_text value "LED D" (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 659C8E3C)
    (at 140.208 107.1245 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J10 (at -0.0254 -2.9972) (layer F.SilkS))
    (fp_text value CTRL_D (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +VDC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 659C8E34)
    (at 156.351751 107.123973 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0 10.085851) (layer F.SilkS))
    (fp_text value CTRL_C (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +VDC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /C))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 135.001 101.6635)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.54 1.9685) (layer F.SilkS))
    (fp_text value 0.1 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(J6-Pad2)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 151.13 101.6635)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.4765 1.9685) (layer F.SilkS))
    (fp_text value 0.1 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 +VDC))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal (layer F.Cu) (tedit 5A00FA1A)
    (at 160.655 68.707 180)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Angled || order number: 1803277 8A 160V")
    (tags "phoenix_contact connector MC_01x02_G_3.81mm")
    (fp_text reference J5 (at 2.905 -2.8 180) (layer F.SilkS))
    (fp_text value "C Out" (at 1.905 9 180) (layer F.Fab))
    (fp_text user %R (at 2.905 3 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal (layer F.Cu) (tedit 5A00FA1A)
    (at 146.3675 68.707 180)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Angled || order number: 1803277 8A 160V")
    (tags "phoenix_contact connector MC_01x02_G_3.81mm")
    (fp_text reference J4 (at 2.905 -2.8 180) (layer F.SilkS))
    (fp_text value Power (at 1.905 9 180) (layer F.Fab))
    (fp_text user %R (at 2.905 3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 65A4E562)
    (at 125.6665 108.3945 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 2.921 7.8105) (layer F.SilkS))
    (fp_text value Input (at 4.385 7.35 180) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 -90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /C))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F5FF02E)
    (at 170.053 64.77)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F5FE685)
    (at 118.745 116.332 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH3 (at 0 -4.2 180) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F5FE681)
    (at 170.053 116.332 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH4 (at 0 -4.2 180) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F5FF032)
    (at 118.7459 64.77)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Aesthetics:OSHW-LOGO-S locked (layer F.Cu) (tedit 200000)
    (at 144.4625 115.7605)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module footprints:logo_cr_5x5 locked (layer B.Cu) (tedit 0)
    (at 133.858 116.586 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "0.33: 350ma\n0.15: 700ma\n0.1:  900ma" (at 152.3365 104.267) (layer F.SilkS))
  (gr_text "0.33: 350ma\n0.15: 700ma\n0.1:  900ma" (at 136.2075 104.2035) (layer F.SilkS))
  (gr_text "Populate board with either:         \n\n- Sparkfun \"FemtoBuck\", COM-1371\n    - Install headers from the front  \nof the board in the      \nlocations outlined here.  \n    - Install FemtoBuck from the    \nfront the board, circuit  \nside up.                 \n\n- Discrete SMD components        \n  - Install U1,U2               \n  - Install R1,R2 based on     \nrequired current, below.\n  - Install R3,R4               \n  - Install C1,C2               \n  - Install D1,D2,D3,D4 observe\npolarity.               \n  - Install L1,L2               " (at 166.5224 83.82) (layer B.SilkS))
  (gr_text "- Pick the constant current\nvalue using R1 & R2: \n- 350ma: 0.33 OHM\n- 700ma: 0.15 OHM\n- 900ma: 0.1 OHM \n- 1/2 Watt         \n- 1% Tolerance     \n- Footprint 1206   \n(3216 Metric)" (at 166.5732 96.4184) (layer B.SilkS))
  (gr_text " -    +\nD Led" (at 130.6195 74.295 180) (layer F.SilkS))
  (gr_text " -    +\nC Led" (at 159.0675 74.295 180) (layer F.SilkS))
  (gr_text " -    +\nPower In" (at 144.7165 74.295 180) (layer F.SilkS))
  (gr_arc (start 115.189 119.817) (end 114.427 119.817) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.609 119.761) (end 173.609 120.579) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.609 61.397) (end 174.427 61.397) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.189 61.341) (end 115.189 60.579) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "DMX-DCC, Rev 1.1\nSparky Bobo Designs" (at 144.399 117.221) (layer B.SilkS))
  (gr_text DMX-DCC (at 144.145 118.11) (layer F.SilkS))
  (gr_line (start 115.189 60.579) (end 173.609 60.579) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.189 120.579) (end 173.609 120.579) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.427 61.397) (end 174.427 119.761) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.427 119.817) (end 114.427 61.341) (layer Edge.Cuts) (width 0.15))
  (gr_text Output (at 170.18 111.633) (layer F.SilkS))
  (gr_text Input (at 119.0625 111.633) (layer F.SilkS))
  (gr_text "D G C" (at 160.147 105.9942 90) (layer F.SilkS))
  (gr_text "D G C" (at 128.397 105.6767 270) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.554 120.015) (xy 114.554 61.087) (xy 114.935 60.706) (xy 173.863 60.706) (xy 174.244 61.087)
        (xy 174.244 120.142) (xy 173.863 120.396) (xy 114.935 120.396)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.554 120.015) (xy 114.554 61.087) (xy 114.935 60.706) (xy 173.863 60.706) (xy 174.244 61.087)
        (xy 174.244 120.142) (xy 173.863 120.396) (xy 114.935 120.396)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.447375 100.23475) (xy 151.971346 100.203) (xy 151.939596 103.0605) (xy 150.4315 103.0605)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.573868 95.377) (xy 153.573868 97.282) (xy 152.748368 97.282) (xy 152.748368 95.377)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.509023 95.377) (xy 137.509023 97.282) (xy 136.683523 97.282) (xy 136.683523 95.377)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.16225 82.677) (xy 155.16225 85.7885) (xy 154.33675 85.7885) (xy 154.33675 82.677)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.03325 82.677) (xy 139.03325 85.979) (xy 138.20775 85.979) (xy 138.20775 82.677)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.239029 100.23475) (xy 135.763 100.203) (xy 135.73125 103.0605) (xy 134.223154 103.0605)
      )
    )
  )
  (zone (net 5) (net_name +VDC) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 79.502) (xy 134.747 76.23175) (xy 143.51 76.2) (xy 143.51 109.22) (xy 131.5085 109.22)
        (xy 131.6355 79.502)
      )
    )
  )
  (zone (net 5) (net_name +VDC) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.8125 79.502) (xy 150.8125 76.2635) (xy 159.385 76.2635) (xy 159.385 109.22) (xy 147.701 109.22)
        (xy 147.701 79.502)
      )
    )
  )
)
