<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.02" y2="0" width="0" layer="20"/>
<wire x1="33.02" y1="0" x2="33.02" y2="27.94" width="0" layer="20"/>
<wire x1="33.02" y1="27.94" x2="0" y2="27.94" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="0" width="0" layer="20"/>
<text>VIN</text>
<text>VIN</text>
<text>VIN</text>
<text>EN</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VOUT</text>
<text>VOUT</text>
<text>GND</text>
<text>MODE</text>
<text>3.0-4.2v</text>
<text>6v</text>
</plain>
<libraries>
<library name="digikey">
<packages>
<package name="VQFN20">
</package>
</packages>
</library>
<library name="AVX_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/04/2012 16:26:10</description>
<packages>
<package name="CAPC2013X94N">
</package>
<package name="CAPC1608X90N">
</package>
</packages>
</library>
<library name="Kemet_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 28/03/2012 12:54:09</description>
<packages>
<package name="CAPC1005X60N">
</package>
<package name="CAPC3216X180N">
</package>
</packages>
</library>
<library name="Murata_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 21/03/2012 17:47:01</description>
<packages>
<package name="CAPC1005X60N">
</package>
<package name="CAPC1608X85N">
</package>
</packages>
</library>
<library name="Vishay_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 16:36:08</description>
<packages>
<package name="RESC1005X40N">
</package>
<package name="RESC3216X71N">
</package>
</packages>
</library>
<library name="Yageo_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 21/03/2012 16:17:53</description>
<packages>
<package name="RESC1608X60N">
</package>
</packages>
</library>
<library name="Coiltronics_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 13/06/2012 12:50:21</description>
<packages>
<package name="INDM7676X355N">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Dialight_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 13/06/2012 13:59:22</description>
<packages>
<package name="LED_597-3311-402F">
</package>
</packages>
</library>
<library name="32bits">
<packages>
<package name="PERIODIC_SYMBOL_BACK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="digikey" package="VQFN20" value="TPS61088VQFN20">
<attribute name="TYPE" value="boost"/>
</element>
<element name="CBST" library="AVX_By_element14_Batch_1" package="CAPC2013X94N" value="100nF">
<attribute name="VOLTAGERATING" value="25V"/>
<attribute name="OC_NEWARK" value="96M1381"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="MPN" value="08053C104KAT2A"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1740665"/>
<attribute name="NAME"/>
</element>
<element name="CCOMP" library="AVX_By_element14_Batch_1" package="CAPC1608X90N" value="680PF">
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_NEWARK" value="55J2711"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="MPN" value="0603YC681JAT2A"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="NAME"/>
</element>
<element name="CCOMP2" library="Kemet_By_element14_Batch_1" package="CAPC1005X60N" value="36pF">
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="29T8949"/>
<attribute name="SUPPLIER" value="KEMET"/>
<attribute name="MPN" value="C0402C360J5GACTU"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="OC_FARNELL" value="1865427"/>
<attribute name="NAME"/>
</element>
<element name="CIN" library="Kemet_By_element14_Batch_1" package="CAPC3216X180N" value="0.47uF">
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="32T6755"/>
<attribute name="SUPPLIER" value="KEMET"/>
<attribute name="MPN" value="C1206F474K5RACAUTO"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1869060"/>
<attribute name="NAME"/>
</element>
<element name="CIN2" library="Murata_By_element14_Batch_1" package="CAPC1005X60N" value="100nF">
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_NEWARK" value="38K1647"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="MPN" value="GRM155R71C104KA88D"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="8819742"/>
<attribute name="NAME"/>
</element>
<element name="COUT" library="Kemet_By_element14_Batch_1" package="CAPC3216X180N" value="0.47uF">
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="32T6755"/>
<attribute name="SUPPLIER" value="KEMET"/>
<attribute name="MPN" value="C1206F474K5RACAUTO"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1869060"/>
<attribute name="NAME"/>
</element>
<element name="C22" library="Kemet_By_element14_Batch_1" package="CAPC1005X60N" value="8.2nF">
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="29T8966"/>
<attribute name="SUPPLIER" value="KEMET"/>
<attribute name="MPN" value="C0402C822K5RACTU"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1865460"/>
<attribute name="NAME"/>
</element>
<element name="CVCC" library="Murata_By_element14_Batch_1" package="CAPC1608X85N" value="1uF">
<attribute name="VOLTAGERATING" value="6.3V"/>
<attribute name="OC_NEWARK" value="97K0609"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="MPN" value="GRM188R60J105KA01D"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="9527699"/>
<attribute name="NAME"/>
</element>
<element name="RCOMP" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="38.3K Ohms">
<attribute name="WATTAGE" value="0.063 W"/>
<attribute name="OC_NEWARK" value="52K7021"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="MPN" value="CRCW040238K3FKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="OC_FARNELL" value="1151219"/>
<attribute name="NAME"/>
</element>
<element name="RFBB" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="118K Ohms">
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="OC_NEWARK" value="52K6643"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="MPN" value="CRCW0402118KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="OC_FARNELL" value="1652743"/>
<attribute name="NAME"/>
</element>
<element name="RFBT" library="Yageo_By_element14_Batch_1" package="RESC1608X60N" value="470K Ohms">
<attribute name="WATTAGE" value="1/10 W"/>
<attribute name="OC_NEWARK" value="68R0098"/>
<attribute name="SUPPLIER" value="Yageo"/>
<attribute name="MPN" value="RC0603FR-07470KL"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="OC_FARNELL" value="1117267"/>
<attribute name="NAME"/>
</element>
<element name="RLIM" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="102K Ohms">
<attribute name="WATTAGE" value="0.063 W"/>
<attribute name="OC_NEWARK" value="52K6611"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="MPN" value="CRCW0402102KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="OC_FARNELL" value="1150767"/>
<attribute name="NAME"/>
</element>
<element name="RT" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="261K Ohms">
<attribute name="WATTAGE" value="0.063 W"/>
<attribute name="OC_NEWARK" value="52K6902"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="MPN" value="CRCW0402261KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="OC_FARNELL" value="1151087"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="Coiltronics_By_element14_Batch_1" package="INDM7676X355N" value="DR73-1R0-R">
<attribute name="PACKAGE" value="SMD"/>
<attribute name="OC_NEWARK" value="29K6167"/>
<attribute name="INDUCTANCE" value="1µH"/>
<attribute name="SUPPLIER" value="COILTRONICS"/>
<attribute name="MPN" value="DR73-1R0-R"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="CURRENTRATING" value="5.28A"/>
<attribute name="OC_FARNELL" value="1463503"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="+6" library="Dialight_By_element14_Batch_1" package="LED_597-3311-402F" value="597-3311-402F">
<attribute name="COLOR" value="Green"/>
<attribute name="MPN" value="597-3311-402F"/>
<attribute name="PACKAGE" value="1206- Green LED"/>
<attribute name="SUPPLIER" value="Dialight"/>
<attribute name="OC_FARNELL" value="1179613"/>
<attribute name="OC_NEWARK" value="30K4956"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="Vishay_By_element14_Batch_1" package="RESC3216X71N" value="200 Ohms">
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="WATTAGE" value="0.25W"/>
<attribute name="MPN" value="CRCW1206200RJNEA"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="OC_FARNELL" value="1540005"/>
<attribute name="OC_NEWARK" value="59M6966"/>
<attribute name="NAME"/>
</element>
<element name="H" library="32bits" package="PERIODIC_SYMBOL_BACK" value="1">
<attribute name="DESC" value="rev.0"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="P$21"/>
<contactref element="CIN" pad="1"/>
<contactref element="CIN2" pad="1"/>
<contactref element="CVCC" pad="2"/>
<contactref element="U1" pad="P$11"/>
<contactref element="U1" pad="P$12"/>
<contactref element="C22" pad="1"/>
<contactref element="RLIM" pad="2"/>
<contactref element="CCOMP2" pad="1"/>
<contactref element="CCOMP" pad="1"/>
<contactref element="RFBB" pad="1"/>
<contactref element="COUT" pad="1"/>
<contactref element="U1" pad="P$22"/>
<contactref element="U1" pad="P$23"/>
<contactref element="U1" pad="P$24"/>
<contactref element="U1" pad="P$20"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="2"/>
<contactref element="+6" pad="1"/>
<contactref element="U1" pad="P$25"/>
</signal>
<signal name="SW">
<contactref element="U1" pad="P$7"/>
<contactref element="U1" pad="P$6"/>
<contactref element="U1" pad="P$5"/>
<contactref element="U1" pad="P$4"/>
<contactref element="CBST" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="RT" pad="2"/>
</signal>
<signal name="BOOT">
<contactref element="U1" pad="P$8"/>
<contactref element="CBST" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="P$9"/>
<contactref element="L1" pad="2"/>
<contactref element="CIN" pad="2"/>
<contactref element="CIN2" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="P$1"/>
<contactref element="CVCC" pad="1"/>
</signal>
<signal name="COMP">
<contactref element="U1" pad="P$18"/>
<contactref element="CCOMP2" pad="2"/>
<contactref element="RCOMP" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RCOMP" pad="2"/>
<contactref element="CCOMP" pad="2"/>
</signal>
<signal name="ILIM">
<contactref element="U1" pad="P$19"/>
<contactref element="RLIM" pad="1"/>
</signal>
<signal name="SS">
<contactref element="U1" pad="P$10"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="VOUT">
<contactref element="U1" pad="P$16"/>
<contactref element="U1" pad="P$15"/>
<contactref element="U1" pad="P$14"/>
<contactref element="RFBT" pad="1"/>
<contactref element="COUT" pad="2"/>
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="6"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="FB">
<contactref element="U1" pad="P$17"/>
<contactref element="RFBT" pad="2"/>
<contactref element="RFBB" pad="2"/>
</signal>
<signal name="FSW">
<contactref element="RT" pad="1"/>
<contactref element="U1" pad="P$3"/>
</signal>
<signal name="EN">
<contactref element="U1" pad="P$2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MODE">
<contactref element="U1" pad="P$13"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="LED_ANODE">
<contactref element="+6" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
