<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="33.528" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="18.288" y2="0" width="0.2032" layer="20"/>
<wire x1="18.288" y1="0" x2="18.288" y2="33.528" width="0.2032" layer="20"/>
<wire x1="18.288" y1="33.528" x2="0" y2="33.528" width="0.2032" layer="20"/>
<text>Reset</text>
<text>v14</text>
<text>Arduino Pro Mini</text>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>GND</text>
<text>RST</text>
<text>RXI</text>
<text>TXO</text>
<text>TXO</text>
<text>RXI</text>
<text>RAW</text>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>VCC</text>
<text>A5</text>
<text>A4</text>
<text>3.3V</text>
<text>5V</text>
<text>10MHz</text>
<text>16MHz</text>
<text>20MHz</text>
<text>8MHz</text>
<text>GND</text>
<text>BLK</text>
<text>GRN</text>
<text>Arduino Pro</text>
<text>Mini</text>
<text>www.arduino.cc</text>
<text>Valid combinations:</text>
<text>168V / 3.3V Reg / 8MHz</text>
<text>168 / 5V Reg / 16MHz</text>
<text>168 / 5V Reg / 20MHz</text>
<text>Mark back accordingly</text>
<text>A7</text>
<text>A6</text>
<text>Original Arduino Mini Design by Team Arduino
Arduino Pro Mini Design by SparkFun Electronics
Revised by Pete Lewis</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SFE-NEW-WEBLOGO">
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="1X12">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="1X06">
</package>
<package name="EIA3216">
</package>
<package name="1X02">
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="TACTILE-SWITCH-SMD-ALT01">
</package>
<package name="RESONATOR-SMD-1:1">
</package>
<package name="0603-LED-ALT1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="Testing" package="0603-LED-ALT1" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Testing" package="0603-LED-ALT1" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="SparkFun" package="SFE-NEW-WEBLOGO" value="LOGO-SFENEW"/>
<element name="U2" library="SparkFun" package="SOT23-5" value="MIC5205">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun" package="1X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun" package="SFE-LOGO-FLAME" value="LOGO-SFESK"/>
<element name="JP2" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="TQFP32-08" value="ATMEGA328">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X06" value="FTDI Basic">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="R1" library="SparkFun" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP8" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="Testing" package="TACTILE-SWITCH-SMD-ALT01" value="Reset">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Testing" package="RESONATOR-SMD-1:1" value="8/16/20MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C13" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="U2" pad="2"/>
<contactref element="C19" pad="C"/>
<contactref element="JP7" pad="9"/>
<contactref element="JP6" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="R11" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="1"/>
<contactref element="JP7" pad="10"/>
<contactref element="JP6" pad="3"/>
<contactref element="U1" pad="29"/>
<contactref element="C2" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="R6" pad="1"/>
<contactref element="JP6" pad="9"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="JP6" pad="10"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="JP6" pad="11"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="TXO">
<contactref element="JP7" pad="12"/>
<contactref element="U1" pad="31"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP6" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="C13" pad="A"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="RAW">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C19" pad="A"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="D9">
<contactref element="JP7" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="D8">
<contactref element="JP7" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="A5">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="28"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="A4">
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="27"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="A3">
<contactref element="JP6" pad="5"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="A2">
<contactref element="JP6" pad="6"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="A1">
<contactref element="JP6" pad="7"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="A0">
<contactref element="JP6" pad="8"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="D2">
<contactref element="JP7" pad="8"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="D3">
<contactref element="JP7" pad="7"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="JP7" pad="6"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D5">
<contactref element="JP7" pad="5"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="D6">
<contactref element="JP7" pad="4"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="D7">
<contactref element="JP7" pad="3"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="D10">
<contactref element="JP6" pad="12"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="8"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="RXI">
<contactref element="JP1" pad="3"/>
<contactref element="JP7" pad="11"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="5"/>
<contactref element="SJ1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R11" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
