(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 534)
    (no_connects 0)
    (area 14.520959 20.548744 202.100181 89.249251)
    (thickness 1.6002)
    (drawings 73)
    (tracks 4533)
    (zones 0)
    (modules 261)
    (nets 200)
  )
  (page A4)
  (title_block
    (title "gruvin9x custom logic board")
    (date "5 feb 2014")
    (rev 4.2d)
    (company gruvin9x)
    (comment 1 "Licensed under the TAPR Open Hardware License (see file,  LICENSE)")
    (comment 2 http://code.google.com/p/gruvin9x/)
    (comment 3 "Copyright 2011 th9xer")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.21082)
    (user_trace_width 0.21082)
    (user_trace_width 0.24892)
    (user_trace_width 0.35052)
    (user_trace_width 0.44958)
    (user_trace_width 0.55118)
    (user_trace_width 0.8001)
    (user_trace_width 1.00076)
    (trace_clearance 0.23114)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.20066)
    (segment_width 0.381)
    (edge_width 0.50038)
    (via_size 0.89916)
    (via_drill 0.50038)
    (via_min_size 0.70104)
    (via_min_drill 0.39878)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.127)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory production/))
  )
  (net 0 "")
  (net 1 +1.2V)
  (net 2 /AVCC)
  (net 3 /AilDR_SW)
  (net 4 /BATT+)
  (net 5 /BATT+_FUSED)
  (net 6 /Back_Light_EL_TTL)
  (net 7 /Battery)
  (net 8 /Buzzer)
  (net 9 /Charge)
  (net 10 /DOWN)
  (net 11 /DOWN_P)
  (net 12 /EXIT)
  (net 13 /EXIT_P)
  (net 14 /EleDR_SW)
  (net 15 /Ext_Power)
  (net 16 /FB_CLOCK)
  (net 17 /Gear_SW)
  (net 18 /Hold_PWR_ON)
  (net 19 /Hov_Pit)
  (net 20 /Hov_Thr)
  (net 21 /I2C_SCL)
  (net 22 /I2C_SDA)
  (net 23 /IDL1_SW)
  (net 24 /IDL2_SW)
  (net 25 /JTAG_TCK)
  (net 26 /JTAG_TDI)
  (net 27 /JTAG_TDO)
  (net 28 /JTAG_TMS)
  (net 29 /Jack_PPM)
  (net 30 /Jack_Presence)
  (net 31 /Jack_Presence_TTL)
  (net 32 /LCD_A0)
  (net 33 /LCD_CS1)
  (net 34 /LCD_DATA0)
  (net 35 /LCD_DATA1)
  (net 36 /LCD_DATA2)
  (net 37 /LCD_DATA3)
  (net 38 /LCD_DATA4)
  (net 39 /LCD_DATA5)
  (net 40 /LCD_DATA6)
  (net 41 /LCD_DATA7)
  (net 42 /LCD_RD)
  (net 43 /LCD_RES)
  (net 44 /LCD_WR)
  (net 45 /LEFT)
  (net 46 /LEFT_P)
  (net 47 /LH_Dwn_P)
  (net 48 /LH_Stick)
  (net 49 /LH_Trim_Dwn)
  (net 50 /LH_Trim_Up)
  (net 51 /LH_Up_P)
  (net 52 /LV_Dwn_P)
  (net 53 /LV_Stick)
  (net 54 /LV_Trim_Dwn)
  (net 55 /LV_Trim_Up)
  (net 56 /LV_Up_P)
  (net 57 /MENU)
  (net 58 /MENU_P)
  (net 59 /Module_PPM)
  (net 60 /PPM_IN)
  (net 61 /PPM_OUT)
  (net 62 /Pit_Trim)
  (net 63 /RESET)
  (net 64 /RF_Power)
  (net 65 /RF_Power_TTL)
  (net 66 /RH_Dwn_P)
  (net 67 /RH_Stick)
  (net 68 /RH_Trim_Dwn)
  (net 69 /RH_Trim_Up)
  (net 70 /RH_Up_P)
  (net 71 /RIGHT)
  (net 72 /RIGHT_P)
  (net 73 /ROT_ENC_1_A)
  (net 74 /ROT_ENC_1_B)
  (net 75 /ROT_ENC_1_PUSH)
  (net 76 /ROT_ENC_2_A)
  (net 77 /ROT_ENC_2_B)
  (net 78 /ROT_ENC_2_PUSH)
  (net 79 /RV_Dwn_P)
  (net 80 /RV_Stick)
  (net 81 /RV_Trim_Dwn)
  (net 82 /RV_Trim_Up)
  (net 83 /RV_Up_P)
  (net 84 /RudDR_SW)
  (net 85 /SD_CS)
  (net 86 /SD_MISO)
  (net 87 /SD_MOSI)
  (net 88 /SD_SCK)
  (net 89 /Sim_Ctrl)
  (net 90 /Spare1\LED-BL-opt)
  (net 91 /Spare2\Vib-opt)
  (net 92 /Speaker)
  (net 93 /Speaker_TTL)
  (net 94 /TCut_SW)
  (net 95 /TELEM_RX)
  (net 96 /TELEM_TX)
  (net 97 /Train_SW)
  (net 98 /UP)
  (net 99 /UP_P)
  (net 100 /USB_D+)
  (net 101 /USB_D-)
  (net 102 /Vcc_3V3)
  (net 103 /Vib-PWM-opt)
  (net 104 AGND)
  (net 105 GND)
  (net 106 N-000010)
  (net 107 N-000011)
  (net 108 N-000013)
  (net 109 N-000014)
  (net 110 N-000015)
  (net 111 N-000016)
  (net 112 N-000021)
  (net 113 N-000022)
  (net 114 N-000023)
  (net 115 N-000024)
  (net 116 N-000036)
  (net 117 N-000037)
  (net 118 N-000039)
  (net 119 N-000057)
  (net 120 N-000058)
  (net 121 N-000059)
  (net 122 N-000060)
  (net 123 N-000071)
  (net 124 N-000074)
  (net 125 N-000081)
  (net 126 N-000082)
  (net 127 N-000084)
  (net 128 N-000085)
  (net 129 N-000086)
  (net 130 N-000087)
  (net 131 N-000088)
  (net 132 N-000089)
  (net 133 N-000090)
  (net 134 N-000094)
  (net 135 N-000107)
  (net 136 N-000108)
  (net 137 N-000109)
  (net 138 N-000110)
  (net 139 N-000111)
  (net 140 N-000112)
  (net 141 N-000113)
  (net 142 N-000114)
  (net 143 N-000115)
  (net 144 N-000116)
  (net 145 N-000117)
  (net 146 N-000118)
  (net 147 N-000119)
  (net 148 N-000120)
  (net 149 N-000121)
  (net 150 N-000129)
  (net 151 N-000130)
  (net 152 N-000131)
  (net 153 N-000132)
  (net 154 N-000133)
  (net 155 N-000134)
  (net 156 N-000135)
  (net 157 N-000136)
  (net 158 N-000144)
  (net 159 N-000145)
  (net 160 N-000148)
  (net 161 N-000150)
  (net 162 N-000151)
  (net 163 N-000152)
  (net 164 N-000153)
  (net 165 N-000154)
  (net 166 N-000155)
  (net 167 N-000156)
  (net 168 N-000157)
  (net 169 N-000158)
  (net 170 N-000159)
  (net 171 N-000161)
  (net 172 N-000166)
  (net 173 N-000167)
  (net 174 N-000168)
  (net 175 N-000169)
  (net 176 N-000170)
  (net 177 N-000173)
  (net 178 N-000174)
  (net 179 N-000175)
  (net 180 N-000176)
  (net 181 N-000179)
  (net 182 N-000180)
  (net 183 N-000182)
  (net 184 N-000183)
  (net 185 N-000185)
  (net 186 N-000186)
  (net 187 N-000187)
  (net 188 N-000188)
  (net 189 N-000189)
  (net 190 N-000190)
  (net 191 N-000191)
  (net 192 N-000193)
  (net 193 N-000196)
  (net 194 N-000208)
  (net 195 N-000209)
  (net 196 N-000211)
  (net 197 N-000212)
  (net 198 N-000213)
  (net 199 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.23114)
    (trace_width 0.21082)
    (via_dia 0.89916)
    (via_drill 0.50038)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +1.2V)
    (add_net /AilDR_SW)
    (add_net /BATT+_FUSED)
    (add_net /Back_Light_EL_TTL)
    (add_net /Battery)
    (add_net /Buzzer)
    (add_net /DOWN)
    (add_net /DOWN_P)
    (add_net /EXIT)
    (add_net /EXIT_P)
    (add_net /EleDR_SW)
    (add_net /FB_CLOCK)
    (add_net /Gear_SW)
    (add_net /Hold_PWR_ON)
    (add_net /Hov_Pit)
    (add_net /Hov_Thr)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /IDL1_SW)
    (add_net /IDL2_SW)
    (add_net /Jack_PPM)
    (add_net /Jack_Presence)
    (add_net /Jack_Presence_TTL)
    (add_net /LEFT)
    (add_net /LEFT_P)
    (add_net /LH_Dwn_P)
    (add_net /LH_Stick)
    (add_net /LH_Trim_Dwn)
    (add_net /LH_Trim_Up)
    (add_net /LH_Up_P)
    (add_net /LV_Dwn_P)
    (add_net /LV_Stick)
    (add_net /LV_Trim_Dwn)
    (add_net /LV_Trim_Up)
    (add_net /LV_Up_P)
    (add_net /MENU)
    (add_net /MENU_P)
    (add_net /Module_PPM)
    (add_net /PPM_IN)
    (add_net /PPM_OUT)
    (add_net /Pit_Trim)
    (add_net /RESET)
    (add_net /RF_Power_TTL)
    (add_net /RH_Dwn_P)
    (add_net /RH_Stick)
    (add_net /RH_Trim_Dwn)
    (add_net /RH_Trim_Up)
    (add_net /RH_Up_P)
    (add_net /RIGHT)
    (add_net /RIGHT_P)
    (add_net /ROT_ENC_1_A)
    (add_net /ROT_ENC_1_PUSH)
    (add_net /ROT_ENC_2_A)
    (add_net /ROT_ENC_2_B)
    (add_net /ROT_ENC_2_PUSH)
    (add_net /RV_Dwn_P)
    (add_net /RV_Stick)
    (add_net /RV_Trim_Dwn)
    (add_net /RV_Trim_Up)
    (add_net /RV_Up_P)
    (add_net /RudDR_SW)
    (add_net /SD_CS)
    (add_net /SD_MISO)
    (add_net /SD_MOSI)
    (add_net /SD_SCK)
    (add_net /Sim_Ctrl)
    (add_net /Spare1\LED-BL-opt)
    (add_net /Spare2\Vib-opt)
    (add_net /Speaker)
    (add_net /Speaker_TTL)
    (add_net /TCut_SW)
    (add_net /TELEM_RX)
    (add_net /TELEM_TX)
    (add_net /Train_SW)
    (add_net /UP)
    (add_net /UP_P)
    (add_net /USB_D+)
    (add_net /USB_D-)
    (add_net /Vib-PWM-opt)
    (add_net AGND)
    (add_net N-000010)
    (add_net N-000011)
    (add_net N-000013)
    (add_net N-000014)
    (add_net N-000015)
    (add_net N-000016)
    (add_net N-000021)
    (add_net N-000022)
    (add_net N-000023)
    (add_net N-000024)
    (add_net N-000036)
    (add_net N-000037)
    (add_net N-000039)
    (add_net N-000057)
    (add_net N-000058)
    (add_net N-000059)
    (add_net N-000060)
    (add_net N-000071)
    (add_net N-000074)
    (add_net N-000081)
    (add_net N-000082)
    (add_net N-000084)
    (add_net N-000085)
    (add_net N-000086)
    (add_net N-000087)
    (add_net N-000088)
    (add_net N-000089)
    (add_net N-000090)
    (add_net N-000094)
    (add_net N-000107)
    (add_net N-000108)
    (add_net N-000109)
    (add_net N-000110)
    (add_net N-000111)
    (add_net N-000112)
    (add_net N-000113)
    (add_net N-000114)
    (add_net N-000115)
    (add_net N-000116)
    (add_net N-000117)
    (add_net N-000118)
    (add_net N-000119)
    (add_net N-000120)
    (add_net N-000121)
    (add_net N-000129)
    (add_net N-000130)
    (add_net N-000131)
    (add_net N-000132)
    (add_net N-000133)
    (add_net N-000134)
    (add_net N-000135)
    (add_net N-000136)
    (add_net N-000144)
    (add_net N-000145)
    (add_net N-000148)
    (add_net N-000150)
    (add_net N-000151)
    (add_net N-000152)
    (add_net N-000153)
    (add_net N-000154)
    (add_net N-000155)
    (add_net N-000156)
    (add_net N-000157)
    (add_net N-000158)
    (add_net N-000159)
    (add_net N-000161)
    (add_net N-000166)
    (add_net N-000167)
    (add_net N-000168)
    (add_net N-000169)
    (add_net N-000170)
    (add_net N-000173)
    (add_net N-000174)
    (add_net N-000175)
    (add_net N-000176)
    (add_net N-000179)
    (add_net N-000180)
    (add_net N-000182)
    (add_net N-000183)
    (add_net N-000185)
    (add_net N-000186)
    (add_net N-000187)
    (add_net N-000188)
    (add_net N-000189)
    (add_net N-000190)
    (add_net N-000191)
    (add_net N-000193)
    (add_net N-000196)
    (add_net N-000208)
    (add_net N-000209)
    (add_net N-000211)
    (add_net N-000212)
    (add_net N-000213)
  )
  (net_class Large ""
    (clearance 0.23114)
    (trace_width 0.50038)
    (via_dia 0.89916)
    (via_drill 0.50038)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /AVCC)
    (add_net /Charge)
    (add_net /RF_Power)
  )
  (net_class Largest ""
    (clearance 0.23114)
    (trace_width 0.8001)
    (via_dia 0.89916)
    (via_drill 0.70104)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /BATT+)
    (add_net /Ext_Power)
    (add_net /Vcc_3V3)
    (add_net GND)
    (add_net VCC)
  )
  (net_class Medium ""
    (clearance 0.23114)
    (trace_width 0.35052)
    (via_dia 0.89916)
    (via_drill 0.50038)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /JTAG_TCK)
    (add_net /JTAG_TDI)
    (add_net /JTAG_TDO)
    (add_net /JTAG_TMS)
    (add_net /ROT_ENC_1_B)
  )
  (net_class Small ""
    (clearance 0.23114)
    (trace_width 0.21082)
    (via_dia 0.8001)
    (via_drill 0.39878)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /LCD_A0)
    (add_net /LCD_CS1)
    (add_net /LCD_DATA0)
    (add_net /LCD_DATA1)
    (add_net /LCD_DATA2)
    (add_net /LCD_DATA3)
    (add_net /LCD_DATA4)
    (add_net /LCD_DATA5)
    (add_net /LCD_DATA6)
    (add_net /LCD_DATA7)
    (add_net /LCD_RD)
    (add_net /LCD_RES)
    (add_net /LCD_WR)
  )
  (module CONN_2MM_5x1 (layer Front) (tedit 51FF1599)
    (at 33.37306 44.45 90)
    (descr "5pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P2 (at 7.366 -1.778 180) (layer F.SilkS))
    (fp_text value CONN_5 (at -0.25908 1.8796 90) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 0 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 /IDL1_SW))
    (pad 2 thru_hole oval (at -1.99898 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 /Gear_SW))
    (pad 1 thru_hole rect (at -4.0005 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 4 thru_hole oval (at 1.99898 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 /IDL2_SW))
    (pad 5 thru_hole oval (at 4.0005 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 /AilDR_SW))
    (model packages3d\connectors\conn_2mm_5x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_4x1 (layer Front) (tedit 51FF1577)
    (at 36.3982 59.2836 90)
    (descr "6pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P12 (at 5.969 -0.0508 180) (layer F.SilkS))
    (fp_text value CONN_4 (at -0.30988 1.85166 90) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 1.016 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 113 N-000022))
    (pad 2 thru_hole oval (at -0.98298 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 114 N-000023))
    (pad 1 thru_hole rect (at -2.9845 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 4 thru_hole oval (at 3.01498 0.00762 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 112 N-000021))
    (model packages3d\connectors\conn_2mm_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_3x1 (layer Front) (tedit 4FA78A96)
    (at 100.68814 81.7372)
    (descr "3pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference K6 (at -0.18034 -4.8895) (layer F.SilkS))
    (fp_text value CONN_3 (at 0.0508 1.89992) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 1.99898 0.00762) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 187 N-000187))
    (pad 2 thru_hole oval (at 0 0.00762) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 186 N-000186))
    (pad 1 thru_hole rect (at -2.00152 0.00762) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d/connectors/conn_2mm_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_2x1 (layer Front) (tedit 51FF14B2)
    (at 36.59124 74.3204 270)
    (descr "2pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P14 (at -5.334 2.032 270) (layer F.SilkS))
    (fp_text value CONN_2 (at 0.81026 2.37998 270) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at 0.98552 0.00762 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 1 thru_hole rect (at -1.016 0.00762 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 129 N-000086))
    (model packages3d\connectors\conn_2mm_2x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_8x1 (layer Front) (tedit 51FF1450)
    (at 132.461 81.77022 180)
    (descr "9pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P13 (at 8.128 5.334 270) (layer F.SilkS))
    (fp_text value CONN_8 (at -0.83058 1.5494 180) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at -2.98196 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 /I2C_SCL))
    (pad 2 thru_hole oval (at -4.98094 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 /I2C_SDA))
    (pad 1 thru_hole rect (at -6.98246 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 4 thru_hole oval (at -0.98298 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 85 /SD_CS))
    (pad 5 thru_hole oval (at 1.01854 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 86 /SD_MISO))
    (pad 6 thru_hole oval (at 3.01752 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 87 /SD_MOSI))
    (pad 7 thru_hole oval (at 5.0165 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 88 /SD_SCK))
    (pad 8 thru_hole oval (at 7.01548 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 102 /Vcc_3V3))
    (model packages3d\connectors\conn_2mm_8x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_6x1 (layer Front) (tedit 51FF11A9)
    (at 195.0974 44.323 270)
    (descr "6pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P3 (at 6.6 4.5 270) (layer F.SilkS))
    (fp_text value CONN_6 (at 0.9398 1.81864 270) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at -1 -0.00038 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 84 /RudDR_SW))
    (pad 2 thru_hole oval (at -2.99898 -0.00038 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 /EleDR_SW))
    (pad 1 thru_hole rect (at -5.0005 -0.00038 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 4 thru_hole oval (at 0.99898 -0.00038 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 104 AGND))
    (pad 5 thru_hole oval (at 3.0005 -0.00038 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 62 /Pit_Trim))
    (pad 6 thru_hole oval (at 4.99948 -0.00038 270) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (model packages3d\connectors\conn_2mm_6x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_4x1 (layer Front) (tedit 51FF13B9)
    (at 186.2582 42.9006 180)
    (descr "6pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P15 (at 6.3 -0.1 270) (layer F.SilkS))
    (fp_text value CONN_4 (at -0.69088 1.61036 180) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 1 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 117 N-000037))
    (pad 2 thru_hole oval (at -0.99898 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 118 N-000039))
    (pad 1 thru_hole rect (at -3.0005 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 4 thru_hole oval (at 2.99898 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 116 N-000036))
    (model packages3d\connectors\conn_2mm_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_3x1 (layer Front) (tedit 51FF12D7)
    (at 163.62426 79.81188 90)
    (descr "3pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference K2 (at 2.80162 4.42722 180) (layer F.SilkS))
    (fp_text value CONN_3 (at -0.12192 1.78054 90) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 1.99898 -0.00038 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 171 N-000161))
    (pad 2 thru_hole oval (at 0 -0.00038 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 169 N-000158))
    (pad 1 thru_hole rect (at -2.00152 -0.00038 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d\connectors\conn_2mm_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_3x1 (layer Front) (tedit 4E6D39EF)
    (at 180.97246 79.74838 90)
    (descr "3pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference K1 (at 4.48056 -3.83032 180) (layer F.SilkS))
    (fp_text value CONN_3 (at 0.16002 1.77038 90) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 1.99898 -0.00038 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 96 /TELEM_TX))
    (pad 2 thru_hole oval (at 0 -0.00038 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 95 /TELEM_RX))
    (pad 1 thru_hole rect (at -2.00152 -0.00038 90) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d\connectors\conn_2mm_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_9x1 (layer Front) (tedit 51FF1152)
    (at 180.3908 33.8582)
    (descr "9pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P4 (at -5.7 4.4) (layer F.SilkS))
    (fp_text value CONN_9 (at -0.64008 2.02946) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at -3.99796 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 55 /LV_Trim_Up))
    (pad 2 thru_hole oval (at -5.99694 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 1 thru_hole rect (at -7.99846 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 54 /LV_Trim_Dwn))
    (pad 4 thru_hole oval (at -1.99898 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 50 /LH_Trim_Up))
    (pad 5 thru_hole oval (at 0.00254 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 49 /LH_Trim_Dwn))
    (pad 6 thru_hole oval (at 2.00152 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 104 AGND))
    (pad 7 thru_hole oval (at 4.0005 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 48 /LH_Stick))
    (pad 8 thru_hole oval (at 5.99948 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 53 /LV_Stick))
    (pad 9 thru_hole oval (at 8.001 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (model packages3d\connectors\conn_2mm_9x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_3x1 (layer Front) (tedit 51FF112F)
    (at 165.49624 34.86658 180)
    (descr "3pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference K5 (at 5.6007 3.2004 180) (layer F.SilkS))
    (fp_text value CONN_3 (at 0.07874 1.77038 180) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 1.99898 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 190 N-000190))
    (pad 2 thru_hole oval (at 0 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 1 thru_hole rect (at -2.00152 -0.00038 180) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 122 N-000060))
    (model packages3d\connectors\conn_2mm_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_5x1 (layer Front) (tedit 51FF108C)
    (at 149.1615 33.62706)
    (descr "5pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference K4 (at -7 1.8 90) (layer F.SilkS))
    (fp_text value CONN_5 (at -0.19812 1.82118) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at 0 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (pad 2 thru_hole oval (at -1.99898 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 102 /Vcc_3V3))
    (pad 1 thru_hole rect (at -4.0005 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 /BATT+_FUSED))
    (pad 4 thru_hole oval (at 1.99898 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 104 AGND))
    (pad 5 thru_hole oval (at 4.0005 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d\connectors\conn_2mm_5x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_6x1 (layer Front) (tedit 4E6D3A14)
    (at 132.8928 33.5788)
    (descr "6pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P6 (at 1.69164 3.59156) (layer F.SilkS))
    (fp_text value CONN_6 (at 0.34036 1.91008) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at -1 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 2 thru_hole oval (at -2.99898 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 64 /RF_Power))
    (pad 1 thru_hole rect (at -5.0005 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 /Charge))
    (pad 4 thru_hole oval (at 0.99898 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 /BATT+))
    (pad 5 thru_hole oval (at 3.0005 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 /Ext_Power))
    (pad 6 thru_hole oval (at 4.99948 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 /Buzzer))
    (model packages3d\connectors\conn_2mm_6x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_12x1 (layer Front) (tedit 4E6D3A25)
    (at 86.0298 34.3408)
    (descr "12pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P7 (at 14.33068 -1.02108) (layer F.SilkS))
    (fp_text value CONN_12 (at -0.06858 1.778) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at -7.00024 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 /Hov_Pit))
    (pad 2 thru_hole oval (at -9.00176 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 94 /TCut_SW))
    (pad 1 thru_hole rect (at -11.00074 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (pad 4 thru_hole oval (at -5.00126 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 97 /Train_SW))
    (pad 5 thru_hole oval (at -2.99974 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 /Hov_Thr))
    (pad 6 thru_hole oval (at -1.00076 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 59 /Module_PPM))
    (pad 7 thru_hole oval (at 0.99822 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 64 /RF_Power))
    (pad 8 thru_hole oval (at 2.99974 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 /Jack_Presence))
    (pad 9 thru_hole oval (at 4.99872 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Jack_PPM))
    (pad 10 thru_hole oval (at 7.00024 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 /Ext_Power))
    (pad 11 thru_hole oval (at 8.99922 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 /Charge))
    (pad 12 thru_hole oval (at 10.9982 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d\connectors\conn_2mm_12x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_9x1 (layer Front) (tedit 51FF0F4B)
    (at 55.1942 33.6804)
    (descr "9pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P5 (at 11.4 -0.9) (layer F.SilkS))
    (fp_text value CONN_9 (at -0.42926 1.89992) (layer F.SilkS) hide)
    (pad 3 thru_hole oval (at -3.99796 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 82 /RV_Trim_Up))
    (pad 2 thru_hole oval (at -5.99694 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 1 thru_hole rect (at -7.99846 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 81 /RV_Trim_Dwn))
    (pad 4 thru_hole oval (at -1.99898 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 68 /RH_Trim_Dwn))
    (pad 5 thru_hole oval (at 0.00254 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 69 /RH_Trim_Up))
    (pad 6 thru_hole oval (at 2.00152 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 104 AGND))
    (pad 7 thru_hole oval (at 4.0005 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 67 /RH_Stick))
    (pad 8 thru_hole oval (at 5.99948 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 80 /RV_Stick))
    (pad 9 thru_hole oval (at 8.001 -0.00038) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (model packages3d\connectors\conn_2mm_9x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module XTAL_HC49US (layer Front) (tedit 50AEECAE)
    (at 129.77876 66.1289)
    (descr "Condensateur = 2 pas")
    (tags C)
    (attr smd)
    (fp_text reference X1 (at 6.94182 0.11176) (layer F.SilkS))
    (fp_text value 16MHz (at -0.20828 -1.41986) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.44094 0) (size 1.50114 1.50114) (drill 0.59944) (layers *.Cu *.Mask F.SilkS)
      (net 16 /FB_CLOCK))
    (pad 2 thru_hole circle (at 2.44094 0) (size 1.50114 1.50114) (drill 0.59944) (layers *.Cu *.Mask F.SilkS)
      (net 158 N-000144))
    (model packages3d\discret\xtal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3739 0.3739 0.3739))
      (rotate (xyz 0 0 90))
    )
  )
  (module CONN30_SMD (layer Front) (tedit 4E11F388)
    (at 116.19992 33.70072 180)
    (attr smd)
    (fp_text reference P8 (at -6.59892 -4.09956 180) (layer F.SilkS))
    (fp_text value CONN_30_LCD_GRUVIN (at 2.32918 1.28016 180) (layer F.SilkS) hide)
    (pad 20 smd rect (at 4.7498 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 136 N-000108))
    (pad 19 smd rect (at 4.2418 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 182 N-000180))
    (pad 18 smd rect (at 3.7465 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 144 N-000116))
    (pad 17 smd rect (at 3.2512 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 135 N-000107))
    (pad 16 smd rect (at 2.7432 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 105 GND) (clearance 0.2032))
    (pad 15 smd rect (at 2.2479 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3) (clearance 0.2032))
    (pad 14 smd rect (at 1.7526 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 41 /LCD_DATA7))
    (pad 13 smd rect (at 1.2446 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 40 /LCD_DATA6))
    (pad 12 smd rect (at 0.7493 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 39 /LCD_DATA5))
    (pad 11 smd rect (at 0.254 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 38 /LCD_DATA4))
    (pad 21 smd rect (at 5.25018 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 138 N-000110))
    (pad 10 smd rect (at -0.254 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 37 /LCD_DATA3))
    (pad 9 smd rect (at -0.7493 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 36 /LCD_DATA2))
    (pad 22 smd rect (at 5.75056 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 137 N-000109))
    (pad 1 smd rect (at -4.7498 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (clearance 0.2032))
    (pad 8 smd rect (at -1.2446 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 35 /LCD_DATA1))
    (pad 7 smd rect (at -1.7526 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 34 /LCD_DATA0))
    (pad 6 smd rect (at -2.2479 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 42 /LCD_RD))
    (pad 5 smd rect (at -2.7432 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 44 /LCD_WR))
    (pad 4 smd rect (at -3.2512 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 32 /LCD_A0))
    (pad 3 smd rect (at -3.7465 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 43 /LCD_RES))
    (pad 2 smd rect (at -4.2418 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 33 /LCD_CS1))
    (pad 23 smd rect (at 6.25094 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 139 N-000111))
    (pad 24 smd rect (at 6.74878 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 141 N-000113))
    (pad 25 smd rect (at 7.24916 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 140 N-000112))
    (pad 26 smd rect (at 7.74954 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 142 N-000114))
    (pad 27 smd rect (at 8.24992 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 143 N-000115))
    (pad 28 smd rect (at 8.7503 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 181 N-000179))
    (pad 29 smd rect (at 9.25068 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask)
      (net 134 N-000094))
    (pad 30 smd rect (at 9.75106 -3.2512 180) (size 0.254 2.032) (layers Front F.Paste F.Mask))
    (pad TAB2 smd rect (at -7.2136 -1.016 180) (size 2.54 3.302) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad TAB1 smd rect (at 12.1666 -1.016 180) (size 2.54 3.302) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model packages3d\smd\conn30_smd.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TQFP_100 (layer Front) (tedit 4E6D3779)
    (at 113.22558 62.92596 180)
    (descr "Module SMD TQFP 100 Pins")
    (tags "CMS TQFP")
    (clearance 0.20066)
    (attr smd)
    (fp_text reference IC1 (at 7.5946 -7.15518 180) (layer F.SilkS))
    (fp_text value ATMEGA2560-A_GRUVIN (at -8.97382 0.4572 270) (layer F.SilkS))
    (pad 100 smd rect (at 7.747 -5.9944 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 2 /AVCC))
    (pad 76 smd rect (at 7.747 5.9944 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 178 N-000174))
    (pad 77 smd rect (at 7.747 5.4864 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 179 N-000175))
    (pad 78 smd rect (at 7.747 5.0038 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 180 N-000176))
    (pad 79 smd rect (at 7.747 4.4958 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 70 /RH_Up_P))
    (pad 80 smd rect (at 7.747 3.9878 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 81 smd rect (at 7.747 3.5052 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 82 smd rect (at 7.747 2.9972 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 150 N-000129))
    (pad 83 smd rect (at 7.747 2.4892 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 151 N-000130))
    (pad 84 smd rect (at 7.747 2.0066 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 152 N-000131))
    (pad 85 smd rect (at 7.747 1.4986 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 156 N-000135))
    (pad 86 smd rect (at 7.747 0.9906 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 153 N-000132))
    (pad 87 smd rect (at 7.747 0.4826 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 154 N-000133))
    (pad 88 smd rect (at 7.747 0 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 155 N-000134))
    (pad 89 smd rect (at 7.747 -0.508 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 157 N-000136))
    (pad 90 smd rect (at 7.747 -1.016 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 26 /JTAG_TDI))
    (pad 91 smd rect (at 7.747 -1.4986 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 27 /JTAG_TDO))
    (pad 92 smd rect (at 7.747 -2.0066 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 28 /JTAG_TMS))
    (pad 93 smd rect (at 7.747 -2.5146 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 25 /JTAG_TCK))
    (pad 94 smd rect (at 7.747 -2.9972 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 188 N-000188))
    (pad 95 smd rect (at 7.747 -3.5052 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 196 N-000211))
    (pad 96 smd rect (at 7.747 -4.0132 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 197 N-000212))
    (pad 97 smd rect (at 7.747 -4.4958 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 198 N-000213))
    (pad 98 smd rect (at 7.747 -5.0038 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 159 N-000145))
    (pad 99 smd rect (at 7.747 -5.5118 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (pad 75 smd rect (at 5.9944 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 172 N-000166))
    (pad 51 smd rect (at -5.9944 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 170 N-000159))
    (pad 52 smd rect (at -5.4864 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 65 /RF_Power_TTL))
    (pad 53 smd rect (at -5.0038 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 6 /Back_Light_EL_TTL))
    (pad 54 smd rect (at -4.4958 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 165 N-000154))
    (pad 55 smd rect (at -3.9878 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 164 N-000153))
    (pad 56 smd rect (at -3.5052 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 163 N-000152))
    (pad 57 smd rect (at -2.9972 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 162 N-000151))
    (pad 58 smd rect (at -2.4892 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 161 N-000150))
    (pad 59 smd rect (at -2.0066 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 145 N-000117))
    (pad 60 smd rect (at -1.4986 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 160 N-000148))
    (pad 61 smd rect (at -0.9906 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 62 smd rect (at -0.4826 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 63 smd rect (at 0 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 47 /LH_Dwn_P))
    (pad 64 smd rect (at 0.508 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 51 /LH_Up_P))
    (pad 65 smd rect (at 1.016 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 52 /LV_Dwn_P))
    (pad 66 smd rect (at 1.4986 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 56 /LV_Up_P))
    (pad 67 smd rect (at 2.0066 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 79 /RV_Dwn_P))
    (pad 68 smd rect (at 2.5146 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 83 /RV_Up_P))
    (pad 69 smd rect (at 2.9972 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 66 /RH_Dwn_P))
    (pad 70 smd rect (at 3.5052 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 166 N-000155))
    (pad 71 smd rect (at 4.0132 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 176 N-000170))
    (pad 72 smd rect (at 4.4958 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 175 N-000169))
    (pad 73 smd rect (at 5.0038 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 174 N-000168))
    (pad 74 smd rect (at 5.5118 7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 173 N-000167))
    (pad 1 smd rect (at 5.9944 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 146 N-000118))
    (pad 2 smd rect (at 5.4864 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 95 /TELEM_RX))
    (pad 3 smd rect (at 5.0038 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 96 /TELEM_TX))
    (pad 4 smd rect (at 4.4958 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 101 /USB_D-))
    (pad 5 smd rect (at 3.9878 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 125 N-000081))
    (pad 6 smd rect (at 3.5052 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 100 /USB_D+))
    (pad 7 smd rect (at 2.9972 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 73 /ROT_ENC_1_A))
    (pad 8 smd rect (at 2.4892 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 74 /ROT_ENC_1_B))
    (pad 9 smd rect (at 2.0066 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 60 /PPM_IN))
    (pad 10 smd rect (at 1.4986 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 11 smd rect (at 0.9906 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 12 smd rect (at 0.4826 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 124 N-000074))
    (pad 13 smd rect (at 0 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 107 N-000011))
    (pad 14 smd rect (at -0.508 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 103 /Vib-PWM-opt))
    (pad 15 smd rect (at -1.016 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 106 N-000010))
    (pad 16 smd rect (at -1.4986 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 111 N-000016))
    (pad 17 smd rect (at -2.0066 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 110 N-000015))
    (pad 18 smd rect (at -2.5146 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 108 N-000013))
    (pad 19 smd rect (at -2.9972 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 85 /SD_CS))
    (pad 20 smd rect (at -3.5052 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 88 /SD_SCK))
    (pad 21 smd rect (at -4.0132 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 87 /SD_MOSI))
    (pad 22 smd rect (at -4.4958 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 86 /SD_MISO))
    (pad 23 smd rect (at -5.0038 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 148 N-000120))
    (pad 24 smd rect (at -5.5118 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 147 N-000119))
    (pad 25 smd rect (at -5.9944 -7.747 180) (size 0.254 1.016) (layers Front F.Paste F.Mask)
      (net 61 /PPM_OUT))
    (pad 26 smd rect (at -7.747 -5.9944 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 93 /Speaker_TTL))
    (pad 27 smd rect (at -7.747 -5.4864 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 109 N-000014))
    (pad 28 smd rect (at -7.747 -5.0038 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 149 N-000121))
    (pad 29 smd rect (at -7.747 -4.4958 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 89 /Sim_Ctrl))
    (pad 30 smd rect (at -7.747 -3.9878 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 63 /RESET))
    (pad 31 smd rect (at -7.747 -3.5052 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 32 smd rect (at -7.747 -2.9972 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 33 smd rect (at -7.747 -2.4892 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 16 /FB_CLOCK))
    (pad 34 smd rect (at -7.747 -2.0066 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 158 N-000144))
    (pad 35 smd rect (at -7.747 -1.4986 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 11 /DOWN_P))
    (pad 36 smd rect (at -7.747 -0.9906 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 99 /UP_P))
    (pad 37 smd rect (at -7.747 -0.4826 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 72 /RIGHT_P))
    (pad 38 smd rect (at -7.747 0 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 46 /LEFT_P))
    (pad 39 smd rect (at -7.747 0.508 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 58 /MENU_P))
    (pad 40 smd rect (at -7.747 1.016 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 13 /EXIT_P))
    (pad 41 smd rect (at -7.747 1.4986 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 31 /Jack_Presence_TTL))
    (pad 42 smd rect (at -7.747 2.0066 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 18 /Hold_PWR_ON))
    (pad 43 smd rect (at -7.747 2.5146 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 21 /I2C_SCL))
    (pad 44 smd rect (at -7.747 2.9972 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 22 /I2C_SDA))
    (pad 45 smd rect (at -7.747 3.5052 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 76 /ROT_ENC_2_A))
    (pad 46 smd rect (at -7.747 4.0132 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 77 /ROT_ENC_2_B))
    (pad 47 smd rect (at -7.747 4.4958 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 75 /ROT_ENC_1_PUSH))
    (pad 48 smd rect (at -7.747 5.0038 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 78 /ROT_ENC_2_PUSH))
    (pad 49 smd rect (at -7.747 5.5118 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 90 /Spare1\LED-BL-opt))
    (pad 50 smd rect (at -7.747 5.9944 180) (size 1.016 0.254) (layers Front F.Paste F.Mask)
      (net 91 /Spare2\Vib-opt))
    (model smd/TQFP_100.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
    (model packages3d\text\ATmega2560.wrl
      (at (xyz 0 0 0.018))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module SW_PUSH_6x4MM (layer Back) (tedit 4F291B87)
    (at 172.90034 66.20002 180)
    (attr smd)
    (fp_text reference SW2 (at 3.23088 3.64998 180) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 -1.016 180) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 2.99974 1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 10 /DOWN))
    (pad 2 thru_hole circle (at 2.99974 -1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (pad 1 thru_hole circle (at -2.99974 1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 10 /DOWN))
    (pad 2 thru_hole circle (at -2.99974 -1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (model packages3d\discret\push_butt_6x4_th.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SW_PUSH_6x4MM (layer Back) (tedit 4F291B5B)
    (at 181.89956 57.0992)
    (attr smd)
    (fp_text reference SW6 (at 3.12928 3.73126) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 -1.016) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 2.99974 1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 45 /LEFT))
    (pad 2 thru_hole circle (at 2.99974 -1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (pad 1 thru_hole circle (at -2.99974 1.99898) (size 2.19964 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 45 /LEFT))
    (pad 2 thru_hole circle (at -2.99974 -1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (model packages3d\discret\push_butt_6x4_th.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SW_PUSH_6x4MM (layer Back) (tedit 4F291B18)
    (at 54.30012 66.7004 180)
    (attr smd)
    (fp_text reference SW4 (at -3.30962 -3.5814 180) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0.10922 -3.3909 180) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 2.99974 1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 12 /EXIT))
    (pad 2 thru_hole circle (at 2.99974 -1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (pad 1 thru_hole circle (at -2.99974 1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 12 /EXIT))
    (pad 2 thru_hole circle (at -2.99974 -1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (model packages3d\discret\push_butt_6x4_th.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SW_PUSH_6x4MM (layer Back) (tedit 4F291AEA)
    (at 54.30012 51.99888 180)
    (attr smd)
    (fp_text reference SW1 (at -3.23088 -3.62966 180) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0.5207 -3.41884 180) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 2.99974 1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 57 /MENU))
    (pad 2 thru_hole circle (at 2.99974 -1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (pad 1 thru_hole circle (at -2.99974 1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 57 /MENU))
    (pad 2 thru_hole circle (at -2.99974 -1.99898 180) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (model packages3d\discret\push_butt_6x4_th.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SW_PUSH_6x4MM (layer Back) (tedit 4F291ABF)
    (at 172.90034 48.19904)
    (attr smd)
    (fp_text reference SW5 (at 3.23088 3.69062) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 -1.016) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 2.99974 1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 98 /UP))
    (pad 2 thru_hole circle (at 2.99974 -1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (pad 1 thru_hole circle (at -2.99974 1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 98 /UP))
    (pad 2 thru_hole circle (at -2.99974 -1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (model packages3d\discret\push_butt_6x4_th.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SW_PUSH_6x4MM (layer Back) (tedit 4F291A96)
    (at 163.90112 57.0992)
    (attr smd)
    (fp_text reference SW3 (at 3.24104 3.68046) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 -1.016) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 2.99974 1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 71 /RIGHT))
    (pad 2 thru_hole circle (at 2.99974 -1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (pad 1 thru_hole circle (at -2.99974 1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 71 /RIGHT))
    (pad 2 thru_hole circle (at -2.99974 -1.99898) (size 2.19964 2.19964) (drill 1.09982) (layers *.Cu *.Mask B.SilkS)
      (net 105 GND))
    (model packages3d\discret\push_butt_6x4_th.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer Front) (tedit 4E6D3619)
    (at 86.27618 70.50024 180)
    (attr smd)
    (fp_text reference L1 (at 1.13538 1.19126 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 2 /AVCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A4D)
    (at 91.9734 69.723 180)
    (attr smd)
    (fp_text reference C2 (at 1.93294 -0.00762 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 67 /RH_Stick))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A49)
    (at 91.9734 68.072 180)
    (attr smd)
    (fp_text reference C3 (at 1.91262 -0.01778 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 53 /LV_Stick))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A3C)
    (at 91.9734 63.07328 180)
    (attr smd)
    (fp_text reference C4 (at 1.90246 -0.01778 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 19 /Hov_Pit))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1D9)
    (at 91.9734 59.74842 180)
    (attr smd)
    (fp_text reference C5 (at 2.12344 0.01778 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 62 /Pit_Trim))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B778A)
    (at 88.9889 39.67988 270)
    (attr smd)
    (fp_text reference C6 (at -1.86182 0.14986 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A47)
    (at 91.9734 66.42354 180)
    (attr smd)
    (fp_text reference C7 (at 1.97358 -0.0762 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 80 /RV_Stick))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A3F)
    (at 91.9734 64.74714 180)
    (attr smd)
    (fp_text reference C8 (at 2.00406 -0.02286 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 48 /LH_Stick))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A42)
    (at 91.9734 61.39942 180)
    (attr smd)
    (fp_text reference C9 (at 1.92278 0 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 20 /Hov_Thr))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A26)
    (at 91.97086 57.9501 180)
    (attr smd)
    (fp_text reference C10 (at 2.24028 0.06096 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 7 /Battery))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E39)
    (at 126.57582 69.57568 180)
    (attr smd)
    (fp_text reference C13 (at 2.08534 0.01524 180) (layer F.SilkS))
    (fp_text value 18p (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 16 /FB_CLOCK))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E15C72F)
    (at 132.58038 69.94906)
    (attr smd)
    (fp_text reference C14 (at -2.19964 0.04064) (layer F.SilkS))
    (fp_text value 18p (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 158 N-000144))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B778F)
    (at 82.02422 40.77462 270)
    (attr smd)
    (fp_text reference C15 (at -1.7653 0.28448 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E370A06)
    (at 88.77554 70.55104 270)
    (attr smd)
    (fp_text reference C17 (at -1.68148 1.02616 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 2 /AVCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E3E)
    (at 126.57582 70.94982)
    (attr smd)
    (fp_text reference C19 (at -2.10566 0.0508) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1C3)
    (at 97.07372 71.3486 180)
    (attr smd)
    (fp_text reference C20 (at -2.24536 -0.03048 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 159 N-000145))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F4B5)
    (at 89.77376 45.60062 180)
    (attr smd)
    (fp_text reference C21 (at 2.0828 0.76962 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B76DE)
    (at 39.02456 48.62576)
    (attr smd)
    (fp_text reference C22 (at 2.25552 0.09398) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 94 /TCut_SW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2A069D)
    (at 151.20112 57.7596)
    (attr smd)
    (fp_text reference C23 (at 0.02794 1.12014) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 14 /EleDR_SW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7D5E0C)
    (at 92.48902 82.40014 270)
    (attr smd)
    (fp_text reference C24 (at 1.71958 0.2794 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 17 /Gear_SW))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E58)
    (at 132.75056 73.8759)
    (attr smd)
    (fp_text reference C25 (at 2.17932 0.32512) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 23 /IDL1_SW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B76E2)
    (at 38.75024 41.9989)
    (attr smd)
    (fp_text reference C26 (at 2.21996 0.09144) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 3 /AilDR_SW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6F48)
    (at 136.72566 45.1993)
    (attr smd)
    (fp_text reference C27 (at 0.05334 -1.01854) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 84 /RudDR_SW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7D5E1D)
    (at 94.08922 82.40014 270)
    (attr smd)
    (fp_text reference C28 (at 1.71958 -0.29972 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 97 /Train_SW))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7D5DFD)
    (at 95.6691 82.40014 270)
    (attr smd)
    (fp_text reference C29 (at -0.0889 -1.12014 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 24 /IDL2_SW))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F596)
    (at 120.36044 40.81018 90)
    (attr smd)
    (fp_text reference C44 (at -0.11938 1.4986 180) (layer F.SilkS))
    (fp_text value 1u (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 135 N-000107))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F5A1)
    (at 113.94948 43.61942 180)
    (attr smd)
    (fp_text reference C45 (at 0.4699 1.0287 180) (layer F.SilkS))
    (fp_text value 1u (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 138 N-000110))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 137 N-000109))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6FD3)
    (at 109.27334 42.9768 270)
    (attr smd)
    (fp_text reference C46 (at -2.13614 0.00254 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 141 N-000113))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6FCB)
    (at 106.47172 42.9768 270)
    (attr smd)
    (fp_text reference C47 (at -2.13614 -0.05842 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 142 N-000114))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6FDF)
    (at 110.67288 42.9768 270)
    (attr smd)
    (fp_text reference C48 (at -2.09804 -0.05588 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 139 N-000111))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6FCF)
    (at 107.8738 42.9768 270)
    (attr smd)
    (fp_text reference C49 (at -2.18694 -0.0254 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 140 N-000112))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6FC7)
    (at 105.07218 42.9768 270)
    (attr smd)
    (fp_text reference C50 (at -2.11582 -0.07874 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 143 N-000115))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F59C)
    (at 119.70004 43.28922 180)
    (attr smd)
    (fp_text reference C51 (at 0.83058 1.01854 180) (layer F.SilkS))
    (fp_text value 1u (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 144 N-000116))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 182 N-000180))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F5A9)
    (at 116.86032 43.63974)
    (attr smd)
    (fp_text reference C52 (at -0.67056 -1.0287) (layer F.SilkS))
    (fp_text value 1u (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 136 N-000108))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 182 N-000180))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4FB495B9)
    (at 93.49994 55.61076 180)
    (attr smd)
    (fp_text reference R1 (at -0.81026 -1.1303 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 7 /Battery))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B77AB)
    (at 97.07372 56.44896)
    (attr smd)
    (fp_text reference R2 (at -0.00254 -1.03886) (layer F.SilkS))
    (fp_text value 2K7 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 7 /Battery))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1C0)
    (at 97.04832 69.723 180)
    (attr smd)
    (fp_text reference R3 (at -2.09042 -0.09652 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 157 N-000136))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 67 /RH_Stick))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1BA)
    (at 97.07372 66.42354 180)
    (attr smd)
    (fp_text reference R4 (at -2.06502 -0.0762 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 154 N-000133))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 80 /RV_Stick))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1B6)
    (at 97.07372 63.07328 180)
    (attr smd)
    (fp_text reference R5 (at -2.13614 -0.02794 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 156 N-000135))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 19 /Hov_Pit))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A5D)
    (at 97.07372 59.74842 180)
    (attr smd)
    (fp_text reference R6 (at -2.07518 0.02794 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 151 N-000130))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 62 /Pit_Trim))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA24D)
    (at 94.0689 78.62062 270)
    (attr smd)
    (fp_text reference R8 (at -1.9177 -0.06096 270) (layer F.SilkS))
    (fp_text value 200R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 147 N-000119))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 97 /Train_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1BD)
    (at 97.07372 68.072 180)
    (attr smd)
    (fp_text reference R9 (at -2.12598 -0.05842 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 155 N-000134))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 53 /LV_Stick))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA1B8)
    (at 97.07626 64.74714 180)
    (attr smd)
    (fp_text reference R10 (at -2.42316 -0.17272 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 153 N-000132))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 48 /LH_Stick))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A5F)
    (at 97.07372 61.39942 180)
    (attr smd)
    (fp_text reference R11 (at -2.27584 -0.01016 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 152 N-000131))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 20 /Hov_Thr))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B9A5B)
    (at 97.07372 58.09742 180)
    (attr smd)
    (fp_text reference R12 (at -2.22504 -0.02286 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 150 N-000129))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 7 /Battery))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2A0699)
    (at 146.89074 57.74944)
    (attr smd)
    (fp_text reference R18 (at 0.05842 1.06172) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8001 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 145 N-000117))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 14 /EleDR_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA24B)
    (at 92.4814 78.63078 270)
    (attr smd)
    (fp_text reference R19 (at -2.25298 0.0508 270) (layer F.SilkS))
    (fp_text value 200R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 146 N-000118))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 17 /Gear_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7B8A97)
    (at 95.65132 78.63078 270)
    (attr smd)
    (fp_text reference R20 (at -2.28092 0.02032 270) (layer F.SilkS))
    (fp_text value 200R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 148 N-000120))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 24 /IDL2_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E47)
    (at 129.07518 72.34936)
    (attr smd)
    (fp_text reference R25 (at -2.21488 0.32004) (layer F.SilkS))
    (fp_text value 10K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 63 /RESET))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E4C)
    (at 129.10058 73.8759)
    (attr smd)
    (fp_text reference R26 (at -2.14122 0.07366) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 149 N-000121))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 23 /IDL1_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6F3F)
    (at 135.17626 41.82364)
    (attr smd)
    (fp_text reference R35 (at -0.08636 -0.96266) (layer F.SilkS))
    (fp_text value 10K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 65 /RF_Power_TTL))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6F2C)
    (at 128.84912 41.89984 90)
    (attr smd)
    (fp_text reference R36 (at -1.81102 0.1016 180) (layer F.SilkS))
    (fp_text value 100K (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 177 N-000173))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6F35)
    (at 125.27534 40.32504 270)
    (attr smd)
    (fp_text reference R37 (at 1.8161 0.0762 360) (layer F.SilkS))
    (fp_text value 150K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 64 /RF_Power))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 177 N-000173))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B700B)
    (at 103.67264 40.07612 270)
    (fp_text reference R38 (at -2.15646 0.0127 270) (layer F.SilkS))
    (fp_text value NC (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 181 N-000179))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D37D6)
    (at 103.67264 42.9768 90)
    (attr smd)
    (fp_text reference R39 (at -0.03302 -0.02286 180) (layer F.SilkS))
    (fp_text value 0R (at -0.93218 0.00762 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 181 N-000179))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D37D9)
    (at 102.17404 42.97426 90)
    (attr smd)
    (fp_text reference R40 (at 0.07366 -0.98298 90) (layer F.SilkS))
    (fp_text value 0R (at -0.91694 0.00508 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 134 N-000094))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E8C9744)
    (at 102.15118 40.09898 270)
    (fp_text reference R41 (at -2.02946 0.94996 270) (layer F.SilkS))
    (fp_text value NC (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 134 N-000094))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3CEB)
    (at 100.65004 49.76114 270)
    (attr smd)
    (fp_text reference R42 (at 2.17932 -0.09144 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 34 /LCD_DATA0))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 180 N-000176))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B704E)
    (at 103.74122 49.76114 270)
    (attr smd)
    (fp_text reference R43 (at 2.13868 -0.01016 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 36 /LCD_DATA2))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 178 N-000174))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7045)
    (at 106.96956 49.74082 270)
    (attr smd)
    (fp_text reference R44 (at 2.11836 -0.01016 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 38 /LCD_DATA4))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 173 N-000167))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3CC5)
    (at 110.14964 49.7205 270)
    (attr smd)
    (fp_text reference R45 (at 2.1082 -0.07112 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 40 /LCD_DATA6))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 175 N-000169))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F67F)
    (at 100.65004 45.8089 270)
    (attr smd)
    (fp_text reference R46 (at -1.72974 0.34036 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 34 /LCD_DATA0))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F679)
    (at 103.74122 45.8089 270)
    (attr smd)
    (fp_text reference R47 (at 0.0508 -0.01778 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 36 /LCD_DATA2))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F672)
    (at 106.9594 45.8089 270)
    (attr smd)
    (fp_text reference R48 (at 0.02032 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 38 /LCD_DATA4))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA4C5)
    (at 110.14964 45.8089 270)
    (attr smd)
    (fp_text reference R49 (at 0.06096 0.01016 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 40 /LCD_DATA6))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B77B5)
    (at 102.1588 49.75098 270)
    (attr smd)
    (fp_text reference R50 (at 2.17932 -0.08128 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 35 /LCD_DATA1))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 179 N-000175))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7049)
    (at 105.31094 49.74082 270)
    (attr smd)
    (fp_text reference R51 (at 2.04978 -0.03048 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 37 /LCD_DATA3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 172 N-000166))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3CC2)
    (at 108.57992 49.7205 270)
    (attr smd)
    (fp_text reference R52 (at 2.13868 -0.1397 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 39 /LCD_DATA5))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 174 N-000168))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3CC9)
    (at 111.72952 49.7205 270)
    (attr smd)
    (fp_text reference R53 (at 2.13868 -0.07874 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 41 /LCD_DATA7))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 176 N-000170))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F67C)
    (at 102.17912 45.8089 270)
    (attr smd)
    (fp_text reference R54 (at 0.03048 -0.07112 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 35 /LCD_DATA1))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F675)
    (at 105.31094 45.79112 270)
    (attr smd)
    (fp_text reference R55 (at 0.06858 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 37 /LCD_DATA3))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F66E)
    (at 108.5596 45.82922 270)
    (attr smd)
    (fp_text reference R56 (at 0.01016 -0.02032 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 39 /LCD_DATA5))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E94D4BF)
    (at 111.7092 45.84954 270)
    (attr smd)
    (fp_text reference R57 (at 0.02032 0.02032 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 41 /LCD_DATA7))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B705C)
    (at 119.7102 49.69002 270)
    (attr smd)
    (fp_text reference R58 (at 2.1082 -0.08128 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 43 /LCD_RES))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 164 N-000153))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7054)
    (at 116.49964 49.64938 270)
    (attr smd)
    (fp_text reference R59 (at 2.08788 -0.08128 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 44 /LCD_WR))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 162 N-000151))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7062)
    (at 121.36882 49.69002 270)
    (attr smd)
    (fp_text reference R60 (at 2.08788 -0.07874 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 33 /LCD_CS1))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 165 N-000154))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7058)
    (at 118.12016 49.6697 270)
    (attr smd)
    (fp_text reference R61 (at 2.04978 -0.0508 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 32 /LCD_A0))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 163 N-000152))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7040)
    (at 114.97056 49.62906 270)
    (attr smd)
    (fp_text reference R62 (at 1.81864 -0.0508 360) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 42 /LCD_RD))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 161 N-000150))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F5C4)
    (at 121.3612 45.93082 270)
    (attr smd)
    (fp_text reference R63 (at -0.12192 -1.20904 270) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 33 /LCD_CS1))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F68E)
    (at 118.12016 45.92066 270)
    (attr smd)
    (fp_text reference R64 (at 0.09906 0.01016 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 32 /LCD_A0))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E94D4C5)
    (at 114.97056 45.88002 270)
    (attr smd)
    (fp_text reference R65 (at 0.1397 0.01016 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 42 /LCD_RD))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F692)
    (at 119.68988 45.94098 270)
    (attr smd)
    (fp_text reference R66 (at 0.05842 -0.0508 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 43 /LCD_RES))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F689)
    (at 116.5098 45.90034 270)
    (attr smd)
    (fp_text reference R67 (at 0.0889 0.04064 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 44 /LCD_WR))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6F43)
    (at 133.70052 45.2247)
    (attr smd)
    (fp_text reference R68 (at -0.02032 -0.95504) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 170 N-000159))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 84 /RudDR_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B76E7)
    (at 38.77564 40.5511)
    (attr smd)
    (fp_text reference R71 (at 2.16408 -0.98044) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 3 /AilDR_SW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 160 N-000148))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B76DB)
    (at 38.9001 46.29912 180)
    (attr smd)
    (fp_text reference R70 (at -2.25044 -0.06096 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 166 N-000155))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 94 /TCut_SW))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E9D)
    (at 171.00042 76.29906 180)
    (attr smd)
    (fp_text reference R69 (at -0.04064 1.03886 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 95 /TELEM_RX))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F3B649C)
    (at 175.3743 80.62468)
    (attr smd)
    (fp_text reference R73 (at -2.17424 0.0762) (layer F.SilkS))
    (fp_text value 1K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 185 N-000185))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 96 /TELEM_TX))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E8C)
    (at 167.89654 81.09966 270)
    (attr smd)
    (fp_text reference R74 (at -2.0701 0.23622 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 169 N-000158))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 195 N-000209))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E92)
    (at 170.29938 83.20024)
    (attr smd)
    (fp_text reference R72 (at -2.17932 0.28956) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 195 N-000209))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6EA9)
    (at 175.3997 82.10042)
    (attr smd)
    (fp_text reference R75 (at 2.09042 0.05842) (layer F.SilkS))
    (fp_text value 1K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 171 N-000161))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 191 N-000191))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module TP (layer Front) (tedit 4E6D330B)
    (at 136.66978 70.52056)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P9 (at 0.39116 -1.67132) (layer F.SilkS))
    (fp_text value CONN_1 (at 1.24968 1.97866) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 2.25044 2.25044) (layers Front F.Paste F.Mask)
      (net 16 /FB_CLOCK))
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6EB0)
    (at 175.3997 83.49996)
    (attr smd)
    (fp_text reference R76 (at 2.09042 0.0508) (layer F.SilkS))
    (fp_text value 3K9 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 191 N-000191))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E6D32DB)
    (at 175.54956 75.25004 180)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q3 (at 0.0635 -0.05334 180) (layer F.SilkS))
    (fp_text value BC857C (at 0.00508 -0.92456 180) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad B smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 185 N-000185))
    (pad C smd rect (at 0 1.016 180) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 191 N-000191))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E6D32D8)
    (at 170.29684 79.10068 180)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q2 (at -0.03302 -0.0381 180) (layer F.SilkS))
    (fp_text value BC847C (at 0.00762 0.75184 180) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 195 N-000209))
    (pad C smd rect (at 0 1.016 180) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 95 /TELEM_RX))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E6D3190)
    (at 131.826 41.79824 90)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at -0.0508 0.04318 90) (layer F.SilkS))
    (fp_text value BC847C (at 0.00762 -0.77724 90) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 177 N-000173))
    (pad C smd rect (at 0 1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 65 /RF_Power_TTL))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E7B4F6C)
    (at 46.9646 79.2734 270)
    (attr smd)
    (fp_text reference R80 (at 0.0508 0.9652 270) (layer F.SilkS))
    (fp_text value 150K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 167 N-000156))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E7B4F65)
    (at 50.165 72.0852 180)
    (attr smd)
    (fp_text reference R81 (at -0.0254 -1.1176 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 168 N-000157))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 167 N-000156))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E6D3752)
    (at 53.87848 71.80072 90)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q4 (at -0.03048 0.04064 90) (layer F.SilkS))
    (fp_text value BC847C (at -0.01016 1.02108 90) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 167 N-000156))
    (pad C smd rect (at 0 1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 60 /PPM_IN))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2A06E5)
    (at 146.29892 46.42612)
    (attr smd)
    (fp_text reference R83 (at 0.01016 -0.95504) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 92 /Speaker))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 115 N-000024))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2A06E8)
    (at 146.28876 48.00092)
    (attr smd)
    (fp_text reference R84 (at 0.09144 1.03886) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 92 /Speaker))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 115 N-000024))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D37F6)
    (at 137.89914 38.61054 180)
    (attr smd)
    (fp_text reference R82 (at 0.09906 -1.09982 180) (layer F.SilkS))
    (fp_text value 1K (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 125 N-000081))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 8 /Buzzer))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6E52)
    (at 132.77596 72.34936 180)
    (attr smd)
    (fp_text reference C16 (at -2.1336 0.32004 180) (layer F.SilkS))
    (fp_text value 1u (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 63 /RESET))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_5x2_GRUVIN (layer Front) (tedit 4E6D39F9)
    (at 191.09944 60.12434 90)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference P10 (at 1.08458 3.64998 90) (layer F.SilkS))
    (fp_text value CONN_5X2 (at -0.15494 -0.01016 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.08 1.27 90) (size 1.69926 1.89992) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /JTAG_TCK))
    (pad 2 thru_hole oval (at -5.08 -1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 3 thru_hole oval (at -2.54 1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /JTAG_TDO))
    (pad 4 thru_hole oval (at -2.54 -1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (pad 5 thru_hole circle (at 0 1.27 90) (size 1.69926 1.69926) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /JTAG_TMS))
    (pad 6 thru_hole circle (at 0 -1.27 90) (size 1.69926 1.69926) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /RESET))
    (pad 7 thru_hole oval (at 2.54 1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (pad 8 thru_hole oval (at 2.54 -1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 5.08 1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /JTAG_TDI))
    (pad 10 thru_hole oval (at 5.08 -1.27 90) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model pin_array/pins_array_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E11EF52)
    (at 187.325 46.8503 270)
    (attr smd)
    (fp_text reference R91 (at 0.97028 -1.42494 360) (layer F.SilkS))
    (fp_text value 200R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 118 N-000039))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 76 /ROT_ENC_2_A))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_3X2_GRUVIN (layer Front) (tedit 4E6D39F4)
    (at 191.00038 72.52462 270)
    (descr "Double rangee de contacts 2 x 4 pins")
    (tags CONN)
    (attr smd)
    (fp_text reference P1 (at 0.05588 -3.64998 270) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 0.20574 0.03048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 270) (size 1.69926 1.89992) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 /SD_MISO))
    (pad 2 thru_hole oval (at -2.54 -1.27 270) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (pad 3 thru_hole oval (at 0 1.27 270) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 /SD_SCK))
    (pad 4 thru_hole oval (at 0 -1.27 270) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 /SD_MOSI))
    (pad 5 thru_hole oval (at 2.54 1.27 270) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /RESET))
    (pad 6 thru_hole oval (at 2.54 -1.27 270) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d\connectors\pins_array_3x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module SOT89_OGI (layer Front) (tedit 4E0B721B)
    (at 85.51926 40.90924)
    (attr smd)
    (fp_text reference U1 (at -1.9304 -1.86944) (layer F.SilkS))
    (fp_text value 78L05 (at 0 0.20066) (layer F.SilkS) hide)
    (pad VO smd rect (at -1.50114 1.89992) (size 0.70104 1.19888) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad GND smd rect (at 0 1.50114) (size 0.70104 1.99898) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad VI smd rect (at 1.50114 1.89992) (size 0.70104 1.19888) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (pad GND smd rect (at 0 -0.89916) (size 2.19964 2.80162) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model packages3d\smd\SOT89.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT89_GIO (layer Front) (tedit 4E84F560)
    (at 85.60054 47.72406)
    (attr smd)
    (fp_text reference U3 (at -2.02946 -1.8542) (layer F.SilkS))
    (fp_text value LN-6206-30 (at -0.67056 2.26568) (layer F.SilkS) hide)
    (pad GND smd rect (at -1.50114 1.89992) (size 0.70104 1.19888) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad VI smd rect (at 0 1.50114) (size 0.70104 1.99898) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad VO smd rect (at 1.50114 1.89992) (size 0.70104 1.19888) (layers Front F.Paste F.Mask)
      (net 102 /Vcc_3V3))
    (pad VI smd rect (at 0 -0.89916) (size 2.19964 2.80162) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model packages3d\smd\SOT89.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DA1)
    (at 41.62552 58.34888)
    (attr smd)
    (fp_text reference R96 (at -1.69672 -0.00762 90) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 113 N-000022))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 74 /ROT_ENC_1_B))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DA7)
    (at 41.69918 60.325)
    (attr smd)
    (fp_text reference R95 (at -1.79832 -0.05588 90) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 114 N-000023))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 73 /ROT_ENC_1_A))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6B36)
    (at 183.27624 46.7995 270)
    (attr smd)
    (fp_text reference R94 (at -0.18034 1.55702 360) (layer F.SilkS))
    (fp_text value 200R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 116 N-000036))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 78 /ROT_ENC_2_PUSH))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6D9C)
    (at 41.62552 56.3245)
    (attr smd)
    (fp_text reference R93 (at -1.74498 -0.01524 90) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 112 N-000021))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 75 /ROT_ENC_1_PUSH))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6B45)
    (at 185.34888 46.8249 270)
    (attr smd)
    (fp_text reference R92 (at 1.87452 1.22936 360) (layer F.SilkS))
    (fp_text value 200R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 117 N-000037))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 77 /ROT_ENC_2_B))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DAF)
    (at 45.47616 58.27522)
    (attr smd)
    (fp_text reference C96 (at 1.89484 -0.03556 90) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 74 /ROT_ENC_1_B))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DB3)
    (at 45.49902 60.325)
    (attr smd)
    (fp_text reference C95 (at 1.87198 0.00508 90) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 73 /ROT_ENC_1_A))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6B22)
    (at 183.2991 50.57394 270)
    (attr smd)
    (fp_text reference C94 (at 1.73482 0.02794 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 78 /ROT_ENC_2_PUSH))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DAC)
    (at 45.47616 56.3245)
    (attr smd)
    (fp_text reference C93 (at 1.89484 -0.01524 90) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 75 /ROT_ENC_1_PUSH))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6B1A)
    (at 185.34888 50.57394 270)
    (attr smd)
    (fp_text reference C92 (at 1.73482 0 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 77 /ROT_ENC_2_B))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6B10)
    (at 187.325 50.57394 270)
    (attr smd)
    (fp_text reference C91 (at 1.73482 -0.0762 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 76 /ROT_ENC_2_A))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B77AD)
    (at 102.51948 58.18124 270)
    (attr smd)
    (fp_text reference C30 (at 0.01016 1.04648 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module HOLE_M2.5 (layer Front) (tedit 4E6D3242)
    (at 158.39948 35.0012)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M2.5 (at -0.03048 0.1397) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M3 (layer Front) (tedit 4DD3F5BB)
    (at 194.5005 34.0995)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M3 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.00126 5.00126) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M2.5 (layer Front) (tedit 4DD948E5)
    (at 156.99994 81.20126)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M2.5 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M3 (layer Front) (tedit 4E6D37A3)
    (at 188.8998 80.40116)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M3 (at -0.50038 2.42824) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.00126 5.00126) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M2.5 (layer Front) (tedit 4E6D3629)
    (at 69.7992 81.20126)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H5 (at -1.14046 -2.68224) (layer F.SilkS) hide)
    (fp_text value HOLE_M2.5 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M3 (layer Front) (tedit 4E6D366F)
    (at 39.90086 80.0989)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M3 (at 0.14986 2.57048) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.00126 5.00126) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M2.5 (layer Front) (tedit 4E6BBB98)
    (at 54.39918 59.4995)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H7 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M2.5 (at -0.04826 -0.01016) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M3 (layer Front) (tedit 4E6D31E5)
    (at 34.30016 34.0995)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M3 (at 2.30886 2.79146) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.00126 5.00126) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module HOLE_M2.5 (layer Front) (tedit 4E6D31F3)
    (at 69.7992 35.0012)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference H9 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value HOLE_M2.5 (at -2.05994 2.9083) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.20066))
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DD1)
    (at 40.37076 70.56882 270)
    (attr smd)
    (fp_text reference R7 (at 0.09144 -1.23952 270) (layer F.SilkS))
    (fp_text value 180K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 123 N-000071))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 129 N-000086))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DCA)
    (at 40.3606 67.42938 270)
    (attr smd)
    (fp_text reference R15 (at -0.06858 -1.12014 270) (layer F.SilkS))
    (fp_text value 100K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 123 N-000071))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SO8E (layer Front) (tedit 4E0B7755)
    (at 44.87926 69.45884)
    (descr "module CMS SOJ 8 pins etroit")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 3.02006 -2.93878) (layer F.SilkS))
    (fp_text value TPS77601 (at 3.2004 -0.06858 90) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask))
    (pad 1 smd rect (at -1.905 2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 7 smd rect (at -0.635 -2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 123 N-000071))
    (pad 6 smd rect (at 0.635 -2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 129 N-000086))
    (pad 5 smd rect (at 1.905 -2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 129 N-000086))
    (pad 2 smd rect (at -0.635 2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 91 /Spare2\Vib-opt))
    (pad 3 smd rect (at 0.635 2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (pad 4 smd rect (at 1.905 2.667) (size 0.508 1.143) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (model smd/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.32 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DE1)
    (at 42.93108 77.43952)
    (attr smd)
    (fp_text reference C33 (at 0.24892 1.17094) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6DC6)
    (at 38.50894 69.0499 270)
    (attr smd)
    (fp_text reference C34 (at -1.81864 0.04826 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 129 N-000086))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B712F)
    (at 61.2902 75.07986 90)
    (attr smd)
    (fp_text reference R30 (at 0 -1.00076 90) (layer F.SilkS))
    (fp_text value 100R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 131 N-000088))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 59 /Module_PPM))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7119)
    (at 52.27066 81.8896 90)
    (attr smd)
    (fp_text reference R29 (at -0.02032 -1.05156 90) (layer F.SilkS))
    (fp_text value 100R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 133 N-000090))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 126 N-000082))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7116)
    (at 57.96026 82.67954 180)
    (attr smd)
    (fp_text reference R28 (at -0.02032 -1.09982 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 131 N-000088))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7113)
    (at 54.97068 82.67954)
    (attr smd)
    (fp_text reference R27 (at 0.02032 1.06172) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 133 N-000090))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7132)
    (at 64.53124 81.3308)
    (attr smd)
    (fp_text reference R23 (at 0.61976 -1.0414) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 130 N-000087))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 61 /PPM_OUT))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B7127)
    (at 62.02934 81.98104 270)
    (attr smd)
    (fp_text reference R16 (at 1.81864 -0.03048 360) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 132 N-000089))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 61 /PPM_OUT))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E6D363D)
    (at 63.62954 78.4606 90)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q7 (at 0.07112 0.04064 90) (layer F.SilkS))
    (fp_text value BC847C (at 0.1016 0.84074 90) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 130 N-000087))
    (pad C smd rect (at 0 1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 131 N-000088))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E6D362F)
    (at 55.47106 80.10906 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q5 (at 0.02032 -0.04826 270) (layer F.SilkS))
    (fp_text value BC847C (at 0.03048 -0.9398 270) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 132 N-000089))
    (pad C smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 133 N-000090))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7B8A92)
    (at 90.90914 78.64094 270)
    (attr smd)
    (fp_text reference R31 (at -2.25044 0 270) (layer F.SilkS))
    (fp_text value 10K2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 127 N-000084))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 198 N-000213))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7D5E07)
    (at 90.8812 82.40014 90)
    (attr smd)
    (fp_text reference R17 (at -1.71958 -1.22174 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 198 N-000213))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA219)
    (at 87.40902 78.80096 90)
    (attr smd)
    (fp_text reference R33 (at 2.21996 0.04064 90) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 197 N-000212))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA216)
    (at 85.68944 78.78064 90)
    (attr smd)
    (fp_text reference R34 (at 2.23012 0.0508 90) (layer F.SilkS))
    (fp_text value 10K2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 128 N-000085))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 197 N-000212))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA20E)
    (at 84.05114 78.7527 90)
    (attr smd)
    (fp_text reference R77 (at 2.19964 0.0889 90) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 196 N-000211))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0BA213)
    (at 82.47888 78.73238 90)
    (attr smd)
    (fp_text reference R79 (at 2.16154 0.06096 90) (layer F.SilkS))
    (fp_text value 10K2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 193 N-000196))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 196 N-000211))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E0B6F31)
    (at 127.09906 41.88968 270)
    (attr smd)
    (fp_text reference C36 (at 1.8415 0.01016 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 177 N-000173))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module TP (layer Front) (tedit 4E6D379C)
    (at 143.80972 79.02956)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P25 (at -0.24892 -1.76022) (layer F.SilkS))
    (fp_text value CONN_1 (at 2.17932 -2.57048) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 2.25044 2.25044) (layers Front F.Paste F.Mask)
      (net 21 /I2C_SCL))
  )
  (module TP (layer Front) (tedit 4E6D3797)
    (at 143.99006 81.89976)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P26 (at 0.05842 1.91008) (layer F.SilkS))
    (fp_text value CONN_1 (at 2.47904 -1.34874) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 2.25044 2.25044) (layers Front F.Paste F.Mask)
      (net 22 /I2C_SDA))
  )
  (module JUMPER_3PAD (layer Front) (tedit 4E6D366A)
    (at 43.7007 81.71942 270)
    (fp_text reference J4 (at 0.381 -1.94056 360) (layer F.SilkS))
    (fp_text value JUMPER_2W (at 0.04064 -0.06858 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0 0 270) (size 1.00076 1.00076) (layers Front F.Paste F.Mask)
      (net 91 /Spare2\Vib-opt))
    (pad 3 smd rect (at 1.6256 0 270) (size 1.00076 1.00076) (layers Front F.Paste F.Mask)
      (net 103 /Vib-PWM-opt))
    (pad 1 smd rect (at -1.6256 0 270) (size 1.00076 1.00076) (layers Front F.Paste F.Mask)
      (net 91 /Spare2\Vib-opt))
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D35E9)
    (at 148.77034 44.01058 270)
    (attr smd)
    (fp_text reference R85 (at -0.1016 1.02108 270) (layer F.SilkS))
    (fp_text value 100K (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 120 N-000058))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 5 /BATT+_FUSED))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_2MM_2x1 (layer Front) (tedit 4E6D3A1B)
    (at 140.51026 45.48886)
    (descr "2pin 2mm pitch t-hole connector")
    (attr smd)
    (fp_text reference P18 (at -1.8796 -2.66954) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.17094 2.3622) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at 2.00152 0.00762) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 92 /Speaker))
    (pad 1 thru_hole rect (at 0 0.00762) (size 1.50114 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (model packages3d\connectors\conn_2mm_2x1.wrl
      (at (xyz 0.08 0.025 0))
      (scale (xyz 0.3739 0.3739 0.3739))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B78)
    (at 138.85164 53.72862)
    (attr smd)
    (fp_text reference R100 (at -2.30124 -0.46736) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 51 /LH_Up_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 50 /LH_Trim_Up))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B92)
    (at 138.84148 56.61914)
    (attr smd)
    (fp_text reference R99 (at -2.08026 0.762) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 56 /LV_Up_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 55 /LV_Trim_Up))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BA8)
    (at 148.67128 67.2592)
    (attr smd)
    (fp_text reference R98 (at -2.1717 0.1016) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 72 /RIGHT_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 71 /RIGHT))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BB8)
    (at 148.64334 70.06844)
    (attr smd)
    (fp_text reference R97 (at -2.05232 0.02032) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 11 /DOWN_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 10 /DOWN))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B7A)
    (at 138.88212 52.27828)
    (attr smd)
    (fp_text reference R90 (at -2.16154 -0.3683) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 47 /LH_Dwn_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 49 /LH_Trim_Dwn))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B88)
    (at 138.84148 55.17896)
    (attr smd)
    (fp_text reference R89 (at -2.10058 0.34036) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 52 /LV_Dwn_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 54 /LV_Trim_Dwn))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B9E)
    (at 148.66112 65.82918)
    (attr smd)
    (fp_text reference R88 (at -3.32232 -0.04826) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 46 /LEFT_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 45 /LEFT))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BB1)
    (at 148.6535 68.65874)
    (attr smd)
    (fp_text reference R87 (at -1.96342 0.03048) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 99 /UP_P))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 98 /UP))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A78)
    (at 51.17084 42.799 90)
    (attr smd)
    (fp_text reference R86 (at -1.78054 0.04826 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 83 /RV_Up_P))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 82 /RV_Trim_Up))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A98)
    (at 55.26024 42.78884 90)
    (attr smd)
    (fp_text reference R78 (at -1.85166 -0.01016 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 70 /RH_Up_P))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 69 /RH_Trim_Up))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3AC8)
    (at 54.24932 67.55892 180)
    (attr smd)
    (fp_text reference R22 (at -0.03048 -1.14046 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 13 /EXIT_P))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 12 /EXIT))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A67)
    (at 47.15002 42.81932 90)
    (attr smd)
    (fp_text reference R21 (at -1.82118 -0.32004 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 79 /RV_Dwn_P))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 81 /RV_Trim_Dwn))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A90)
    (at 53.13934 42.77106 90)
    (attr smd)
    (fp_text reference R14 (at -1.79832 0.07112 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 66 /RH_Dwn_P))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 68 /RH_Trim_Dwn))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3AB1)
    (at 54.24932 52.9209 180)
    (attr smd)
    (fp_text reference R13 (at -0.0508 -1.14808 180) (layer F.SilkS))
    (fp_text value 200R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 58 /MENU_P))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 57 /MENU))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A5E)
    (at 47.13986 38.44036 90)
    (attr smd)
    (fp_text reference C59 (at -0.06858 -1.0795 90) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 81 /RV_Trim_Dwn))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A80)
    (at 53.13934 38.44036 90)
    (attr smd)
    (fp_text reference C58 (at -1.91008 0.9398 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 68 /RH_Trim_Dwn))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3AA8)
    (at 54.229 51.3207 180)
    (attr smd)
    (fp_text reference C57 (at 0 1.07188 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 57 /MENU))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B39)
    (at 143.13916 52.26812)
    (attr smd)
    (fp_text reference C56 (at -0.0889 -0.99822) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 49 /LH_Trim_Dwn))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B5C)
    (at 143.13154 55.18912)
    (attr smd)
    (fp_text reference C55 (at 2.12852 -0.14986) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 54 /LV_Trim_Dwn))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BBF)
    (at 152.96134 65.82664)
    (attr smd)
    (fp_text reference C54 (at 2.1082 0.0127) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 45 /LEFT))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BD3)
    (at 152.96896 68.6689)
    (attr smd)
    (fp_text reference C53 (at 3.61188 0.02032) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 98 /UP))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A70)
    (at 51.16068 38.44036 90)
    (attr smd)
    (fp_text reference C43 (at -0.6985 -1.0795 90) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 82 /RV_Trim_Up))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3A89)
    (at 55.25008 38.49116 90)
    (attr smd)
    (fp_text reference C42 (at -1.76784 1.27 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 69 /RH_Trim_Up))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3AC0)
    (at 54.20106 65.86982 180)
    (attr smd)
    (fp_text reference C41 (at -0.04826 1.01092 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 12 /EXIT))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B5B)
    (at 143.13154 53.71846)
    (attr smd)
    (fp_text reference C40 (at 2.159 0.00254) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 50 /LH_Trim_Up))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B5E)
    (at 143.13154 56.60898)
    (attr smd)
    (fp_text reference C39 (at 2.1082 -0.01016) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 55 /LV_Trim_Up))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BCC)
    (at 152.96896 67.24904)
    (attr smd)
    (fp_text reference C38 (at 3.47218 0.27178) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 71 /RIGHT))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3BDB)
    (at 152.93086 70.0786)
    (attr smd)
    (fp_text reference C37 (at 3.6703 0.0508) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 10 /DOWN))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT89_OGI (layer Front) (tedit 4E6D3B1C)
    (at 157.51048 43.61942 90)
    (attr smd)
    (fp_text reference U2 (at -1.7399 -1.81864 90) (layer F.SilkS))
    (fp_text value 78L05 (at -2.96926 0.1016 180) (layer F.SilkS) hide)
    (pad VO smd rect (at -1.50114 1.89992 90) (size 0.70104 1.19888) (layers Front F.Paste F.Mask)
      (net 119 N-000057))
    (pad GND smd rect (at 0 1.50114 90) (size 0.70104 1.99898) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad VI smd rect (at 1.50114 1.89992 90) (size 0.70104 1.19888) (layers Front F.Paste F.Mask)
      (net 190 N-000190))
    (pad GND smd rect (at 0 -0.89916 90) (size 2.19964 2.80162) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model packages3d\smd\SOT89.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E7CC873)
    (at 162.7505 42.56024 90)
    (attr smd)
    (fp_text reference C60 (at 0.96012 -1.47066 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 190 N-000190))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E7CC879)
    (at 161.35096 44.48048 270)
    (attr smd)
    (fp_text reference C61 (at 0.5588 -1.44018 360) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 119 N-000057))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D35CF)
    (at 150.6093 41.33088)
    (attr smd)
    (fp_text reference R101 (at 2.33172 0.02032) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 121 N-000059))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 120 N-000058))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer Front) (tedit 4E205BB9)
    (at 151.77008 44.00042 90)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q6 (at -0.07874 0.01016 90) (layer F.SilkS))
    (fp_text value Si2319DS (at -2.09042 -0.22098 180) (layer F.SilkS))
    (pad S smd rect (at -0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 5 /BATT+_FUSED))
    (pad G smd rect (at 0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 120 N-000058))
    (pad D smd rect (at 0 1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 190 N-000190))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module JUMPER_3PAD (layer Front) (tedit 4E6D316D)
    (at 126.54026 50.72126)
    (fp_text reference J1 (at -1.3589 1.70942) (layer F.SilkS))
    (fp_text value JUMPER_2W (at 0.02032 -0.04064) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0 0) (size 1.00076 1.00076) (layers Front F.Paste F.Mask)
      (net 6 /Back_Light_EL_TTL))
    (pad 3 smd rect (at 1.6256 0) (size 1.00076 1.00076) (layers Front F.Paste F.Mask)
      (net 90 /Spare1\LED-BL-opt))
    (pad 1 smd rect (at -1.6256 0) (size 1.00076 1.00076) (layers Front F.Paste F.Mask)
      (net 6 /Back_Light_EL_TTL))
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3B10)
    (at 167.88892 38.02126)
    (attr smd)
    (fp_text reference R102 (at 2.29108 -0.2413) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 119 N-000057))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 122 N-000060))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3430)
    (at 108.21924 76.77912 270)
    (attr smd)
    (fp_text reference R104 (at -1.62814 -0.39878 360) (layer F.SilkS))
    (fp_text value 68R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 100 /USB_D+))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 187 N-000187))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D343B)
    (at 103.77932 74.3204 180)
    (attr smd)
    (fp_text reference R105 (at -0.07874 0.92964 180) (layer F.SilkS))
    (fp_text value 68R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 101 /USB_D-))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 186 N-000186))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3428)
    (at 104.67848 76.75118 270)
    (attr smd)
    (fp_text reference R106 (at 1.61798 0 360) (layer F.SilkS))
    (fp_text value 1K5 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 186 N-000186))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2AE3A9)
    (at 70.43928 76.21016 90)
    (attr smd)
    (fp_text reference R107 (at -0.43942 -1.72974 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 73 /ROT_ENC_1_A))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2AE3D5)
    (at 174.97044 55.61076 180)
    (attr smd)
    (fp_text reference R108 (at -0.05842 0.96012 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 76 /ROT_ENC_2_A))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2AE3BA)
    (at 72.46874 72.63892 180)
    (attr smd)
    (fp_text reference R109 (at 0.32766 0.9779 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 74 /ROT_ENC_1_B))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E2AE3E4)
    (at 173.87062 57.8612 180)
    (attr smd)
    (fp_text reference R110 (at 0.02032 0.97028 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 77 /ROT_ENC_2_B))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_DIODE (layer Front) (tedit 4E6D32FC)
    (at 170.29684 81.8007 180)
    (attr smd)
    (fp_text reference D1 (at -1.8542 -0.03048 180) (layer F.SilkS))
    (fp_text value DIODESIL (at -0.0635 1.0414 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 195 N-000209))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sod523 (layer Front) (tedit 4E8C980E)
    (at 106.50982 76.77912 90)
    (descr SOD523)
    (attr smd)
    (fp_text reference D3 (at 1.72974 -0.02032 180) (layer F.SilkS))
    (fp_text value 3V6 (at -0.42164 0.05842 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8509 0 90) (size 0.59944 0.8001) (layers Front F.Paste F.Mask)
      (net 187 N-000187))
    (pad 1 smd rect (at -0.8509 0 90) (size 0.59944 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sod523 (layer Front) (tedit 4E8C9808)
    (at 102.91826 76.77912 90)
    (descr SOD523)
    (attr smd)
    (fp_text reference D4 (at 1.29794 -1.14046 180) (layer F.SilkS))
    (fp_text value 3V6 (at -0.42164 0.09144 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8509 0 90) (size 0.59944 0.8001) (layers Front F.Paste F.Mask)
      (net 186 N-000186))
    (pad 1 smd rect (at -0.8509 0 90) (size 0.59944 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_DIODE (layer Front) (tedit 4E6D3382)
    (at 36.62934 69.0499 270)
    (attr smd)
    (fp_text reference D16 (at -1.80086 0.07874 360) (layer F.SilkS))
    (fp_text value DIODESCH (at -2.60096 1.23952 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 129 N-000086))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_DIODE (layer Front) (tedit 4E6D3653)
    (at 57.21096 76.37018 90)
    (attr smd)
    (fp_text reference D17 (at 1.7399 0.12954 180) (layer F.SilkS))
    (fp_text value DIODESCH (at 0.0508 -1.05156 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 132 N-000089))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 89 /Sim_Ctrl))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3494)
    (at 88.94064 74.48042 270)
    (attr smd)
    (fp_text reference C62 (at -2.2479 0.09144 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-IGO (layer Front) (tedit 4E6BBAF4)
    (at 91.60002 73.72096 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U5 (at -2.25044 0 270) (layer F.SilkS))
    (fp_text value REF3012 (at -0.55118 -0.98806 270) (layer F.SilkS) hide)
    (pad VO smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 1 +1.2V))
    (pad VI smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad GND smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_3X1_SMP_GRUVIN (layer Front) (tedit 4E6D31ED)
    (at 72.24014 41.021)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference K3 (at 0.254 -2.159) (layer F.SilkS))
    (fp_text value CONN_3 (at 0.04064 0.12954) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.74904 0) (size 1.99898 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 2 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Back_Light_EL_TTL))
    (pad 3 thru_hole circle (at 3.74904 0) (size 1.99898 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (model packages3d\display\backlight_driver_board.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
  )
  (module PIN_ARRAY_3x1_GRUVIN (layer Front) (tedit 4E6D3A48)
    (at 85.29066 83.45932 180)
    (descr "Double rangee de contacts 2 x 4 pins")
    (tags CONN)
    (fp_text reference P21 (at 5.50164 -0.3683 180) (layer F.SilkS))
    (fp_text value CONN_3 (at 0.18034 -0.61976 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 180) (size 1.69926 1.89992) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 127 N-000084))
    (pad 2 thru_hole oval (at 0 1.27 180) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 128 N-000085))
    (pad 3 thru_hole oval (at 2.54 1.27 180) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 193 N-000196))
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E6D3400)
    (at 95.48114 72.84974)
    (attr smd)
    (fp_text reference R24 (at -2.2606 0.14986) (layer F.SilkS))
    (fp_text value 200R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 1 +1.2V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 188 N-000188))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-BCE (layer Front) (tedit 4E7BA587)
    (at 151.1554 38.6842)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q8 (at 0.01524 0.04572) (layer F.SilkS))
    (fp_text value BC847C (at -0.10414 -1.0541) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 189 N-000189))
    (pad C smd rect (at 0 1.016) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 121 N-000059))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E7B4FC3)
    (at 146.812 41.7068)
    (attr smd)
    (fp_text reference R32 (at -0.0762 -1.016) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 6 /Back_Light_EL_TTL))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 189 N-000189))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206_GRUVIN_POL (layer Front) (tedit 4E7B589B)
    (at 79.24038 41.2496 270)
    (attr smd)
    (fp_text reference C12 (at 0 0 360) (layer F.SilkS))
    (fp_text value 47u (at -1.651 0.06096 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206_GRUVIN_POL (layer Front) (tedit 4E7B589B)
    (at 91.19108 40.94988 270)
    (attr smd)
    (fp_text reference C1 (at 0 0 360) (layer F.SilkS))
    (fp_text value 10u (at -1.651 0.06096 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206_GRUVIN_POL (layer Front) (tedit 4E7B589B)
    (at 49.34966 76.68006 90)
    (attr smd)
    (fp_text reference C35 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47u (at -1.651 0.06096 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 29 /Jack_PPM))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 168 N-000157))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206_GRUVIN_POL (layer Front) (tedit 4E7B589B)
    (at 52.30114 76.68006 90)
    (attr smd)
    (fp_text reference C18 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47u (at -1.651 0.06096 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 126 N-000082))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 29 /Jack_PPM))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206_GRUVIN_POL (layer Front) (tedit 4E7B589B)
    (at 43.99026 64.40932)
    (attr smd)
    (fp_text reference C31 (at 0 0 90) (layer F.SilkS))
    (fp_text value 47u (at -1.651 0.06096 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 129 N-000086))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206_GRUVIN_POL (layer Front) (tedit 4E7B589B)
    (at 135.1788 47.9552)
    (attr smd)
    (fp_text reference C11 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10u (at -1.651 0.06096 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 93 /Speaker_TTL))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 115 N-000024))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1210_GRUVIN_POL (layer Front) (tedit 4E7B5854)
    (at 43.01998 75.11034)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C32 (at 0.06096 0.0508 90) (layer F.SilkS))
    (fp_text value 22u (at -1.36906 -0.04064 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.524 0) (size 1.27 2.54) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 1.524 0) (size 1.27 2.54) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.2 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 4E9880F1)
    (at 142.44066 38.42004)
    (attr smd)
    (fp_text reference F1 (at -0.02794 0.72898) (layer F.SilkS))
    (fp_text value FUSE (at -0.01016 -0.44958) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers Front F.Paste F.Mask)
      (net 5 /BATT+_FUSED))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module TP_SML (layer Front) (tedit 4E84F645)
    (at 123.95962 56.1594)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P23 (at -1.38938 -1.09982) (layer F.SilkS))
    (fp_text value CONN_1 (at -0.14986 -2.4892) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.50114 1.50114) (layers Front F.Paste F.Mask)
      (net 91 /Spare2\Vib-opt))
  )
  (module TP_SML (layer Front) (tedit 4E84F640)
    (at 126.29896 56.1594)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P24 (at 1.3208 -1.15824) (layer F.SilkS))
    (fp_text value CONN_1 (at 1.25222 1.45034) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.50114 1.50114) (layers Front F.Paste F.Mask)
      (net 90 /Spare1\LED-BL-opt))
  )
  (module SOT23-BCE (layer Front) (tedit 4E84F429)
    (at 96.30918 46.49978 90)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q9 (at 0.0508 0.03048 90) (layer F.SilkS))
    (fp_text value BC847C (at 0.0508 -0.86868 90) (layer F.SilkS) hide)
    (pad E smd rect (at -0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad B smd rect (at 0.889 -1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 194 N-000208))
    (pad C smd rect (at 0 1.016 90) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 192 N-000193))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23GDS (layer Front) (tedit 4E84F3CA)
    (at 94.43974 41.03116 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q10 (at -0.0508 -0.04064 270) (layer F.SilkS))
    (fp_text value Si2319DS (at -1.97104 -0.1397 360) (layer F.SilkS))
    (pad S smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 15 /Ext_Power))
    (pad G smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 183 N-000182))
    (pad D smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module sod523 (layer Front) (tedit 4E8C97FD)
    (at 92.72016 46.08068 180)
    (descr SOD523)
    (attr smd)
    (fp_text reference D2 (at -0.92964 -0.91948 180) (layer F.SilkS))
    (fp_text value 5V1 (at -0.42926 -0.04826 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8509 0 180) (size 0.59944 0.8001) (layers Front F.Paste F.Mask)
      (net 31 /Jack_Presence_TTL))
    (pad 1 smd rect (at -0.8509 0 180) (size 0.59944 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F4EB)
    (at 92.14104 48.02124)
    (attr smd)
    (fp_text reference R103 (at -1.72212 -0.4318 90) (layer F.SilkS))
    (fp_text value 1K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 31 /Jack_Presence_TTL))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 30 /Jack_Presence))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F58A)
    (at 92.21978 51.22926)
    (attr smd)
    (fp_text reference R111 (at -2.44094 0.07112) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 18 /Hold_PWR_ON))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 194 N-000208))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4FB495B2)
    (at 93.49994 53.04028 180)
    (attr smd)
    (fp_text reference R112 (at 0.01016 -1.14046 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 194 N-000208))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 184 N-000183))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E84F432)
    (at 97.08896 41.94048 90)
    (attr smd)
    (fp_text reference R113 (at 0.96012 1.6383 180) (layer F.SilkS))
    (fp_text value 100K (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 183 N-000182))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 15 /Ext_Power))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4FB598EB)
    (at 96.34982 44.1198 180)
    (attr smd)
    (fp_text reference R114 (at -1.81102 -0.21082 270) (layer F.SilkS))
    (fp_text value 5K1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 192 N-000193))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 183 N-000182))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_DIODE (layer Front) (tedit 4E84F587)
    (at 92.16898 49.62906)
    (attr smd)
    (fp_text reference D5 (at -1.88976 0.7112) (layer F.SilkS))
    (fp_text value DIODESCH (at -0.64008 0.07112) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 31 /Jack_Presence_TTL))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 184 N-000183))
    (model packages3d\smd\sod523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4FB59866)
    (at 95.20936 49.0093)
    (attr smd)
    (fp_text reference C63 (at 2.08026 1.08966) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 194 N-000208))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E932BFF)
    (at 92.63126 44.62018 180)
    (attr smd)
    (fp_text reference R115 (at -1.6891 0.07112 270) (layer F.SilkS))
    (fp_text value 100K (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 30 /Jack_Presence))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E932C18)
    (at 89.04986 43.58894 270)
    (attr smd)
    (fp_text reference R116 (at 0.25146 1.03886 270) (layer F.SilkS))
    (fp_text value NC (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 4 /BATT+))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 30 /Jack_Presence))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4E94D534)
    (at 113.52022 47.5107 90)
    (attr smd)
    (fp_text reference C64 (at 1.64084 -0.21082 180) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F3C1054)
    (at 175.54956 78.04912 180)
    (attr smd)
    (fp_text reference R117 (at -0.10922 -1.0414 180) (layer F.SilkS))
    (fp_text value 1K (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 185 N-000185))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_5X2_GRUVIN (layer Front) (tedit 4F7B73B7)
    (at 114.04092 81.10982)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference P20 (at 4.8006 -3.66014) (layer F.SilkS))
    (fp_text value CONN_8 (at -0.24892 -3.40868) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.08 1.27) (size 1.69926 1.89992) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 GND))
    (pad 2 thru_hole oval (at -5.08 -1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 199 VCC))
    (pad 3 thru_hole oval (at -2.54 1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 124 N-000074))
    (pad 4 thru_hole oval (at -2.54 -1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 N-000011))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.69926 1.69926) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 /Vib-PWM-opt))
    (pad 6 thru_hole circle (at 0 -1.27) (size 1.69926 1.69926) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 N-000010))
    (pad 7 thru_hole oval (at 2.54 1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 111 N-000016))
    (pad 8 thru_hole oval (at 2.54 -1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 N-000015))
    (pad 9 thru_hole oval (at 5.08 1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 108 N-000013))
    (pad 10 thru_hole oval (at 5.08 -1.27) (size 1.69926 1.99898) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 N-000014))
    (model pin_array/pins_array_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4F7920F3)
    (at 111.99114 73.62952 270)
    (attr smd)
    (fp_text reference C65 (at 0.0508 -0.92964 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 199 VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_GRUVIN (layer Front) (tedit 4FB495A8)
    (at 95.20936 50.56124)
    (attr smd)
    (fp_text reference R118 (at 0.04064 1.15824) (layer F.SilkS))
    (fp_text value 10K (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 0.8001) (layers Front F.Paste F.Mask)
      (net 194 N-000208))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer Front) (tedit 42806E04)
    (at 97.16008 54.2798 180)
    (attr smd)
    (fp_text reference L2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 105 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 104 AGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TP_SML (layer Front) (tedit 4FB598C7)
    (at 97.47504 48.63592)
    (fp_text reference P11 (at 1.3208 -1.01854) (layer F.SilkS))
    (fp_text value CONN_1 (at 0.78994 0.35052) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.30048 1.30048) (layers Front F.Paste F.Mask)
      (net 192 N-000193))
  )
  (dimension 55.100091 (width 0.3048) (layer Dwgs.User)
    (gr_text "55.100 mm" (at 21.12496 57.440336 89.89601503) (layer Dwgs.User))
    (feature1 (pts (xy 26.4 85) (xy 19.449363 84.987386)))
    (feature2 (pts (xy 26.5 29.9) (xy 19.549363 29.887386)))
    (crossbar (pts (xy 22.800557 29.893286) (xy 22.700557 84.993286)))
    (arrow1a (pts (xy 22.700557 84.993286) (xy 22.116182 83.86572)))
    (arrow1b (pts (xy 22.700557 84.993286) (xy 23.289021 83.867849)))
    (arrow2a (pts (xy 22.800557 29.893286) (xy 22.212093 31.018723)))
    (arrow2b (pts (xy 22.800557 29.893286) (xy 23.384932 31.020852)))
  )
  (dimension 169.20003 (width 0.3048) (layer Dwgs.User)
    (gr_text "169.200 mm" (at 114.397207 22.224343 0.03386274991) (layer Dwgs.User))
    (feature1 (pts (xy 199 26.9) (xy 198.996247 20.548744)))
    (feature2 (pts (xy 29.8 27) (xy 29.796247 20.648744)))
    (crossbar (pts (xy 29.798168 23.899943) (xy 198.998168 23.799943)))
    (arrow1a (pts (xy 198.998168 23.799943) (xy 197.872012 24.387029)))
    (arrow1b (pts (xy 198.998168 23.799943) (xy 197.871318 23.214189)))
    (arrow2a (pts (xy 29.798168 23.899943) (xy 30.925018 24.485697)))
    (arrow2b (pts (xy 29.798168 23.899943) (xy 30.924324 23.312857)))
  )
  (gr_text 1 (at 106.92892 82.4611) (layer F.SilkS))
  (gr_text G (at 98.5901 84.07908) (layer F.SilkS))
  (gr_text - (at 100.69068 83.96986) (layer F.SilkS))
  (gr_text USB (at 100.08108 74.15022) (layer F.SilkS))
  (gr_text + (at 102.6795 84.0105) (layer F.SilkS))
  (gr_text "http://gruvin9x.googlecode.com\nG9X RC Controller V4.2d (Dirty Epic). TAPR Licence\nSee project site for details" (at 145.10004 60.50026) (layer F.SilkS))
  (gr_text "LED\nB/lite" (at 166.7002 39.81958) (layer F.SilkS))
  (gr_text 1 (at 167.87114 31.20898 90) (layer F.SilkS))
  (gr_text Telemetry (at 172.49902 71.60006) (layer F.SilkS))
  (gr_text "T\nR\nG" (at 185.01106 78.03896) (layer F.SilkS))
  (gr_text "T\nR\nG" (at 160.25114 77.57922) (layer F.SilkS))
  (gr_text Sp2 (at 49.87036 59.92114) (layer F.SilkS))
  (gr_text Sp1 (at 128.66878 56.18988) (layer F.SilkS))
  (gr_text Sp2 (at 123.8504 57.83072) (layer F.SilkS))
  (gr_text SDA (at 147.41906 82.77098) (layer F.SilkS))
  (gr_text SCL (at 147.3708 79.13878) (layer F.SilkS))
  (gr_text PORTH (at 113.3094 77.34046) (layer F.SilkS))
  (gr_text ADC (at 79.00924 79.57058) (layer F.SilkS))
  (gr_text Vib (at 35.8902 78.56982) (layer F.SilkS))
  (gr_text "Rotenc B" (at 44.38904 54.4703) (layer F.SilkS))
  (gr_text "Rotenc A" (at 186.29884 39.10076) (layer F.SilkS))
  (gr_text "Aux\nPwr" (at 155.22956 37.6809) (layer F.SilkS))
  (gr_text 1 (at 106.44886 71.74992) (layer F.SilkS))
  (gr_text 1 (at 66.5988 41.1607) (layer F.SilkS))
  (gr_text 1 (at 122.3391 39.2811) (layer F.SilkS))
  (gr_text 1 (at 172.16882 31.20898 90) (layer F.SilkS))
  (gr_text 1 (at 142.60068 32.34944) (layer F.SilkS))
  (gr_text 1 (at 126.3904 37.59962) (layer F.SilkS))
  (gr_text 1 (at 72.57034 36.76904) (layer F.SilkS))
  (gr_text 1 (at 44.62018 32.53994) (layer F.SilkS))
  (gr_text 1 (at 37.00018 49.42078) (layer F.SilkS))
  (gr_text 1 (at 39.7002 72.9996) (layer F.SilkS))
  (gr_text 1 (at 40.08882 63.71082) (layer F.SilkS))
  (gr_text 1 (at 89.18956 79.71028) (layer F.SilkS))
  (gr_text 1 (at 98.82124 78.52918) (layer F.SilkS))
  (gr_text 1 (at 142.05966 79.44104) (layer F.SilkS))
  (gr_text 1 (at 187.44946 69.09054) (layer F.SilkS))
  (gr_text 1 (at 194.81038 65.44056) (layer F.SilkS))
  (gr_text 1 (at 197.69074 38.97884) (layer F.SilkS))
  (gr_text 1 (at 189.34938 46.17974) (layer F.SilkS))
  (gr_text "EL B/lite" (at 72.18934 43.68038) (layer F.SilkS))
  (gr_text Spkr (at 141.50086 49.57064) (layer F.SilkS))
  (gr_text Clk (at 139.76096 71.02094) (layer F.SilkS))
  (gr_text LCD (at 113.20018 39.63924) (layer F.SilkS))
  (gr_text JTAG (at 187.4012 60.59932 90) (layer F.SilkS))
  (gr_text "SD / MMC" (at 132.44068 77.76972) (layer F.SilkS))
  (gr_text ISP (at 187.30976 72.46874 90) (layer F.SilkS))
  (gr_text TTL (at 180.79974 74.30008) (layer F.SilkS))
  (gr_text RS232 (at 164.09924 74.20102) (layer F.SilkS))
  (gr_arc (start 36.79952 88.99906) (end 36.57092 82.94878) (angle 47) (layer Edge.Cuts) (width 0.50038))
  (gr_arc (start 192.32626 88.99906) (end 188.00064 84.74964) (angle 47.5) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 41.09974 84.74964) (end 187.92444 84.74964) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 198.74992 30.24886) (end 30.24886 30.24886) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 33.25114 77.7494) (end 36.5506 82.94878) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 196.25056 77.7494) (end 192.54978 82.94878) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 196.25056 53.74894) (end 196.25056 77.7494) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 198.74992 50.7492) (end 196.25056 53.74894) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 33.25114 53.74894) (end 33.25114 77.7494) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 30.24886 50.7492) (end 33.25114 53.74894) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 30.24886 30.24886) (end 30.24886 50.7492) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (gr_line (start 198.74992 30.24886) (end 198.74992 50.7492) (angle 90) (layer Edge.Cuts) (width 0.50038))
  (zone (net 105) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (mode segment) (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.89952 87.80018) (xy 202.10018 27.44978) (xy 27.54884 27.65044) (xy 27.54884 87.00008)
      )
    )
  )
  (zone (net 105) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (mode segment) (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.60082 86.79942) (xy 199.60082 28.39974) (xy 28.69692 28.19908) (xy 28.69946 28.19908) (xy 28.39974 28.19908)
        (xy 28.69692 28.19908) (xy 28.30068 85.99932)
      )
    )
  )
)
