(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Z80-FDC: RC2014 Compatible FDC and RTC Module")
    (date "2021-01-25")
    (rev "1.2")
    (company "Designed by Sergey Kiselev")
    (comment 2 "Licensed under CERN-OHL-S: https://cern-ohl.web.cern.ch")
    (comment 3 "Documentation and design files: https://github.com/skiselev/Z80-FDC")
    (comment 4 "Z80-FDC is an open source hardware project")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "Net-(C9-Pad1)")
  (net 4 "/A15")
  (net 5 "/A14")
  (net 6 "/A13")
  (net 7 "/A12")
  (net 8 "/A11")
  (net 9 "/A10")
  (net 10 "/A9")
  (net 11 "/A8")
  (net 12 "/A7")
  (net 13 "/A6")
  (net 14 "/A5")
  (net 15 "/A4")
  (net 16 "/A3")
  (net 17 "/A2")
  (net 18 "/A1")
  (net 19 "/A0")
  (net 20 "/~{M1}")
  (net 21 "/~{RESET}")
  (net 22 "/CPU_CLK")
  (net 23 "/~{INT}")
  (net 24 "/~{MREQ}")
  (net 25 "/~{WR}")
  (net 26 "/~{RD}")
  (net 27 "/~{IORQ}")
  (net 28 "/D0")
  (net 29 "/D1")
  (net 30 "/D2")
  (net 31 "/D3")
  (net 32 "/D4")
  (net 33 "/D5")
  (net 34 "/D6")
  (net 35 "/D7")
  (net 36 "/~{RFSH}")
  (net 37 "/~{BUSACK}")
  (net 38 "/~{HALT}")
  (net 39 "/~{BUSREQ}")
  (net 40 "/~{WAIT}")
  (net 41 "/~{NMI}")
  (net 42 "/TXDA")
  (net 43 "/RXDA")
  (net 44 "/USR1")
  (net 45 "Net-(C10-Pad1)")
  (net 46 "/~{DENSEL}")
  (net 47 "unconnected-(J1-Pad4)")
  (net 48 "unconnected-(J1-Pad6)")
  (net 49 "/~{INDEX}")
  (net 50 "/~{MEA}")
  (net 51 "/~{DSB}")
  (net 52 "/~{DSA}")
  (net 53 "/~{MEB}")
  (net 54 "/~{DIR}")
  (net 55 "/UART_CLK")
  (net 56 "/~{STEP}")
  (net 57 "/~{WDATA}")
  (net 58 "/~{WE}")
  (net 59 "/~{TRK0}")
  (net 60 "/~{HDSEL}")
  (net 61 "/~{RDATA}")
  (net 62 "/~{WP}")
  (net 63 "/~{DC}")
  (net 64 "unconnected-(J4-Pad4)")
  (net 65 "/RESET")
  (net 66 "/USR2")
  (net 67 "/USR3")
  (net 68 "/~{FDC_CS}")
  (net 69 "/~{DACK}")
  (net 70 "unconnected-(U1-Pad15)")
  (net 71 "unconnected-(U1-Pad16)")
  (net 72 "/~{DOR_WR}")
  (net 73 "/~{CCR_WR}")
  (net 74 "unconnected-(U1-Pad22)")
  (net 75 "unconnected-(U1-Pad38)")
  (net 76 "/RTC_CE")
  (net 77 "/RTC_IO")
  (net 78 "/RTC_CLK")
  (net 79 "/RTC_WE")
  (net 80 "/RTC_IN")
  (net 81 "/~{RTC_WR}")
  (net 82 "Net-(U4-Pad4)")
  (net 83 "unconnected-(U4-Pad7)")
  (net 84 "unconnected-(U4-Pad9)")
  (net 85 "unconnected-(U4-Pad10)")
  (net 86 "/~{RTC_CS}")
  (net 87 "unconnected-(U4-Pad15)")
  (net 88 "/~{RTC_RD}")
  (net 89 "Net-(R1-Pad2)")
  (net 90 "unconnected-(U3-Pad5)")
  (net 91 "unconnected-(U3-Pad2)")
  (net 92 "Net-(C8-Pad1)")
  (net 93 "Net-(U2-Pad2)")
  (net 94 "Net-(U2-Pad3)")
  (footprint "My_Components:Conn_Pin_Header_10x1_2.54mm_Right_Angle" (layer "F.Cu")
    (tedit 626C4E3B)
    (at 179.07 124.46)
    (descr "Pin Header, 10x1, 2.54mm pitch")
    (tags "CONN 10x1")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 5.715 5.08) (layer "F.SilkS"))
    (fp_text value "RC2014_EXT" (at 6.0325 6.985) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "/~{RFSH}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "unconnected-(J4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "/UART_CLK") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "/~{BUSACK}") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "/~{HALT}") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "/~{BUSREQ}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "/~{WAIT}") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "/~{NMI}") (pinfunction "Pin_10") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 130.2258 95.631)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "3.2mm" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "My_Components:Conn_Pin_Header_39x1_2.54mm_Right_Angle" (layer "F.Cu")
    (tedit 626C4DFD)
    (at 175.26 127)
    (descr "Pin Header, 39x1, 2.54mm pitch")
    (tags "CONN 39x1")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value "RC2014_BUS" (at 0 4.445) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "/A15") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "/A14") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "/A13") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "/A12") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at -38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "/A11") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "/A10") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "/A9") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "/A8") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at -27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "/A7") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at -25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "/A6") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at -22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "/A5") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at -20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "/A4") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/A3") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "/A2") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at -12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "/A1") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at -10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "/A0") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "/~{M1}") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "/~{RESET}") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "/CPU_CLK") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "/~{INT}") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "/~{MREQ}") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "/~{WR}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "/~{RD}") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "/~{IORQ}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "/D0") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "/D1") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "/D2") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "/D3") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "/D4") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "/D5") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "/D6") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle (at 35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "/D7") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole circle (at 38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "/TXDA") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole circle (at 40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "/RXDA") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole circle (at 43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "/USR1") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole circle (at 45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "/USR2") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole circle (at 48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "/USR3") (pinfunction "Pin_39") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 185.42 102.87 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at -2.54 -1.905 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.5875 -1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 129.54 103.505 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at -2.54 -1.905 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.5875 -1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 157.48 102.87 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 2.54 1.905 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at -1.5875 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_TE_2-644488-2_2P_2.54mm" (layer "F.Cu")
    (tedit 6271FC4E)
    (at 162.56 86.36 180)
    (descr "Connector, Friction Lock, 2 Positions, 2.54mm Pitch")
    (tags "CONN FRICTION LOCK 2P")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 7.112 5.3975) (layer "F.SilkS"))
    (fp_text value "Floppy 5V" (at 6.985 3.81) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 129.54 115.57 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 2.54 1.905 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at -1.5875 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 162.56 96.52)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at -2.54 -1.905 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.5875 -1.905) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 157.48 115.57 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 2.54 1.905 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at -1.5875 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 6001348F)
    (at 220.98 100.33 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C10" (at -2.2225 -1.905 90) (layer "F.SilkS"))
    (fp_text value "15pF" (at 1.905 -1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask "F.SilkS")
      (net 45 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Elec_Radial_6.3mm" (layer "F.Cu")
    (tedit 61A5155F)
    (at 157.48 122.428 -90)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 0.508 -4.572 180) (layer "F.SilkS"))
    (fp_text value "47uF" (at 2.032 -4.572 180) (layer "F.SilkS"))
    (fp_text user "+" (at -2.794 -2.794 -90) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -1.25 0 270) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.25 0 270) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/c_vert_c2v10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Crystal_HC-49U_Vert" (layer "F.Cu")
    (tedit 60825482)
    (at 215.9 105.41 -90)
    (descr "Quartz Crystal, HC-49U, Vertical")
    (tags "QUARTZ CRYSTAL HC49U VERT")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "Y1" (at 2.54 3.4925 90) (layer "F.SilkS"))
    (fp_text value "16MHz" (at -1.905 3.4925 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.44094 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "Net-(C10-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.44094 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(C9-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "discret/crystal_hc18u_vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Crystal_32K_Horiz" (layer "F.Cu")
    (tedit 603D2699)
    (at 159.931316 91.4475 90)
    (descr "crystal resonator for RTC, 32768 Hz")
    (tags "CRYSTAL RTC")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y2" (at 0.96 13.423684) (layer "F.SilkS"))
    (fp_text value "32768Hz" (at -0.6275 13.423684) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 93 "Net-(U2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 94 "Net-(U2-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -1.5875 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad "3" thru_hole circle locked (at 1.5875 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (model "discret/c_vert_c1v5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Res_762" (layer "F.Cu")
    (tedit 626C4978)
    (at 182.88 115.57 -90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags "RESISTOR")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "R2" (at 5.715 0 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at -6.0325 -2.54 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 65 "/RESET") (pintype "passive"))
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP14_300" (layer "F.Cu")
    (tedit 619D8A4B)
    (at 170.18 115.57)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -6.35 5.715) (layer "F.SilkS"))
    (fp_text value "74HCT125" (at 5.08 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "/~{M1}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "input"))
    (pad "3" thru_hole circle locked (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 89 "Net-(R1-Pad2)") (pintype "tri_state"))
    (pad "4" thru_hole circle locked (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "/~{RESET}") (pintype "input"))
    (pad "5" thru_hole circle locked (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 65 "/RESET") (pintype "tri_state"))
    (pad "7" thru_hole circle locked (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "/D0") (pintype "tri_state"))
    (pad "9" thru_hole circle locked (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 77 "/RTC_IO") (pintype "input"))
    (pad "10" thru_hole circle locked (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 88 "/~{RTC_RD}") (pintype "input"))
    (pad "11" thru_hole circle locked (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 77 "/RTC_IO") (pintype "tri_state"))
    (pad "12" thru_hole circle locked (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "/RTC_IN") (pintype "input"))
    (pad "13" thru_hole circle locked (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 79 "/RTC_WE") (pintype "input"))
    (pad "14" thru_hole circle locked (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP16_300" (layer "F.Cu")
    (tedit 619D8A53)
    (at 143.51 115.57)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at -7.62 5.715) (layer "F.SilkS"))
    (fp_text value "74HCT138" (at 5.3975 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "/A3") (pinfunction "A0") (pintype "input"))
    (pad "2" thru_hole circle locked (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "/A4") (pinfunction "A1") (pintype "input"))
    (pad "3" thru_hole circle locked (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "/A7") (pinfunction "A2") (pintype "input"))
    (pad "4" thru_hole circle locked (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 82 "Net-(U4-Pad4)") (pinfunction "E1") (pintype "input"))
    (pad "5" thru_hole circle locked (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 89 "Net-(R1-Pad2)") (pinfunction "E2") (pintype "input"))
    (pad "6" thru_hole circle locked (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "/A6") (pinfunction "E3") (pintype "input"))
    (pad "7" thru_hole circle locked (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 83 "unconnected-(U4-Pad7)") (pinfunction "O7") (pintype "output+no_connect"))
    (pad "8" thru_hole circle locked (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole circle locked (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 84 "unconnected-(U4-Pad9)") (pinfunction "O6") (pintype "output+no_connect"))
    (pad "10" thru_hole circle locked (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 85 "unconnected-(U4-Pad10)") (pinfunction "O5") (pintype "output+no_connect"))
    (pad "11" thru_hole circle locked (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 86 "/~{RTC_CS}") (pinfunction "O4") (pintype "output"))
    (pad "12" thru_hole circle locked (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 72 "/~{DOR_WR}") (pinfunction "O3") (pintype "output"))
    (pad "13" thru_hole circle locked (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 68 "/~{FDC_CS}") (pinfunction "O2") (pintype "output"))
    (pad "14" thru_hole circle locked (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 73 "/~{CCR_WR}") (pinfunction "O1") (pintype "output"))
    (pad "15" thru_hole circle locked (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 87 "unconnected-(U4-Pad15)") (pinfunction "O0") (pintype "output+no_connect"))
    (pad "16" thru_hole circle locked (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP14_300" (layer "F.Cu")
    (tedit 619D8A4B)
    (at 170.18 102.87)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at -6.35 5.715) (layer "F.SilkS"))
    (fp_text value "74HCT32" (at 5.3975 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 86 "/~{RTC_CS}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "/~{WR}") (pintype "input"))
    (pad "3" thru_hole circle locked (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 81 "/~{RTC_WR}") (pintype "output"))
    (pad "4" thru_hole circle locked (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 72 "/~{DOR_WR}") (pintype "input"))
    (pad "5" thru_hole circle locked (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "/~{RD}") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 69 "/~{DACK}") (pintype "output"))
    (pad "7" thru_hole circle locked (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 82 "Net-(U4-Pad4)") (pintype "output"))
    (pad "9" thru_hole circle locked (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "/~{IORQ}") (pintype "input"))
    (pad "10" thru_hole circle locked (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "/A5") (pintype "input"))
    (pad "11" thru_hole circle locked (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 88 "/~{RTC_RD}") (pintype "output"))
    (pad "12" thru_hole circle locked (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "/~{RD}") (pintype "input"))
    (pad "13" thru_hole circle locked (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 86 "/~{RTC_CS}") (pintype "input"))
    (pad "14" thru_hole circle locked (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP8_300" (layer "F.Cu")
    (tedit 619E89A5)
    (at 153.67 91.44 90)
    (descr "8 pins DIL package, round pads")
    (tags "DIP DIL DIP8 DIL8")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -3.81 -5.715 90) (layer "F.SilkS"))
    (fp_text value "DS1302+" (at 6.096 0 180) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC2") (pintype "power_in"))
    (pad "2" thru_hole circle locked (at -1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 93 "Net-(U2-Pad2)") (pinfunction "X1") (pintype "input"))
    (pad "3" thru_hole circle locked (at 1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 94 "Net-(U2-Pad3)") (pinfunction "X2") (pintype "input"))
    (pad "4" thru_hole circle locked (at 3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 76 "/RTC_CE") (pinfunction "CE") (pintype "input"))
    (pad "6" thru_hole circle locked (at 1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 77 "/RTC_IO") (pinfunction "I/O") (pintype "bidirectional"))
    (pad "7" thru_hole circle locked (at -1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 78 "/RTC_CLK") (pinfunction "SCLK") (pintype "input"))
    (pad "8" thru_hole circle locked (at -3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 92 "Net-(C8-Pad1)") (pinfunction "VCC1") (pintype "power_in"))
    (model "dil/dil_8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_SIL6" (layer "F.Cu")
    (tedit 603D2E41)
    (at 184.15 92.71)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RN1" (at -5.08 2.54) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 2.54) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "common") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "/~{DC}") (pinfunction "R1") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "/~{RDATA}") (pinfunction "R2") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "/~{WP}") (pinfunction "R3") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 59 "/~{TRK0}") (pinfunction "R4") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 "/~{INDEX}") (pinfunction "R5") (pintype "passive"))
  )
  (footprint "My_Components:Cap_Super_Radial_13.5mm" (layer "F.Cu")
    (tedit 626ABAF1)
    (at 140.97 89.535 180)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at 1.5875 -7.62) (layer "F.SilkS"))
    (fp_text value "0.22F" (at -2.2225 -7.62) (layer "F.SilkS"))
    (fp_text user "+" (at -5.3975 -5.3975) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -2.5 0 180) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 92 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/c_vert_c2v10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_PLCC44_TH" (layer "F.Cu")
    (tedit 61A920C2)
    (at 199.39 106.68 90)
    (descr "PLCC44 Socket, Through Hole")
    (tags "PLCC PLCC44")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -12.3825 -3.81 180) (layer "F.SilkS"))
    (fp_text value "37C65" (at -12.3825 3.81 180) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at 1.27 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "/~{RD}") (pinfunction "~{RD}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -1.27 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "/~{WR}") (pinfunction "~{WR}") (pintype "input"))
    (pad "3" thru_hole circle locked (at -1.27 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 68 "/~{FDC_CS}") (pinfunction "~{CS}") (pintype "input"))
    (pad "4" thru_hole circle locked (at -3.81 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "5" thru_hole circle locked (at -3.81 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 69 "/~{DACK}") (pinfunction "~{DACK}") (pintype "input"))
    (pad "6" thru_hole circle locked (at -6.35 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "TC") (pintype "input"))
    (pad "7" thru_hole circle locked (at -8.89 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "/D0") (pinfunction "DB0") (pintype "tri_state"))
    (pad "8" thru_hole circle locked (at -6.35 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "/D1") (pinfunction "DB1") (pintype "tri_state"))
    (pad "9" thru_hole circle locked (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "/D2") (pinfunction "DB2") (pintype "tri_state"))
    (pad "10" thru_hole circle locked (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/D3") (pinfunction "DB3") (pintype "tri_state"))
    (pad "11" thru_hole circle locked (at -8.89 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "/D4") (pinfunction "DB4") (pintype "tri_state"))
    (pad "12" thru_hole circle locked (at -6.35 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "/D5") (pinfunction "DB5") (pintype "tri_state"))
    (pad "13" thru_hole circle locked (at -8.89 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "/D6") (pinfunction "DB6") (pintype "tri_state"))
    (pad "14" thru_hole circle locked (at -6.35 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "/D7") (pinfunction "DB7") (pintype "tri_state"))
    (pad "15" thru_hole circle locked (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 70 "unconnected-(U1-Pad15)") (pinfunction "DMA") (pintype "output+no_connect"))
    (pad "16" thru_hole circle locked (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 71 "unconnected-(U1-Pad16)") (pinfunction "IRQ") (pintype "output+no_connect"))
    (pad "17" thru_hole circle locked (at -8.89 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "~{DCHGEN}") (pintype "input"))
    (pad "18" thru_hole circle locked (at -6.35 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 72 "/~{DOR_WR}") (pinfunction "~{LDOR}") (pintype "input"))
    (pad "19" thru_hole circle locked (at -6.35 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 73 "/~{CCR_WR}") (pinfunction "~{LDCR}") (pintype "input"))
    (pad "20" thru_hole circle locked (at -3.81 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 65 "/RESET") (pinfunction "RST") (pintype "input"))
    (pad "21" thru_hole circle locked (at -3.81 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "/~{RDATA}") (pinfunction "~{RDD}") (pintype "input"))
    (pad "22" thru_hole circle locked (at -1.27 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 74 "unconnected-(U1-Pad22)") (pinfunction "~{XT2}") (pintype "input+no_connect"))
    (pad "23" thru_hole circle locked (at -1.27 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "XT2") (pintype "input"))
    (pad "24" thru_hole circle locked (at 1.27 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "DRV") (pintype "input"))
    (pad "25" thru_hole circle locked (at 1.27 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(C9-Pad1)") (pinfunction "~{XT1}") (pintype "input"))
    (pad "26" thru_hole circle locked (at 3.81 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "Net-(C10-Pad1)") (pinfunction "XT1") (pintype "input"))
    (pad "27" thru_hole circle locked (at 3.81 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "PCVAL") (pintype "input"))
    (pad "28" thru_hole circle locked (at 6.35 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 60 "/~{HDSEL}") (pinfunction "~{HS}") (pintype "output"))
    (pad "29" thru_hole circle locked (at 8.89 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 58 "/~{WE}") (pinfunction "~{WE}") (pintype "output"))
    (pad "30" thru_hole circle locked (at 6.35 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 57 "/~{WDATA}") (pinfunction "~{WD}") (pintype "output"))
    (pad "31" thru_hole circle locked (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 54 "/~{DIR}") (pinfunction "~{DIRC}") (pintype "output"))
    (pad "32" thru_hole circle locked (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 56 "/~{STEP}") (pinfunction "~{STEP}") (pintype "output"))
    (pad "33" thru_hole circle locked (at 8.89 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 52 "/~{DSA}") (pinfunction "~{DS1}") (pintype "output"))
    (pad "34" thru_hole circle locked (at 6.35 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle locked (at 8.89 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 51 "/~{DSB}") (pinfunction "~{DS2}") (pintype "output"))
    (pad "36" thru_hole circle locked (at 6.35 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 "/~{MEA}") (pinfunction "~{DS3}/~{MO1}") (pintype "output"))
    (pad "37" thru_hole circle locked (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 "/~{MEB}") (pinfunction "~{DS4}/~{MO2}") (pintype "output"))
    (pad "38" thru_hole circle locked (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 75 "unconnected-(U1-Pad38)") (pinfunction "~{HDL}") (pintype "output+no_connect"))
    (pad "39" thru_hole circle locked (at 8.89 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "/~{DENSEL}") (pinfunction "~{RWC}/~{RPM}") (pintype "output"))
    (pad "40" thru_hole circle locked (at 6.35 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "/~{DC}") (pinfunction "~{DCHG}") (pintype "input"))
    (pad "41" thru_hole circle locked (at 6.35 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "/~{WP}") (pinfunction "~{WP}") (pintype "input"))
    (pad "42" thru_hole circle locked (at 3.81 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 59 "/~{TRK0}") (pinfunction "~{TR00}") (pintype "input"))
    (pad "43" thru_hole circle locked (at 3.81 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 "/~{INDEX}") (pinfunction "~{IDX}") (pintype "input"))
    (pad "44" thru_hole circle locked (at 1.27 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
  )
  (footprint "My_Components:IC_DIP16_300" (layer "F.Cu")
    (tedit 619D8A53)
    (at 143.51 102.87)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -7.62 5.715) (layer "F.SilkS"))
    (fp_text value "74HCT174" (at 6.35 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "/~{RESET}") (pinfunction "~{Mr}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 91 "unconnected-(U3-Pad2)") (pinfunction "Q0") (pintype "output+no_connect"))
    (pad "3" thru_hole circle locked (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/D3") (pinfunction "D0") (pintype "input"))
    (pad "4" thru_hole circle locked (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "/D0") (pinfunction "D1") (pintype "input"))
    (pad "5" thru_hole circle locked (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 90 "unconnected-(U3-Pad5)") (pinfunction "Q1") (pintype "output+no_connect"))
    (pad "6" thru_hole circle locked (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "/D5") (pinfunction "D2") (pintype "input"))
    (pad "7" thru_hole circle locked (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 79 "/RTC_WE") (pinfunction "Q2") (pintype "output"))
    (pad "8" thru_hole circle locked (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole circle locked (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 81 "/~{RTC_WR}") (pinfunction "Cp") (pintype "input"))
    (pad "10" thru_hole circle locked (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 "/RTC_IN") (pinfunction "Q3") (pintype "output"))
    (pad "11" thru_hole circle locked (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "/D7") (pinfunction "D3") (pintype "input"))
    (pad "12" thru_hole circle locked (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 78 "/RTC_CLK") (pinfunction "Q4") (pintype "output"))
    (pad "13" thru_hole circle locked (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "/D6") (pinfunction "D4") (pintype "input"))
    (pad "14" thru_hole circle locked (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "/D4") (pinfunction "D5") (pintype "input"))
    (pad "15" thru_hole circle locked (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 76 "/RTC_CE") (pinfunction "Q5") (pintype "output"))
    (pad "16" thru_hole circle locked (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Res_762" (layer "F.Cu")
    (tedit 626C4978)
    (at 185.42 115.57 -90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags "RESISTOR")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "R1" (at 5.715 0 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at -6.0325 2.54 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 89 "Net-(R1-Pad2)") (pintype "passive"))
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_17x2_2.54mm_Shrouded" (layer "F.Cu")
    (tedit 61A9C916)
    (at 193.04 83.82 180)
    (descr "Pin Header, 13x2, 2.54mm pitch, shrouded")
    (tags "CONN PIN HEADER 13x2")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 4.7625 -5.715) (layer "F.SilkS"))
    (fp_text value "Floppy" (at -5.08 -5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -20.32 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -20.32 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "/~{DENSEL}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -17.78 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -17.78 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle locked (at -15.24 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at -15.24 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle locked (at -12.7 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at -12.7 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "/~{INDEX}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at -10.16 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at -10.16 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "/~{MEA}") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle locked (at -7.62 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle locked (at -7.62 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "/~{DSB}") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle locked (at -5.08 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle locked (at -5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "/~{DSA}") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle locked (at -2.54 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle locked (at -2.54 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "/~{MEB}") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle locked (at 0 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle locked (at 0 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "/~{DIR}") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle locked (at 2.54 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle locked (at 2.54 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "/~{STEP}") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle locked (at 5.08 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle locked (at 5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "/~{WDATA}") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle locked (at 7.62 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle locked (at 7.62 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "/~{WE}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle locked (at 10.16 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle locked (at 10.16 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "/~{TRK0}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle locked (at 12.7 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle locked (at 12.7 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 "/~{WP}") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle locked (at 15.24 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle locked (at 15.24 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "/~{RDATA}") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle locked (at 17.78 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle locked (at 17.78 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 "/~{HDSEL}") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle locked (at 20.32 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle locked (at 20.32 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "/~{DC}") (pinfunction "Pin_34") (pintype "passive"))
    (model "pin_array/pins_array_13x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 220.6625 93.0275)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_Open_Hardware_Small" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 220.98 110.49 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at 2.54 1.905 90) (layer "F.SilkS"))
    (fp_text value "47pF" (at -1.5875 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 220.6625 93.0275 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (property "Sheetfile" "Z80-FDC.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Logo_Open_Hardware_Small" (at 0.75 0) (layer "B.Fab") hide)
  )
  (gr_line (start 140.6271 78.8924) (end 219.2026 78.8924) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 125.1966 127.7366) (end 125.1966 94.3229) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 125.49418 93.60448) (end 139.90868 79.18998) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 224.3026 127.7366) (mid 224.00502 128.45502) (end 223.2866 128.7526) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 224.3026 83.9924) (end 224.3026 127.7366) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 223.2866 128.7526) (end 126.2126 128.7526) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 125.1966 94.3229) (mid 125.273939 93.934094) (end 125.49418 93.60448) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 139.90868 79.18998) (mid 140.238294 78.969739) (end 140.6271 78.8924) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 126.2126 128.7526) (mid 125.49418 128.45502) (end 125.1966 127.7366) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 219.2026 78.8924) (mid 222.808845 80.386155) (end 224.3026 83.9924) (layer "Edge.Cuts") (width 0.05))
  (gr_text "~{M1}" (at 172.72 122.8725) (layer "B.SilkS"))
  (gr_text "D6" (at 208.28 125.4125) (layer "B.SilkS"))
  (gr_text "D5" (at 205.74 125.4125) (layer "B.SilkS"))
  (gr_text "D4" (at 203.2 125.4125) (layer "B.SilkS"))
  (gr_text "D3" (at 200.66 125.4125) (layer "B.SilkS"))
  (gr_text "D2" (at 198.12 125.4125) (layer "B.SilkS"))
  (gr_text "D1" (at 195.58 125.4125) (layer "B.SilkS"))
  (gr_text "D0" (at 193.04 125.4125) (layer "B.SilkS"))
  (gr_text "TXDA" (at 213.36 125.4125) (layer "B.SilkS"))
  (gr_text "RXDA" (at 215.9 125.4125) (layer "B.SilkS"))
  (gr_text "USR1" (at 218.44 125.4125) (layer "B.SilkS"))
  (gr_text "USR3" (at 220.98 123.5075) (layer "B.SilkS"))
  (gr_text "A0" (at 165.1 125.4125) (layer "B.SilkS"))
  (gr_text "A1" (at 162.56 125.4125) (layer "B.SilkS"))
  (gr_text "A2" (at 160.02 125.4125) (layer "B.SilkS"))
  (gr_text "A4" (at 154.94 125.4125) (layer "B.SilkS"))
  (gr_text "A3" (at 160.02 123.5075) (layer "B.SilkS"))
  (gr_text "A5" (at 152.4 125.4125) (layer "B.SilkS"))
  (gr_text "A6" (at 149.86 125.4125) (layer "B.SilkS"))
  (gr_text "A7" (at 147.32 125.4125) (layer "B.SilkS"))
  (gr_text "A8" (at 144.78 125.4125) (layer "B.SilkS"))
  (gr_text "A9" (at 142.24 125.4125) (layer "B.SilkS"))
  (gr_text "A10" (at 139.7 125.4125) (layer "B.SilkS"))
  (gr_text "A11" (at 137.16 125.4125) (layer "B.SilkS"))
  (gr_text "A12" (at 134.62 125.4125) (layer "B.SilkS"))
  (gr_text "A13" (at 132.08 125.4125) (layer "B.SilkS"))
  (gr_text "A14" (at 129.54 125.4125) (layer "B.SilkS"))
  (gr_text "A15" (at 127 125.4125) (layer "B.SilkS"))
  (gr_text "USR2" (at 220.98 125.4125) (layer "B.SilkS"))
  (gr_text "~{IORQ}" (at 190.5 122.8725) (layer "B.SilkS"))
  (gr_text "~{NMI}" (at 190.5 121.285) (layer "B.SilkS"))
  (gr_text "~{RD}" (at 187.96 122.8725) (layer "B.SilkS"))
  (gr_text "~{WAIT}" (at 187.96 121.285) (layer "B.SilkS"))
  (gr_text "~{BREQ}" (at 185.42 121.285) (layer "B.SilkS"))
  (gr_text "~{WR}" (at 185.42 122.8725) (layer "B.SilkS"))
  (gr_text "~{HALT}" (at 182.88 121.285) (layer "B.SilkS"))
  (gr_text "~{MREQ}" (at 182.88 122.8725) (layer "B.SilkS"))
  (gr_text "~{BACK}" (at 180.34 121.285) (layer "B.SilkS"))
  (gr_text "~{INT}" (at 180.34 122.8725) (layer "B.SilkS"))
  (gr_text "~{CLK1}" (at 177.8 122.8725) (layer "B.SilkS"))
  (gr_text "~{CLK2}" (at 177.8 121.285) (layer "B.SilkS"))
  (gr_text "~{RESET}" (at 175.26 121.76125) (layer "B.SilkS"))
  (gr_text "~{RFSH}" (at 172.4025 121.285) (layer "B.SilkS"))
  (gr_text "VCC" (at 170.18 122.8725) (layer "B.SilkS"))
  (gr_text "GND" (at 167.64 122.8725) (layer "B.SilkS"))
  (gr_text "Flock - Floppy Disk Controller and Real Time Clock - Version 1.0\nCopyright (C) 2022 Sergey Kiselev" (at 220.6625 87.63) (layer "B.SilkS"))
  (gr_text "Designed\nin\nOregon" (at 217.17 118.11) (layer "B.SilkS"))
  (gr_text "D7" (at 210.82 125.4125) (layer "B.SilkS"))
  (gr_text "FDC I/O Registers:\nMSR(r):    0x50   CCR(w)/DIR(r): 0x48\nData(r/w): 0x51   DOR(w)/TC(r):  0x58 " (at 156.21 115.57) (layer "B.SilkS"))
  (gr_text "Module's I/O Addresses:\nFloppy Disk Controller (FDC): 0x48 - 0x5F\nReal Time Clock (RTC):       0xC0 - 0xC7\n" (at 187.96 115.57) (layer "B.SilkS"))
  (gr_text "Licensed under CERN-OHL-S:\nhttps://cern-ohl.web.cern.ch" (at 216.8525 95.25) (layer "B.SilkS"))
  (gr_text "GND" (at 167.63541 121.285) (layer "B.SilkS"))
  (gr_text "!" (at 185.1025 103.1875) (layer "B.SilkS"))
  (gr_text "J2 is an unfused 5V power supply for a single 3.5{dblquote} floppy disk drive\nAvoid overloading and short-circuiting\n" (at 182.88 103.1875) (layer "B.SilkS"))
  (gr_text "Design files and documentation:\ngithub.com/skiselev/Flock" (at 216.8525 91.44) (layer "B.SilkS"))
  (gr_text "VCC" (at 170.170852 121.285) (layer "B.SilkS"))
  (gr_text "www.malinov.com" (at 217.17 124.46) (layer "F.SilkS"))
  (gr_text "Flock - FDC and RTC - Version 1.0\nCopyright (C) 2022 Sergey Kiselev" (at 128.905 123.698) (layer "F.SilkS"))
  (gr_text "1" (at 220.98 82.55) (layer "F.SilkS"))
  (gr_text "Designed\nin\nOregon" (at 217.404336 118.11) (layer "F.SilkS"))
  (gr_text "-" (at 161.29 88.265) (layer "F.SilkS"))
  (gr_text "1" (at 127 124.46) (layer "F.SilkS"))
  (gr_text "+" (at 163.83 88.265) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.25 128.75)
        (xy 125.25 128.75)
        (xy 125.25 93.75)
        (xy 140.25 78.75)
        (xy 224.25 78.75)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.25 128.75)
        (xy 125.25 128.75)
        (xy 125.25 93.75)
        (xy 140.25 78.75)
        (xy 224.25 78.75)
      )
    )
  )
)
