(kicad_pcb (version 20171130) (host pcbnew "(5.0.2-5)-5")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 109)
    (zones 0)
    (modules 23)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.33)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/"))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module badgelife_sao_v169bis:Badgelife-SAOv169-SAO-2x3 (layer F.Cu) (tedit 5D36323F)
    (at 58.33872 68.42252)
    (descr "Through hole straight IDC box header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x03 2.54mm double row")
    (fp_text reference "#SAO" (at 0 -5.842) (layer B.SilkS) hide)
    (fp_text value Badgelife-SAOv169-SAO-2x3 (at 0 -7.7) (layer F.Fab))
    (fp_text user GPIO2 (at 3.937 3.048) (layer F.SilkS))
    (fp_text user SCL (at 0 3.048) (layer F.SilkS))
    (fp_text user GND (at -2.54 3.048 unlocked) (layer F.SilkS))
    (fp_text user GPIO1 (at 3.937 -2.794 unlocked) (layer B.SilkS))
    (fp_text user SDA (at 0 -2.794 unlocked) (layer F.SilkS))
    (fp_text user VCC (at -2.54 -2.794 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0.06 0.02 270) (layer F.Fab))
    (fp_text user VCC (at -2.54 -2.794 unlocked) (layer B.SilkS))
    (fp_text user SDA (at 0 -2.794 unlocked) (layer B.SilkS))
    (fp_text user GPIO1 (at 3.937 -2.794 unlocked) (layer F.SilkS))
    (fp_text user GND (at -2.54 3.048 unlocked) (layer B.SilkS))
    (fp_text user SCL (at 0 3.048) (layer B.SilkS))
    (fp_text user GPIO2 (at 3.937 3.048) (layer B.SilkS))
    (pad 5 thru_hole circle (at 2.6 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 2.6 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0.06 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0.06 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -2.48 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -2.48 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl
      (offset (xyz -2.5 1.2 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module mrmeeseeks:Power_Rail-01x09 (layer F.Cu) (tedit 5AC7D21B)
    (at 31.02864 50.37074 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.Fab) hide)
    (fp_text value Conn_01x09 (at 0 17.57 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 9 thru_hole rect (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x09 (layer F.Cu) (tedit 5AC7D21B)
    (at 61.68644 50.22342 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.Fab) hide)
    (fp_text value Conn_01x09 (at 0 17.57 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 9 thru_hole rect (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x08 (layer F.Cu) (tedit 5AC7D1EA)
    (at 33.99536 53.05044 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.Fab) hide)
    (fp_text value Conn_01x08 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:badgelife-shitty-label-gnd (layer F.Cu) (tedit 0)
    (at 73.62952 23.79472)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:Power_Rail-01x08 (layer F.Cu) (tedit 5AC7D1EA)
    (at 64.66332 27.0891 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.Fab) hide)
    (fp_text value Conn_01x08 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:badgelife-shitty-label-gnd (layer F.Cu) (tedit 0)
    (at 42.45356 23.85568)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-label-3.3v (layer F.Cu) (tedit 0)
    (at 74.13752 55.54472)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 67.17538 50.04562 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5D36193E)
    (at 36.42868 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 51.67268 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 46.57268 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 41.50868 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Power_Rail-01x08 (layer F.Cu) (tedit 5AC7D1EA)
    (at 64.60236 53.0098 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.Fab) hide)
    (fp_text value Conn_01x08 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 8 thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x08 (layer F.Cu) (tedit 5AC7D1EA)
    (at 33.86836 27.15006 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.Fab) hide)
    (fp_text value Conn_01x08 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 8 thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x09 (layer F.Cu) (tedit 5AC7D21B)
    (at 85.1154 50.06848 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.Fab) hide)
    (fp_text value Conn_01x09 (at 0 17.57 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 9 thru_hole rect (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x09 (layer F.Cu) (tedit 5D3623F9)
    (at 54.49824 50.28438 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.Fab) hide)
    (fp_text value Conn_01x09 (at 0 17.57 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 9 thru_hole rect (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 72.25538 50.04562 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 77.31938 50.04562 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 82.41938 50.04562 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 180) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:badgelife-shitty-label-3.3v (layer F.Cu) (tedit 0)
    (at 42.70756 55.58028)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-label-sda (layer F.Cu) (tedit 0)
    (at 57.15 40.132 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-label-scl (layer F.Cu) (tedit 0)
    (at 28.42768 40.21328 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text "based on DC26 proto board by @ANDnXOR\nupdated by @helenleigh & @pdp7 for DC27" (at 57.912 57.658) (layer B.SilkS))
  (gr_text github.com/OSHPark/badgelife_dev_board (at 58.42 22.352) (layer B.SilkS))
  (gr_text v1.69bis (at 58.42 60.452) (layer F.SilkS))
  (gr_text "#badgelife" (at 58.42 21.844) (layer F.Mask))
  (gr_text "#badgelife" (at 58.42 21.844) (layer F.Cu))
  (gr_text GPIO1 (at 59.182 39.878 90) (layer F.SilkS))
  (gr_text GPIO2 (at 87.884 40.132 270) (layer F.SilkS))
  (gr_line (start 31.496 61.722) (end 39.116 61.722) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 22.606 53.086) (end 31.496 61.722) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 22.606 26.67) (end 22.606 53.086) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30.988 18.796) (end 22.606 26.67) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.598 18.796) (end 30.988 18.796) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.726 27.432) (end 85.598 18.796) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.726 53.34) (end 93.726 27.432) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 62.23) (end 93.726 53.34) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.216 62.23) (end 85.09 62.23) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.818 69.85) (end 77.216 62.23) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.818 75.184) (end 67.818 69.85) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.514 75.184) (end 67.818 75.184) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.514 70.104) (end 48.514 75.184) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 39.116 61.722) (end 48.514 70.104) (layer Edge.Cuts) (width 0.15))
)
