<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="10.5" y1="24" x2="10.5" y2="11" width="0" layer="20"/>
<wire x1="10.5" y1="11" x2="11.5" y2="10" width="0" layer="20" curve="90"/>
<wire x1="11.5" y1="10" x2="46" y2="10" width="0" layer="20"/>
<wire x1="46" y1="10" x2="47" y2="11" width="0" layer="20" curve="90"/>
<wire x1="47" y1="11" x2="47" y2="24" width="0" layer="20"/>
<wire x1="47" y1="24" x2="46" y2="25" width="0" layer="20" curve="90"/>
<wire x1="46" y1="25" x2="11.5" y2="25" width="0" layer="20"/>
<wire x1="11.5" y1="25" x2="10.5" y2="24" width="0" layer="20" curve="90"/>
<text>JAW 2023-01</text>
<text>www.A791RL.com</text>
<text>gm/sio</text>
<text>3v3</text>
<text>5v</text>
<text>RTS</text>
<text>Rx</text>
<text>Tx</text>
<text>V</text>
<text>CTS</text>
<text>Gnd</text>
<text>Gnd</text>
<text>CTS</text>
<text>V</text>
<text>Tx</text>
<text>Rx</text>
<text>RTS</text>
<text>nRST
3v3</text>
<text>A5
A6</text>
<text>B0
A7</text>
<text>Gnd
B1</text>
<text>B7
B6</text>
<text>B3
A15</text>
<text>B3
A15</text>
<text>B7
B6</text>
<text>Gnd
B1</text>
<text>B0
A7</text>
<text>A5
A6</text>
<text>nRST
3v3</text>
</plain>
<libraries>
<library name="jaw-ic">
<packages>
<package name="QFN32EP-5MM">
</package>
</packages>
</library>
<library name="jaw-conn">
<packages>
<package name="HEADER-3X2-PTH1.27">
</package>
<package name="HEADER-6X1-PTH">
</package>
<package name="HEADER-6X2-PTH">
</package>
<package name="USBC_GCT4110">
</package>
</packages>
</library>
<library name="jaw">
<packages>
<package name="SOT-23-3@1">
</package>
<package name="SMD0603">
</package>
<package name="SMD0603D">
</package>
<package name="ROBOTMAN-LOGO">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="jaw-ic" package="QFN32EP-5MM" value="STM32L432/32-QFN32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jaw" package="SMD0603" value="5k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="SMD0603" value="5k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="jaw" package="SOT-23-3@1" value="mcp1700 /3v3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="SMD0603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="SMD0603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="jaw" package="SMD0603D" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="jaw-conn" package="HEADER-6X1-PTH" value="HEADER-6X1-PTH">
<attribute name="NAME"/>
</element>
<element name="CN1" library="jaw-conn" package="HEADER-3X2-PTH1.27" value="DO NOT PLACE"/>
<element name="CONN1" library="jaw-conn" package="HEADER-6X2-PTH" value="HEADER-6X2-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="jaw" package="ROBOTMAN-LOGO" value="ROBOTMAN-LOGO"/>
<element name="U$1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="J2" library="jaw-conn" package="USBC_GCT4110" value="USB-C-GCT4110">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="VR1" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="16"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="J1" pad="P$1"/>
<contactref element="CN1" pad="2"/>
<contactref element="U1" pad="EP"/>
<contactref element="CONN1" pad="8"/>
<contactref element="J2" pad="P4"/>
<contactref element="J2" pad="P3"/>
<contactref element="J2" pad="P1"/>
<contactref element="J2" pad="P2"/>
<contactref element="J2" pad="A1B12"/>
<contactref element="J2" pad="B1A12"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="VR1" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="CONN1" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="BOOT0">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="31"/>
<contactref element="CN1" pad="5"/>
</signal>
<signal name="NRST">
<contactref element="C7" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="CN1" pad="6"/>
<contactref element="CONN1" pad="2"/>
</signal>
<signal name="USBDM">
<contactref element="U1" pad="21"/>
<contactref element="J2" pad="B7"/>
<contactref element="J2" pad="A7"/>
</signal>
<signal name="USBDP">
<contactref element="U1" pad="22"/>
<contactref element="J2" pad="A6"/>
<contactref element="J2" pad="B6"/>
</signal>
<signal name="VUSB">
<contactref element="C1" pad="1"/>
<contactref element="VR1" pad="3"/>
<contactref element="CN1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="J2" pad="B4A9"/>
<contactref element="J2" pad="A4B9"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="19"/>
<contactref element="CN1" pad="4"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="20"/>
<contactref element="CN1" pad="3"/>
</signal>
<signal name="TX2">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="RX2">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="CTS">
<contactref element="J1" pad="P$2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="RTS">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="P$6"/>
</signal>
<signal name="IOLED1">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="IOLED2">
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SPISCK">
<contactref element="CONN1" pad="4"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="SPIMISO">
<contactref element="CONN1" pad="3"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="SPIMOSI">
<contactref element="CONN1" pad="5"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="I2CCL">
<contactref element="CONN1" pad="9"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="I2CDA">
<contactref element="CONN1" pad="10"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="SPINSS">
<contactref element="CONN1" pad="6"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="DPYCS">
<contactref element="CONN1" pad="7"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="10"/>
</signal>
<signal name="IOB3">
<contactref element="U1" pad="26"/>
<contactref element="CONN1" pad="12"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="27"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="24"/>
</signal>
<signal name="IOA15">
<contactref element="U1" pad="25"/>
<contactref element="CONN1" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="2"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="A5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="B5"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
