(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/InA_0")
  (net 2 "GND")
  (net 3 "/InB_0")
  (net 4 "Vs")
  (net 5 "Net-(U2-FILTER)")
  (net 6 "/2.5V_0")
  (net 7 "/2.5V_1")
  (net 8 "Net-(U1-FILTER)")
  (net 9 "/InA_1")
  (net 10 "/InB_1")
  (net 11 "/2.5V_2")
  (net 12 "Net-(U5-FILTER)")
  (net 13 "/InA_2")
  (net 14 "/InB_2")
  (net 15 "/2.5V_3")
  (net 16 "Net-(U7-FILTER)")
  (net 17 "/InA_3")
  (net 18 "/InB_3")
  (net 19 "/2.5V_4")
  (net 20 "Net-(U9-FILTER)")
  (net 21 "/InA_4")
  (net 22 "/InB_4")
  (net 23 "/2.5V_5")
  (net 24 "Net-(U11-FILTER)")
  (net 25 "/InA_5")
  (net 26 "/InB_5")
  (net 27 "/2.5V_6")
  (net 28 "Net-(U13-FILTER)")
  (net 29 "/InA_6")
  (net 30 "/InB_6")
  (net 31 "/2.5V_7")
  (net 32 "Net-(U15-FILTER)")
  (net 33 "/InA_7")
  (net 34 "/InB_7")
  (net 35 "/gnd")
  (net 36 "/N{slash}C")
  (net 37 "/AIN70")
  (net 38 "/AIN68")
  (net 39 "/AIN66")
  (net 40 "/Vmux-")
  (net 41 "/AIN62")
  (net 42 "/AIN61")
  (net 43 "/AIN59")
  (net 44 "/AIN57")
  (net 45 "/AIN55")
  (net 46 "/AIN53")
  (net 47 "/AIN51")
  (net 48 "/AIN49")
  (net 49 "/AIN71")
  (net 50 "/AIN69")
  (net 51 "/AIN67")
  (net 52 "/AIN65")
  (net 53 "/Vmux+")
  (net 54 "/AIN63")
  (net 55 "/AGND")
  (net 56 "/AIN60")
  (net 57 "/AIN58")
  (net 58 "/AIN56")
  (net 59 "/AIN54")
  (net 60 "/AIN52")
  (net 61 "/AIN50")
  (net 62 "/AIN48")
  (net 63 "Net-(U3-OUTB)")
  (net 64 "Net-(U3-INB-)")
  (net 65 "Net-(U3-OUTA)")
  (net 66 "Net-(U3-INA-)")
  (net 67 "Net-(U3-INB+)")
  (net 68 "Net-(U3-INA+)")
  (net 69 "Net-(U2-EN)")
  (net 70 "Net-(U1-EN)")
  (net 71 "Net-(U4-OUTA)")
  (net 72 "Net-(U4-INA-)")
  (net 73 "Net-(U4-INA+)")
  (net 74 "Net-(U4-INB+)")
  (net 75 "Net-(U4-INB-)")
  (net 76 "Net-(U4-OUTB)")
  (net 77 "Net-(U5-EN)")
  (net 78 "Net-(U6-OUTA)")
  (net 79 "Net-(U6-INA-)")
  (net 80 "Net-(U6-INA+)")
  (net 81 "Net-(U6-INB+)")
  (net 82 "Net-(U6-INB-)")
  (net 83 "Net-(U6-OUTB)")
  (net 84 "Net-(U7-EN)")
  (net 85 "Net-(U8-OUTA)")
  (net 86 "Net-(U8-INA-)")
  (net 87 "Net-(U8-INA+)")
  (net 88 "Net-(U8-INB+)")
  (net 89 "Net-(U8-INB-)")
  (net 90 "Net-(U8-OUTB)")
  (net 91 "Net-(U9-EN)")
  (net 92 "Net-(U10-OUTA)")
  (net 93 "Net-(U10-INA-)")
  (net 94 "Net-(U10-INA+)")
  (net 95 "Net-(U10-INB+)")
  (net 96 "Net-(U10-INB-)")
  (net 97 "Net-(U10-OUTB)")
  (net 98 "Net-(U11-EN)")
  (net 99 "Net-(U12-OUTA)")
  (net 100 "Net-(U12-INA-)")
  (net 101 "Net-(U12-INA+)")
  (net 102 "Net-(U12-INB+)")
  (net 103 "Net-(U12-INB-)")
  (net 104 "Net-(U12-OUTB)")
  (net 105 "Net-(U13-EN)")
  (net 106 "Net-(U14-OUTA)")
  (net 107 "Net-(U14-INA-)")
  (net 108 "Net-(U14-INA+)")
  (net 109 "Net-(U14-INB+)")
  (net 110 "Net-(U14-INB-)")
  (net 111 "Net-(U14-OUTB)")
  (net 112 "Net-(U15-EN)")
  (net 113 "Net-(U16-OUTA)")
  (net 114 "Net-(U16-INA-)")
  (net 115 "Net-(U16-INA+)")
  (net 116 "Net-(U16-INB+)")
  (net 117 "Net-(U16-INB-)")
  (net 118 "Net-(U16-OUTB)")
  (net 119 "/AIN64")
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 122.57945 105.0347 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "/InB_2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 169.34085 109.4524)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 21 "/InA_4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 130.91065 109.1495)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 13 "/InA_2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 111.5728 145.6436 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R81" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 55 "/AGND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 131.26625 105.6189)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "/InA_2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 170.28065 71.3632)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R53" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 25 "/InA_5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 165.48005 126.064 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C30" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 106.023648 113.669399)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 123.279349 92.3182 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C52" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 159.63805 82.6154 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R59" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "Net-(U12-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(U12-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 165.40385 120.4252 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U10" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(U10-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(U10-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(U10-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Net-(U10-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(U10-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "Net-(U10-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 197.1548 109.3216 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C41" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 30 "/InB_6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 123.97645 113.7723 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/InB_2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(U6-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 204.7349 79.660824 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R76" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/InA_7") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(U16-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 201.0918 120.2436 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U14" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(U14-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(U14-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "Net-(U14-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "Net-(U14-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "Net-(U14-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "Net-(U14-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 118.426049 86.6032 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R40" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U8-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/AIN59") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 125.920949 91.734 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 101.121448 104.195199)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 6 "/2.5V_0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 88.533249 120.133699 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U3" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(U3-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(U3-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(U3-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(U3-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(U3-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(U3-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 92.470249 109.160899)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "/InA_0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 84.951701 75.4507 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 10 "/InB_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 165.98805 85.8666 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U12" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "Net-(U12-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "Net-(U12-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "Net-(U12-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "Net-(U12-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "Net-(U12-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "Net-(U12-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 127.04985 125.7611 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 162.99085 79.5166 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R58" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/InB_5") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(U12-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 85.536049 113.783699 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/InB_0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(U3-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 198.5264 126.4666 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C55" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 135.054748 80.9009 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 16 "Net-(U7-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 178.576249 69.9281)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R51" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 23 "/2.5V_5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 214.351299 73.145724)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C43" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 31 "/2.5V_7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 138.432948 70.1567)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 15 "/2.5V_3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 119.494749 82.844 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R39" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(U8-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U8-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 199.2231 92.335424 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C56" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 144.464049 113.658)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 82.183249 116.882499 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(U3-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(U3-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 213.679999 104.3051)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R61" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 27 "/2.5V_6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 161.46685 109.5032 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C29" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 22 "/InB_4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 97.743248 114.939399 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 5 "Net-(U2-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 159.05385 117.174 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R49" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U10-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(U10-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 144.667249 111.0418)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 77 "Net-(U5-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 183.097449 111.3447)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R42" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 91 "Net-(U9-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 84.139049 105.046099 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "/InB_0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 91.835101 79.9211 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/InA_1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(U4-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 140.10545 112.19115 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U5" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "*" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U5-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(U5-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/2.5V_2") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/2.5V_2") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 94.781649 125.774399 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(U3-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/AIN62") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 183.681649 76.7861)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R52" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 98 "Net-(U11-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.137349 71.5918)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "/InA_3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 122.847549 79.7452 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/InB_3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(U8-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 194.7418 116.9924 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R69" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "Net-(U14-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(U14-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 92.825849 105.630299)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "/InA_0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.093149 87.3633 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(U8-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(U8-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 106.226848 111.053199)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 69 "Net-(U2-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 204.0382 113.792 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R66" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/InA_6") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(U14-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 126.97365 120.1223 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U6" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "Net-(U6-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(U6-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(U6-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(U6-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(U6-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(U6-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 169.92505 74.8938)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C34" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 25 "/InA_5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 88.964901 92.0115 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 133.22205 125.763 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(U6-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/AIN56") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm_Pad" (layer "F.Cu")
    (at 81 146)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 201.7885 86.112424 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U16" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "Net-(U16-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(U16-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "Net-(U16-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "Net-(U16-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "Net-(U16-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(U16-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 139.561849 104.1838)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 11 "/2.5V_2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 85.891501 80.0227 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/InB_1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(U4-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 214.2236 112.31245 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U13" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(U13-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "Net-(U13-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/2.5V_6") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/2.5V_6") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 201.8647 91.751224 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C48" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 175.198049 80.6723 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C33" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 24 "Net-(U11-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 210.998499 80.918124 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C45" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 32 "Net-(U15-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 157.98515 120.9332 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R50" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(U10-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/AIN53") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 177.966649 107.4585)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 19 "/2.5V_4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 143.335148 79.6309)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 84.494501 71.2851 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "/InB_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 143.538348 77.0147)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 84 "Net-(U7-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 121.907749 75.1732 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 18 "/InB_3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 163.42265 92.0896 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C54" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 190.7794 138.1252)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R82" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 119 "/AIN64") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 125.844749 86.0952 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U8" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(U8-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(U8-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(U8-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(U8-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(U8-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(U8-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 197.8515 75.190424 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C47" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 34 "/InB_7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 207.3402 121.5117 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R65" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(U14-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "Net-(U14-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 106.5823 77.2922)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 70 "Net-(U1-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 213.654599 107.2769)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C37" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 27 "/2.5V_6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.093149 91.7359 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(U8-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/AIN58") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 136.183649 114.928 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 12 "Net-(U5-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 214.376699 70.173924)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R71" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 31 "/2.5V_7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 139.536449 107.1556)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 11 "/2.5V_2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 121.450549 71.0076 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R37" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 18 "/InB_3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 95.137101 92.0134 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(U4-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/AIN60") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 178.550849 72.8999)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C31" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 23 "/2.5V_5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 206.0811 71.609024)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R73" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 33 "/InA_7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.470001 86.8807 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U4-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/AIN61") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 124.40825 126.3453 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C51" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 194.3698 86.620424 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R80" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(U16-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/AIN51") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 128.791149 79.6436 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/InA_3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U8-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 172.23645 91.5073 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R54" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(U12-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/AIN54") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 101.096048 107.166999)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 6 "/2.5V_0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 195.4385 82.861224 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R79" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(U16-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(U16-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 168.93445 79.415 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R56" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/InA_5") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "Net-(U12-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 177.992049 104.4867)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R41" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 19 "/2.5V_4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 161.59385 70.779 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R57" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 26 "/InB_5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 162.05105 74.9446 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C35" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 26 "/InB_5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 166.06425 91.5054 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C36" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm_Pad" (layer "F.Cu")
    (at 221 51)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 207.3402 125.8843 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R64" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "Net-(U14-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/AIN48") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 109.204 138.1506 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R83" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 119 "/AIN64") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 179.11985 77.93545 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U11" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "*" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U11-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "Net-(U11-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/2.5V_5") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/2.5V_5") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 219.278899 79.648124)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C44" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 161.00965 105.3376 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R47" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 22 "/InB_4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 129.781749 75.1224)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 17 "/InA_3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 138.976549 78.16405 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U7" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(U7-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(U7-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/2.5V_3") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/2.5V_3") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 82.538701 83.1215 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(U4-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U4-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 94.781649 121.401799 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(U3-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(U3-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 92.825701 75.3999)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 9 "/InA_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:D8" (layer "F.Cu")
    (at 88.888701 86.3727 180)
    (tags "OPA2335AIDR ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_keywords" "OPA2335AIDR")
    (attr smd)
    (fp_text reference "U4" (at 0.08 -3.51 180 unlocked) (layer "F.SilkS"))
    (fp_text value "OPA2335AIDR" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.7178 -3.6068) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -2.7178 -3.6068) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.03 4.02 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(U4-OUTA)") (pinfunction "OUTA") (pintype "output"))
    (pad "2" smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(U4-INA-)") (pinfunction "INA-") (pintype "input"))
    (pad "3" smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(U4-INA+)") (pinfunction "INA+") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(U4-INB+)") (pinfunction "INB+") (pintype "input"))
    (pad "6" smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(U4-INB-)") (pinfunction "INB-") (pintype "input"))
    (pad "7" smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(U4-OUTB)") (pinfunction "OUTB") (pintype "output"))
    (pad "8" smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "V+") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 86.323301 92.5957 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C50" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 201.168 125.8824 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C42" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 182.894249 113.9609)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 162.40665 114.0752 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R48" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/InB_4") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(U10-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 93.181301 71.8693)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "/InA_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.114549 120.641699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(U3-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/AIN63") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 214.9203 78.181274 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U15" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "*" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(U15-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "Net-(U15-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/2.5V_7") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/2.5V_7") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 120.62365 116.8711 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(U6-INB-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U6-OUTB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 85.967849 126.356699 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C49" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 205.7255 75.139624)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C46" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 33 "/InA_7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 196.6976 105.156 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R67" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "/InB_6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 205.0288 109.2708)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C40" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 29 "/InA_6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 88.609449 125.772499 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 101.665049 112.202549 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U2" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "*" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(U2-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(U2-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/2.5V_0") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/2.5V_0") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 183.478449 79.4023)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C32" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 158.56935 86.3746 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R60" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(U12-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/AIN55") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 129.92005 113.6707 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/InA_2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(U6-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 101.4515 73.406)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 7 "/2.5V_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 208.0369 87.380524 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R75" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(U16-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(U16-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 218.785399 111.1631)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R62" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 105 "Net-(U13-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 84.596249 109.211699 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "/InB_0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 119.55495 120.6303 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U6-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/AIN57") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 218.582199 113.7793)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C38" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 198.7913 79.762424 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R78" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/InB_7") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(U16-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 171.65225 121.6933 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R45" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(U10-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(U10-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 95.137101 87.6408 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(U4-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(U4-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 123.03665 109.2003 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 14 "/InB_2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm_Pad" (layer "F.Cu")
    (at 81 51)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 171.65225 126.0659 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R44" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(U10-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/AIN52") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 174.613849 115.2309 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 20 "Net-(U9-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:CON40_2X20_DUK_FTSH_SAI" (layer "F.Cu")
    (at 152.4762 56.6928 180)
    (tags "FTSH-120-01-L-DV-K ")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "FTSH-120-01-L-DV-K")
    (attr smd)
    (fp_text reference "J1" (at 0.17 0.02 180 unlocked) (layer "F.SilkS"))
    (fp_text value "FTSH-120-01-L-DV-K" (at -0.04 -5.06 180 unlocked) (layer "F.Fab"))
    (fp_text user "39" (at -13.6906 2.0574 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at 13.208 2.032 180 unlocked) (layer "F.SilkS"))
    (fp_text user "40" (at -13.8176 -2.0828 180 unlocked) (layer "F.SilkS"))
    (fp_text user "2" (at 13.208 -2.032 180 unlocked) (layer "F.SilkS"))
    (fp_text user "40" (at -13.8176 -2.1082 180 unlocked) (layer "F.Fab"))
    (fp_text user "39" (at -13.6906 2.0574 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.01 7.77 180 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at 13.208 2.032 180 unlocked) (layer "F.Fab"))
    (fp_text user "2" (at 13.208 -2.032 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 12.065 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/2.5V_0") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 12.065 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/InB_0") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 10.795 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/2.5V_0") (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at 10.795 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/InA_0") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at 9.525 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/2.5V_1") (pinfunction "5") (pintype "unspecified"))
    (pad "6" smd rect (at 9.525 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/InB_1") (pinfunction "6") (pintype "unspecified"))
    (pad "7" smd rect (at 8.255 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/2.5V_1") (pinfunction "7") (pintype "unspecified"))
    (pad "8" smd rect (at 8.255 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/InA_1") (pinfunction "8") (pintype "unspecified"))
    (pad "9" smd rect (at 6.985 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/2.5V_3") (pinfunction "9") (pintype "unspecified"))
    (pad "10" smd rect (at 6.985 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/InB_3") (pinfunction "10") (pintype "unspecified"))
    (pad "11" smd rect (at 5.715 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/2.5V_3") (pinfunction "11") (pintype "unspecified"))
    (pad "12" smd rect (at 5.715 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/InA_3") (pinfunction "12") (pintype "unspecified"))
    (pad "13" smd rect (at 4.445 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/2.5V_2") (pinfunction "13") (pintype "unspecified"))
    (pad "14" smd rect (at 4.445 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/InB_2") (pinfunction "14") (pintype "unspecified"))
    (pad "15" smd rect (at 3.175 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/2.5V_2") (pinfunction "15") (pintype "unspecified"))
    (pad "16" smd rect (at 3.175 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/InA_2") (pinfunction "16") (pintype "unspecified"))
    (pad "17" smd rect (at 1.905 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/2.5V_4") (pinfunction "17") (pintype "unspecified"))
    (pad "18" smd rect (at 1.905 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/InB_5") (pinfunction "18") (pintype "unspecified"))
    (pad "19" smd rect (at 0.635 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/2.5V_4") (pinfunction "19") (pintype "unspecified"))
    (pad "20" smd rect (at 0.635 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/InA_5") (pinfunction "20") (pintype "unspecified"))
    (pad "21" smd rect (at -0.635 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/2.5V_5") (pinfunction "21") (pintype "unspecified"))
    (pad "22" smd rect (at -0.635 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/InB_4") (pinfunction "22") (pintype "unspecified"))
    (pad "23" smd rect (at -1.905 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/2.5V_5") (pinfunction "23") (pintype "unspecified"))
    (pad "24" smd rect (at -1.905 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/InA_4") (pinfunction "24") (pintype "unspecified"))
    (pad "25" smd rect (at -3.175 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/2.5V_6") (pinfunction "25") (pintype "unspecified"))
    (pad "26" smd rect (at -3.175 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/InB_7") (pinfunction "26") (pintype "unspecified"))
    (pad "27" smd rect (at -4.445 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/2.5V_6") (pinfunction "27") (pintype "unspecified"))
    (pad "28" smd rect (at -4.445 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/InA_7") (pinfunction "28") (pintype "unspecified"))
    (pad "29" smd rect (at -5.715 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/2.5V_7") (pinfunction "29") (pintype "unspecified"))
    (pad "30" smd rect (at -5.715 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/InB_6") (pinfunction "30") (pintype "unspecified"))
    (pad "31" smd rect (at -6.985 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/2.5V_7") (pinfunction "31") (pintype "unspecified"))
    (pad "32" smd rect (at -6.985 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/InA_6") (pinfunction "32") (pintype "unspecified"))
    (pad "33" smd rect (at -8.255 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "33") (pintype "unspecified"))
    (pad "34" smd rect (at -8.255 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "34") (pintype "unspecified"))
    (pad "35" smd rect (at -9.525 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "35") (pintype "unspecified"))
    (pad "36" smd rect (at -9.525 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "36") (pintype "unspecified"))
    (pad "37" smd rect (at -10.795 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "37") (pintype "unspecified"))
    (pad "38" smd rect (at -10.795 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "38") (pintype "unspecified"))
    (pad "39" smd rect (at -12.065 2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "39") (pintype "unspecified"))
    (pad "40" smd rect (at -12.065 -2.032 180) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "40") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 98.0987 81.1784 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 8 "Net-(U1-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 210.301799 115.0493 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C39" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 28 "Net-(U13-FILTER)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 178.53565 112.49405 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U9" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U9-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(U9-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/2.5V_4") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/2.5V_4") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 91.479649 113.682099 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/InA_0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(U3-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 197.3943 71.024824 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R77" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 34 "/InB_7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 193.6731 120.7516 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R70" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(U14-OUTB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/AIN49") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 219.482099 77.031924)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R72" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 112 "Net-(U15-EN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:AMPHENOL_L717TSCH37POL2RM8" (layer "F.Cu")
    (at 151.4222 141.5264)
    (property "MANUFACTURER" "Amphenol FCi")
    (property "MAXIMUM_PACKAGE_HEIGHT" "12mm")
    (property "PARTREV" "3")
    (property "SNAPEDA_PN" "L717TSCH37POL2RM8")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -31.775 -8.16) (layer "F.SilkS"))
    (fp_text value "L717TSCH37POL2RM8" (at -18.44 8.16) (layer "F.Fab"))
    (pad "01" thru_hole rect (at -24.93 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "01") (pintype "passive") (solder_mask_margin 0.102))
    (pad "02" thru_hole circle (at -22.16 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 36 "/N{slash}C") (pinfunction "02") (pintype "passive") (solder_mask_margin 0.102))
    (pad "03" thru_hole circle (at -19.39 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 37 "/AIN70") (pinfunction "03") (pintype "passive") (solder_mask_margin 0.102))
    (pad "04" thru_hole circle (at -16.62 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 38 "/AIN68") (pinfunction "04") (pintype "passive") (solder_mask_margin 0.102))
    (pad "05" thru_hole circle (at -13.85 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 39 "/AIN66") (pinfunction "05") (pintype "passive") (solder_mask_margin 0.102))
    (pad "06" thru_hole circle (at -11.08 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "06") (pintype "passive") (solder_mask_margin 0.102))
    (pad "07" thru_hole circle (at -8.31 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 36 "/N{slash}C") (pinfunction "07") (pintype "passive") (solder_mask_margin 0.102))
    (pad "08" thru_hole circle (at -5.54 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "08") (pintype "passive") (solder_mask_margin 0.102))
    (pad "09" thru_hole circle (at -2.77 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 40 "/Vmux-") (pinfunction "09") (pintype "passive") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 0 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "10") (pintype "passive") (solder_mask_margin 0.102))
    (pad "11" thru_hole circle (at 2.77 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 41 "/AIN62") (pinfunction "11") (pintype "passive") (solder_mask_margin 0.102))
    (pad "12" thru_hole circle (at 5.54 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 42 "/AIN61") (pinfunction "12") (pintype "passive") (solder_mask_margin 0.102))
    (pad "13" thru_hole circle (at 8.31 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 43 "/AIN59") (pinfunction "13") (pintype "passive") (solder_mask_margin 0.102))
    (pad "14" thru_hole circle (at 11.08 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 44 "/AIN57") (pinfunction "14") (pintype "passive") (solder_mask_margin 0.102))
    (pad "15" thru_hole circle (at 13.85 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 45 "/AIN55") (pinfunction "15") (pintype "passive") (solder_mask_margin 0.102))
    (pad "16" thru_hole circle (at 16.62 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 46 "/AIN53") (pinfunction "16") (pintype "passive") (solder_mask_margin 0.102))
    (pad "17" thru_hole circle (at 19.39 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 47 "/AIN51") (pinfunction "17") (pintype "passive") (solder_mask_margin 0.102))
    (pad "18" thru_hole circle (at 22.16 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 48 "/AIN49") (pinfunction "18") (pintype "passive") (solder_mask_margin 0.102))
    (pad "19" thru_hole circle (at 24.93 -1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "19") (pintype "passive") (solder_mask_margin 0.102))
    (pad "20" thru_hole circle (at -23.545 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 36 "/N{slash}C") (pinfunction "20") (pintype "passive") (solder_mask_margin 0.102))
    (pad "21" thru_hole circle (at -20.775 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 49 "/AIN71") (pinfunction "21") (pintype "passive") (solder_mask_margin 0.102))
    (pad "22" thru_hole circle (at -18.005 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 50 "/AIN69") (pinfunction "22") (pintype "passive") (solder_mask_margin 0.102))
    (pad "23" thru_hole circle (at -15.235 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 51 "/AIN67") (pinfunction "23") (pintype "passive") (solder_mask_margin 0.102))
    (pad "24" thru_hole circle (at -12.465 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 52 "/AIN65") (pinfunction "24") (pintype "passive") (solder_mask_margin 0.102))
    (pad "25" thru_hole circle (at -9.695 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 36 "/N{slash}C") (pinfunction "25") (pintype "passive") (solder_mask_margin 0.102))
    (pad "26" thru_hole circle (at -6.925 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 36 "/N{slash}C") (pinfunction "26") (pintype "passive") (solder_mask_margin 0.102))
    (pad "27" thru_hole circle (at -4.155 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 4 "Vs") (pinfunction "27") (pintype "passive") (solder_mask_margin 0.102))
    (pad "28" thru_hole circle (at -1.385 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 53 "/Vmux+") (pinfunction "28") (pintype "passive") (solder_mask_margin 0.102))
    (pad "29" thru_hole circle (at 1.385 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 54 "/AIN63") (pinfunction "29") (pintype "passive") (solder_mask_margin 0.102))
    (pad "30" thru_hole circle (at 4.155 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 55 "/AGND") (pinfunction "30") (pintype "passive") (solder_mask_margin 0.102))
    (pad "31" thru_hole circle (at 6.925 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 56 "/AIN60") (pinfunction "31") (pintype "passive") (solder_mask_margin 0.102))
    (pad "32" thru_hole circle (at 9.695 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 57 "/AIN58") (pinfunction "32") (pintype "passive") (solder_mask_margin 0.102))
    (pad "33" thru_hole circle (at 12.465 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 58 "/AIN56") (pinfunction "33") (pintype "passive") (solder_mask_margin 0.102))
    (pad "34" thru_hole circle (at 15.235 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 59 "/AIN54") (pinfunction "34") (pintype "passive") (solder_mask_margin 0.102))
    (pad "35" thru_hole circle (at 18.005 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 60 "/AIN52") (pinfunction "35") (pintype "passive") (solder_mask_margin 0.102))
    (pad "36" thru_hole circle (at 20.775 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 61 "/AIN50") (pinfunction "36") (pintype "passive") (solder_mask_margin 0.102))
    (pad "37" thru_hole circle (at 23.545 1.42) (size 1.575 1.575) (drill 1.05) (layers "*.Cu" "*.Mask")
      (net 62 "/AIN48") (pinfunction "37") (pintype "passive") (solder_mask_margin 0.102))
    (pad "S1" thru_hole circle (at -31.75 0) (size 4.246 4.246) (drill 3.23) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
    (pad "S2" thru_hole circle (at 31.75 0) (size 4.246 4.246) (drill 3.23) (layers "*.Cu" "*.Mask")
      (net 35 "/gnd") (pinfunction "SHIELD__1") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 101.4769 70.4342)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 7 "/2.5V_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 162.83845 126.6482 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C53" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 133.22205 121.3904 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(U6-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(U6-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 198.0946 113.8936 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R68" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/InB_6") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "Net-(U14-INB+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 169.69645 105.9218)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 21 "/InA_4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 172.23645 87.1347 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R55" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(U12-INA-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(U12-OUTA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 138.407548 73.1285)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 15 "/2.5V_3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DownloadedParts:MAX6070" (layer "F.Cu")
    (at 102.020501 78.44155 90)
    (tags "MAX6070AAUT25+T ")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_keywords" "MAX6070AAUT25+T")
    (attr smd)
    (fp_text reference "U1" (at 0.03 -2.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MAX6070AAUT25+T" (at -0.01 5.14 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.61925 -2.6518 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.61925 -2.6518 90) (layer "F.SilkS"))
    (fp_text user "*" (at -0.01 3.04 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.4953 -1.4224 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4224 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(U1-FILTER)") (pinfunction "FILTER") (pintype "input"))
    (pad "2" smd rect (at -1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(U1-EN)") (pinfunction "EN") (pintype "unspecified"))
    (pad "4" smd rect (at 1.36525 0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vs") (pinfunction "IN") (pintype "input"))
    (pad "5" smd rect (at 1.36525 0 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/2.5V_1") (pinfunction "OUTS") (pintype "output"))
    (pad "6" smd rect (at 1.36525 -0.950001 90) (size 0.9779 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/2.5V_1") (pinfunction "OUTF") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 205.3844 105.7402)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R63" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "/InA_6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 106.3791 79.9084)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -0.0215) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Vs") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 208.0369 91.753124 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R74" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(U16-OUTA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/AIN50") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm_Pad" (layer "F.Cu")
    (at 221 146)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (property "Sheetfile" "Tile resistance jig readout 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 168.35025 113.9736 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Resistance measurement.kicad_sch")
    (property "Sheetname" "Resistance measurement4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R46" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/InA_4") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(U10-INA+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 76.6318 46.2026) (end 225.6028 150.4188)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Ch3" (at 144.945549 66.7023) (layer "F.SilkS"))
  (gr_text "SLAC 1k resistance measurement board v1" (at 93.2688 52.0954) (layer "F.SilkS"))
  (gr_text "Ch1" (at 107.176701 66.9544) (layer "F.SilkS"))
  (gr_text "Ch4" (at 184.19595 100.8799) (layer "F.SilkS"))
  (gr_text "Ch7" (at 219.7463 66.632524) (layer "F.SilkS"))
  (gr_text "Ch5" (at 184.19985 66.6388) (layer "F.SilkS"))
  (gr_text "Ch6" (at 220.2942 101.0666) (layer "F.SilkS"))
  (gr_text "Ch0" (at 107.151449 100.893199) (layer "F.SilkS"))
  (gr_text "Ch2" (at 144.90605 100.8799) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 225.5012 46.0756)
        (xy 225.5012 150.2664)
        (xy 76.6318 150.4188)
        (xy 76.6318 46.2026)
      )
    )
  )
)
