<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.635" x2="13.9575" y2="0.635" width="0" layer="20"/>
<wire x1="13.9575" y1="0.635" x2="13.9575" y2="28.565" width="0" layer="20"/>
<wire x1="13.9575" y1="28.565" x2="0" y2="28.565" width="0" layer="20"/>
<wire x1="0" y1="28.565" x2="0" y2="0.635" width="0" layer="20"/>
<text>HVR-A1E XLR module battery mod</text>
<text>rev1 / 2016 / tibounise.com</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-10_PAD">
</package>
</packages>
</library>
<library name="rc-master-smd">
<description>&lt;b&gt;R/C MASTER-SMD! - v1.01 (07/03/2007)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD ONLY resistors and capacitors by various manufacturers. The pad sizes, spacing and silkscreen widths have been tweaked for use in dense fine pitch layouts where space, alignment and precision are critical. In general these components are designed for routing in grid increments of 5 mils&lt;/p&gt;
&lt;p&gt;* Silkscreen line elements are a minimum of 8 mils in width. All components have text sizes of 0.032"  or 0.04".&lt;/p&gt;
&lt;p&gt;* A silkscreen text values use a ratio of 18 in all cases.&lt;/p&gt;
&lt;p&gt;* ALL PADS AND PART OUTLINES ARE SNAPPED TO A 5 MIL GRID!&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All components are prefixed using the following conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;
&lt;/author&gt;

&lt;p&gt;2009-02-03 changed by Ivan A-R &lt;ivan@tuxotronic.org&gt;&lt;/p&gt;</description>
<packages>
<package name="CD32">
<description>SMD Power Inductors CD32 Series (3.5*3.5mm)</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="TP4056">
<packages>
<package name="SOP-8">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X04-1.27MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-PowerIC" package="QFN-10_PAD" value="TPS61200">
<attribute name="PROD_ID" value="IC-10035"/>
</element>
<element name="L1" library="rc-master-smd" package="CD32" value="4.7uH">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="100n">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="100n">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="220K">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="2M2"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="2M7">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="220K">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10u">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="10u">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="10u">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="100n">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="NAME"/>
</element>
<element name="IC1" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="10u">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="1.2K">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="1206" value="400m">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="BAT">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="PWROUT">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04-1.27MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X04-1.27MM" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="13"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="15"/>
<contactref element="R2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="10"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="V_BATT">
<contactref element="IC1" pad="5"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="VIN">
<contactref element="IC1" pad="8"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="L1" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="4"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="CHRG">
<contactref element="IC1" pad="7"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="STDBY">
<contactref element="IC1" pad="6"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="VBCK">
<contactref element="C4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="JP5" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
